{"text_format":"3","workbook":"xls","n_sheets":9,"sheets":["1.焦炉-管道","2.焦炉-钢构","3.化产-管道","4.化产-钢构","5.干熄焦-管道","6.干熄焦-钢构","7.工程预算表","数据源","Sheet10"],"not_rendered":{"external_links":6,"defined_names":31,"comments":11},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"1.焦炉-管道","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"hidden":true,"merged":[[0,0,0,7]],"flags":["formulas_cached_only"]}
["2023年广西钢铁焦化厂钢结构及管道除锈防腐检修工程-焦炉管道"]
["车间","区域","施工环境描述","材料名称","直径mm","材料长度\nm","面积/㎡","备注","区域腐蚀程度","推荐使用涂料"]
["焦炉车间","1#-4#炉机侧管廊架到进地下室","施工作业面从室外地坪至管廊架顶部，高度约14m左右，作业环境存在一氧化碳中毒、高温烫伤、、高空坠落等危险源。","焦炉煤气管道",800,280,{"v":703.3600000000001,"d":"703.36"},null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","机侧管廊架","施工作业面从室外地坪至管廊架顶部，高度约14m左右，作业环境存在一氧化碳中毒、高温烫伤、、高空坠落等危险源。","焦炉煤气管道",2000,300,{"v":1884,"d":"1884.00"},null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","机侧管廊架3#炉到4#炉","施工作业面从室外地坪至管廊架顶部，高度约14m左右，作业环境存在一氧化碳中毒、高温烫伤、、高空坠落等危险源。","焦炉煤气管道",900,470,1328.22,null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","1#-4#炉机侧管廊架到进地下室","施工作业面从室外地坪至管廊架顶部，高度约14.5m左右，作业环境存在一氧化碳中毒、高温烫伤、、高空坠落等危险源。","高炉煤气管道",1200,280,1055.04,null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","机侧管廊架","施工作业面从室外地坪至管廊架顶部，高度约14.5m左右，作业环境存在一氧化碳中毒、高温烫伤、、高空坠落等危险源。","高炉煤气管道",2000,500,{"v":3140,"d":"3140.00"},null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","1#-4#炉地下室到炉顶","施工作业面从地下室至管廊架顶部，高度约6m左右，作业环境存在一氧化碳中毒、高空坠落等危险源。","高炉煤气放散管",400,140,{"v":175.84000000000003,"d":"175.84"},null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","1#-4#炉地下室到炉顶","施工作业面从地下室至管廊架顶部，高度约6m左右，作业环境存在一氧化碳中毒、高空坠落等危险源。","焦炉煤气放散管",200,70,{"v":43.96000000000001,"d":"43.96"},null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","1#2#装煤除烟囱","施工作业面从地面至烟囱顶部，高度约30m左右，作业环境存在一氧化碳中毒、高空坠落等危险源。","1#2#装煤除烟囱",1800,30,169.56,null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","1#2#装煤除尘","施工作业面从地面至管架，高度约17.6m左右，作业环境存在一氧化碳中毒、高空坠落等危险源。","1#2#装煤除进气管",1600,23.87,{"v":119.92288000000002,"d":"119.92"},null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","3#4#装煤除烟囱","施工作业面从地面至烟囱顶部，高度约30m左右，作业环境存在一氧化碳中毒、高空坠落等危险源。","3#4#装煤除烟囱",1800,30,169.56,null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","3#4#装煤除尘","施工作业面从地面至管架，高度约17.6m左右，作业环境存在一氧化碳中毒、高空坠落等危险源。","3#4#装煤除进气管",1600,23.87,{"v":119.92288000000002,"d":"119.92"},null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","1#2#出焦除尘烟囱","施工作业面从地面至烟囱顶部，高度约30m左右，作业环境存在一氧化碳中毒、高空坠落等危险源。","1#2#出焦除尘烟囱",3200,30,{"v":301.44000000000005,"d":"301.44"},null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","1#2#出焦除尘","施工作业面从地面至管架，高度约17.6m左右，作业环境存在一氧化碳中毒、高空坠落等危险源。","1#2#出焦除尘进气管",1600,37.62,{"v":189.00288000000003,"d":"189.00"},null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","3#4#出焦除尘烟囱","施工作业面从地面至烟囱顶部，高度约30m左右，作业环境存在一氧化碳中毒、高空坠落等危险源。","3#4#出焦除尘烟囱",3200,30,{"v":301.44000000000005,"d":"301.44"},null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","3#4#出焦除尘","施工作业面从地面至管架，高度约17.6m左右，作业环境存在一氧化碳中毒、高空坠落等危险源。","3#4#出焦除尘进气管",1600,37.62,{"v":189.00288000000003,"d":"189.00"},null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","1#2#炉机侧除尘烟囱","施工作业面从地面至烟囱顶部，高度约30m左右，作业环境存在一氧化碳中毒、高空坠落等危险源。","1#2#炉机侧除尘烟囱",2000,30,{"v":188.4,"d":"188.40"},null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","1#2#炉机侧除尘进气管","施工作业面从地面至管架，高度约17.6m左右，作业环境存在一氧化碳中毒、高空坠落等危险源。","1#2#炉机侧除尘进气管",1600,30.78,{"v":154.63872000000003,"d":"154.64"},null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","3#4#炉机侧除尘烟囱","施工作业面从地面至烟囱顶部，高度约30m左右，作业环境存在一氧化碳中毒、高空坠落等危险源。","3#4#炉机侧除尘烟囱",2000,30,{"v":188.4,"d":"188.40"},null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","3#4#炉机侧除尘进气管","施工作业面从地面至管架，高度约17.6m左右，作业环境存在一氧化碳中毒、高空坠落等危险源。","3#4#炉机侧除尘进气管",1600,30.78,{"v":154.63872000000003,"d":"154.64"},null,"一般性腐蚀","环氧富锌漆"]
["焦炉车间","1#2#炉机侧管廊架","施工作业面从室外地坪至管廊架顶部，高度约14.5m左右，作业环境存在一氧化碳中毒、高温烫伤、、高空坠落等危险源。","荒煤气管道",2000,130,{"v":816.4,"d":"816.40"},null,"一般性腐蚀","环氧富锌漆"]
["汇总",{"$nulls":5},{"v":11392.74896,"d":"11392.75"},null,null,20]

{"sheet":"2.焦炉-钢构","index":1,"n_rows":703,"n_cols":18,"rows_kept":703,"merged":[[702,0,702,8],[702,9,702,11],[702,13,702,14]],"flags":["formulas_cached_only"]}
["2024年广西钢铁集团焦化厂除锈防腐检修工程-焦炉钢构"]
["钢构及平台","钢构展开面积计算（忽略截断面）     无翼板、腹板概念的钢材例如方钢，长边按腹板计，短边按翼板计。圆钢直径计入“F”列单元格。",{"$nulls":11},"平台防腐"]
["区域/部位","材料型号","规格","数量：根","单根长","腹板H","翼板B","翼板厚t2","腹板厚t1","面积：㎡","重合情况","手动计算","序号","单面","双面","备注","区域腐蚀程度","推荐使用涂料"]
["标高10.31米、4#拦焦车轨道梁","H/工字钢","H1720*542*10*20",1,13450,1720,542,20,10,{"v":75.1586,"d":"75.159"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、4#拦焦车轨道梁","H/工字钢","H1720*542*10*20",8,12500,1720,542,20,10,{"v":558.8,"d":"558.800"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、4#拦焦车轨道梁","H/工字钢","H1720*542*10*20",1,13200,1720,542,20,10,{"v":73.7616,"d":"73.762"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、4#拦焦车轨道梁","H/工字钢","H1720*542*10*20",2,4000,1720,542,20,10,44.704,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、4#拦焦车轨道梁","H/工字钢","H1720*542*10*20",1,11900,1720,542,20,10,{"v":66.4972,"d":"66.497"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、4#拦焦车轨道梁","H/工字钢","H1720*542*10*20",1,11900,1720,542,20,10,{"v":66.4972,"d":"66.497"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、4#拦焦车轨道梁","H/工字钢","H1720*542*10*20",1,12800,1720,542,20,10,{"v":71.5264,"d":"71.526"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、4#拦焦车轨道梁","H/工字钢","H1720*542*10*20",1,4850,1720,542,20,10,{"v":27.1018,"d":"27.102"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、3#拦焦车轨道梁","H/工字钢","H1720*542*10*20",1,5700,1720,542,20,10,{"v":31.8516,"d":"31.852"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、3#拦焦车轨道梁","H/工字钢","H1720*542*10*20",1,4300,1720,542,20,10,{"v":24.0284,"d":"24.028"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、3#拦焦车轨道梁","H/工字钢","H2212*542*10*20",1,14950,2212,542,20,10,{"v":98.2514,"d":"98.251"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、3#拦焦车轨道梁","H/工字钢","H1720*542*10*20",5,13500,1720,542,20,10,{"v":377.19,"d":"377.190"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、3#拦焦车轨道梁","H/工字钢","H1712*542*10*20",1,13500,1712,542,20,10,75.222,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、3#拦焦车轨道梁","H/工字钢","H1712*542*10*20",1,13500,1712,542,20,10,75.222,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、3#拦焦车轨道梁","H/工字钢","H1720*542*10*20",2,4000,1720,542,20,10,44.704,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、3#拦焦车轨道梁","H/工字钢","H1712*542*10*20",1,11000,1712,542,20,10,61.292,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、3#拦焦车轨道梁","H/工字钢","H2212*542*10*20",1,10300,2212,542,20,10,{"v":67.6916,"d":"67.692"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、3#拦焦车轨道梁","H/工字钢","H2212*542*10*20",1,10300,2212,542,20,10,{"v":67.6916,"d":"67.692"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、4#炉电机车滑线支架","H/工字钢","HN350*175*7/11",7,12500,350,175,11,7,121.275,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、4#炉电机车滑线支架","H/工字钢","HN350*175*7/11",7,12500,350,175,11,7,121.275,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、4#炉电机车滑线支架","H/工字钢","HN350*175*7/11",2,11900,350,175,11,7,{"v":32.9868,"d":"32.987"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、4#炉电机车滑线支架","H/工字钢","HN350*175*7/11",2,11900,350,175,11,7,{"v":32.9868,"d":"32.987"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、3#炉电机车滑线支架","H/工字钢","HN350*175*7/11",7,12500,350,175,11,7,121.275,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、3#炉电机车滑线支架","H/工字钢","HN350*175*7/11",7,12500,350,175,11,7,121.275,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、3#炉电机车滑线支架","H/工字钢","HN350*175*7/11",2,11900,350,175,11,7,{"v":32.9868,"d":"32.987"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、3#炉电机车滑线支架","H/工字钢","HN350*175*7/11",2,11900,350,175,11,7,{"v":32.9868,"d":"32.987"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、4#炉电机车滑线支架","2L型钢","2L80*6",110,1600,80,80,6,6,{"v":56.32,"d":"56.320"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、4#炉电机车滑线支架","2L型钢","2L80*6",127,2200,80,80,6,6,89.408,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、3#炉电机车滑线支架","2L型钢","2L80*6",110,1600,80,80,6,6,{"v":56.32,"d":"56.320"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、3#炉电机车滑线支架","2L型钢","2L80*6",127,2200,80,80,6,6,89.408,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、4#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",4,8282,390,300,16,10,{"v":64.93088,"d":"64.931"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、4#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",9,8282,390,300,16,10,{"v":146.09448,"d":"146.094"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、4#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",4,8282,390,300,16,10,{"v":64.93088,"d":"64.931"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、4#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",4,8282,390,300,16,10,{"v":64.93088,"d":"64.931"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、4#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",4,8282,390,300,16,10,{"v":64.93088,"d":"64.931"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、4#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",4,8282,390,300,16,10,{"v":64.93088,"d":"64.931"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、3#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",1,8282,390,300,16,10,{"v":16.23272,"d":"16.233"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、3#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",1,8282,390,300,16,10,{"v":16.23272,"d":"16.233"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、3#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",10,8282,390,300,16,10,{"v":162.3272,"d":"162.327"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、3#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",3,8282,390,300,16,10,{"v":48.69816,"d":"48.698"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、3#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",2,8282,390,300,16,10,{"v":32.46544,"d":"32.465"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、3#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",2,8282,390,300,16,10,{"v":32.46544,"d":"32.465"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、4#炉拦焦车第二轨支架","H/工字钢","HN350*175*7/11",2,115750,350,175,11,7,320.859,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、3#炉拦焦车第二轨支架","H/工字钢","HN350*175*7/11",2,127450,350,175,11,7,{"v":353.2914,"d":"353.291"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、4#炉拦焦车第二轨支架","L型钢","L80*6",110,1600,80,80,6,6,{"v":56.32,"d":"56.320"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、3#炉拦焦车第二轨支架","L型钢","L80*6",127,2200,80,80,6,6,89.408,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、4#炉拦焦车第二轨拉条","2L型钢","2L125*10",232,3450,125,125,10,20,{"v":400.2,"d":"400.200"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、3#炉拦焦车第二轨拉条","2L型钢","2L125*10",232,3450,125,125,10,20,{"v":400.2,"d":"400.200"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、4#炉除尘立柱","H/工字钢","HW400*200*8*13",4,17970,400,200,13,8,{"v":113.85792,"d":"113.858"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、4#炉除尘立柱","H/工字钢","HW400*200*8*13",10,17970,400,200,13,8,{"v":284.6448,"d":"284.645"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、4#炉除尘立柱","H/工字钢","HW400*200*8*13",4,17970,400,200,13,8,{"v":113.85792,"d":"113.858"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、4#炉除尘立柱","H/工字钢","HW400*200*8*13",4,17970,400,200,13,8,{"v":113.85792,"d":"113.858"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、4#炉除尘立柱","H/工字钢","HW400*200*8*13",2,17970,400,200,13,8,{"v":56.92896,"d":"56.929"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、4#炉除尘立柱","H/工字钢","HW400*200*8*13",2,17970,400,200,13,8,{"v":56.92896,"d":"56.929"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、3#炉除尘立柱","H/工字钢","HW400*200*8*13",4,17970,400,200,13,8,{"v":113.85792,"d":"113.858"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、3#炉除尘立柱","H/工字钢","HW400*200*8*13",4,17970,400,200,13,8,{"v":113.85792,"d":"113.858"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、3#炉除尘立柱","H/工字钢","HW400*200*8*13",13,17970,400,200,13,8,{"v":370.03824,"d":"370.038"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、3#炉除尘立柱","H/工字钢","HW400*200*8*13",4,17970,400,200,13,8,{"v":113.85792,"d":"113.858"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、3#炉除尘立柱","H/工字钢","HW400*200*8*13",4,17970,400,200,13,8,{"v":113.85792,"d":"113.858"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、3#炉除尘立柱","H/工字钢","HW400*200*8*13",3,17970,400,200,13,8,{"v":85.39344,"d":"85.393"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31、4#炉拦焦车滑线支架","H/工字钢","HN350*175*7/11",2,178350,350,175,11,7,{"v":494.3862,"d":"494.386"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31、3#炉电机车滑线支架","H/工字钢","HN350*175*7/11",2,169350,350,175,11,7,{"v":469.4382,"d":"469.438"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31、4#炉电机车滑线支架","2L型钢","2L80*6",110,1600,80,80,6,6,{"v":56.32,"d":"56.320"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31、4#炉电机车滑线支架","2L型钢","2L80*6",127,2200,80,80,6,6,89.408,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31、3#炉电机车滑线支架","2L型钢","2L80*6",110,1600,80,80,6,6,{"v":56.32,"d":"56.320"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31、3#炉电机车滑线支架","2L型钢","2L80*6",127,2200,80,80,6,6,89.408,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、4#炉除尘立柱支架","2L型钢","2L140*10",24,4200,140,140,10,20,56.448,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、4#炉除尘立柱支架","2L型钢","2L140*10",54,4200,140,140,10,20,127.008,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、4#炉除尘立柱支架","2L型钢","2L140*10",24,4200,140,140,10,20,56.448,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、4#炉除尘立柱支架","2L型钢","2L140*10",24,4200,140,140,10,20,56.448,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、4#炉除尘立柱支架","2L型钢","2L140*10",24,4200,140,140,10,20,56.448,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、4#炉除尘立柱支架","2L型钢","2L140*10",24,4200,140,140,10,20,56.448,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、3#炉除尘立柱支架","2L型钢","2L140*10",6,4200,140,140,10,20,14.112,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、3#炉除尘立柱支架","2L型钢","2L140*10",6,4200,140,140,10,20,14.112,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、3#炉除尘立柱支架","2L型钢","2L140*10",60,4200,140,140,10,20,{"v":141.12,"d":"141.120"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、3#炉除尘立柱支架","2L型钢","2L140*10",18,4200,140,140,10,20,42.336,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、3#炉除尘立柱支架","2L型钢","2L140*10",12,4200,140,140,10,20,28.224,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、3#炉除尘立柱支架","2L型钢","2L140*10",12,4200,140,140,10,20,28.224,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、4#炉除尘立柱支架","2L型钢","2L140*10",40,2200,140,140,10,20,{"v":49.28,"d":"49.280"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、4#炉除尘立柱支架","2L型钢","2L140*10",90,4200,140,140,10,20,{"v":211.68,"d":"211.680"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、4#炉除尘立柱支架","2L型钢","2L140*10",40,4200,140,140,10,20,{"v":94.08,"d":"94.080"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、4#炉除尘立柱支架","2L型钢","2L140*10",40,4200,140,140,10,20,{"v":94.08,"d":"94.080"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、4#炉除尘立柱支架","2L型钢","2L140*10",40,4200,140,140,10,20,{"v":94.08,"d":"94.080"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、4#炉除尘立柱支架","2L型钢","2L140*10",40,4200,140,140,10,20,{"v":94.08,"d":"94.080"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、3#炉除尘立柱支架","2L型钢","2L140*10",10,4200,140,140,10,20,{"v":23.52,"d":"23.520"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、3#炉除尘立柱支架","2L型钢","2L140*10",10,4200,140,140,10,20,{"v":23.52,"d":"23.520"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、3#炉除尘立柱支架","2L型钢","2L140*10",100,4200,140,140,10,20,{"v":235.2,"d":"235.200"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、3#炉除尘立柱支架","2L型钢","2L140*10",30,4200,140,140,10,20,{"v":70.56,"d":"70.560"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、3#炉除尘立柱支架","2L型钢","2L140*10",20,4200,140,140,10,20,{"v":47.04,"d":"47.040"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、3#炉除尘立柱支架","2L型钢","2L140*10",20,2200,140,140,10,20,{"v":24.64,"d":"24.640"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、4#炉除尘平台架","H/工字钢","HW300*300*10*15",2,178350,300,300,10,15,631.359,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、3#炉除尘平台架","H/工字钢","HW300*300*10*15",2,169350,300,300,10,15,599.499,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、4#炉除尘平台架","L型钢","L90*8",268,3750,90,90,8,8,{"v":361.8,"d":"361.800"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、3#炉除尘平台架","L型钢","L90*8",263,3750,90,90,8,8,{"v":355.05,"d":"355.050"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、1#拦焦车轨道梁","H/工字钢","H1720*542*10*20",1,13450,1720,542,20,10,{"v":75.1586,"d":"75.159"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、1#拦焦车轨道梁","H/工字钢","H1720*542*10*20",8,12500,1720,542,20,10,{"v":558.8,"d":"558.800"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、1#拦焦车轨道梁","H/工字钢","H1720*542*10*20",1,13200,1720,542,20,10,{"v":73.7616,"d":"73.762"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、1#拦焦车轨道梁","H/工字钢","H1720*542*10*20",2,4000,1720,542,20,10,44.704,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、1#拦焦车轨道梁","H/工字钢","H1720*542*10*20",1,11900,1720,542,20,10,{"v":66.4972,"d":"66.497"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、1#拦焦车轨道梁","H/工字钢","H1720*542*10*20",1,11900,1720,542,20,10,{"v":66.4972,"d":"66.497"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、1#拦焦车轨道梁","H/工字钢","H1720*542*10*20",1,12800,1720,542,20,10,{"v":71.5264,"d":"71.526"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、1#拦焦车轨道梁","H/工字钢","H1720*542*10*20",1,4850,1720,542,20,10,{"v":27.1018,"d":"27.102"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、2#拦焦车轨道梁","H/工字钢","H1720*542*10*20",1,5700,1720,542,20,10,{"v":31.8516,"d":"31.852"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、2#拦焦车轨道梁","H/工字钢","H1720*542*10*20",1,4300,1720,542,20,10,{"v":24.0284,"d":"24.028"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、2#拦焦车轨道梁","H/工字钢","H2212*542*10*20",1,14950,2212,542,20,10,{"v":98.2514,"d":"98.251"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、2#拦焦车轨道梁","H/工字钢","H1720*542*10*20",5,13500,1720,542,20,10,{"v":377.19,"d":"377.190"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、2#拦焦车轨道梁","H/工字钢","H1712*542*10*20",1,13500,1712,542,20,10,75.222,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、2#拦焦车轨道梁","H/工字钢","H1712*542*10*20",1,13500,1712,542,20,10,75.222,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、2#拦焦车轨道梁","H/工字钢","H1720*542*10*20",2,4000,1720,542,20,10,44.704,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、2#拦焦车轨道梁","H/工字钢","H1712*542*10*20",1,11000,1712,542,20,10,61.292,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、2#拦焦车轨道梁","H/工字钢","H2212*542*10*20",1,10300,2212,542,20,10,{"v":67.6916,"d":"67.692"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31米、2#拦焦车轨道梁","H/工字钢","H2212*542*10*20",1,10300,2212,542,20,10,{"v":67.6916,"d":"67.692"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、1#炉电机车滑线支架","H/工字钢","HN350*175*7/11",7,12500,350,175,11,7,121.275,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、1#炉电机车滑线支架","H/工字钢","HN350*175*7/11",7,12500,350,175,11,7,121.275,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、1#炉电机车滑线支架","H/工字钢","HN350*175*7/11",2,11900,350,175,11,7,{"v":32.9868,"d":"32.987"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、1#炉电机车滑线支架","H/工字钢","HN350*175*7/11",2,11900,350,175,11,7,{"v":32.9868,"d":"32.987"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、2#炉电机车滑线支架","H/工字钢","HN350*175*7/11",7,12500,350,175,11,7,121.275,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、2#炉电机车滑线支架","H/工字钢","HN350*175*7/11",7,12500,350,175,11,7,121.275,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、2#炉电机车滑线支架","H/工字钢","HN350*175*7/11",2,11900,350,175,11,7,{"v":32.9868,"d":"32.987"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、2#炉电机车滑线支架","H/工字钢","HN350*175*7/11",2,11900,350,175,11,7,{"v":32.9868,"d":"32.987"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、1#炉电机车滑线支架","2L型钢","2L80*6",110,1600,80,80,6,6,{"v":56.32,"d":"56.320"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、1#炉电机车滑线支架","2L型钢","2L80*6",127,2200,80,80,6,6,89.408,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、2#炉电机车滑线支架","2L型钢","2L80*6",110,1600,80,80,6,6,{"v":56.32,"d":"56.320"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高5.9米、2#炉电机车滑线支架","2L型钢","2L80*6",127,2200,80,80,6,6,89.408,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、1#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",4,8282,390,300,16,10,{"v":64.93088,"d":"64.931"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、1#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",9,8282,390,300,16,10,{"v":146.09448,"d":"146.094"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、1#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",4,8282,390,300,16,10,{"v":64.93088,"d":"64.931"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、1#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",4,8282,390,300,16,10,{"v":64.93088,"d":"64.931"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、1#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",4,8282,390,300,16,10,{"v":64.93088,"d":"64.931"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、1#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",4,8282,390,300,16,10,{"v":64.93088,"d":"64.931"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、2#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",1,8282,390,300,16,10,{"v":16.23272,"d":"16.233"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、2#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",1,8282,390,300,16,10,{"v":16.23272,"d":"16.233"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、2#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",10,8282,390,300,16,10,{"v":162.3272,"d":"162.327"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、2#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",3,8282,390,300,16,10,{"v":48.69816,"d":"48.698"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、2#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",2,8282,390,300,16,10,{"v":32.46544,"d":"32.465"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、2#炉拦焦车第二轨立柱","H/工字钢","HM390*300*10*16",2,8282,390,300,16,10,{"v":32.46544,"d":"32.465"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、2#炉拦焦车第二轨立柱","H/工字钢","HN350*175*7/11",2,115750,350,175,11,7,320.859,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、2#炉拦焦车第二轨支架","H/工字钢","HN350*175*7/11",2,127450,350,175,11,7,{"v":353.2914,"d":"353.291"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、1#炉拦焦车第二轨支架","L型钢","L80*6",110,1600,80,80,6,6,{"v":56.32,"d":"56.320"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.282米、2#炉拦焦车第二轨支架","L型钢","L80*6",127,2200,80,80,6,6,89.408,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉拦焦车第二轨拉条","2L型钢","2L125*10",232,3450,125,125,10,20,{"v":400.2,"d":"400.200"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、2#炉拦焦车第二轨拉条","2L型钢","2L125*10",232,3450,125,125,10,20,{"v":400.2,"d":"400.200"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘立柱","H/工字钢","HW400*200*8*13",4,17970,400,200,13,8,{"v":113.85792,"d":"113.858"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘立柱","H/工字钢","HW400*200*8*13",10,17970,400,200,13,8,{"v":284.6448,"d":"284.645"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘立柱","H/工字钢","HW400*200*8*13",4,17970,400,200,13,8,{"v":113.85792,"d":"113.858"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘立柱","H/工字钢","HW400*200*8*13",4,17970,400,200,13,8,{"v":113.85792,"d":"113.858"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘立柱","H/工字钢","HW400*200*8*13",2,17970,400,200,13,8,{"v":56.92896,"d":"56.929"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘立柱","H/工字钢","HW400*200*8*13",2,17970,400,200,13,8,{"v":56.92896,"d":"56.929"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、2#炉除尘立柱","H/工字钢","HW400*200*8*13",4,17970,400,200,13,8,{"v":113.85792,"d":"113.858"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、2#炉除尘立柱","H/工字钢","HW400*200*8*13",4,17970,400,200,13,8,{"v":113.85792,"d":"113.858"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、2#炉除尘立柱","H/工字钢","HW400*200*8*13",13,17970,400,200,13,8,{"v":370.03824,"d":"370.038"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、2#炉除尘立柱","H/工字钢","HW400*200*8*13",4,17970,400,200,13,8,{"v":113.85792,"d":"113.858"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、2#炉除尘立柱","H/工字钢","HW400*200*8*13",4,17970,400,200,13,8,{"v":113.85792,"d":"113.858"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、2#炉除尘立柱","H/工字钢","HW400*200*8*13",3,17970,400,200,13,8,{"v":85.39344,"d":"85.393"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31、1#炉拦焦车滑线支架","H/工字钢","HN350*175*7/11",2,178350,350,175,11,7,{"v":494.3862,"d":"494.386"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31、2#炉拦焦车滑线支架","H/工字钢","HN350*175*7/11",2,169350,350,175,11,7,{"v":469.4382,"d":"469.438"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31、1#炉拦焦车滑线支架","2L型钢","2L80*6",110,1600,80,80,6,6,{"v":56.32,"d":"56.320"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31、2#炉拦焦车滑线支架","2L型钢","2L80*6",127,2200,80,80,6,6,89.408,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31、1#炉拦焦车滑线支架","2L型钢","2L80*6",110,1600,80,80,6,6,{"v":56.32,"d":"56.320"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高10.31、2#炉拦焦车滑线支架","2L型钢","2L80*6",127,2200,80,80,6,6,89.408,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、1#炉除尘立柱支架","2L型钢","2L140*10",24,4200,140,140,10,20,56.448,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、1#炉除尘立柱支架","2L型钢","2L140*10",54,4200,140,140,10,20,127.008,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、1#炉除尘立柱支架","2L型钢","2L140*10",24,4200,140,140,10,20,56.448,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、1#炉除尘立柱支架","2L型钢","2L140*10",24,4200,140,140,10,20,56.448,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、1#炉除尘立柱支架","2L型钢","2L140*10",24,4200,140,140,10,20,56.448,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、1#炉除尘立柱支架","2L型钢","2L140*10",24,4200,140,140,10,20,56.448,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、2#炉除尘立柱支架","2L型钢","2L140*10",6,4200,140,140,10,20,14.112,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、2#炉除尘立柱支架","2L型钢","2L140*10",6,4200,140,140,10,20,14.112,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、2#炉除尘立柱支架","2L型钢","2L140*10",60,4200,140,140,10,20,{"v":141.12,"d":"141.120"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、2#炉除尘立柱支架","2L型钢","2L140*10",18,4200,140,140,10,20,42.336,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、2#炉除尘立柱支架","2L型钢","2L140*10",12,4200,140,140,10,20,28.224,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高8.82、2#炉除尘立柱支架","2L型钢","2L140*10",12,4200,140,140,10,20,28.224,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘立柱支架","2L型钢","2L140*10",40,2200,140,140,10,20,{"v":49.28,"d":"49.280"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘立柱支架","2L型钢","2L140*10",90,4200,140,140,10,20,{"v":211.68,"d":"211.680"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘立柱支架","2L型钢","2L140*10",40,4200,140,140,10,20,{"v":94.08,"d":"94.080"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘立柱支架","2L型钢","2L140*10",40,4200,140,140,10,20,{"v":94.08,"d":"94.080"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘立柱支架","2L型钢","2L140*10",40,4200,140,140,10,20,{"v":94.08,"d":"94.080"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘立柱支架","2L型钢","2L140*10",40,4200,140,140,10,20,{"v":94.08,"d":"94.080"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘立柱支架","2L型钢","2L140*10",10,4200,140,140,10,20,{"v":23.52,"d":"23.520"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘立柱支架","2L型钢","2L140*10",10,4200,140,140,10,20,{"v":23.52,"d":"23.520"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘立柱支架","2L型钢","2L140*10",100,4200,140,140,10,20,{"v":235.2,"d":"235.200"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘立柱支架","2L型钢","2L140*10",30,4200,140,140,10,20,{"v":70.56,"d":"70.560"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘立柱支架","2L型钢","2L140*10",20,4200,140,140,10,20,{"v":47.04,"d":"47.040"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘立柱支架","2L型钢","2L140*10",20,2200,140,140,10,20,{"v":24.64,"d":"24.640"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘平台架","H/工字钢","HW300*300*10*15",2,178350,300,300,10,15,631.359,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、2#炉除尘平台架","H/工字钢","HW300*300*10*15",2,169350,300,300,10,15,599.499,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、1#炉除尘平台架","L型钢","L90*8",268,3750,90,90,8,8,{"v":361.8,"d":"361.800"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.975、2#炉除尘平台架","L型钢","L90*8",263,3750,90,90,8,8,{"v":355.05,"d":"355.050"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高25.4、备煤B114皮带立柱","H/工字钢","H650*280*8*16",2,25200,650,280,16,8,{"v":121.1616,"d":"121.162"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高25.9、备煤B114皮带立柱","H/工字钢","H650*280*8*16",2,25300,650,280,16,8,{"v":121.6424,"d":"121.642"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高26.6、备煤B114皮带立柱","H/工字钢","H650*280*8*16",2,26000,700,280,16,8,130.208,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高27.7、备煤B114皮带立柱","H/工字钢","H650*280*8*16",2,26500,700,280,16,8,132.712,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高27.7、备煤B114皮带立柱","H/工字钢","H650*280*8*16",4,27100,300,240,12,6,{"v":167.8032,"d":"167.803"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高28.4、备煤B114皮带立柱","H/工字钢","H700*270*8*12",2,24200,700,270,12,8,{"v":119.2576,"d":"119.258"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高29.5、备煤B114皮带立柱","H/工字钢","H700*270*8*12",2,24600,700,270,12,8,{"v":121.2288,"d":"121.229"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高30.7、备煤B114皮带立柱","H/工字钢","H750*300*8*16",2,25000,750,300,16,8,{"v":134.2,"d":"134.200"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高30.7、备煤B114皮带立柱","H/工字钢","H750*300*8*16",2,25500,750,300,16,8,136.884,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高33、备煤B114皮带立柱","H/工字钢","H300*300*6*14",4,33000,300,300,14,6,236.016,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高31.3、备煤B114皮带立柱","H/工字钢","H800*300*8*16",2,26800,800,300,16,8,{"v":149.2224,"d":"149.222"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高31.9、备煤B114皮带立柱","H/工字钢","H800*300*8*16",2,27500,800,300,16,8,{"v":153.12,"d":"153.120"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高32.4、备煤B114皮带立柱","H/工字钢","H800*320*8*16",2,28300,800,320,16,8,{"v":162.1024,"d":"162.102"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高33、备煤B114皮带立柱","H/工字钢","H800*320*8*16",2,28900,800,320,16,8,{"v":165.5392,"d":"165.539"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高13.8、备煤B114皮带立柱支架","2L型钢","2L80*6",6,7433,80,80,6,12,{"v":14.27136,"d":"14.271"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高13.8、备煤B114皮带立柱支架","2L型钢","2L125*8",3,5270,125,125,8,16,7.905,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高25.4、备煤B114皮带立柱支架","2L型钢","2L90*6",4,7100,90,90,6,12,10.224,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高25.4、备煤B114皮带立柱支架","2L型钢","2L110*8",3,4860,110,110,8,16,{"v":6.4152,"d":"6.415"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高13.8、备煤B114皮带立柱支架","2L型钢","2L80*6",6,7433,80,80,6,12,{"v":14.27136,"d":"14.271"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高13.8、备煤B114皮带立柱支架","2L型钢","2L125*8",3,5270,125,125,8,16,7.905,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高25.9、备煤B114皮带立柱支架","2L型钢","2L80*6",6,7433,80,80,6,12,{"v":14.27136,"d":"14.271"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高25.9、备煤B114皮带立柱支架","2L型钢","2L110*8",3,4860,110,110,8,16,{"v":6.4152,"d":"6.415"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高14.1、备煤B114皮带立柱支架","2L型钢","2L90*6",6,7433,90,90,6,12,{"v":16.05528,"d":"16.055"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高14.1、备煤B114皮带立柱支架","2L型钢","2L125*8",3,5270,125,125,8,16,7.905,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高26.6、备煤B114皮带立柱支架","2L型钢","2L90*6",6,7433,90,90,6,12,{"v":16.05528,"d":"16.055"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高26.6、备煤B114皮带立柱支架","2L型钢","2L110*8",3,4860,110,110,8,16,{"v":6.4152,"d":"6.415"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高14.6、备煤B114皮带立柱支架","2L型钢","2L90*6",6,7433,90,90,6,12,{"v":16.05528,"d":"16.055"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高14.6、备煤B114皮带立柱支架","2L型钢","2L125*8",3,5270,125,125,8,16,7.905,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高27.7、备煤B114皮带立柱支架","2L型钢","2L90*6",6,7433,90,90,6,12,{"v":16.05528,"d":"16.055"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高27.7、备煤B114皮带立柱支架","2L型钢","2L110*8",3,4860,110,110,8,16,{"v":6.4152,"d":"6.415"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高14.6、备煤B114皮带立柱支架","2L型钢","2L100*6",8,7433,100,100,6,12,{"v":23.7856,"d":"23.786"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高14.6、备煤B114皮带立柱支架","2L型钢","2L90*6",6,5270,90,90,6,12,{"v":11.3832,"d":"11.383"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高27.7、备煤B114皮带立柱支架","2L型钢","2L100*8",4,4860,100,100,8,16,7.776,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高14.6、备煤B114皮带立柱支架","2L型钢","2L100*6",8,7433,100,100,6,12,{"v":23.7856,"d":"23.786"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高14.6、备煤B114皮带立柱支架","2L型钢","2L90*6",6,5270,90,90,6,12,{"v":11.3832,"d":"11.383"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高27.7、备煤B114皮带立柱支架","2L型钢","2L100*8",4,4860,100,100,8,16,7.776,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高15、备煤B114皮带立柱支架","2L型钢","2L75*6",8,5270,75,75,6,12,12.648,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高12.6、备煤B114皮带立柱支架","2L型钢","2K125*8",2,5500,125,125,8,16,{"v":5.5,"d":"5.500"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高28.4、备煤B114皮带立柱支架","2L型钢","2L110*8",6,4860,110,110,8,16,{"v":12.8304,"d":"12.830"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高28.4、备煤B114皮带立柱支架","2L型钢","2L75*6",6,4860,75,75,6,12,8.748,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高15、备煤B114皮带立柱支架","2L型钢","2L75*6",8,5270,75,75,6,12,12.648,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高14.2、备煤B114皮带立柱支架","2L型钢","2K125*8",2,5500,125,125,8,16,{"v":5.5,"d":"5.500"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高29.5、备煤B114皮带立柱支架","2L型钢","2L110*8",6,4860,110,110,8,16,{"v":12.8304,"d":"12.830"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高29.5、备煤B114皮带立柱支架","2L型钢","2L75*6",8,5270,75,75,6,12,12.648,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高15.2、备煤B114皮带立柱支架","2L型钢","2L75*6",8,5270,75,75,6,12,12.648,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高14.8、备煤B114皮带立柱支架","2L型钢","2K125*8",2,6000,125,125,8,16,{"v":6,"d":"6.000"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高30.7、备煤B114皮带立柱支架","2L型钢","2L110*8",6,4860,110,110,8,16,{"v":12.8304,"d":"12.830"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高30.7、备煤B114皮带立柱支架","2L型钢","2L75*6",8,5270,75,75,6,12,12.648,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高16、备煤B114皮带立柱支架","2L型钢","2L90*6",8,5520,90,90,6,12,{"v":15.8976,"d":"15.898"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高15.4、备煤B114皮带立柱支架","2L型钢","2K125*8",2,6000,125,125,8,16,{"v":6,"d":"6.000"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高30.7、备煤B114皮带立柱支架","2L型钢","2L110*8",6,4860,110,110,8,16,{"v":12.8304,"d":"12.830"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高30.7、备煤B114皮带立柱支架","2L型钢","2L90*6",8,5520,90,90,6,12,{"v":15.8976,"d":"15.898"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高16、备煤B114皮带立柱支架","2L型钢","2L100*6",8,5270,100,100,6,12,16.864,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高15.4、备煤B114皮带立柱支架","2L型钢","2L90*6",4,5120,90,90,6,12,{"v":7.3728,"d":"7.373"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高31.3、备煤B114皮带立柱支架","2L型钢","2L90*6",6,4860,90,90,6,12,{"v":10.4976,"d":"10.498"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高31.3、备煤B114皮带立柱支架","2L型钢","2L100*6",6,4560,100,100,6,12,10.944,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高16、备煤B114皮带立柱支架","2L型钢","2L100*6",8,5270,100,100,6,12,16.864,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高15.4、备煤B114皮带立柱支架","2L型钢","2L90*6",4,5120,90,90,6,12,{"v":7.3728,"d":"7.373"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高31.9、备煤B114皮带立柱支架","2L型钢","2L90*6",6,4860,90,90,6,12,{"v":10.4976,"d":"10.498"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高31.9、备煤B114皮带立柱支架","2L型钢","2L100*6",6,4560,100,100,6,12,10.944,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高16.2、备煤B114皮带立柱支架","2L型钢","2L80*6",10,5700,80,80,6,12,{"v":18.24,"d":"18.240"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高16.2、备煤B114皮带立柱支架","2L型钢","2L125*8",4,6000,125,125,8,16,{"v":12,"d":"12.000"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高31.3、备煤B114皮带立柱支架","2L型钢","2L110*10",4,4650,110,110,10,20,8.184,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高31.3、备煤B114皮带立柱支架","2L型钢","2L110*10",3,4230,110,110,10,20,{"v":5.5836,"d":"5.584"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高16.2、备煤B114皮带立柱支架","2L型钢","2L80*6",10,5700,80,80,6,12,{"v":18.24,"d":"18.240"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高16.2、备煤B114皮带立柱支架","2L型钢","2L125*8",4,6000,125,125,8,16,{"v":12,"d":"12.000"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高31.9、备煤B114皮带立柱支架","2L型钢","2L110*10",4,4650,110,110,10,20,8.184,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高31.9、备煤B114皮带立柱支架","2L型钢","2L110*10",3,4230,110,110,10,20,{"v":5.5836,"d":"5.584"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高16.2、备煤B114皮带立柱支架","2L型钢","2L100*6",8,5700,100,100,6,12,{"v":18.24,"d":"18.240"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高16.2、备煤B114皮带立柱支架","2L型钢","2L125*8",4,6000,125,125,8,16,{"v":12,"d":"12.000"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高32.4、备煤B114皮带立柱支架","2L型钢","2L90*6",8,4650,90,90,6,16,13.392,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高32.4、备煤B114皮带立柱支架","2L型钢","2L110*10",4,4230,110,110,10,20,{"v":7.4448,"d":"7.445"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高16.2、备煤B114皮带立柱支架","2L型钢","2L100*6",8,5700,100,100,6,12,{"v":18.24,"d":"18.240"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高16.2、备煤B114皮带立柱支架","2L型钢","2L125*8",4,6000,125,125,8,16,{"v":12,"d":"12.000"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高33、备煤B114皮带立柱支架","2L型钢","2L90*6",8,4650,90,90,6,16,13.392,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高33、备煤B114皮带立柱支架","2L型钢","2L110*10",4,4230,110,110,10,20,{"v":7.4448,"d":"7.445"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高33、备煤B114皮带通廊底部",null,"152429*4000",{"$nulls":6},"",null,null,0,{"v":609.716,"d":"609.72"},null,"平台板、仅防腐单面","一般性腐蚀","环氧富锌漆"]
["标高33、备煤B114皮带通廊底部",null,"148572*4000",{"$nulls":6},"",null,null,0,{"v":594.288,"d":"594.29"},null,"平台板、仅防腐单面","一般性腐蚀","环氧富锌漆"]
["标高33、备煤B114皮带通廊底部",null,"146625*4000",{"$nulls":6},"",null,null,0,{"v":586.5,"d":"586.50"},null,"平台板、仅防腐单面","一般性腐蚀","环氧富锌漆"]
["标高42.8、备煤B115皮带立柱","H/工字钢","H950*350*12*25",2,42600,950,350,25,12,{"v":279.1152,"d":"279.115"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高34.9、备煤B115皮带立柱","H/工字钢","H800*300*12*20",2,34750,800,300,20,12,192.932,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高23、备煤B115皮带立柱支架","2L型钢","2L110*7",8,10000,110,110,7,14,{"v":35.2,"d":"35.200"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高23、备煤B115皮带立柱支架","L型钢","L50*6",4,7800,50,50,6,6,{"v":6.24,"d":"6.240"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高42.8、备煤B115皮带立柱支架","2L型钢","2L110*7",8,8200,110,110,7,14,28.864,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高42.8、备煤B115皮带立柱支架","L型钢","L50*6",4,6200,50,50,6,6,{"v":4.96,"d":"4.960"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.7、备煤B115皮带立柱支架","2L型钢","2L110*7",6,8920,110,110,7,14,{"v":23.5488,"d":"23.549"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.7、备煤B115皮带立柱支架","L型钢","L50*6",3,7000,50,50,6,6,{"v":4.2,"d":"4.200"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高34.9、备煤B115皮带立柱支架","2L型钢","2L90*6",8,7200,90,90,6,12,20.736,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高34.9、备煤B115皮带立柱支架","L型钢","L50*6",4,6720,50,50,6,6,5.376,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高42.8、备煤B115皮带通廊底部",null,"90000*4000",{"$nulls":6},"",null,null,0,{"v":360,"d":"360.00"},null,"平台板、仅防腐单面","一般性腐蚀","环氧富锌漆"]
["标高42.8、备煤B113皮带立柱","H/工字钢","H950*350*12*25",2,42600,950,350,25,12,{"v":279.1152,"d":"279.115"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高34.9、备煤B113皮带立柱","H/工字钢","H800*300*12*20",2,34750,800,300,20,12,192.932,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高23、备煤B113皮带立柱支架","2L型钢","2L110*7",8,10000,110,110,7,14,{"v":35.2,"d":"35.200"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高23、备煤B113皮带立柱支架","L型钢","L50*6",4,7800,50,50,6,6,{"v":6.24,"d":"6.240"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高42.8、备煤B113皮带立柱支架","2L型钢","2L110*7",8,8200,110,110,7,14,28.864,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高42.8、备煤B113皮带立柱支架","L型钢","L50*6",4,6200,50,50,6,6,{"v":4.96,"d":"4.960"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.7、备煤B113皮带立柱支架","2L型钢","2L110*7",6,8920,110,110,7,14,{"v":23.5488,"d":"23.549"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.7、备煤B113皮带立柱支架","L型钢","L50*6",3,7000,50,50,6,6,{"v":4.2,"d":"4.200"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高34.9、备煤B113皮带立柱支架","2L型钢","2L90*6",8,7200,90,90,6,12,20.736,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高34.9、备煤B113皮带立柱支架","L型钢","L50*6",4,6720,50,50,6,6,5.376,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高42.8、备煤B113皮带通廊底部",null,"90000*4000",{"$nulls":6},"",null,null,0,{"v":360,"d":"360.00"},null,"平台板、仅防腐单面","一般性腐蚀","环氧富锌漆"]
["标高4.3、备煤B112皮带立柱","H/工字钢","H400*250*8*14",2,4300,400,250,14,8,{"v":15.3424,"d":"15.342"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高12.1、备煤B112皮带立柱","H/工字钢","H400*250*8*14",2,11900,400,250,14,8,{"v":42.4592,"d":"42.459"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高19.5、备煤B112皮带立柱","H/工字钢","H530*250*8*14",2,19300,530,250,14,8,{"v":78.8984,"d":"78.898"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高27、备煤B112皮带立柱","H/工字钢","H680*280*10*16",2,26600,680,280,16,10,130.872,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高4.3、备煤B112皮带立柱支架","L型钢","L110*8",2,5656,110,110,8,8,{"v":4.97728,"d":"4.977"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高4.3、备煤B112皮带立柱支架","2L型钢","2L80*6",1,4000,80,80,6,12,{"v":1.28,"d":"1.280"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高12.1、备煤B112皮带立柱支架","L型钢","L110*8",6,5656,110,110,8,8,{"v":14.93184,"d":"14.932"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高12.1、备煤B112皮带立柱支架","2L型钢","2L80*6",3,4000,80,80,6,12,{"v":3.84,"d":"3.840"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高19.5、备煤B112皮带立柱支架","L型钢","L110*8",10,6800,110,110,8,8,{"v":29.92,"d":"29.920"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高19.5、备煤B112皮带立柱支架","L型钢","L110*8",6,5656,110,110,8,8,{"v":14.93184,"d":"14.932"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高19.5、备煤B112皮带立柱支架","2L型钢","2L100*8",3,5500,100,100,8,8,{"v":6.6,"d":"6.600"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高19.5、备煤B112皮带立柱支架","2L型钢","2L90*8",2,5000,90,90,8,8,{"v":3.6,"d":"3.600"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高27、备煤B112皮带立柱支架","2L型钢","2L80*6",8,5656,80,80,6,12,{"v":14.47936,"d":"14.479"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高27、备煤B112皮带立柱支架","2L型钢","2L125*8",3,5500,125,125,8,16,{"v":8.25,"d":"8.250"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高27、备煤B112皮带立柱支架","2L型钢","2L90*8",4,5000,90,90,8,8,{"v":7.2,"d":"7.200"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高27、备煤B112皮带立柱支架","L型钢","L110*8",6,4800,110,110,8,8,12.672,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高27、备煤B112皮带通廊底部",null,"138416*4000",{"$nulls":6},"",null,null,0,{"v":553.664,"d":"553.66"},null,"平台板、仅防腐单面","一般性腐蚀","环氧富锌漆"]
["标高24.3、备煤B104皮带立柱","H/工字钢","H650*250*10*16",2,23900,650,250,16,10,108.984,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高24.3、备煤B104皮带立柱支架","2L型钢","2L80*6",8,5656,80,80,6,12,{"v":14.47936,"d":"14.479"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高24.3、备煤B104皮带立柱支架","2L型钢","2L90*6",4,5000,90,90,6,12,{"v":7.2,"d":"7.200"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高24.3、备煤B104皮带立柱支架","2L型钢","2L125*8",3,5500,125,125,8,16,{"v":8.25,"d":"8.250"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高24.3、备煤B104皮带立柱支架","2L型钢","2L100*10",4,5000,100,100,10,20,{"v":8,"d":"8.000"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高24.3、备煤B104皮带通廊底部",null,"59311*4000",{"$nulls":6},"",null,null,0,{"v":237.244,"d":"237.24"},null,"平台板、仅防腐单面","一般性腐蚀","环氧富锌漆"]
["标高15.8、备煤B101\\B102皮带立柱","H/工字钢","H500*300*12*16",2,15750,500,300,16,12,68.544,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高15.8、备煤B101\\B102皮带立柱","H/工字钢","H400*300*10*16",2,8250,400,300,16,10,{"v":32.67,"d":"32.670"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高15.8、备煤B101\\B102皮带立柱支架","2L型钢","2L110*7",4,11313,110,110,7,14,{"v":19.91088,"d":"19.911"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高15.8、备煤B101\\B102皮带立柱支架","2L型钢","2L160*10",4,8000,160,160,10,20,{"v":20.48,"d":"20.480"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高15.8、备煤B101\\B102皮带立柱支架","2L型钢","2L110*7",2,11313,110,110,7,14,{"v":9.95544,"d":"9.955"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高15.8、备煤B101\\B102皮带立柱支架","2L型钢","2L160*10",2,8000,160,160,10,20,{"v":10.24,"d":"10.240"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高15.8、备煤B101\\B102皮带通廊底部",null,"42925*8000",{"$nulls":6},"",null,null,0,{"v":343.4,"d":"343.40"},null,"平台板、仅防腐单面","一般性腐蚀","环氧富锌漆"]
["标高17.9、备煤B103皮带立柱","H/工字钢","H420*240*10*14",2,17700,420,240,14,10,63.012,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.9、备煤B103皮带立柱支架","L型钢","L110*8",8,6300,110,110,8,8,22.176,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.9、备煤B103皮带立柱支架","2L型钢","2L100*6",4,5500,100,100,8,16,{"v":8.8,"d":"8.800"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.9、备煤B103皮带通廊底部",null,"26244*4000",{"$nulls":6},"",null,null,0,104.976,null,"平台板、仅防腐单面","一般性腐蚀","环氧富锌漆"]
["标高25、备煤B107~109皮带通廊底部",null,"3*10000*4000",{"$nulls":6},"",null,null,0,120,null,"平台板、仅防腐单面","一般性腐蚀","环氧富锌漆"]
["标高21.9、1#2#装煤除尘仓体","其他","2*23870*9000",{"$nulls":6},"需手动计算","无重合面",429.66,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高21.9、1#2#装煤除尘仓体","其他","2*11576*9000",{"$nulls":6},"需手动计算","无重合面",208.368,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、1#2#装煤除尘仓体立柱","H/工字钢","H200*200*8*12",16,5400,200,200,12,8,{"v":102.2976,"d":"102.298"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、1#2#装煤除尘仓体立柱","L型钢","L60*6",56,6200,60,60,6,6,83.328,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高21.9、3#4#装煤除尘仓体","其他","2*23870*9000",{"$nulls":6},"需手动计算","无重合面",429.66,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高21.9、3#4#装煤除尘仓体","其他","2*11576*9000",{"$nulls":6},"需手动计算","无重合面",208.368,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、3#4#装煤除尘仓体立柱","H/工字钢","H200*200*8*12",16,5400,200,200,12,8,{"v":102.2976,"d":"102.298"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、3#4#装煤除尘仓体立柱支架\n","L型钢","L60*6",56,6200,60,60,6,6,83.328,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、1#2#出焦除尘仓体","其他","2*37620*9000",{"$nulls":6},"需手动计算","无重合面",677.16,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、1#2#出焦除尘仓体","其他","2*11576*9000",{"$nulls":6},"需手动计算","无重合面",208.368,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、1#2#出焦除尘立柱","H/工字钢","H200*200*8*12",24,5400,200,200,12,8,{"v":153.4464,"d":"153.446"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、1#2#出焦除尘立柱支架","L型钢","L60*6",44,6200,60,60,6,6,65.472,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、3#4#出焦除尘仓体","其他","2*37620*9000",{"$nulls":6},"需手动计算","无重合面",677.16,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、3#4#出焦除尘仓体","其他","2*11576*9000",{"$nulls":6},"需手动计算","无重合面",208.368,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、3#4#出焦除尘立柱","H/工字钢","H200*200*8*12",24,5400,200,200,12,8,{"v":153.4464,"d":"153.446"},"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、3#4#出焦除尘立柱支架","L型钢","L60*6",44,6200,60,60,6,6,65.472,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、1#2#炉机侧除尘仓体","其他","2*30780*9000",{"$nulls":6},"需手动计算","无重合面",554.04,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、1#2#炉机侧除尘仓体","其他","2*11576*9000",{"$nulls":6},"需手动计算","无重合面",208.368,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、1#2#炉机侧除尘立柱","H/工字钢","H200*200*8*12",20,5400,200,200,12,8,127.872,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、1#2#炉机侧除尘立柱支架","L型钢","L60*6",36,6200,60,60,6,6,53.568,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、3#4#炉机侧除尘仓体","其他","2*30780*9000",{"$nulls":6},"需手动计算","无重合面",554.04,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、3#4#炉机侧除尘仓体","其他","2*11576*9000",{"$nulls":6},"需手动计算","无重合面",208.368,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、3#4#炉机侧除尘立柱","H/工字钢","H200*200*8*12",20,5400,200,200,12,8,127.872,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高17.6、3#4#炉机侧除尘立柱支架","L型钢","L60*6",36,6200,60,60,6,6,53.568,"无重合面",null,0,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["标高21.49、1#炉集气管操作台铺板","其他","1224/39.25*3",{"$nulls":6},"需手动计算","无重合面",93.55,1,null,null,"A1822.030214CO003-5-1（根据吨钢重量计算面积）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=1200",48,1200,100,68,4.5,7.6,{"v":19.3536,"d":"19.354"},"无重合面",null,2,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=500",48,500,100,68,4.5,7.6,8.064,"无重合面",null,3,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=3700",12,3700,100,68,4.5,7.6,{"v":14.9184,"d":"14.918"},"无重合面",null,4,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=2060",84,2060,100,68,4.5,7.6,{"v":58.14144,"d":"58.141"},"无重合面",null,5,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=1500",42,1500,100,68,4.5,7.6,21.168,"无重合面",null,6,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台踢脚板","方（扁）钢","4*100   L=140m",1,140000,100,{"$nulls":3},{"v":28,"d":"28.000"},"无重合面",null,7,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台围栏","圆钢","Φ16 L=140m",2,140000,16,{"$nulls":3},{"v":14.0672,"d":"14.067"},"无重合面",null,8,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台围栏","圆钢","Φ33.5*3.25   L=140m",1,140000,40,{"$nulls":3},17.584,"无重合面",null,9,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台菱形花纹板","其他","t5   150㎡",1,{"$nulls":5},"需手动计算","无重合面",{"v":150,"d":"150.00"},10,null,null,"A1822.030214CO003-5-1图上已表明花纹板面积","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=1196",2,1196,200,100,5.8,8,{"v":1.4352,"d":"1.435"},"无重合面",null,11,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=446",13,446,200,100,5.8,8,{"v":3.4788,"d":"3.479"},"无重合面",null,12,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=872",4,872,200,100,5.8,8,{"v":2.0928,"d":"2.093"},"无重合面",null,13,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台梁柱","方（扁）钢","16*200*200",24,200,16,200,null,null,{"v":2.0736,"d":"2.074"},"无重合面",null,14,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台梁柱","L型钢","200*200*8*12   L=1644",52,1644,200,200,8,12,{"v":68.3904,"d":"68.390"},"无重合面",null,15,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台梁柱","L型钢","160*65*8.5*8.5  L=3294",11,3294,160,65,8.5,8.5,{"v":16.3053,"d":"16.305"},"无重合面",null,16,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台梁柱","L型钢","200*200*8*12   L=3294",13,3294,200,200,8,12,{"v":34.2576,"d":"34.258"},"无重合面",null,17,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台梁柱","L型钢","160*65*8.5*8.5  L=1644",98,1644,160,65,8.5,8.5,{"v":72.5004,"d":"72.500"},"无重合面",null,18,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台梁柱","L型钢","160*65*8.5*8.5  L=1706",2,1706,160,65,8.5,8.5,{"v":1.5354,"d":"1.535"},"无重合面",null,19,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=970",2,970,200,100,5.8,8,1.164,"无重合面",null,20,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=819",2,819,200,100,5.8,8,{"v":0.9828,"d":"0.983"},"无重合面",null,21,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=1640",60,1640,200,100,5.8,8,{"v":59.04,"d":"59.040"},"无重合面",null,22,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、1#炉集气管操作台梁柱","L型钢","160*65*8.5*8.5  L=1640",60,1640,160,65,8.5,8.5,{"v":44.28,"d":"44.280"},"无重合面",null,23,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、1#炉集气管操作台梯子","方（扁）钢","8*270*800",8,800,270,"800",null,null,13.696,"无重合面",null,24,null,null,"A1822.030214CO003-6-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、1#炉集气管操作台梯子","圆钢","Φ16  L=1332",8,1332,16,{"$nulls":3},{"v":0.5353574400000001,"d":"0.535"},"无重合面",null,25,null,null,"A1822.030214CO003-6-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、1#炉集气管操作台梯子","圆钢","Φ33.5*3.25   L=7260",2,7260,40,{"$nulls":3},{"v":1.8237120000000002,"d":"1.824"},"无重合面",null,26,null,null,"A1822.030214CO003-6-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、1#炉集气管操作台梯子","L型钢","50*50*5   L=792",1,792,50,50,5,null,{"v":0.1584,"d":"0.158"},"无重合面",null,27,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、1#炉集气管操作台梯子","L型钢","200*100*5.5*8   L=1091",2,1091,200,100,5.5,8,{"v":1.3092,"d":"1.309"},"无重合面",null,28,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、1#炉集气管操作台梯子","方（扁）钢","8*800*1150",1,1150,800,"150",null,null,2.185,"无重合面",null,29,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、1#炉集气管操作台梯子","L型钢","4*100   L=2000",1,2000,100,{"$nulls":3},{"v":0.4,"d":"0.400"},"无重合面",null,30,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、1#炉集气管操作台梯子","L型钢","300*150*6.5*9  L=2800",2,2800,300,150,6.5,9,{"v":5.04,"d":"5.040"},"无重合面",null,31,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、1#炉集气管操作台梯子","L型钢","300*150*6.5*9  L=1630",2,1630,300,150,6.5,9,2.934,"无重合面",null,32,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、1#炉集气管操作台梯子","L型钢","300*150*6.5*9  L=2510",2,2510,300,150,6.5,9,4.518,"无重合面",null,33,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、1#炉集气管操作台梯子","方（扁）钢","16*300*675",2,675,300,"675",null,null,{"v":2.6325,"d":"2.633"},"无重合面",null,34,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、1#炉集气管操作台梯子","方（扁）钢","10*300*894",2,894,300,"894",null,null,{"v":4.269744,"d":"4.270"},"无重合面",null,35,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、1#炉集气管操作台梯子","方（扁）钢","8*290*800",7,800,290,"800",null,null,12.208,"无重合面",null,36,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、1#炉集气管操作台梯子","圆钢","Φ16  L=13m",1,13000,16,{"$nulls":3},{"v":0.65312,"d":"0.653"},"无重合面",null,37,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、1#炉集气管操作台梯子","圆钢","Φ33.5*3.25   L=20m",1,20000,40,{"$nulls":3},2.512,"无重合面",null,38,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台铺板","其他","1224/39.25*3",{"$nulls":6},"需手动计算","无重合面",93.55,39,null,null,"A1822.030214CO003-5-1（根据吨钢重量计算面积）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=1200",48,1200,100,68,4.5,7.6,{"v":19.3536,"d":"19.354"},"无重合面",null,40,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=500",48,500,100,68,4.5,7.6,8.064,"无重合面",null,41,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=3700",12,3700,100,68,4.5,7.6,{"v":14.9184,"d":"14.918"},"无重合面",null,42,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=2060",84,2060,100,68,4.5,7.6,{"v":58.14144,"d":"58.141"},"无重合面",null,43,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=1500",42,1500,100,68,4.5,7.6,21.168,"无重合面",null,44,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台踢脚板","方（扁）钢","4*100   L=140m",1,140000,100,4,null,null,{"v":29.12,"d":"29.120"},"无重合面",null,45,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台围栏","圆钢","Φ16 L=140m",2,140000,16,{"$nulls":3},{"v":14.0672,"d":"14.067"},"无重合面",null,46,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台围栏","圆钢","Φ33.5*3.25   L=140m",1,140000,40,{"$nulls":3},17.584,"无重合面",null,47,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台菱形花纹板","其他","t5   150㎡",1,{"$nulls":5},"需手动计算","无重合面",{"v":150,"d":"150.00"},48,null,null,"A1822.030214CO003-5-1图上已表明花纹板面积","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=1196",2,1196,200,100,5.8,8,{"v":1.4352,"d":"1.435"},"无重合面",null,49,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=446",13,446,200,100,5.8,8,{"v":3.4788,"d":"3.479"},"无重合面",null,50,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=872",4,872,200,100,5.8,8,{"v":2.0928,"d":"2.093"},"无重合面",null,51,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台梁柱","方（扁）钢","16*200*200",24,200,16,200,null,null,{"v":2.0736,"d":"2.074"},"无重合面",null,52,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台梁柱","L型钢","200*200*8*12   L=1644",52,1644,200,200,8,12,{"v":68.3904,"d":"68.390"},"无重合面",null,53,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台梁柱","L型钢","160*65*8.5*8.5  L=3294",11,3294,160,65,8.5,8.5,{"v":16.3053,"d":"16.305"},"无重合面",null,54,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台梁柱","L型钢","200*200*8*12   L=3294",13,3294,200,200,8,12,{"v":34.2576,"d":"34.258"},"无重合面",null,55,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台梁柱","L型钢","160*65*8.5*8.5  L=1644",98,1644,160,65,8.5,8.5,{"v":72.5004,"d":"72.500"},"无重合面",null,56,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台梁柱","L型钢","160*65*8.5*8.5  L=1706",2,1706,160,65,8.5,8.5,{"v":1.5354,"d":"1.535"},"无重合面",null,57,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=970",2,970,200,100,5.8,8,1.164,"无重合面",null,58,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=819",2,819,200,100,5.8,8,{"v":0.9828,"d":"0.983"},"无重合面",null,59,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=1640",60,1640,200,100,5.8,8,{"v":59.04,"d":"59.040"},"无重合面",null,60,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、2#炉集气管操作台梁柱","L型钢","160*65*8.5*8.5  L=1640",60,1640,160,65,8.5,8.5,{"v":44.28,"d":"44.280"},"无重合面",null,61,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、2#炉集气管操作台梯子","方（扁）钢","8*270*800",8,800,270,"800",null,null,13.696,"无重合面",null,62,null,null,"A1822.030214CO003-6-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、2#炉集气管操作台梯子","圆钢","Φ16  L=1332",8,1332,16,{"$nulls":3},{"v":0.5353574400000001,"d":"0.535"},"无重合面",null,63,null,null,"A1822.030214CO003-6-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、2#炉集气管操作台梯子","圆钢","Φ33.5*3.25   L=7260",2,7260,40,{"$nulls":3},{"v":1.8237120000000002,"d":"1.824"},"无重合面",null,64,null,null,"A1822.030214CO003-6-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、2#炉集气管操作台梯子","L型钢","50*50*5   L=792",1,792,50,50,5,null,{"v":0.1584,"d":"0.158"},"无重合面",null,65,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、2#炉集气管操作台梯子","L型钢","200*100*5.5*8   L=1091",2,1091,200,100,5.5,8,{"v":1.3092,"d":"1.309"},"无重合面",null,66,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、2#炉集气管操作台梯子","方（扁）钢","8*800*1150",1,1150,800,"150",null,null,2.185,"无重合面",null,67,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、2#炉集气管操作台梯子","L型钢","4*100   L=2000",1,2000,100,{"$nulls":3},{"v":0.4,"d":"0.400"},"无重合面",null,68,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、2#炉集气管操作台梯子","L型钢","300*150*6.5*9  L=2800",2,2800,300,150,6.5,9,{"v":5.04,"d":"5.040"},"无重合面",null,69,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、2#炉集气管操作台梯子","L型钢","300*150*6.5*9  L=1630",2,1630,300,150,6.5,9,2.934,"无重合面",null,70,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、2#炉集气管操作台梯子","L型钢","300*150*6.5*9  L=2510",2,2510,300,150,6.5,9,4.518,"无重合面",null,71,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、2#炉集气管操作台梯子","方（扁）钢","16*300*675",2,675,300,"675",null,null,{"v":2.6325,"d":"2.633"},"无重合面",null,72,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、2#炉集气管操作台梯子","方（扁）钢","10*300*894",2,894,300,"894",null,null,{"v":4.269744,"d":"4.270"},"无重合面",null,73,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、2#炉集气管操作台梯子","方（扁）钢","8*290*800",7,800,290,"800",null,null,12.208,"无重合面",null,74,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、2#炉集气管操作台梯子","圆钢","Φ16  L=13m",1,13000,16,{"$nulls":3},{"v":0.65312,"d":"0.653"},"无重合面",null,75,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、2#炉集气管操作台梯子","圆钢","Φ33.5*3.25   L=20m",1,20000,40,{"$nulls":3},2.512,"无重合面",null,76,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台铺板","其他","1224/39.25*3",{"$nulls":6},"需手动计算","无重合面",93.55,77,null,null,"A1822.030214CO003-5-1（根据吨钢重量计算面积）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=1200",48,1200,100,68,4.5,7.6,{"v":19.3536,"d":"19.354"},"无重合面",null,78,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=500",48,500,100,68,4.5,7.6,8.064,"无重合面",null,79,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=3700",12,3700,100,68,4.5,7.6,{"v":14.9184,"d":"14.918"},"无重合面",null,80,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=2060",84,2060,100,68,4.5,7.6,{"v":58.14144,"d":"58.141"},"无重合面",null,81,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=1500",42,1500,100,68,4.5,7.6,21.168,"无重合面",null,82,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台踢脚板","方（扁）钢","4*100   L=140m",1,140000,100,4,null,null,{"v":29.12,"d":"29.120"},"无重合面",null,83,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台围栏","圆钢","Φ16 L=140m",2,140000,16,{"$nulls":3},{"v":14.0672,"d":"14.067"},"无重合面",null,84,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台围栏","圆钢","Φ33.5*3.25   L=140m",1,140000,40,{"$nulls":3},17.584,"无重合面",null,85,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台菱形花纹板","其他","t5   150㎡",1,{"$nulls":5},"需手动计算","无重合面",{"v":150,"d":"150.00"},86,null,null,"A1822.030214CO003-5-1图上已表明花纹板面积","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=1196",2,1196,200,100,5.8,8,{"v":1.4352,"d":"1.435"},"无重合面",null,87,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=446",13,446,200,100,5.8,8,{"v":3.4788,"d":"3.479"},"无重合面",null,88,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=872",4,872,200,100,5.8,8,{"v":2.0928,"d":"2.093"},"无重合面",null,89,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台梁柱","方（扁）钢","16*200*200",24,200,16,200,null,null,{"v":2.0736,"d":"2.074"},"无重合面",null,90,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台梁柱","L型钢","200*200*8*12   L=1644",52,1644,200,200,8,12,{"v":68.3904,"d":"68.390"},"无重合面",null,91,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台梁柱","L型钢","160*65*8.5*8.5  L=3294",11,3294,160,65,8.5,8.5,{"v":16.3053,"d":"16.305"},"无重合面",null,92,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台梁柱","L型钢","200*200*8*12   L=3294",13,3294,200,200,8,12,{"v":34.2576,"d":"34.258"},"无重合面",null,93,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台梁柱","L型钢","160*65*8.5*8.5  L=1644",98,1644,160,65,8.5,8.5,{"v":72.5004,"d":"72.500"},"无重合面",null,94,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台梁柱","L型钢","160*65*8.5*8.5  L=1706",2,1706,160,65,8.5,8.5,{"v":1.5354,"d":"1.535"},"无重合面",null,95,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=970",2,970,200,100,5.8,8,1.164,"无重合面",null,96,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=819",2,819,200,100,5.8,8,{"v":0.9828,"d":"0.983"},"无重合面",null,97,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=1640",60,1640,200,100,5.8,8,{"v":59.04,"d":"59.040"},"无重合面",null,98,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、3#炉集气管操作台梁柱","L型钢","160*65*8.5*8.5  L=1640",60,1640,160,65,8.5,8.5,{"v":44.28,"d":"44.280"},"无重合面",null,99,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、3#炉集气管操作台梯子","方（扁）钢","8*270*800",8,800,270,"800",null,null,13.696,"无重合面",null,100,null,null,"A1822.030214CO003-6-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、3#炉集气管操作台梯子","圆钢","Φ16  L=1332",8,1332,16,{"$nulls":3},{"v":0.5353574400000001,"d":"0.535"},"无重合面",null,101,null,null,"A1822.030214CO003-6-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、3#炉集气管操作台梯子","圆钢","Φ33.5*3.25   L=7260",2,7260,40,{"$nulls":3},{"v":1.8237120000000002,"d":"1.824"},"无重合面",null,102,null,null,"A1822.030214CO003-6-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、3#炉集气管操作台梯子","L型钢","50*50*5   L=792",1,792,50,50,5,null,{"v":0.1584,"d":"0.158"},"无重合面",null,103,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、3#炉集气管操作台梯子","L型钢","200*100*5.5*8   L=1091",2,1091,200,100,5.5,8,{"v":1.3092,"d":"1.309"},"无重合面",null,104,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、3#炉集气管操作台梯子","方（扁）钢","8*800*1150",1,1150,800,"150",null,null,2.185,"无重合面",null,105,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、3#炉集气管操作台梯子","L型钢","4*100   L=2000",1,2000,100,{"$nulls":3},{"v":0.4,"d":"0.400"},"无重合面",null,106,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、3#炉集气管操作台梯子","L型钢","300*150*6.5*9  L=2800",2,2800,300,150,6.5,9,{"v":5.04,"d":"5.040"},"无重合面",null,107,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、3#炉集气管操作台梯子","L型钢","300*150*6.5*9  L=1630",2,1630,300,150,6.5,9,2.934,"无重合面",null,108,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、3#炉集气管操作台梯子","L型钢","300*150*6.5*9  L=2510",2,2510,300,150,6.5,9,4.518,"无重合面",null,109,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、3#炉集气管操作台梯子","方（扁）钢","16*300*675",2,675,300,"675",null,null,{"v":2.6325,"d":"2.633"},"无重合面",null,110,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、3#炉集气管操作台梯子","方（扁）钢","10*300*894",2,894,300,"894",null,null,{"v":4.269744,"d":"4.270"},"无重合面",null,111,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、3#炉集气管操作台梯子","方（扁）钢","8*290*800",7,800,290,"800",null,null,12.208,"无重合面",null,112,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、3#炉集气管操作台梯子","圆钢","Φ16  L=13m",1,13000,16,{"$nulls":3},{"v":0.65312,"d":"0.653"},"无重合面",null,113,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、3#炉集气管操作台梯子","圆钢","Φ33.5*3.25   L=20m",1,20000,40,{"$nulls":3},2.512,"无重合面",null,114,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台铺板","其他","1224/39.25*3",{"$nulls":6},"需手动计算","无重合面",93.55,115,null,null,"A1822.030214CO003-5-1（根据吨钢重量计算面积）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=1200",48,1200,100,68,4.5,7.6,{"v":19.3536,"d":"19.354"},"无重合面",null,116,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=500",48,500,100,68,4.5,7.6,8.064,"无重合面",null,117,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=3700",12,3700,100,68,4.5,7.6,{"v":14.9184,"d":"14.918"},"无重合面",null,118,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=2060",84,2060,100,68,4.5,7.6,{"v":58.14144,"d":"58.141"},"无重合面",null,119,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台工字钢","L型钢","100*68*4.5*7.6  L=1500",42,1500,100,68,4.5,7.6,21.168,"无重合面",null,120,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台踢脚板","方（扁）钢","4*100   L=140m",1,140000,100,4,null,null,{"v":29.12,"d":"29.120"},"无重合面",null,121,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台围栏","圆钢","Φ16 L=140m",2,140000,16,{"$nulls":3},{"v":14.0672,"d":"14.067"},"无重合面",null,122,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台围栏","圆钢","Φ33.5*3.25   L=140m",1,140000,40,{"$nulls":3},17.584,"无重合面",null,123,null,null,"A1822.030214CO003-5-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台菱形花纹板","其他","t5   150㎡",1,{"$nulls":5},"需手动计算","无重合面",{"v":150,"d":"150.00"},124,null,null,"A1822.030214CO003-5-1图上已表明花纹板面积","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=1196",2,1196,200,100,5.8,8,{"v":1.4352,"d":"1.435"},"无重合面",null,125,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=446",13,446,200,100,5.8,8,{"v":3.4788,"d":"3.479"},"无重合面",null,126,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=872",4,872,200,100,5.8,8,{"v":2.0928,"d":"2.093"},"无重合面",null,127,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台梁柱","方（扁）钢","16*200*200",24,200,16,200,null,null,{"v":2.0736,"d":"2.074"},"无重合面",null,128,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台梁柱","L型钢","200*200*8*12   L=1644",52,1644,200,200,8,12,{"v":68.3904,"d":"68.390"},"无重合面",null,129,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台梁柱","L型钢","160*65*8.5*8.5  L=3294",11,3294,160,65,8.5,8.5,{"v":16.3053,"d":"16.305"},"无重合面",null,130,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台梁柱","L型钢","200*200*8*12   L=3294",13,3294,200,200,8,12,{"v":34.2576,"d":"34.258"},"无重合面",null,131,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台梁柱","L型钢","160*65*8.5*8.5  L=1644",98,1644,160,65,8.5,8.5,{"v":72.5004,"d":"72.500"},"无重合面",null,132,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台梁柱","L型钢","160*65*8.5*8.5  L=1706",2,1706,160,65,8.5,8.5,{"v":1.5354,"d":"1.535"},"无重合面",null,133,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=970",2,970,200,100,5.8,8,1.164,"无重合面",null,134,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=819",2,819,200,100,5.8,8,{"v":0.9828,"d":"0.983"},"无重合面",null,135,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台梁柱","L型钢","200*100*5.8*8  L=1640",60,1640,200,100,5.8,8,{"v":59.04,"d":"59.040"},"无重合面",null,136,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高21.49、4#炉集气管操作台梁柱","L型钢","160*65*8.5*8.5  L=1640",60,1640,160,65,8.5,8.5,{"v":44.28,"d":"44.280"},"无重合面",null,137,null,null,"A1822.030214CO003-4-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、4#炉集气管操作台梯子","方（扁）钢","8*270*800",8,800,270,"800",null,null,13.696,"无重合面",null,138,null,null,"A1822.030214CO003-6-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、4#炉集气管操作台梯子","圆钢","Φ16  L=1332",8,1332,16,{"$nulls":3},{"v":0.5353574400000001,"d":"0.535"},"无重合面",null,139,null,null,"A1822.030214CO003-6-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、4#炉集气管操作台梯子","圆钢","Φ33.5*3.25   L=7260",2,7260,40,{"$nulls":3},{"v":1.8237120000000002,"d":"1.824"},"无重合面",null,140,null,null,"A1822.030214CO003-6-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、4#炉集气管操作台梯子","L型钢","50*50*5   L=792",1,792,50,50,5,null,{"v":0.1584,"d":"0.158"},"无重合面",null,141,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、4#炉集气管操作台梯子","L型钢","200*100*5.5*8   L=1091",2,1091,200,100,5.5,8,{"v":1.3092,"d":"1.309"},"无重合面",null,142,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、4#炉集气管操作台梯子","方（扁）钢","8*800*1150",1,1150,800,"150",null,null,2.185,"无重合面",null,143,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、4#炉集气管操作台梯子","L型钢","4*100   L=2000",1,2000,100,{"$nulls":3},{"v":0.4,"d":"0.400"},"无重合面",null,144,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、4#炉集气管操作台梯子","L型钢","300*150*6.5*9  L=2800",2,2800,300,150,6.5,9,{"v":5.04,"d":"5.040"},"无重合面",null,145,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、4#炉集气管操作台梯子","L型钢","300*150*6.5*9  L=1630",2,1630,300,150,6.5,9,2.934,"无重合面",null,146,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、4#炉集气管操作台梯子","L型钢","300*150*6.5*9  L=2510",2,2510,300,150,6.5,9,4.518,"无重合面",null,147,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、4#炉集气管操作台梯子","方（扁）钢","16*300*675",2,675,300,"675",null,null,{"v":2.6325,"d":"2.633"},"无重合面",null,148,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、4#炉集气管操作台梯子","方（扁）钢","10*300*894",2,894,300,"894",null,null,{"v":4.269744,"d":"4.270"},"无重合面",null,149,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、4#炉集气管操作台梯子","方（扁）钢","8*290*800",7,800,290,"800",null,null,12.208,"无重合面",null,150,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、4#炉集气管操作台梯子","圆钢","Φ16  L=13m",1,13000,16,{"$nulls":3},{"v":0.65312,"d":"0.653"},"无重合面",null,151,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["标高17.52、4#炉集气管操作台梯子","圆钢","Φ33.5*3.25   L=20m",1,20000,40,{"$nulls":3},2.512,"无重合面",null,152,null,null,"A1822.030214CO003-7-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["1#电机车东西南北面",null,"0.7*0.3*4+1.15*9+1.15*9+0.7*0.3*4+4.67*1.27+4.67*1.27",{"$nulls":6},"",null,null,152,{"v":34.2418,"d":"34.24"},null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#电机车电气室外墙","其他","7.3*2.7*2+3.4*2.4*2",{"$nulls":6},"需手动计算","无重合面",55.74,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#电机车一层平台",null,"4.7*0.8*2+1.3*7.4",{"$nulls":6},"",null,null,152,null,34.28,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#电机车底部","其他","9*4.67",{"$nulls":6},"需手动计算","无重合面",42.03,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#电机车二层平台",null,"7.4*2.4+1.85*1+1.6*0.9+1.85*0.9",{"$nulls":6},"",null,null,152,null,{"v":45.43000000000001,"d":"45.43"},"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#电机车操作室外墙","其他","3.5*2.3*2+2.55*2.3*2",{"$nulls":6},"需手动计算","无重合面",27.83,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#电机车车顶","其他","3*4.3",{"$nulls":6},"需手动计算","无重合面",12.899999999999999,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#电机车楼梯与栏杆","其他","0.29*36*0.96+25",{"$nulls":6},"需手动计算","无重合面",35.0224,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#电机车行走支架","其他","0.58*1.95*4+2.3*2*4",{"$nulls":6},"需手动计算","无重合面",22.924,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#电机车东西南北面",null,"0.7*0.3*4+1.15*9+1.15*9+0.7*0.3*4+4.67*1.27+4.67*1.27",{"$nulls":6},"",null,null,152,{"v":34.2418,"d":"34.24"},null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#电机车电气室外墙","其他","7.3*2.7*2+3.4*2.4*2",{"$nulls":6},"需手动计算","无重合面",55.74,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#电机车一层平台",null,"4.7*0.8*2+1.3*7.4",{"$nulls":6},"",null,null,152,null,34.28,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#电机车底部","其他","9*4.67",{"$nulls":6},"需手动计算","无重合面",42.03,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#电机车二层平台",null,"7.4*2.4+1.85*1+1.6*0.9+1.85*0.9",{"$nulls":6},"",null,null,152,null,{"v":45.43000000000001,"d":"45.43"},"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#电机车操作室外墙","其他","3.5*2.3*2+2.55*2.3*2",{"$nulls":6},"需手动计算","无重合面",27.83,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#电机车车顶","其他","3*4.3",{"$nulls":6},"需手动计算","无重合面",12.899999999999999,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#电机车楼梯与栏杆","其他","0.29*36*0.96+25",{"$nulls":6},"需手动计算","无重合面",35.0224,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#电机车行走支架","其他","0.58*1.95*4+2.3*2*4",{"$nulls":6},"需手动计算","无重合面",22.924,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#电机车东西南北面",null,"0.7*0.3*4+1.15*9+1.15*9+0.7*0.3*4+4.67*1.27+4.67*1.27",{"$nulls":6},"",null,null,152,{"v":34.2418,"d":"34.24"},null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#电机车电气室外墙","其他","7.3*2.7*2+3.4*2.4*2",{"$nulls":6},"需手动计算","无重合面",55.74,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#电机车一层平台",null,"4.7*0.8*2+1.3*7.4",{"$nulls":6},"",null,null,152,null,34.28,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#电机车底部","其他","9*4.67",{"$nulls":6},"需手动计算","无重合面",42.03,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#电机车二层平台",null,"7.4*2.4+1.85*1+1.6*0.9+1.85*0.9",{"$nulls":6},"",null,null,152,null,{"v":45.43000000000001,"d":"45.43"},"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#电机车操作室外墙","其他","3.5*2.3*2+2.55*2.3*2",{"$nulls":6},"需手动计算","无重合面",27.83,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#电机车车顶","其他","3*4.3",{"$nulls":6},"需手动计算","无重合面",12.899999999999999,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#电机车楼梯与栏杆","其他","0.29*36*0.96+25",{"$nulls":6},"需手动计算","无重合面",35.0224,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#电机车行走支架","其他","0.58*1.95*4+2.3*2*4",{"$nulls":6},"需手动计算","无重合面",22.924,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#电机车东西南北面",null,"0.7*0.3*4+1.15*9+1.15*9+0.7*0.3*4+4.67*1.27+4.67*1.27",{"$nulls":6},"",null,null,152,{"v":34.2418,"d":"34.24"},null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#电机车电气室外墙","其他","7.3*2.7*2+3.4*2.4*2",{"$nulls":6},"需手动计算","无重合面",55.74,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#电机车一层平台",null,"4.7*0.8*2+1.3*7.4",{"$nulls":6},"",null,null,152,null,34.28,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#电机车底部","其他","9*4.67",{"$nulls":6},"需手动计算","无重合面",42.03,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#电机车二层平台",null,"7.4*2.4+1.85*1+1.6*0.9+1.85*0.9",{"$nulls":6},"",null,null,152,null,{"v":45.43000000000001,"d":"45.43"},"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#电机车操作室外墙","其他","3.5*2.3*2+2.55*2.3*2",{"$nulls":6},"需手动计算","无重合面",27.83,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#电机车车顶","其他","3*4.3",{"$nulls":6},"需手动计算","无重合面",12.899999999999999,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#电机车楼梯与栏杆","其他","0.29*36*0.96+25",{"$nulls":6},"需手动计算","无重合面",35.0224,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#电机车行走支架","其他","0.58*1.95*4+2.3*2*4",{"$nulls":6},"需手动计算","无重合面",22.924,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#台车侧面","其他","13.2*0.86*2+5*1.5*2+0.36*0.87*4",{"$nulls":6},"需手动计算","无重合面",38.956799999999994,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#台车八卦梁支架","其他","1.16*5.5*12+0.56*3.6*8+0.26*3.6*8",{"$nulls":6},"需手动计算","无重合面",100.176,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#台车面","其他","6.5*0.85*2+3.14*5*2",{"$nulls":6},"需手动计算","无重合面",42.45,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#台车大梁","其他","0.85*1.05*8",{"$nulls":6},"需手动计算","无重合面",7.14,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#台车小平台","其他","1*2.3*2",{"$nulls":6},"需手动计算","无重合面",4.6,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#台车栏杆","其他","6.6*0.38*2",{"$nulls":6},"需手动计算","无重合面",5.016,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#台车底","其他","13.2*5",{"$nulls":6},"需手动计算","无重合面",66,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#台车行走支架","其他","2.5*0.9*4+2.5*0.6*4",{"$nulls":6},"需手动计算","无重合面",15,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#台车侧面","其他","13.2*0.86*2+5*1.5*2+0.36*0.87*4",{"$nulls":6},"需手动计算","无重合面",38.956799999999994,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#台车八卦梁支架","其他","1.16*5.5*12+0.56*3.6*8+0.26*3.6*8",{"$nulls":6},"需手动计算","无重合面",100.176,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#台车台车面","其他","6.5*0.85*2+3.14*5*2",{"$nulls":6},"需手动计算","无重合面",42.45,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#台车大梁","其他","0.85*1.05*8",{"$nulls":6},"需手动计算","无重合面",7.14,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#台车小平台","其他","1*2.3*2",{"$nulls":6},"需手动计算","无重合面",4.6,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#台车栏杆","其他","6.6*0.38*2",{"$nulls":6},"需手动计算","无重合面",5.016,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#台车底","其他","13.2*5",{"$nulls":6},"需手动计算","无重合面",66,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#台车行走支架","其他","2.5*0.9*4+2.5*0.6*4",{"$nulls":6},"需手动计算","无重合面",15,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#台车侧面","其他","13.2*0.86*2+5*1.5*2+0.36*0.87*4",{"$nulls":6},"需手动计算","无重合面",38.956799999999994,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#台车八卦梁支架","其他","1.16*5.5*12+0.56*3.6*8+0.26*3.6*8",{"$nulls":6},"需手动计算","无重合面",100.176,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#台车台车面","其他","6.5*0.85*2+3.14*5*2",{"$nulls":6},"需手动计算","无重合面",42.45,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#台车大梁","其他","0.85*1.05*8",{"$nulls":6},"需手动计算","无重合面",7.14,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#台车小平台","其他","1*2.3*2",{"$nulls":6},"需手动计算","无重合面",4.6,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#台车栏杆","其他","6.6*0.38*2",{"$nulls":6},"需手动计算","无重合面",5.016,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#台车底","其他","13.2*5",{"$nulls":6},"需手动计算","无重合面",66,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#台车行走支架","其他","2.5*0.9*4+2.5*0.6*4",{"$nulls":6},"需手动计算","无重合面",15,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#台车侧面","其他","13.2*0.86*2+5*1.5*2+0.36*0.87*4",{"$nulls":6},"需手动计算","无重合面",38.956799999999994,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#台车八卦梁支架","其他","1.16*5.5*12+0.56*3.6*8+0.26*3.6*8",{"$nulls":6},"需手动计算","无重合面",100.176,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#台车台车面","其他","6.5*0.85*2+3.14*5*2",{"$nulls":6},"需手动计算","无重合面",42.45,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#台车大梁","其他","0.85*1.05*8",{"$nulls":6},"需手动计算","无重合面",7.14,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#台车小平台","其他","1*2.3*2",{"$nulls":6},"需手动计算","无重合面",4.6,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#台车栏杆","其他","6.6*0.38*2",{"$nulls":6},"需手动计算","无重合面",5.016,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#台车底","其他","13.2*5",{"$nulls":6},"需手动计算","无重合面",66,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#台车行走支架","其他","2.5*0.9*4+2.5*0.6*4",{"$nulls":6},"需手动计算","无重合面",15,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["5#台车侧面","其他","13.2*0.86*2+5*1.5*2+0.36*0.87*4",{"$nulls":6},"需手动计算","无重合面",38.956799999999994,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["5#台车八卦梁支架","其他","1.16*5.5*12+0.56*3.6*8+0.26*3.6*8",{"$nulls":6},"需手动计算","无重合面",100.176,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["5#台车台车面","其他","6.5*0.85*2+3.14*5*2",{"$nulls":6},"需手动计算","无重合面",42.45,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["5#台车大梁","其他","0.85*1.05*8",{"$nulls":6},"需手动计算","无重合面",7.14,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["5#台车小平台","其他","1*2.3*2",{"$nulls":6},"需手动计算","无重合面",4.6,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["5#台车栏杆","其他","6.6*0.38*2",{"$nulls":6},"需手动计算","无重合面",5.016,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["5#台车底","其他","13.2*5",{"$nulls":6},"需手动计算","无重合面",66,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["5#台车行走支架","其他","2.5*0.9*4+2.5*0.6*4",{"$nulls":6},"需手动计算","无重合面",15,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["6#台车侧面","其他","13.2*0.86*2+5*1.5*2+0.36*0.87*4",{"$nulls":6},"需手动计算","无重合面",38.956799999999994,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["6#台车八卦梁支架","其他","1.16*5.5*12+0.56*3.6*8+0.26*3.6*8",{"$nulls":6},"需手动计算","无重合面",100.176,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["6#台车台车面","其他","6.5*0.85*2+3.14*5*2",{"$nulls":6},"需手动计算","无重合面",42.45,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["6#台车大梁","其他","0.85*1.05*8",{"$nulls":6},"需手动计算","无重合面",7.14,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["6#台车小平台","其他","1*2.3*2",{"$nulls":6},"需手动计算","无重合面",4.6,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["6#台车栏杆","其他","6.6*0.38*2",{"$nulls":6},"需手动计算","无重合面",5.016,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["6#台车底","其他","13.2*5",{"$nulls":6},"需手动计算","无重合面",66,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["6#台车行走支架","其他","2.5*0.9*4+2.5*0.6*4",{"$nulls":6},"需手动计算","无重合面",15,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#拦焦车清门台车","其他","8*1.5*3",{"$nulls":6},"需手动计算","无重合面",36,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#拦焦车除尘挡板","其他","7*1.3*2",{"$nulls":6},"需手动计算","无重合面",18.2,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#拦焦车水箱房","其他","6.4*2.2*2+3*2.2*2",{"$nulls":6},"需手动计算","无重合面",41.36000000000001,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#拦焦车一层平台",null,"8.4*2+8.4*0.9+4.5*4.5",{"$nulls":6},"",null,null,152,null,89.22,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#拦焦车电阻室","其他","2.5*2.2*4",{"$nulls":6},"需手动计算","无重合面",22,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#拦焦车操作室","其他","2.5*2.2*4",{"$nulls":6},"需手动计算","无重合面",22,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#拦焦车电气室","其他","5.5*2.8*2+3*2.8*2",{"$nulls":6},"需手动计算","无重合面",47.599999999999994,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#拦焦车三层平台",null,"8.4*7",{"$nulls":6},"",null,null,152,null,{"v":117.60000000000001,"d":"117.60"},"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#拦焦车液压站","其他","3*3*2+6*3*2",{"$nulls":6},"需手动计算","无重合面",54,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#拦焦车清门台车","其他","8*1.5*3",{"$nulls":6},"需手动计算","无重合面",36,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#拦焦车除尘挡板","其他","7*1.3*2",{"$nulls":6},"需手动计算","无重合面",18.2,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#拦焦车水箱房","其他","6.4*2.2*2+3*2.2*2",{"$nulls":6},"需手动计算","无重合面",41.36000000000001,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#拦焦车一层平台",null,"8.4*2+8.4.*0.9+4.5*4.5",{"$nulls":6},"",null,null,152,null,89.22,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#拦焦车电阻室","其他","2.5*2.2*4",{"$nulls":6},"需手动计算","无重合面",22,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#拦焦车操作室","其他","2.5*2.2*4",{"$nulls":6},"需手动计算","无重合面",22,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#拦焦车电气室","其他","5.5*2.8*2+3*2.8*2",{"$nulls":6},"需手动计算","无重合面",47.599999999999994,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#拦焦车三层平台",null,"8.4*7",{"$nulls":6},"",null,null,152,null,{"v":117.60000000000001,"d":"117.60"},"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#拦焦车液压站","其他","3*3*2+6*3*2",{"$nulls":6},"需手动计算","无重合面",54,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#拦焦车清门台车","其他","8*1.5*3",{"$nulls":6},"需手动计算","无重合面",36,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#拦焦车除尘挡板","其他","7*1.3*2",{"$nulls":6},"需手动计算","无重合面",18.2,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#拦焦车水箱房","其他","6.4*2.2*2+3*2.2*2",{"$nulls":6},"需手动计算","无重合面",41.36000000000001,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#拦焦车一层平台",null,"8.4*2+8.4.*0.9+4.5*4.5",{"$nulls":6},"",null,null,152,null,89.22,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#拦焦车电阻室","其他","2.5*2.2*4",{"$nulls":6},"需手动计算","无重合面",22,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#拦焦车操作室","其他","2.5*2.2*4",{"$nulls":6},"需手动计算","无重合面",22,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#拦焦车电气室","其他","5.5*2.8*2+3*2.8*2",{"$nulls":6},"需手动计算","无重合面",47.599999999999994,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#拦焦车三层平台",null,"8.4*7",{"$nulls":6},"",null,null,152,null,{"v":117.60000000000001,"d":"117.60"},"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#拦焦车液压站","其他","3*3*2+6*3*2",{"$nulls":6},"需手动计算","无重合面",54,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#拦焦车清门台车","其他","8*1.5*3",{"$nulls":6},"需手动计算","无重合面",36,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#拦焦车除尘挡板","其他","7*1.3*2",{"$nulls":6},"需手动计算","无重合面",18.2,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#拦焦车水箱房","其他","6.4*2.2*2+3*2.2*2",{"$nulls":6},"需手动计算","无重合面",41.36000000000001,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#拦焦车一层平台",null,"8.4*2+8.4.*0.9+4.5*4.5",{"$nulls":6},"",null,null,152,null,89.22,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#拦焦车电阻室","其他","2.5*2.2*4",{"$nulls":6},"需手动计算","无重合面",22,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#拦焦车操作室","其他","2.5*2.2*4",{"$nulls":6},"需手动计算","无重合面",22,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#拦焦车电气室","其他","5.5*2.8*2+3*2.8*2",{"$nulls":6},"需手动计算","无重合面",47.599999999999994,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#拦焦车三层平台",null,"8.4*7",{"$nulls":6},"",null,null,152,null,{"v":117.60000000000001,"d":"117.60"},"现场测量计算","一般性腐蚀","环氧富锌漆"]
["4#拦焦车液压站","其他","3*3*2+6*3*2",{"$nulls":6},"需手动计算","无重合面",54,152,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#加煤车操作室","其他","4*3*4",{"$nulls":6},"需手动计算","无重合面",48,153,null,null,"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["1#加煤车液压站","其他","8.27*3+8.27*3*2+3*3*2",{"$nulls":6},"需手动计算","无重合面",92.42999999999999,154,null,null,"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["1#加煤车电气室","其他","9.3*3+9.3*3*2+3*3*2",{"$nulls":6},"需手动计算","无重合面",101.7,155,null,null,"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["1#加煤车二层平台",null,"15.2*14－8.27*3－9.3*3+15.2*14",{"$nulls":6},"",null,null,156,null,372.89,"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["1#加煤车三层平台",null,"1.09*14+0.9*2.6+3.05*2.6+1.16*2.6",{"$nulls":6},"",null,null,157,null,{"v":57.092,"d":"57.09"},"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["1#加煤车煤斗","其他","2.3*3.6*4*4",{"$nulls":6},"需手动计算","无重合面",132.48,158,null,null,"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["1#加煤车东西面挡板","其他","2*15*2-3.41*2-1.74*2-2.3*2",{"$nulls":6},"需手动计算","无重合面",45.1,159,null,null,"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["2#加煤车操作室","其他","4*3*4",{"$nulls":6},"需手动计算","无重合面",48,160,null,null,"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["2#加煤车液压站","其他","8.27*3+8.27*3*2+3*3*2",{"$nulls":6},"需手动计算","无重合面",92.42999999999999,161,null,null,"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["2#加煤车电气室","其他","9.3*3+9.3*3*2+3*3*2",{"$nulls":6},"需手动计算","无重合面",101.7,162,null,null,"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["2#加煤车二层平台",null,"15.2*14－8.27*3－9.3*3+15.2*14",{"$nulls":6},"",null,null,163,null,372.89,"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["2#加煤车三层平台",null,"1.09*14+0.9*2.6+3.05*2.6+1.16*2.6",{"$nulls":6},"",null,null,164,null,{"v":57.092,"d":"57.09"},"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["2#加煤车煤斗","其他","2.3*3.6*4*4",{"$nulls":6},"需手动计算","无重合面",132.48,165,null,null,"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["2#加煤车东西面挡板","其他","2*15*2-3.41*2-1.74*2-2.3*2",{"$nulls":6},"需手动计算","无重合面",45.1,166,null,null,"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["3#加煤车操作室","其他","4*3*4",{"$nulls":6},"需手动计算","无重合面",48,167,null,null,"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["3#加煤车液压站","其他","8.27*3+8.27*3*2+3*3*2",{"$nulls":6},"需手动计算","无重合面",92.42999999999999,168,null,null,"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["3#加煤车电气室","其他","9.3*3+9.3*3*2+3*3*2",{"$nulls":6},"需手动计算","无重合面",101.7,169,null,null,"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["3#加煤车二层平台",null,"15.2*14－8.27*3－9.3*3+15.2*14",{"$nulls":6},"",null,null,170,null,372.89,"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["3#加煤车三层平台",null,"1.09*14+0.9*2.6+3.05*2.6+1.16*2.6",{"$nulls":6},"",null,null,171,null,{"v":57.092,"d":"57.09"},"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["3#加煤车煤斗","其他","2.3*3.6*4*4",{"$nulls":6},"需手动计算","无重合面",132.48,172,null,null,"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["3#加煤车东西面挡板","其他","2*15*2-3.41*2-1.74*2-2.3*2",{"$nulls":6},"需手动计算","无重合面",45.1,173,null,null,"现场测量计算","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["1#推焦车一层平台",null,"20*21*2",{"$nulls":6},"",null,null,173,null,{"v":840,"d":"840.00"},"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#推焦车二层平台",null,"15*10+3*11+10*3-2.1*4.6",{"$nulls":6},"",null,null,173,null,406.68,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#推焦车电气室电阻室","其他","3*6*2+3*5.5*2+5.5*6",{"$nulls":6},"需手动计算","无重合面",102,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#推焦车操作室","其他","3*2.1*2+3*4.6*2",{"$nulls":6},"需手动计算","无重合面",40.2,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#推焦车除尘管","其他","8*1.2*2+8*1.4*2+9*12*2",{"$nulls":6},"需手动计算","无重合面",257.6,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#推焦车平煤杆防护板","其他","21.2*0.8",{"$nulls":6},"需手动计算","无重合面",16.96,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#推焦车南面除尘罩","其他","9*3.8+9*2.85",{"$nulls":6},"需手动计算","无重合面",59.849999999999994,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#推焦车北面除尘罩","其他","9*3.8+9*2.85",{"$nulls":6},"需手动计算","无重合面",59.849999999999994,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#推焦车液压站","其他","10*3*3+3*3*2",{"$nulls":6},"需手动计算","无重合面",108,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#推焦车水箱房","其他","3*6.5*3+3*3*2",{"$nulls":6},"需手动计算","无重合面",76.5,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#推焦车炉门工休息室","其他","3*2.1*5",{"$nulls":6},"需手动计算","无重合面",31.500000000000004,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#推焦车储气罐","其他","2*3.14*0.8*0.8+2*3.14*0.8*5",{"$nulls":6},"需手动计算","无重合面",29.139200000000006,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#推焦车推焦杆防护板","其他","18*2*2",{"$nulls":6},"需手动计算","无重合面",72,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["1#推焦车大梁支架","其他","17.5*0.5*4+25*1*3",{"$nulls":6},"需手动计算","无重合面",110,173,null,null,"预估值","一般性腐蚀","环氧富锌漆"]
["2#推焦车一层平台","其他","20*21*2",{"$nulls":6},"需手动计算","无重合面",null,173,null,{"v":840,"d":"840.00"},"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#推焦车二层平台","其他","15*10+3*11+10*3-2.1*4.6",{"$nulls":6},"需手动计算","无重合面",null,173,null,406.68,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#推焦车电气室电阻室","其他","3*6*2+3*5.5*2+5.5*6",{"$nulls":6},"需手动计算","无重合面",102,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#推焦车操作室","其他","3*2.1*2+3*4.6*2",{"$nulls":6},"需手动计算","无重合面",40.2,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#推焦车除尘管","其他","8*1.2*2+8*1.4*2+9*12*2",{"$nulls":6},"需手动计算","无重合面",257.6,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#推焦车平煤杆防护板","其他","21.2*0.8",{"$nulls":6},"需手动计算","无重合面",16.96,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#推焦车南面除尘罩","其他","9*3.8+9*2.85",{"$nulls":6},"需手动计算","无重合面",59.849999999999994,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#推焦车北面除尘罩","其他","9*3.8+9*2.85",{"$nulls":6},"需手动计算","无重合面",59.849999999999994,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#推焦车液压站","其他","10*3*3+3*3*2",{"$nulls":6},"需手动计算","无重合面",108,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#推焦车水箱房","其他","3*6.5*3+3*3*2",{"$nulls":6},"需手动计算","无重合面",76.5,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#推焦车炉门工休息室","其他","3*2.1*5",{"$nulls":6},"需手动计算","无重合面",31.500000000000004,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#推焦车储气罐","其他","2*3.14*0.8*0.8+2*3.14*0.8*5",{"$nulls":6},"需手动计算","无重合面",29.139200000000006,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#推焦车推焦杆防护板","其他","18*2*2",{"$nulls":6},"需手动计算","无重合面",72,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["2#推焦车大梁支架","其他","17.5*0.5*4+25*1*3",{"$nulls":6},"需手动计算","无重合面",110,173,null,null,"预估值","一般性腐蚀","环氧富锌漆"]
["3#推焦车一层平台","其他","20*21*2",{"$nulls":6},"需手动计算","无重合面",null,173,null,{"v":840,"d":"840.00"},"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#推焦车二层平台","其他","15*10+3*11+10*3-2.1*4.6",{"$nulls":6},"需手动计算","无重合面",null,173,null,406.68,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#推焦车电气室电阻室","其他","3*6*2+3*5.5*2+5.5*6",{"$nulls":6},"需手动计算","无重合面",102,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#推焦车操作室","其他","3*2.1*2+3*4.6*2",{"$nulls":6},"需手动计算","无重合面",40.2,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#推焦车除尘管","其他","8*1.2*2+8*1.4*2+9*12*2",{"$nulls":6},"需手动计算","无重合面",257.6,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#推焦车平煤杆防护板","其他","21.2*0.8",{"$nulls":6},"需手动计算","无重合面",16.96,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#推焦车南面除尘罩","其他","9*3.8+9*2.85",{"$nulls":6},"需手动计算","无重合面",59.849999999999994,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#推焦车北面除尘罩","其他","9*3.8+9*2.85",{"$nulls":6},"需手动计算","无重合面",59.849999999999994,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#推焦车液压站","其他","10*3*3+3*3*2",{"$nulls":6},"需手动计算","无重合面",108,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#推焦车水箱房","其他","3*6.5*3+3*3*2",{"$nulls":6},"需手动计算","无重合面",76.5,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#推焦车炉门工休息室","其他","3*2.1*5",{"$nulls":6},"需手动计算","无重合面",31.500000000000004,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#推焦车储气罐","其他","2*3.14*0.8*0.8+2*3.14*0.8*5",{"$nulls":6},"需手动计算","无重合面",29.139200000000006,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#推焦车推焦杆防护板","其他","18*2*2",{"$nulls":6},"需手动计算","无重合面",72,173,null,null,"现场测量计算","一般性腐蚀","环氧富锌漆"]
["3#推焦车大梁支架","其他","17.5*0.5*4+25*1*3",{"$nulls":6},"需手动计算","无重合面",110,173,null,null,"预估值","一般性腐蚀","环氧富锌漆"]
["机侧水封槽","其他","800*15。长800米，每米防腐面积为15平方米",{"$nulls":6},"需手动计算","无重合面",12000,173,null,null,"包括水封槽以及钢结构支架","一般性腐蚀","环氧富锌漆"]
["101皮带除尘装置","其他","5.3*4.2+5.3*12*2+4.2*12*2",{"$nulls":6},"需手动计算","无重合面",250.26,173,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["102皮带除尘装置","其他","2.8*2.7+2.8*10*2+2.7*10*2",{"$nulls":6},"需手动计算","无重合面",117.56,173,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["103皮带除尘装置","其他","7*7+7*12*4",{"$nulls":6},"需手动计算","无重合面",385,173,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["筛分楼除尘装置","其他","22*7.7+22*12*2+7.7*12*2",{"$nulls":6},"需手动计算","无重合面",882.2,173,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["104皮带除尘装置","其他","3*2.7+3*9*2+2.7*2*2",{"$nulls":6},"需手动计算","无重合面",72.9,173,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["105皮带除尘装置","其他","3*2.7+3*9*2+2.7*2*2",{"$nulls":6},"需手动计算","无重合面",72.9,173,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["1#煤塔除尘","其他","4.1*4+4.1*10*2+4*10*2",{"$nulls":6},"需手动计算","无重合面",178.4,173,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["2#煤塔除尘","其他","4.1*4+4.1*10*2+4*10*2",{"$nulls":6},"需手动计算","无重合面",178.4,173,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["110皮带","其他","长度35米，每米支架防腐面积4㎡，共计35*4",{"$nulls":6},"需手动计算","无重合面",140,173,null,null,"包括皮带支架、溜槽、皮带通廊、通廊钢结构立柱及转运站楼梯扶手等","一般性腐蚀","环氧富锌漆"]
["111皮带","其他","长度35米，每米支架防腐面积4㎡，共计35*4",{"$nulls":6},"需手动计算","无重合面",140,173,null,null,"包括皮带支架、溜槽、皮带通廊、通廊钢结构立柱及转运站楼梯扶手等","一般性腐蚀","环氧富锌漆"]
["一回转皮带","其他","长度10米，每米支架防腐面积4㎡，共计10*4",{"$nulls":6},"需手动计算","无重合面",40,173,null,null,"包括皮带支架、溜槽、皮带通廊、通廊钢结构立柱及转运站楼梯扶手等","一般性腐蚀","环氧富锌漆"]
["二回转皮带","其他","长度10米，每米支架防腐面积4㎡，共计10*4",{"$nulls":6},"需手动计算","无重合面",40,173,null,null,"包括皮带支架、溜槽、皮带通廊、通廊钢结构立柱及转运站楼梯扶手等","一般性腐蚀","环氧富锌漆"]
["T101皮带","其他","长度10米，每米支架防腐面积4㎡，共计10*4",{"$nulls":6},"需手动计算","无重合面",40,173,null,null,"包括皮带支架、溜槽、皮带通廊、通廊钢结构立柱及转运站楼梯扶手等","一般性腐蚀","环氧富锌漆"]
["T102皮带","其他","长度50米，每米支架防腐面积4㎡，每米通廊防腐面积40㎡，共计50*4+50*40",{"$nulls":6},"需手动计算","无重合面",2200,173,null,null,"包括皮带支架、溜槽、皮带通廊、通廊钢结构立柱及转运站楼梯扶手等","一般性腐蚀","环氧富锌漆"]
["汇总",{"$nulls":8},{"v":2178.19189376,"d":"2178.19"},null,2233.33,null,{"v":0,"d":"0.00"},{"v":1289.946,"d":"1289.95"}]
["工程量汇总",{"$nulls":8},{"v":4411.52189376,"d":"钢结构： 4411.52㎡"},{"$nulls":3},{"v":1289.946,"d":"平台： 1289.95㎡"}]

{"sheet":"3.化产-管道","index":2,"n_rows":172,"n_cols":11,"rows_kept":172,"merged":[[0,0,0,8]],"flags":["formulas_cached_only"]}
["2024年广西钢铁集团焦化厂除锈防腐检修工程-化产管道"]
["车间","序号","区域","施工环境描述","材料名称","直径mm","材料长度\n","面积/㎡","备注","腐蚀程度","推荐采用防腐涂料"]
["化产环水",1,"初冷器电捕","作业高度约8m，作业环境存在煤气中毒、高空坠落等危险源。","初冷器出口煤气管",1020,94.5,{"v":302.6646,"d":"302.66"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",2,"初冷器电捕","作业高度约4m，作业环境存在煤气中毒、高空坠落等危险源。","电捕旁通煤气管",1020,70,{"v":224.19600000000003,"d":"224.20"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",2,"初冷器电捕","作业高度约4m，作业环境存在煤气中毒、高空坠落等危险源。","煤气鼓风机出口煤气管",1620,307,{"v":1561.6476,"d":"1561.65"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",3,"初冷器电捕","作业高度约4m，作业环境存在煤气中毒、高空坠落等危险源。","电捕进口至煤气鼓风机煤气管",1820,86,{"v":491.4728,"d":"491.47"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",4,"初冷器电捕","作业高度约3-17m，作业环境存在煤气中毒、高空坠落等危险源。","电捕焦油器1",6200,14.2,{"v":276.4456,"d":"276.45"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",5,"初冷器电捕","作业高度约3-17m，作业环境存在煤气中毒、高空坠落等危险源。","电捕焦油器2",6200,14.2,{"v":276.4456,"d":"276.45"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",6,"初冷器电捕","作业高度约3-17m，作业环境存在煤气中毒、高空坠落等危险源。","电捕焦油器3",6200,14.2,{"v":276.4456,"d":"276.45"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",7,"初冷器电捕","作业高度约3-17m，作业环境存在煤气中毒、高空坠落等危险源。","电捕焦油器4",6200,14.2,{"v":276.4456,"d":"276.45"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",8,"初冷器电捕","作业高度约8m，作业环境存在煤气中毒、高空坠落等危险源。","大循环煤气管",630,300,593.46,null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",9,"洗涤一系","作业高度约8m，作业环境存在煤气中毒、高空坠落等危险源。","（脱硫塔、两用塔、洗氨塔）进富液槽富液管",480,70,{"v":105.504,"d":"105.50"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",10,"洗涤一系","作业高度约1m，作业环境存在煤气中毒、高空坠落等危险源。","富液泵进口富液管",530,21,{"v":34.9482,"d":"34.95"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",11,"洗涤一系","作业高度约6m，作业环境存在煤气中毒、高空坠落等危险源。","富液泵出口至脱酸蒸氨富液管",325,229.1,{"v":233.79655000000002,"d":"233.80"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",11,"洗涤一系","作业高度约0.5m，作业环境存在煤气中毒、高空坠落等危险源。","脱酸蒸氨二楼富液至脱氨水富液换热器富液管",219,8.6,{"v":5.913876,"d":"5.91"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",11,"洗涤一系","作业高度约0.5m，作业环境存在煤气中毒、高空坠落等危险源。","脱酸蒸氨二楼换热器富液进口富液管",133,15.1,{"v":6.306062000000001,"d":"6.31"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",12,"洗涤二系","作业高度约8m，作业环境存在煤气中毒、高空坠落等危险源。","（脱硫塔、两用塔、洗氨塔）进富液槽富液管",480,70,{"v":105.504,"d":"105.50"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",13,"洗涤二系","作业高度约1m，作业环境存在煤气中毒、高空坠落等危险源。","富液泵进口富液管",530,21,{"v":34.9482,"d":"34.95"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",14,"洗涤二系","作业高度约6m，作业环境存在煤气中毒、高空坠落等危险源。","富液泵出口至脱酸蒸氨富液管",325,191.8,{"v":195.73190000000005,"d":"195.73"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",14,"洗涤二系","作业高度约0.5m，作业环境存在煤气中毒、高空坠落等危险源。","脱酸蒸氨二楼富液至脱氨水富液换热器富液管",219,8.6,{"v":5.913876,"d":"5.91"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",14,"洗涤二系","作业高度约0.5m，作业环境存在煤气中毒、高空坠落等危险源。","脱酸蒸氨二楼换热器富液进口富液管",133,15.1,{"v":6.306062000000001,"d":"6.31"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",15,"洗涤一系","作业高度约10m，作业环境存在煤气中毒、高空坠落等危险源。","一系洗涤煤气管至精脱硫点煤气管",1620,260,{"v":1322.568,"d":"1322.57"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",15,"精脱硫一系","作业高度约3m，作业环境存在煤气中毒、高空坠落等危险源。","一系精脱硫塔煤气进出口管",920,40,{"v":115.552,"d":"115.55"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",15,"精脱硫一系","作业高度约1m，作业环境存在煤气中毒、高空坠落等危险源。","一系精脱硫塔再生煤气管道",480,58,{"v":87.41760000000001,"d":"87.42"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",16,"精脱硫一系","作业高度约15m，作业环境存在煤气中毒、高空坠落等危险源。","精脱硫至TOP1点煤气管",2020,250,{"v":1585.7,"d":"1585.70"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",17,"洗涤二系","作业高度约10m，作业环境存在煤气中毒、高空坠落等危险源。","二系洗涤煤气管至精脱硫点煤气管",1620,260,{"v":1322.568,"d":"1322.57"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",17,"精脱硫二系","作业高度约3m，作业环境存在煤气中毒、高空坠落等危险源。","二系精脱硫塔煤气进出口管",920,40,{"v":115.552,"d":"115.55"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",17,"精脱硫二系","作业高度约1m，作业环境存在煤气中毒、高空坠落等危险源。","二系精脱硫塔再生煤气管道",480,58,{"v":87.41760000000001,"d":"87.42"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",18,"洗涤一系","作业高度约5-45m，作业环境存在煤气中毒、高空坠落等危险源。","一系洗苯塔",6000,40,781.86,"加顶部","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",19,"洗涤二系","作业高度约5-45m，作业环境存在煤气中毒、高空坠落等危险源。","二系洗苯塔",6000,40,781.86,"加顶部","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",20,"洗涤一系","作业高度约1-7m，作业环境存在煤气中毒、高空坠落等危险源。","一系富液槽",8000,7,226.08,"加顶部","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",21,"洗涤二系","作业高度约1-7m，作业环境存在煤气中毒、高空坠落等危险源。","二系富液槽",8000,7,226.08,"加顶部","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",21,"脱酸蒸氨","作业高度约1-5m，作业环境存在氨水泄漏、高空坠落等危险源。","富液陶瓷过滤器1",3200,6,{"v":68.3264,"d":"68.33"},"加底、顶部","一般性腐蚀","环氧富锌漆"]
["化产环水",21,"脱酸蒸氨","作业高度约1-5m，作业环境存在氨水泄漏、高空坠落等危险源。","富液陶瓷过滤器2",3200,6,{"v":68.3264,"d":"68.33"},"加底、顶部","一般性腐蚀","环氧富锌漆"]
["化产环水",21,"脱酸蒸氨","作业高度约1-5m，作业环境存在氨水泄漏、高空坠落等危险源。","富液陶瓷过滤器3",3200,6,{"v":68.3264,"d":"68.33"},"加底、顶部","一般性腐蚀","环氧富锌漆"]
["化产环水",21,"脱酸蒸氨","作业高度约1-5m，作业环境存在氨水泄漏、高空坠落等危险源。","富液陶瓷过滤器4",3200,6,{"v":68.3264,"d":"68.33"},"加底、顶部","一般性腐蚀","环氧富锌漆"]
["化产环水",21,"脱酸蒸氨","作业高度约1-5m，作业环境存在氨水泄漏、高空坠落等危险源。","富液陶瓷过滤器5",3200,6,{"v":68.3264,"d":"68.33"},"加底、顶部","一般性腐蚀","环氧富锌漆"]
["化产环水",21,"脱酸蒸氨","作业高度约1-6m，作业环境存在氨水泄漏、高空坠落等危险源。","脱酸蒸氨一段贫液至回流贫液管",159,50,{"v":24.963,"d":"24.96"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"脱酸蒸氨","作业高度约1m，作业环境存在氨水泄漏、高空坠落等危险源。","脱酸蒸氨至一段贫液至洗涤一系二段贫液",219,190.5,{"v":130.99923,"d":"131.00"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"脱酸蒸氨","作业高度约1m，作业环境存在氨水泄漏、高空坠落等危险源。","脱酸蒸氨至一段贫液至洗涤二系二段贫液",219,152.5,{"v":104.86815000000001,"d":"104.87"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"脱酸蒸氨","作业高度约7m，作业环境存在氨水泄漏、高空坠落等危险源。","脱酸蒸氨旧装车平台至洗涤一系脱氨水管",159,111,{"v":55.417860000000005,"d":"55.42"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"脱酸蒸氨","作业高度约7m，作业环境存在氨水泄漏、高空坠落等危险源。","脱酸蒸氨旧装车平台至洗涤二系脱氨水管",159,75.5,{"v":37.69413,"d":"37.69"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"脱酸蒸氨","作业高度约1m，作业环境存在氨水泄漏、高空坠落等危险源。","脱酸蒸氨脱氨水换热器零星脱氨水管",159,20,{"v":9.9852,"d":"9.99"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约2-7m，作业环境存在氨水泄漏、高空坠落等危险源。","中间槽到二号槽剩余氨水管",273,13,{"v":11.143860000000002,"d":"11.14"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约2-7m，作业环境存在氨水泄漏、高空坠落等危险源。","中间槽到一号槽剩余氨水管",273,7,{"v":6.000540000000001,"d":"6.00"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约2-7m，作业环境存在氨水泄漏、高空坠落等危险源。","一二号槽到大槽剩余氨水管",273,40,{"v":34.2888,"d":"34.29"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约2-7m，作业环境存在氨水泄漏、高空坠落等危险源。","二号槽到大槽剩余氨水管",273,29.5,{"v":25.287990000000004,"d":"25.29"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约2-7m，作业环境存在氨水泄漏、高空坠落等危险源。","大槽到陶瓷过滤器剩余氨水管",273,21,{"v":18.001620000000003,"d":"18.00"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约2-7m，作业环境存在氨水泄漏、高空坠落等危险源。","一二号槽到陶瓷过滤器剩余氨水管",273,13.5,{"v":11.572470000000001,"d":"11.57"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约1m，作业环境存在氨水泄漏、高空坠落等危险源。","二系剩余氨水中间泵进口管",273,8,{"v":6.857760000000001,"d":"6.86"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约2-7m，作业环境存在氨水泄漏、高空坠落等危险源。","二系剩余氨水中间泵出口管至气浮除油机",159,16,{"v":7.988160000000001,"d":"7.99"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约1-3m，作业环境存在氨水泄漏、高空坠落等危险源。","二系高压氨水泵进口管",108,7,{"v":2.3738400000000004,"d":"2.37"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约3-7m，作业环境存在氨水泄漏、高空坠落等危险源。","二系高压氨水泵出口管到管廊架",108,15,{"v":5.0868,"d":"5.09"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约1m，作业环境存在氨水泄漏、高空坠落等危险源。","二系剩余氨水泵进口管",219,6,{"v":4.12596,"d":"4.13"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约2m，作业环境存在氨水泄漏、高空坠落等危险源。","二系剩余氨水泵出口管至陶瓷过滤器",159,38,{"v":18.971880000000002,"d":"18.97"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约1-10m，作业环境存在氨水泄漏、高空坠落等危险源。","冷凝渣泵出口管至三台刮渣机",108,69,{"v":23.39928,"d":"23.40"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约1-7m，作业环境存在氨水泄漏、高空坠落等危险源。","冷凝渣泵刮渣机底部至渣泵进口管",108,43,{"v":14.582160000000002,"d":"14.58"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约1-5m，作业环境存在氨水泄漏、高空坠落等危险源。","乳化液泵分离器至泵进口",325,38,{"v":38.77900000000001,"d":"38.78"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约1-7m，作业环境存在氨水泄漏、高空坠落等危险源。","乳化液泵出口至管廊架",325,56,{"v":57.14800000000001,"d":"57.15"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约2-7m，作业环境存在氨水泄漏、高空坠落等危险源。","陶瓷过滤器出口至管廊架",159,51,{"v":25.46226,"d":"25.46"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约2-7m，作业环境存在氨水泄漏、高空坠落等危险源。","循环氨水泵分离槽至三台循环氨水泵进口",1020,23,{"v":73.6644,"d":"73.66"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约1-3m，作业环境存在氨水泄漏、高空坠落等危险源。","循环氨水泵循环氨水泵出口",530,20,{"v":33.284000000000006,"d":"33.28"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约8m，作业环境存在氨水泄漏、高空坠落等危险源。","刮渣机进口管",820,23,{"v":59.2204,"d":"59.22"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"二系焦油氨水分离区","作业高度约2-7m，作业环境存在氨水泄漏、高空坠落等危险源。","刮渣机出口至分离器",1020,36,{"v":115.30080000000001,"d":"115.30"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约1-3m，作业环境存在氨水泄漏、高空坠落等危险源。","2台高压氨水泵进出口管",108,53,{"v":17.973360000000003,"d":"17.97"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约3-7m，作业环境存在氨水泄漏、高空坠落等危险源。","2台剩余氨水中间泵出口管",159,3,{"v":1.4977800000000001,"d":"1.50"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约1m，作业环境存在氨水泄漏、高空坠落等危险源。","2台剩余氨水中间泵进口管管",273,5,{"v":4.2861,"d":"4.29"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约2m，作业环境存在氨水泄漏、高空坠落等危险源。","2台剩余氨水泵出口管",159,60,{"v":29.955600000000004,"d":"29.96"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约1-3m，作业环境存在氨水泄漏、高空坠落等危险源。","4台循环氨水泵进出口小管",530,82,{"v":136.4644,"d":"136.46"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约1m，作业环境存在氨水泄漏、高空坠落等危险源。","4台循环氨水泵进口大管",1020,22,{"v":70.4616,"d":"70.46"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约1-5m，作业环境存在氨水泄漏、高空坠落等危险源。","2台乳化液泵进口管",273,40,{"v":34.2888,"d":"34.29"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约1-7m，作业环境存在氨水泄漏、高空坠落等危险源。","2台乳化液泵出口管",273,46,{"v":39.432120000000005,"d":"39.43"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约2-7m，作业环境存在氨水泄漏、高空坠落等危险源。","刮渣机出口大管",1020,38,{"v":121.70640000000002,"d":"121.71"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约2-7m，作业环境存在氨水泄漏、高空坠落等危险源。","刮渣机出口小管",830,35,{"v":91.217,"d":"91.22"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约8m，作业环境存在氨水泄漏、高空坠落等危险源。","刮渣机进口小管",830,15,{"v":39.092999999999996,"d":"39.09"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约8m，作业环境存在氨水泄漏、高空坠落等危险源。","刮渣机进口总管",1020,32,{"v":102.48960000000001,"d":"102.49"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约1m，作业环境存在氨水泄漏、高空坠落等危险源。","刮渣机排苯渣管",89,47,{"v":13.13462,"d":"13.13"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约8m，作业环境存在氨水泄漏、高空坠落等危险源。","刮渣机初冷器两系乳化液回流管",325,70,{"v":71.43500000000002,"d":"71.44"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约2-7m，作业环境存在氨水泄漏、高空坠落等危险源。","气浮除油机出口管",273,10,{"v":8.5722,"d":"8.57"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约2-7m，作业环境存在氨水泄漏、高空坠落等危险源。","气浮除油机去地槽管",159,20,{"v":9.9852,"d":"9.99"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约1-3m，作业环境存在氨水泄漏、高空坠落等危险源。","气浮除油机接剩余氨水泵进口管",219,20,{"v":13.753200000000001,"d":"13.75"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约1m，作业环境存在氨水泄漏、高空坠落等危险源。","气浮除油机射流泵进出口管",108,30,{"v":10.1736,"d":"10.17"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约1-3m，作业环境存在氨水泄漏、高空坠落等危险源。","氨水焦油分离器至循环氨水泵循环氨水管",530,20,{"v":33.284000000000006,"d":"33.28"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",21,"一系焦油氨水分离区","作业高度约2-7m，作业环境存在氨水泄漏、高空坠落等危险源。","氨水焦油分离器至剩余氨水槽剩余氨水管",273,200,{"v":171.44400000000002,"d":"171.44"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",22,"一二系焦油氨水分离区","作业高度约1-3m，作业环境存在氨水泄漏、高空坠落等危险源。","气浮除油机机体1#",2500,8,{"v":62.800000000000004,"d":"62.80"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",23,"一二系焦油氨水分离区","作业高度约1-3m，作业环境存在氨水泄漏、高空坠落等危险源。","气浮除油机机体2#",2500,8,{"v":62.800000000000004,"d":"62.80"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",24,"一二系焦油氨水分离区","作业高度约1-3m，作业环境存在氨水泄漏、高空坠落等危险源。","气浮除油机机体3#",2500,8,{"v":62.800000000000004,"d":"62.80"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",25,"一二系焦油氨水分离区","作业高度约1-3m，作业环境存在氨水泄漏、高空坠落等危险源。","气浮除油机机体4#",2500,8,{"v":62.800000000000004,"d":"62.80"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",26,"一二系焦油氨水分离区","作业高度约8m，作业环境存在氨水泄漏、高空坠落等危险源。","刮渣机机体1#-6#","15M²/台",3,{"v":45,"d":"45.00"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",26,"一二系焦油氨水分离区","作业高度约1-9m，作业环境存在氨水泄漏、高空坠落等危险源。","焦油氨水分离槽1#",12500,9.5,{"v":497.5016,"d":"497.50"},"加顶部","一般性腐蚀","环氧富锌漆"]
["化产环水",26,"一二系焦油氨水分离区","作业高度约1-9m，作业环境存在氨水泄漏、高空坠落等危险源。","焦油氨水分离槽2#",12500,9.5,{"v":497.5016,"d":"497.50"},"加顶部","一般性腐蚀","环氧富锌漆"]
["化产环水",26,"一二系焦油氨水分离区","作业高度约1-9m，作业环境存在氨水泄漏、高空坠落等危险源。","焦油氨水分离槽3#",12500,9.5,{"v":497.5016,"d":"497.50"},"加顶部","一般性腐蚀","环氧富锌漆"]
["化产环水",26,"一二系焦油氨水分离区","作业高度约1-9m，作业环境存在氨水泄漏、高空坠落等危险源。","焦油氨水分离槽4#",12500,9.5,{"v":497.5016,"d":"497.50"},"加顶部","一般性腐蚀","环氧富锌漆"]
["化产环水",27,"一二系焦油氨水分离区","作业高度约1-8m，作业环境存在氨水泄漏、高空坠落等危险源。","剩余氨水小槽1#",12000,8,414.48,"加顶部","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",28,"一二系焦油氨水分离区","作业高度约1-8m，作业环境存在氨水泄漏、高空坠落等危险源。","剩余氨水小槽2#",12000,8,414.48,"加顶部","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",29,"一二系焦油氨水分离区","作业高度约1-8m，作业环境存在氨水泄漏、高空坠落等危险源。","剩余氨水小槽3#",12000,8,414.48,"加顶部","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",30,"一二系焦油氨水分离区","作业高度约1-8m，作业环境存在氨水泄漏、高空坠落等危险源。","剩余氨水小槽4#",12000,8,414.48,"加顶部","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",30,"一二系焦油氨水分离区","作业高度约1-8m，作业环境存在氨水泄漏、高空坠落等危险源。","剩余氨水大槽1#",14000,8,505.54,"加顶部","一般性腐蚀","环氧富锌漆"]
["化产环水",30,"一二系焦油氨水分离区","作业高度约1-8m，作业环境存在氨水泄漏、高空坠落等危险源。","剩余氨水大槽2#",14000,8,505.54,"加顶部","一般性腐蚀","环氧富锌漆"]
["化产环水",31,"一二系焦油氨水分离区","作业高度约1-7m，作业环境存在氨水泄漏、高空坠落等危险源。","陶瓷过滤器本体1#",3032,7,{"v":66.64336,"d":"66.64"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",32,"一二系焦油氨水分离区","作业高度约1-7m，作业环境存在氨水泄漏、高空坠落等危险源。","陶瓷过滤器本体2#",3032,7,{"v":66.64336,"d":"66.64"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",33,"一二系焦油氨水分离区","作业高度约1-7m，作业环境存在氨水泄漏、高空坠落等危险源。","陶瓷过滤器本体3#",3032,7,{"v":66.64336,"d":"66.64"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",34,"一二系焦油氨水分离区","作业高度约1-7m，作业环境存在氨水泄漏、高空坠落等危险源。","陶瓷过滤器本体4#",3032,7,{"v":66.64336,"d":"66.64"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",34,"机侧外线","作业高度约10m，作业环境存在氨水泄漏、高空坠落等危险源。","一系冷凝至3#4#焦炉循环氨水管",530,220,{"v":366.124,"d":"366.12"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"机侧外线","作业高度约10m，作业环境存在氨水泄漏、高空坠落等危险源。","一系冷凝至3#4#焦炉高压氨水管",159,220,{"v":109.83720000000001,"d":"109.84"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"机侧外线","作业高度约10m，作业环境存在乳化液泄漏、高空坠落等危险源。","一系冷凝至初冷器乳化液管",273,106,{"v":90.86532000000001,"d":"90.87"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"机侧外线","作业高度约10m，作业环境存在氨水泄漏、高空坠落等危险源。","一系冷凝至初冷器循环氨水管",219,106,{"v":72.89196000000001,"d":"72.89"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"机侧外线","作业高度约10m，作业环境存在氨水泄漏、高空坠落等危险源。","冷凝至脱酸蒸氨剩余氨水管",159,350,{"v":174.741,"d":"174.74"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"机侧外线","作业高度约10m，作业环境存在混合液泄漏、高空坠落等危险源。","一系气液分离器至刮渣机混合液管",101,150,{"v":47.571000000000005,"d":"47.57"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"机侧外线","作业高度约10m，作业环境存在氨水泄漏、高空坠落等危险源。","二系冷凝至1#2#焦炉循环氨水管",1020,200,{"v":640.5600000000001,"d":"640.56"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"机侧外线","作业高度约10m，作业环境存在氨水泄漏、高空坠落等危险源。","二系冷凝至1#2#焦炉高压氨水管",159,200,{"v":99.852,"d":"99.85"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"机侧外线","作业高度约10m，作业环境存在乳化液泄漏、高空坠落等危险源。","二系冷凝至初冷器乳化液管",273,165,{"v":141.4413,"d":"141.44"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"机侧外线","作业高度约10m，作业环境存在氨水泄漏、高空坠落等危险源。","二系冷凝至初冷器循环氨水管",219,165,{"v":113.46390000000001,"d":"113.46"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"机侧外线","作业高度约10m，作业环境存在混合液泄漏、高空坠落等危险源。","二系气液分离器至刮渣机混合液管",1020,50,{"v":160.14000000000001,"d":"160.14"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"机侧外线","作业高度约10m，作业环境存在氨水泄漏、高空坠落等危险源。","洗涤至冷凝终冷水采出管",89,206,{"v":57.56876,"d":"57.57"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"机侧外线","作业高度约10m，作业环境存在废水泄漏、高空坠落等危险源。","废水事故池至二系刮渣机事故池送水管",108,160,{"v":54.25920000000001,"d":"54.26"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"机侧外线","作业高度约10m，作业环境存在外排水泄漏、高空坠落等危险源。","外排水至炼铁（减温减压站处）外排水管",273,500,{"v":428.61000000000007,"d":"428.61"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"机侧外线","作业高度约10m，作业环境存在粗苯泄漏、高空坠落等危险源。","粗苯至油库粗苯送油管",108,600,{"v":203.472,"d":"203.47"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"机侧外线","作业高度约8m，作业环境存在蒸氨废水泄漏、高空坠落等危险源。","脱酸蒸氨至水处理蒸氨废水管",133,420,{"v":175.40040000000002,"d":"175.40"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"油库","作业高度约1m，作业环境存在粗苯泄漏等危险源。","油库粗苯槽回流管",89,30,{"v":8.383799999999999,"d":"8.38"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"油库","作业高度约2m，作业环境存在粗苯泄漏等危险源。","油库粗苯装车泵进口管",159,65,{"v":32.4519,"d":"32.45"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"油库","作业高度约3m，作业环境存在粗苯泄漏等危险源。","油库北区进粗苯槽",108,37.5,{"v":12.717,"d":"12.72"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"污水处理","作业高度约水上1m，作业环境存在落水、溺水等危险源。","一级一系一段好氧池总管曝气管（南北两根）",530,30,{"v":49.926,"d":"49.93"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"污水处理","作业高度约水上1m，作业环境存在落水、溺水等危险源。","一级一系二段好氧池总管曝气管（南北两根）",530,30,{"v":49.926,"d":"49.93"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"污水处理","作业高度约水上1m，作业环境存在落水、溺水等危险源。","一级一系三段好氧池总管曝气管（南北两根）",530,45,{"v":74.88900000000001,"d":"74.89"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"污水处理","作业高度约水上1m，作业环境存在落水、溺水等危险源。","一级二系一段好氧池总管曝气管（南北两根）",530,30,{"v":49.926,"d":"49.93"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"污水处理","作业高度约水上1m，作业环境存在落水、溺水等危险源。","一级二系二段好氧池总管曝气管（南北两根）",530,30,{"v":49.926,"d":"49.93"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",34,"污水处理","作业高度约水上1m，作业环境存在落水、溺水等危险源。","一级二系三段好氧池总管曝气管（南北两根）",530,45,{"v":74.88900000000001,"d":"74.89"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",35,"污水处理","作业高度约水上1m，作业环境存在落水、溺水等危险源。","一级一系一段好氧池曝气管支管",159,210,{"v":104.84460000000001,"d":"104.84"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",36,"污水处理","作业高度约水上1m，作业环境存在落水、溺水等危险源。","一级一系二段好氧池曝气管支管",159,210,{"v":104.84460000000001,"d":"104.84"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",37,"污水处理","作业高度约水上1m，作业环境存在落水、溺水等危险源。","一级一系三段好氧池曝气管支管",159,210,{"v":104.84460000000001,"d":"104.84"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",38,"污水处理","作业高度约水上1m，作业环境存在落水、溺水等危险源。","一级二系一段好氧池曝气管支管",159,210,{"v":104.84460000000001,"d":"104.84"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",39,"污水处理","作业高度约水上1m，作业环境存在落水、溺水等危险源。","一级二系二段好氧池曝气管支管",159,210,{"v":104.84460000000001,"d":"104.84"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",40,"污水处理","作业高度约水上1m，作业环境存在落水、溺水等危险源。","一级二系三段好氧池曝气管支管",159,210,{"v":104.84460000000001,"d":"104.84"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",40,"污水处理","作业高度约水上1m，作业环境存在落水、溺水等危险源。","二级一系好氧池总管曝气管（南北两根）",530,34,{"v":56.582800000000006,"d":"56.58"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",40,"污水处理","作业高度约水上1m，作业环境存在落水、溺水等危险源。","二级二系好氧池总管曝气管（南北两根）",530,34,{"v":56.582800000000006,"d":"56.58"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",41,"污水处理","作业高度约水上1m，作业环境存在落水、溺水等危险源。","二级一系好氧池曝气管支管",159,200,{"v":99.852,"d":"99.85"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",42,"污水处理","作业高度约水上1m，作业环境存在落水、溺水等危险源。","二级二系好氧池曝气管支管",159,200,{"v":99.852,"d":"99.85"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",43,"循环水","作业高度约2-8m，作业环境存在高空坠落等危险源。","制冷水至低温水池进水管（来自制冷集水池）",830,12,{"v":31.2744,"d":"31.27"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",44,"循环水","作业高度约2-8m，作业环境存在高空坠落等危险源。","制冷水至制冷水池进水管（来自制冷集水池）",830,18,{"v":46.9116,"d":"46.91"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",45,"循环水","作业高度约2-8m，作业环境存在高空坠落等危险源。","工艺水至工艺水池进水管（来自工艺水集水池）",830,42,{"v":109.46039999999999,"d":"109.46"},null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["化产环水",45,"循环水","作业高度约1m。","工艺水泵进口管",920,18,{"v":51.998400000000004,"d":"52.00"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",45,"循环水","作业高度约1m。","低温水泵进口管",920,9,{"v":25.999200000000002,"d":"26.00"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",45,"循环水","作业高度约1m。","制冷水泵进口管",920,12,{"v":34.665600000000005,"d":"34.67"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",45,"洗涤二系","作业高度约8m，作业环境存在煤气中毒、高空坠落等危险源。",{"$nulls":3},{"v":0,"d":"0.00"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",45,{"$nulls":5},{"v":0,"d":"0.00"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水",45,{"$nulls":5},{"v":0,"d":"0.00"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水",45,{"$nulls":5},{"v":0,"d":"0.00"},null,"一般性腐蚀","环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["化产环水","",{"$nulls":5},{"v":0,"d":"0.00"},null,null,"环氧富锌漆"]
["汇总",{"$nulls":6},{"v":12911.83609,"d":"12911.84㎡"}]

{"sheet":"4.化产-钢构","index":3,"n_rows":3825,"n_cols":19,"rows_kept":3825,"merged":[[3824,0,3824,8],[3824,9,3824,11],[3824,13,3824,14]],"flags":["formulas_cached_only"]}
["2024年广西钢铁集团焦化厂除锈防腐检修工程-化产钢构"]
["平台及钢结构防腐","钢构展开面积计算（忽略截断面）     无翼板、腹板概念的钢材例如方钢，长边按腹板计，短边按翼板计。圆钢直径计入“F”列单元格。",{"$nulls":11},"平台防腐"]
["区域/部位","材料型号","规格","数量：根","单根长","腹板H","翼板B","翼板厚t2","腹板厚t1","面积：㎡","重合情况","手动计算","序号","单面","双面","备注","腐蚀程度","推荐采用防腐涂料","辅助列"]
["洗涤一系进口预留阀楼梯槽钢","[槽钢","[16b（160*63*6.5）",2,{"v":16000,"d":"16000.00"},160,63,6.5,6.5,{"v":12.768,"d":"12.77"},"腹板重合",null,1,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系进口预留阀楼梯花纹板","方（扁）钢","800*320*6",56,{"v":800,"d":"800.00"},320,6,0,0,{"v":29.2096,"d":"29.21"},"无重合面",null,2,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系进口预留阀楼梯扁铁","方（扁）钢","/",4,{"v":16000,"d":"16000.00"},50,4,0,0,{"v":6.912,"d":"6.91"},"无重合面",null,3,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系进口预留阀楼梯圆钢","圆钢","/",16,{"v":1900,"d":"1900.00"},48,0,0,0,{"v":4.581888,"d":"4.58"},"无重合面",null,4,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系进口预留阀楼梯支撑","H/工字钢","HW125X125X6.5/9",4,{"v":7000,"d":"7000.00"},125,125,6.5,9,{"v":20.496,"d":"20.50"},"无重合面",null,5,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系眼镜阀平台槽钢","[槽钢","[16b（160*63*6.5）",2,{"v":35000,"d":"35000.00"},160,63,6.5,6.5,27.93,"腹板重合",null,6,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系眼镜阀平台槽钢","[槽钢","[16b（160*63*6.5）",16,{"v":1000,"d":"1000.00"},160,63,6.5,6.5,{"v":6.384,"d":"6.38"},"腹板重合",null,7,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系眼镜阀平台槽钢","[槽钢","[16b（160*63*6.5）",8,{"v":3100,"d":"3100.00"},160,63,6.5,6.5,{"v":9.8952,"d":"9.90"},"腹板重合",null,8,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系眼镜阀平台支撑槽钢","[槽钢","[16b（160*63*6.5）",2,{"v":17600,"d":"17600.00"},160,63,6.5,6.5,{"v":14.0448,"d":"14.04"},"腹板重合",null,9,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系眼镜阀平台花纹板","方（扁）钢","1000*6",35,{"v":1000,"d":"1000.00"},1000,6,0,0,70.42,"无重合面",null,10,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系眼镜阀平台扁铁","方（扁）钢","/",35,{"v":4000,"d":"4000.00"},50,4,0,0,15.12,"无重合面",null,11,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系眼镜阀平台踢腿板","方（扁）钢","/",35,{"v":2000,"d":"2000.00"},100,4,0,0,14.56,"无重合面",null,12,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系眼镜阀平台圆钢","圆钢","/",4,{"v":35000,"d":"35000.00"},48,0,0,0,{"v":21.1008,"d":"21.10"},"无重合面",null,13,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系眼镜阀楼梯槽钢","[槽钢","[16b（160*63*6.5）",22,{"v":3600,"d":"3600.00"},160,63,6.5,6.5,{"v":31.6008,"d":"31.60"},"腹板重合",null,14,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系眼镜阀楼梯花纹板","方（扁）钢","/",110,{"v":800,"d":"800.00"},320,6,0,0,{"v":57.376,"d":"57.38"},"无重合面",null,15,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系眼镜阀楼梯扁铁","方（扁）钢","/",44,{"v":3600,"d":"3600.00"},50,6,0,0,{"v":17.7408,"d":"17.74"},"无重合面",null,16,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系眼镜阀楼梯圆钢","圆钢","/",11,{"v":15200,"d":"15200.00"},48,null,0,0,{"v":25.200384,"d":"25.20"},"无重合面",null,17,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系进口预留阀楼梯槽钢","[槽钢","[16b（160*63*6.5）",2,{"v":16000,"d":"16000.00"},160,63,6.5,6.5,{"v":17.888,"d":"17.89"},"无重合面",null,18,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系进口预留阀楼梯花纹板","方（扁）钢","/",56,{"v":800,"d":"800.00"},320,6,0,0,{"v":29.2096,"d":"29.21"},"无重合面",null,19,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系进口预留阀楼梯扁铁","方（扁）钢","/",16,{"v":4000,"d":"4000.00"},50,4,0,0,{"v":6.912,"d":"6.91"},"无重合面",null,20,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系进口预留阀楼梯圆钢","圆钢","/",16,{"v":1900,"d":"1900.00"},48,0,0,0,{"v":4.581888,"d":"4.58"},"无重合面",null,21,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系进口预留阀楼梯支撑","H/工字钢","HW125X125X6.5/9",4,{"v":7000,"d":"7000.00"},125,125,6.5,9,{"v":20.496,"d":"20.50"},"无重合面",null,22,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系眼镜阀平台槽钢","[槽钢","[16b（160*63*6.5）",2,{"v":35000,"d":"35000.00"},160,63,6.5,6.5,27.93,"腹板重合",null,23,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系眼镜阀平台槽钢","[槽钢","[16b（160*63*6.5）",16,{"v":1000,"d":"1000.00"},160,63,6.5,6.5,{"v":6.384,"d":"6.38"},"腹板重合",null,24,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系眼镜阀平台槽钢","[槽钢","[16b（160*63*6.5）",8,{"v":3100,"d":"3100.00"},160,63,6.5,6.5,{"v":9.8952,"d":"9.90"},"腹板重合",null,25,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系眼镜阀平台支撑槽钢","[槽钢","[16b（160*63*6.5）",2,{"v":17600,"d":"17600.00"},160,63,6.5,6.5,{"v":19.6768,"d":"19.68"},"无重合面",null,26,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系眼镜阀平台花纹板","方（扁）钢","1000*6",35,{"v":1000,"d":"1000.00"},1000,6,0,0,70.42,"无重合面",null,27,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系眼镜阀平台扁铁","方（扁）钢","/",35,{"v":4000,"d":"4000.00"},50,6,0,0,15.68,"无重合面",null,28,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系眼镜阀平台踢腿板","方（扁）钢","/",35,{"v":2000,"d":"2000.00"},100,6,0,0,14.84,"无重合面",null,29,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系眼镜阀平台圆钢","圆钢","/",35,{"v":4000,"d":"4000.00"},48,0,0,0,{"v":21.1008,"d":"21.10"},"无重合面",null,30,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系眼镜阀楼梯槽钢","[槽钢","[16b（160*63*6.5）",22,{"v":3600,"d":"3600.00"},160,63,6.5,6.5,{"v":44.2728,"d":"44.27"},"无重合面",null,31,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系眼镜阀楼梯花纹板","方（扁）钢","/",110,{"v":800,"d":"800.00"},320,6,0,0,{"v":57.376,"d":"57.38"},"无重合面",null,32,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系眼镜阀楼梯扁铁","方（扁）钢","/",44,{"v":3600,"d":"3600.00"},50,4,0,0,{"v":17.1072,"d":"17.11"},"无重合面",null,33,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系眼镜阀楼梯圆钢","圆钢","/",11,{"v":15200,"d":"15200.00"},48,0,0,0,{"v":25.200384,"d":"25.20"},"无重合面",null,34,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕眼镜阀楼梯槽钢","[槽钢","[16b（160*63*6.5）",16,{"v":3800,"d":"3800.00"},160,63,6.5,6.5,{"v":33.9872,"d":"33.99"},"无重合面",null,35,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕眼镜阀楼梯花纹板","方（扁）钢","/",13.299999999999999,{"v":800,"d":"800.00"},320,6,0,0,{"v":6.93728,"d":"6.94"},"无重合面",null,36,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕眼镜阀楼梯扁铁","方（扁）钢","/",32,{"v":3800,"d":"3800.00"},50,4,0,0,{"v":13.1328,"d":"13.13"},"无重合面",null,37,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕眼镜阀楼梯圆钢","圆钢","/",8,{"v":15600,"d":"15600.00"},48,0,0,0,{"v":18.809856,"d":"18.81"},"无重合面",null,38,null,null,"新建整改平台楼梯（总图除外）","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["外线G74-G78  A-A\\B-B面","H/工字钢","HW175*175*7*10",8,{"v":3500,"d":"3500.00"},150,150,7,10,24.64,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  A-A\\B-B面","H/工字钢","HW175*175*7*10",24,{"v":2200,"d":"2200.00"},150,150,7,10,{"v":46.464,"d":"46.46"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  A-A\\B-B面","H/工字钢","HW200*200*8*12",16,{"v":2200,"d":"2200.00"},200,200,8,12,{"v":41.3952,"d":"41.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  A-A\\B-B面","H/工字钢","HW200*200*8*12",16,{"v":6300,"d":"6300.00"},200,200,8,12,{"v":118.5408,"d":"118.54"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  A-A\\B-B面 ","L型钢","ZC-2:L75*6",124,{"v":4862.616612903225,"d":"4862.62"},75,75,6,6,{"v":180.889338,"d":"180.89"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  A-A\\B-B面","2L型钢","ZC-1:TN100*100*5.5*8",4,{"v":2778.434435493268,"d":"2778.43"},100,100,5.5,8,{"v":4.445495096789228,"d":"4.45"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  A-A\\B-B面","2L型钢","ZC-3:TN125*125*6*9",8,{"v":5000,"d":"5000.00"},125,125,6,9,{"v":20,"d":"20.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  A-A\\B-B面","2L型钢","ZC-3:TN125*125*6*9",2,{"v":4000,"d":"4000.00"},125,125,6,9,{"v":4,"d":"4.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  A-A\\B-B面","2L型钢","ZC-3:TN125*125*6*9",8,{"v":3900,"d":"3900.00"},125,125,6,9,{"v":15.6,"d":"15.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  A-A\\B-B面","2L型钢","ZC-3:TN125*125*6*9",2,{"v":2500,"d":"2500.00"},125,125,6,9,{"v":2.5,"d":"2.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  A-A\\B-B面","2L型钢","ZC-3:TN125*125*6*9",4,{"v":3500,"d":"3500.00"},125,125,6,9,{"v":7,"d":"7.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  A-A\\B-B面","2L型钢","TN150*150*6.5*9",8,{"v":3500,"d":"3500.00"},150,150,6.5,9,{"v":16.8,"d":"16.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  A-A\\B-B面","2L型钢","TN175*175*7*11",4,{"v":3000,"d":"3000.00"},175,175,7,11,{"v":8.4,"d":"8.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  8.5米平面","H/工字钢","HM244*175*7*11",35,{"v":4000,"d":"4000.00"},244,175,7,11,163.24,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  8.5米平面","H/工字钢","HM244*175*7*11",2,{"v":24000,"d":"24000.00"},244,175,7,11,{"v":55.968,"d":"55.97"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  8.5米平面","H/工字钢","HM244*175*7*11",2,{"v":22500,"d":"22500.00"},244,175,7,11,52.47,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  8.5米平面","H/工字钢","HN400*200*8*13",2,{"v":9000,"d":"9000.00"},400,200,8,13,{"v":28.332,"d":"28.33"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  8.5米平面","H/工字钢","HW450*200*9*14",8,{"v":11000,"d":"11000.00"},450,200,9,14,{"v":147.136,"d":"147.14"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  8.5米平面","L型钢","L75*6",42,{"v":4910,"d":"4910.00"},75,75,6,6,{"v":61.866,"d":"61.87"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  8.5米平面","L型钢","ZC-4:L80*8",16,{"v":4597.298587006803,"d":"4597.30"},80,80,8,8,{"v":23.538168765474833,"d":"23.54"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  8.5米平面","L型钢","L80*8",4,{"v":10320,"d":"10320.00"},80,80,8,8,{"v":13.2096,"d":"13.21"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78   6.3米平面","H/工字钢","HM244*175*7*11",35,{"v":4000,"d":"4000.00"},244,175,7,11,163.24,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78   6.3米平面","H/工字钢","HM244*175*7*11",2,{"v":24000,"d":"24000.00"},244,175,7,11,{"v":55.968,"d":"55.97"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78   6.3米平面","H/工字钢","HM244*175*7*11",2,{"v":22500,"d":"22500.00"},244,175,7,11,52.47,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78   6.3米平面","H/工字钢","HN400*200*8*13",2,{"v":9000,"d":"9000.00"},400,200,8,13,{"v":28.332,"d":"28.33"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78   6.3米平面","H/工字钢","HW450*200*9*14",8,{"v":11000,"d":"11000.00"},450,200,9,14,{"v":147.136,"d":"147.14"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78   6.3米平面","L型钢","L100*10",2,{"v":99500,"d":"99500.00"},100,100,10,10,{"v":59.7,"d":"59.70"},"翼板重合",null,38,null,{"v":139.3,"d":"139.30"},"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["外线G74-G78   6.3米平面","L型钢","L75*6",42,{"v":4910,"d":"4910.00"},75,75,6,6,{"v":46.3995,"d":"46.40"},"翼板重合",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78   6.3米平面","L型钢","L80*8",2,{"v":5600,"d":"5600.00"},80,80,8,8,{"v":2.688,"d":"2.69"},"翼板重合",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78   6.3米平面","L型钢","L80*8",2,{"v":4720,"d":"4720.00"},80,80,8,8,{"v":2.2656,"d":"2.27"},"翼板重合",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78   10米平面","H/工字钢","HM244*175*7*11",2,{"v":22500,"d":"22500.00"},244,175,7,11,{"v":44.595,"d":"44.60"},"翼板重合",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78   10米平面","H/工字钢","HM244*175*7*11",9,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":35.676,"d":"35.68"},"翼板重合",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78   10米平面","L型钢","L100*10",2,{"v":22500,"d":"22500.00"},100,100,10,10,{"v":13.5,"d":"13.50"},"翼板重合",null,38,null,{"v":31.5,"d":"31.50"},"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["外线G74-G78   10米平面","L型钢","L75*6",14,{"v":4910,"d":"4910.00"},75,75,6,6,{"v":15.4665,"d":"15.47"},"翼板重合",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78   10米平面","L型钢","L80*8",2,{"v":5600,"d":"5600.00"},80,80,8,8,{"v":2.688,"d":"2.69"},"翼板重合",null,38,null,null,"总图内所有管架、410NC02102-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  C-C面","2L型钢","TN125*125*6*9",6,{"v":4000,"d":"4000.00"},125,125,6,9,{"v":12,"d":"12.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  C-C面","2L型钢","TN125*125*6*9",24,{"v":5000,"d":"5000.00"},125,125,6,9,{"v":60,"d":"60.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线G74-G78  C1-C1面","2L型钢","TN125*125*6*9",4,{"v":5000,"d":"5000.00"},125,125,6,9,{"v":10,"d":"10.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K78a-K78e   C-C面","2L型钢","TN125*125*6*9",16,{"v":3900,"d":"3900.00"},125,125,6,9,{"v":31.2,"d":"31.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K78a-K78e   C-C面","2L型钢","TN125*125*6*9",4,{"v":2500,"d":"2500.00"},125,125,6,9,{"v":5,"d":"5.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K78a-K78e   B-B面","H/工字钢","HW200*200*8*12",6,{"v":6300,"d":"6300.00"},200,200,8,12,{"v":44.4528,"d":"44.45"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K78a-K78e   B-B面","2L型钢","TN125*125*6*9",8,{"v":3900,"d":"3900.00"},125,125,6,9,{"v":15.6,"d":"15.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K78a-K78e   B-B面","2L型钢","TN125*125*6*9",2,{"v":2500,"d":"2500.00"},125,125,6,9,{"v":2.5,"d":"2.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K78a-K78e   A-A面","H/工字钢","HW200*200*8*12",10,{"v":6300,"d":"6300.00"},200,200,8,12,{"v":74.088,"d":"74.09"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K78a-K78e   A-A面","2L型钢","TN125*125*6*9",8,{"v":3900,"d":"3900.00"},125,125,6,9,{"v":15.6,"d":"15.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K78a-K78e   A-A面","2L型钢","TN125*125*6*9",2,{"v":2500,"d":"2500.00"},125,125,6,9,{"v":2.5,"d":"2.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K78a-K78e   6.3米平面","H/工字钢","HN350*175*7*11",2,{"v":6000,"d":"6000.00"},350,175,7,11,{"v":16.536,"d":"16.54"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K78a-K78e   6.3米平面","H/工字钢","HM194*150*6*9",18,{"v":2500,"d":"2500.00"},194,150,6,9,43.65,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K78a-K78e   6.3米平面","H/工字钢","HW450*200*9*14",4,{"v":10000,"d":"10000.00"},450,200,9,14,66.88,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K78a-K78e   6.3米平面","H/工字钢","HW450*200*9*14",4,{"v":12000,"d":"12000.00"},450,200,9,14,{"v":80.256,"d":"80.26"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K78a-K78e   6.3米平面","L型钢","L100*10",2,{"v":34500,"d":"34500.00"},100,100,10,10,{"v":20.7,"d":"20.70"},"翼板重合",null,38,null,{"v":48.3,"d":"48.30"},"总图内所有管架、410NC02102-3","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["外线K78a-K78e   6.3米平面","L型钢","L100*10",2,{"v":18000,"d":"18000.00"},100,100,10,10,{"v":10.8,"d":"10.80"},"翼板重合",null,38,null,{"v":25.2,"d":"25.20"},"总图内所有管架、410NC02102-3","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["外线K78a-K78e   6.3米平面","L型钢","L75*6",18,{"v":3900,"d":"3900.00"},75,75,6,6,{"v":15.795,"d":"15.80"},"翼板重合",null,38,null,null,"总图内所有管架、410NC02102-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84   6.3米平面","H/工字钢","HM244*175*7*11",24,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":111.936,"d":"111.94"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84   6.3米平面","H/工字钢","HM244*175*7*11",2,{"v":70000,"d":"70000.00"},244,175,7,11,163.24,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84   6.3米平面","L型钢","L75*6",4,{"v":4850,"d":"4850.00"},75,75,6,6,5.82,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84   6.3米平面","L型钢","L75*6",18,{"v":5000,"d":"5000.00"},75,75,6,6,{"v":27,"d":"27.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84   6.3米平面","L型钢","L80*8",2,{"v":5000,"d":"5000.00"},80,80,8,8,{"v":3.2,"d":"3.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84   6.3米平面","L型钢","L80*8",2,{"v":5650,"d":"5650.00"},80,80,8,8,{"v":3.616,"d":"3.62"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84    B-B面","2L型钢","TN125*125*6*9",16,{"v":5000,"d":"5000.00"},125,125,6,9,{"v":40,"d":"40.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84    B-B面","2L型钢","TN125*125*6*9",4,{"v":4000,"d":"4000.00"},125,125,6,9,{"v":8,"d":"8.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84    8米平面","H/工字钢","HM244*175*7*11",26,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":121.264,"d":"121.26"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84    8米平面","H/工字钢","HM244*175*7*11",2,{"v":3000,"d":"3000.00"},244,175,7,11,{"v":6.996,"d":"7.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84    8米平面","L型钢","L80*8",2,{"v":5000,"d":"5000.00"},80,80,8,8,{"v":3.2,"d":"3.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84    8米平面","L型钢","L80*8",2,{"v":5650,"d":"5650.00"},80,80,8,8,{"v":3.616,"d":"3.62"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84  A-A面","H/工字钢","HW150*150*7*10",20,{"v":2100,"d":"2100.00"},150,150,7,10,36.96,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84  A-A面","H/工字钢","HW150*150*7*10",42,{"v":1500,"d":"1500.00"},150,150,7,10,55.44,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84  A-A面","H/工字钢","HW175*175*7*10",16,{"v":3200,"d":"3200.00"},150,150,7,10,{"v":45.056,"d":"45.06"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84  A-A面","H/工字钢","HW200*200*8*12",14,{"v":3200,"d":"3200.00"},200,200,8,12,{"v":52.6848,"d":"52.68"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84  A-A面","H/工字钢","HW200*200*8*12",14,{"v":1500,"d":"1500.00"},200,200,8,12,{"v":24.696,"d":"24.70"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84  A-A面","H/工字钢","HW200*200*8*12",14,{"v":6000,"d":"6000.00"},200,200,8,12,{"v":98.784,"d":"98.78"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84  A-A面","2L型钢","TN100*100*5.5*8",8,{"v":2000,"d":"2000.00"},100,100,5.5,8,{"v":6.4,"d":"6.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84  A-A面","2L型钢","TN100*100*5.5*8",38,{"v":2300,"d":"2300.00"},100,100,5.5,8,34.96,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84  A-A面","2L型钢","TN100*100*5.5*8",16,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":9.6,"d":"9.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84  A-A面","2L型钢","TN125*125*6*9",12,{"v":4200,"d":"4200.00"},125,125,6,9,{"v":25.2,"d":"25.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84  A-A面","2L型钢","TN125*125*6*9",2,{"v":3000,"d":"3000.00"},125,125,6,9,{"v":3,"d":"3.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84  A-A面","2L型钢","TN125*125*6*9",2,{"v":4000,"d":"4000.00"},125,125,6,9,{"v":4,"d":"4.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84  A-A面","2L型钢","TN125*125*6*9",12,{"v":5000,"d":"5000.00"},125,125,6,9,{"v":30,"d":"30.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84  A-A面","2L型钢","TN150*150*6.5*9",20,{"v":2100,"d":"2100.00"},150,150,6.5,9,{"v":25.2,"d":"25.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84   9.5米平面","H/工字钢","HM244*175*7*11",24,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":111.936,"d":"111.94"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84   9.5米平面","H/工字钢","HM244*175*7*11",2,{"v":70000,"d":"70000.00"},244,175,7,11,163.24,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84   9.5米平面","L型钢","L75*6",4,{"v":4850,"d":"4850.00"},75,75,6,6,5.82,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84   9.5米平面","L型钢","L75*6",18,{"v":5000,"d":"5000.00"},75,75,6,6,{"v":27,"d":"27.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84   9.5米平面","L型钢","L80*8",2,{"v":5000,"d":"5000.00"},80,80,8,8,{"v":3.2,"d":"3.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84   9.5米平面","L型钢","L80*8",2,{"v":5650,"d":"5650.00"},80,80,8,8,{"v":3.616,"d":"3.62"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84   11米平面","H/工字钢","HM244*175*7*11",24,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":111.936,"d":"111.94"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84   11米平面","H/工字钢","HM244*175*7*11",2,{"v":70000,"d":"70000.00"},244,175,7,11,163.24,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84   11米平面","L型钢","L100*10",2,{"v":70000,"d":"70000.00"},100,100,10,10,{"v":42,"d":"42.00"},"翼板重合",null,38,null,{"v":98,"d":"98.00"},"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["外线GK80-GK84   11米平面","L型钢","L75*6",4,{"v":4850,"d":"4850.00"},75,75,6,6,5.82,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84   11米平面","L型钢","L75*6",18,{"v":5000,"d":"5000.00"},75,75,6,6,{"v":27,"d":"27.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84   11米平面","L型钢","L80*8",2,{"v":5000,"d":"5000.00"},80,80,8,8,{"v":3.2,"d":"3.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK80-GK84   11米平面","L型钢","L80*8",2,{"v":5650,"d":"5650.00"},80,80,8,8,{"v":3.616,"d":"3.62"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   6.3米平面","H/工字钢","HN350*175*7*11",2,{"v":7500,"d":"7500.00"},350,175,7,11,20.67,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   6.3米平面","H/工字钢","HN350*175*7*11",2,{"v":8000,"d":"8000.00"},350,175,7,11,{"v":22.048,"d":"22.05"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   6.3米平面","H/工字钢","HM244*175*7*11",2,{"v":40500,"d":"40500.00"},244,175,7,11,{"v":94.446,"d":"94.45"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   6.3米平面","H/工字钢","HM244*175*7*11",27,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":125.928,"d":"125.93"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   6.3米平面","H/工字钢","HN400*200*8*13",2,{"v":9000,"d":"9000.00"},400,200,8,13,{"v":28.332,"d":"28.33"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   6.3米平面","L型钢","L75*6",12,{"v":5000,"d":"5000.00"},75,75,6,6,{"v":18,"d":"18.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   6.3米平面","L型钢","L80*8",6,{"v":5660,"d":"5660.00"},80,80,8,8,{"v":10.8672,"d":"10.87"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   9.5米平面","H/工字钢","HN350*175*7*11",2,{"v":7500,"d":"7500.00"},350,175,7,11,20.67,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   9.5米平面","H/工字钢","HN350*175*7*11",2,{"v":8000,"d":"8000.00"},350,175,7,11,{"v":22.048,"d":"22.05"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   9.5米平面","H/工字钢","HM244*175*7*11",2,{"v":20000,"d":"20000.00"},244,175,7,11,46.64,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   9.5米平面","H/工字钢","HM244*175*7*11",27,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":125.928,"d":"125.93"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   9.5米平面","H/工字钢","HM294*200*8*12",2,{"v":20500,"d":"20500.00"},294,200,8,12,{"v":55.924,"d":"55.92"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   9.5米平面","H/工字钢","HN400*200*8*13",2,{"v":9000,"d":"9000.00"},400,200,8,13,{"v":28.332,"d":"28.33"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   9.5米平面","L型钢","L75*6",12,{"v":5000,"d":"5000.00"},75,75,6,6,{"v":18,"d":"18.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   9.5米平面","L型钢","L80*8",6,{"v":5660,"d":"5660.00"},80,80,8,8,{"v":10.8672,"d":"10.87"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   8米平面","H/工字钢","HN350*175*7*11",2,{"v":7500,"d":"7500.00"},350,175,7,11,20.67,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   8米平面","H/工字钢","HN350*175*7*11",2,{"v":8000,"d":"8000.00"},350,175,7,11,{"v":22.048,"d":"22.05"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   8米平面","H/工字钢","HM244*175*7*11",31,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":144.584,"d":"144.58"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   8米平面","H/工字钢","HN400*200*8*13",2,{"v":9000,"d":"9000.00"},400,200,8,13,{"v":28.332,"d":"28.33"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a   8米平面","L型钢","L80*8",6,{"v":5660,"d":"5660.00"},80,80,8,8,{"v":10.8672,"d":"10.87"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  A-A面B-B面总和","H/工字钢","HW150*150*7*10",8,{"v":2100,"d":"2100.00"},150,150,7,10,{"v":14.784,"d":"14.78"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  A-A面B-B面总和","H/工字钢","HW150*150*7*10",10,{"v":1500,"d":"1500.00"},150,150,7,10,{"v":13.2,"d":"13.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  A-A面B-B面总和","H/工字钢","HW175*175*7*10",18,{"v":3200,"d":"3200.00"},150,150,7,10,{"v":50.688,"d":"50.69"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  A-A面B-B面总和","H/工字钢","HW200*200*8*12",8,{"v":4700,"d":"4700.00"},200,200,8,12,{"v":44.2176,"d":"44.22"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  A-A面B-B面总和","H/工字钢","HW200*200*8*12",4,{"v":11000,"d":"11000.00"},200,200,8,12,{"v":51.744,"d":"51.74"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  A-A面B-B面总和","H/工字钢","HW200*200*8*12",8,{"v":6000,"d":"6000.00"},200,200,8,12,{"v":56.448,"d":"56.45"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  A-A面B-B面总和","2L型钢","TN100*100*5.5*8",20,{"v":2100,"d":"2100.00"},100,100,5.5,8,{"v":16.8,"d":"16.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  A-A面B-B面总和","2L型钢","TN100*100*5.5*8",8,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":4.8,"d":"4.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  A-A面B-B面总和","2L型钢","TN125*125*6*9",24,{"v":5000,"d":"5000.00"},125,125,6,9,{"v":60,"d":"60.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  A-A面B-B面总和","2L型钢","TN125*125*6*9",6,{"v":4000,"d":"4000.00"},125,125,6,9,{"v":12,"d":"12.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  A-A面B-B面总和","2L型钢","TN150*150*6.5*9",4,{"v":2100,"d":"2100.00"},150,150,6.5,9,5.04,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  A-A面B-B面总和","2L型钢","TN175*175*7*11",8,{"v":2100,"d":"2100.00"},175,175,7,11,11.76,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  A-A面B-B面总和","2L型钢","TN175*175*7*11",4,{"v":1500,"d":"1500.00"},175,175,7,11,{"v":4.2,"d":"4.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  A-A面B-B面总和","2L型钢","TN175*175*7*11",4,{"v":5120,"d":"5120.00"},175,175,7,11,{"v":14.336,"d":"14.34"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  A-A面B-B面总和","2L型钢","TN200*200*8*13",4,{"v":2500,"d":"2500.00"},200,200,8,13,{"v":8,"d":"8.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a    11米平面","H/工字钢","HN350*175*7*11",2,{"v":7500,"d":"7500.00"},350,175,7,11,20.67,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a    11米平面","H/工字钢","HN350*175*7*11",2,{"v":8000,"d":"8000.00"},350,175,7,11,{"v":22.048,"d":"22.05"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a    11米平面","H/工字钢","HM244*175*7*11",31,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":144.584,"d":"144.58"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a    11米平面","H/工字钢","HN400*200*8*13",2,{"v":9000,"d":"9000.00"},400,200,8,13,{"v":28.332,"d":"28.33"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a    11米平面","L型钢","L100*10",2,{"v":52000,"d":"52000.00"},100,100,10,10,{"v":31.2,"d":"31.20"},"翼板重合",null,38,null,{"v":72.8,"d":"72.80"},"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["外线GK86-Gk88a    11米平面","L型钢","L100*10",2,{"v":20500,"d":"20500.00"},100,100,10,10,{"v":12.3,"d":"12.30"},"翼板重合",null,38,null,{"v":28.7,"d":"28.70"},"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["外线GK86-Gk88a    11米平面","L型钢","L100*10",null,{"v":0,"d":"0.00"},100,100,10,10,{"v":0,"d":"0.00"},"无重合面",null,38,null,{"v":28.8,"d":"28.80"},"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["外线GK86-Gk88a    11米平面","L型钢","L100*10",6,{"v":5660,"d":"5660.00"},100,100,10,10,{"v":13.584,"d":"13.58"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-Gk88a    11米平面","L型钢","L75*6",22,{"v":5000,"d":"5000.00"},75,75,6,6,{"v":33,"d":"33.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  E-E面F-F面总和","2L型钢","TN125*125*6*9",20,{"v":5000,"d":"5000.00"},125,125,6,9,{"v":50,"d":"50.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  E-E面F-F面总和","2L型钢","TN125*125*6*9",5,{"v":4000,"d":"4000.00"},125,125,6,9,{"v":10,"d":"10.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  C-C面D-D面总和","H/工字钢","HW200*200*8*12",2,{"v":3200,"d":"3200.00"},200,200,8,12,{"v":7.5264,"d":"7.53"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  C-C面D-D面总和","H/工字钢","HW200*200*8*12",2,{"v":1500,"d":"1500.00"},200,200,8,12,{"v":3.528,"d":"3.53"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK86-GK88a  C-C面D-D面总和","H/工字钢","HW200*200*8*12",2,{"v":6000,"d":"6000.00"},200,200,8,12,{"v":14.112,"d":"14.11"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   6.3米平面","H/工字钢","HM244*175*7*11",2,{"v":78000,"d":"78000.00"},244,175,7,11,{"v":181.896,"d":"181.90"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   6.3米平面","H/工字钢","HM244*175*7*11",2,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":9.328,"d":"9.33"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   6.3米平面","H/工字钢","HM244*175*7*11",2,{"v":5000,"d":"5000.00"},244,175,7,11,11.66,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   6.3米平面","H/工字钢","HN400*200*8*13",2,{"v":9000,"d":"9000.00"},400,200,8,13,{"v":28.332,"d":"28.33"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   6.3米平面","H/工字钢","HW200*200*8*12",32,{"v":5000,"d":"5000.00"},200,200,8,12,188.16,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   6.3米平面","L型钢","L80*8",28,{"v":5800,"d":"5800.00"},80,80,8,8,{"v":51.968,"d":"51.97"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   6.3米平面","L型钢","L80*8",6,{"v":6400,"d":"6400.00"},80,80,8,8,{"v":12.288,"d":"12.29"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   4.2米平面","H/工字钢","HM244*175*7*11",2,{"v":40000,"d":"40000.00"},244,175,7,11,93.28,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   4.2米平面","H/工字钢","HW200*200*8*12",15,{"v":5000,"d":"5000.00"},200,200,8,12,{"v":88.2,"d":"88.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   4.2米平面","L型钢","L80*8",12,{"v":5800,"d":"5800.00"},80,80,8,8,{"v":22.272,"d":"22.27"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   4.2米平面","L型钢","L80*8",2,{"v":6400,"d":"6400.00"},80,80,8,8,{"v":4.096,"d":"4.10"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  11米平面","H/工字钢","HM244*175*7*11",8,{"v":12000,"d":"12000.00"},244,175,7,11,{"v":111.936,"d":"111.94"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  11米平面","H/工字钢","HM244*175*7*11",8,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":37.312,"d":"37.31"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  11米平面","H/工字钢","HM244*175*7*11",6,{"v":5000,"d":"5000.00"},244,175,7,11,34.98,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  11米平面","H/工字钢","HM294*200*8*12",2,{"v":18000,"d":"18000.00"},294,200,8,12,{"v":49.104,"d":"49.10"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  11米平面","H/工字钢","HN400*200*8*13",2,{"v":9000,"d":"9000.00"},400,200,8,13,{"v":28.332,"d":"28.33"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  11米平面","H/工字钢","HW200*200*8*12",26,{"v":5000,"d":"5000.00"},200,200,8,12,152.88,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  11米平面","L型钢","L100*10",2,{"v":87000,"d":"87000.00"},100,100,10,10,{"v":52.2,"d":"52.20"},"翼板重合",null,38,null,{"v":121.8,"d":"121.80"},"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["外线GK89-GK95  11米平面","L型钢","L80*8",28,{"v":5800,"d":"5800.00"},80,80,8,8,{"v":51.968,"d":"51.97"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  11米平面","L型钢","L80*8",6,{"v":6400,"d":"6400.00"},80,80,8,8,{"v":12.288,"d":"12.29"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   9.5米平面","H/工字钢","HM244*175*7*11",8,{"v":12000,"d":"12000.00"},244,175,7,11,{"v":111.936,"d":"111.94"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   9.5米平面","H/工字钢","HM244*175*7*11",8,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":37.312,"d":"37.31"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   9.5米平面","H/工字钢","HM244*175*7*11",26,{"v":5000,"d":"5000.00"},244,175,7,11,151.58,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   9.5米平面","H/工字钢","HM294*200*8*12",2,{"v":18000,"d":"18000.00"},294,200,8,12,{"v":49.104,"d":"49.10"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   9.5米平面","H/工字钢","HN400*200*8*13",2,{"v":9000,"d":"9000.00"},400,200,8,13,{"v":28.332,"d":"28.33"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   9.5米平面","H/工字钢","HW200*200*8*12",6,{"v":5000,"d":"5000.00"},200,200,8,12,35.28,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   9.5米平面","L型钢","L80*8",28,{"v":5800,"d":"5800.00"},80,80,8,8,{"v":51.968,"d":"51.97"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   9.5米平面","L型钢","L80*8",6,{"v":6400,"d":"6400.00"},80,80,8,8,{"v":12.288,"d":"12.29"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   8米平面","H/工字钢","HM244*175*7*11",8,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":37.312,"d":"37.31"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   8米平面","H/工字钢","HM244*175*7*11",26,{"v":5000,"d":"5000.00"},244,175,7,11,151.58,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   8米平面","H/工字钢","HN400*200*8*13",2,{"v":9000,"d":"9000.00"},400,200,8,13,{"v":28.332,"d":"28.33"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   8米平面","H/工字钢","HW200*200*8*12",6,{"v":5000,"d":"5000.00"},200,200,8,12,35.28,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   8米平面","L型钢","L80*8",4,{"v":5800,"d":"5800.00"},80,80,8,8,{"v":7.424,"d":"7.42"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95   8米平面","L型钢","L80*8",6,{"v":6400,"d":"6400.00"},80,80,8,8,{"v":12.288,"d":"12.29"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   2.8M平面","2L型钢","TN125*125*6*9",11,{"v":4000,"d":"4000.00"},125,125,6,9,{"v":22,"d":"22.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95 E-E面","2L型钢","TN150*150*6.5*9",4,{"v":6300,"d":"6300.00"},150,150,6.5,9,15.12,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95 D-D面","2L型钢","TN150*150*6.5*9",6,{"v":6300,"d":"6300.00"},150,150,6.5,9,22.68,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95 C-C面","2L型钢","TN125*125*6*9",4,{"v":5800,"d":"5800.00"},125,125,6,9,{"v":11.6,"d":"11.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95 C-C面","2L型钢","TN125*125*6*9",1,{"v":5000,"d":"5000.00"},125,125,6,9,{"v":2.5,"d":"2.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95 B-B面","2L型钢","TN125*125*6*9",8,{"v":5800,"d":"5800.00"},125,125,6,9,{"v":23.2,"d":"23.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95 B-B面","2L型钢","TN125*125*6*9",2,{"v":5000,"d":"5000.00"},125,125,6,9,{"v":5,"d":"5.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95 A-A面","2L型钢","TN125*125*6*9",14,{"v":5800,"d":"5800.00"},125,125,6,9,{"v":40.6,"d":"40.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95 A-A面","2L型钢","TN125*125*6*9",2,{"v":5000,"d":"5000.00"},125,125,6,9,{"v":5,"d":"5.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","H/工字钢","HW150*150*7*10",8,{"v":2100,"d":"2100.00"},150,150,7,10,{"v":14.784,"d":"14.78"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","H/工字钢","HW150*150*7*10",20,{"v":1500,"d":"1500.00"},150,150,7,10,{"v":26.4,"d":"26.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","H/工字钢","HW150*150*7*10",4,{"v":2000,"d":"2000.00"},150,150,7,10,7.04,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","H/工字钢","HW175*175*7*10",2,{"v":2100,"d":"2100.00"},150,150,7,10,{"v":3.696,"d":"3.70"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","H/工字钢","HW175*175*7*10",5,{"v":1500,"d":"1500.00"},150,150,7,10,{"v":6.6,"d":"6.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","H/工字钢","HW175*175*7*10",17,{"v":3200,"d":"3200.00"},150,150,7,10,{"v":47.872,"d":"47.87"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","H/工字钢","HW200*200*8*12",3,{"v":4700,"d":"4700.00"},200,200,8,12,{"v":16.5816,"d":"16.58"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","H/工字钢","HW200*200*8*12",2,{"v":6800,"d":"6800.00"},200,200,8,12,{"v":15.9936,"d":"15.99"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","H/工字钢","HW200*200*8*12",2,{"v":11000,"d":"11000.00"},200,200,8,12,{"v":25.872,"d":"25.87"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","H/工字钢","HW200*200*8*12",3,{"v":6000,"d":"6000.00"},200,200,8,12,{"v":21.168,"d":"21.17"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","H/工字钢","HW200*200*8*12",2,{"v":3900,"d":"3900.00"},200,200,8,12,{"v":9.1728,"d":"9.17"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","H/工字钢","HW250*250*9*14",3,{"v":6800,"d":"6800.00"},250,250,9,14,{"v":30.0288,"d":"30.03"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","H/工字钢","HW250*250*9*14",2,{"v":3900,"d":"3900.00"},250,250,9,14,{"v":11.4816,"d":"11.48"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","2L型钢","TN100*100*5.5*8",19,{"v":2100,"d":"2100.00"},100,100,5.5,8,15.96,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","2L型钢","TN100*100*5.5*8",10,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":6,"d":"6.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","2L型钢","TN125*125*6*9",14,{"v":5000,"d":"5000.00"},125,125,6,9,{"v":35,"d":"35.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","2L型钢","TN125*125*6*9",2,{"v":4000,"d":"4000.00"},125,125,6,9,{"v":4,"d":"4.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","2L型钢","TN150*150*6.5*9",10,{"v":2100,"d":"2100.00"},150,150,6.5,9,{"v":12.6,"d":"12.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","2L型钢","TN150*150*6.5*9",2,{"v":5000,"d":"5000.00"},150,150,6.5,9,{"v":6,"d":"6.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  G-G面","2L型钢","TN150*150*6.5*9",4,{"v":5600,"d":"5600.00"},150,150,6.5,9,13.44,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","H/工字钢","HW150*150*7*10",8,{"v":2100,"d":"2100.00"},150,150,7,10,{"v":14.784,"d":"14.78"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","H/工字钢","HW150*150*7*10",20,{"v":1500,"d":"1500.00"},150,150,7,10,{"v":26.4,"d":"26.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","H/工字钢","HW150*150*7*10",4,{"v":2000,"d":"2000.00"},150,150,7,10,7.04,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","H/工字钢","HW175*175*7*10",2,{"v":2100,"d":"2100.00"},150,150,7,10,{"v":3.696,"d":"3.70"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","H/工字钢","HW175*175*7*10",5,{"v":1500,"d":"1500.00"},150,150,7,10,{"v":6.6,"d":"6.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","H/工字钢","HW175*175*7*10",17,{"v":3200,"d":"3200.00"},150,150,7,10,{"v":47.872,"d":"47.87"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","H/工字钢","HW200*200*8*12",3,{"v":4700,"d":"4700.00"},200,200,8,12,{"v":16.5816,"d":"16.58"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","H/工字钢","HW200*200*8*12",2,{"v":6800,"d":"6800.00"},200,200,8,12,{"v":15.9936,"d":"15.99"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","H/工字钢","HW200*200*8*12",2,{"v":11000,"d":"11000.00"},200,200,8,12,{"v":25.872,"d":"25.87"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","H/工字钢","HW200*200*8*12",3,{"v":6000,"d":"6000.00"},200,200,8,12,{"v":21.168,"d":"21.17"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","H/工字钢","HW200*200*8*12",2,{"v":3900,"d":"3900.00"},200,200,8,12,{"v":9.1728,"d":"9.17"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","H/工字钢","HW250*250*9*14",3,{"v":6800,"d":"6800.00"},250,250,9,14,{"v":30.0288,"d":"30.03"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","H/工字钢","HW250*250*9*14",2,{"v":3900,"d":"3900.00"},250,250,9,14,{"v":11.4816,"d":"11.48"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","2L型钢","TN100*100*5.5*8",19,{"v":2100,"d":"2100.00"},100,100,5.5,8,15.96,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","2L型钢","TN100*100*5.5*8",10,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":6,"d":"6.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","2L型钢","TN125*125*6*9",8,{"v":5000,"d":"5000.00"},125,125,6,9,{"v":20,"d":"20.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","2L型钢","TN125*125*6*9",2,{"v":4000,"d":"4000.00"},125,125,6,9,{"v":4,"d":"4.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","2L型钢","TN150*150*6.5*9",10,{"v":2100,"d":"2100.00"},150,150,6.5,9,{"v":12.6,"d":"12.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","2L型钢","TN150*150*6.5*9",2,{"v":5000,"d":"5000.00"},150,150,6.5,9,{"v":6,"d":"6.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK89-GK95  F-F面","2L型钢","TN150*150*6.5*9",4,{"v":5600,"d":"5600.00"},150,150,6.5,9,13.44,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   9.5M平面","H/工字钢","HM244*175*7*11",36,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":167.904,"d":"167.90"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   9.5M平面","H/工字钢","HM244*175*7*11",2,{"v":101500,"d":"101500.00"},244,175,7,11,{"v":236.698,"d":"236.70"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   9.5M平面","H/工字钢","HW200*200*8*12",5,{"v":4000,"d":"4000.00"},200,200,8,12,23.52,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   9.5M平面","H/工字钢","HW200*200*8*12",2,{"v":18500,"d":"18500.00"},200,200,8,12,{"v":43.512,"d":"43.51"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   9.5M平面","L型钢","L100*10",2,{"v":120000,"d":"120000.00"},100,100,10,10,{"v":72,"d":"72.00"},"翼板重合",null,38,null,{"v":168,"d":"168.00"},"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["外线K96~GK103   9.5M平面","L型钢","L75*6",78,{"v":5000,"d":"5000.00"},75,75,6,6,{"v":117,"d":"117.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   9.5M平面","L型钢","L75*6",2,{"v":5660,"d":"5660.00"},75,75,6,6,{"v":3.396,"d":"3.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   8M平面","H/工字钢","HM244*175*7*11",36,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":167.904,"d":"167.90"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   8M平面","H/工字钢","HM244*175*7*11",2,{"v":101500,"d":"101500.00"},244,175,7,11,{"v":236.698,"d":"236.70"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   8M平面","H/工字钢","HW200*200*8*12",5,{"v":4000,"d":"4000.00"},200,200,8,12,23.52,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   8M平面","H/工字钢","HW200*200*8*12",2,{"v":18500,"d":"18500.00"},200,200,8,12,{"v":43.512,"d":"43.51"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   8M平面","L型钢","L75*6",78,{"v":5000,"d":"5000.00"},75,75,6,6,{"v":117,"d":"117.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   8M平面","L型钢","L75*6",2,{"v":5660,"d":"5660.00"},75,75,6,6,{"v":3.396,"d":"3.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   6.3M平面","H/工字钢","HM244*175*7*11",41,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":191.224,"d":"191.22"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   6.3M平面","H/工字钢","HM244*175*7*11",2,{"v":120000,"d":"120000.00"},244,175,7,11,279.84,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   6.3M平面","L型钢","L75*6",44,{"v":5000,"d":"5000.00"},75,75,6,6,{"v":66,"d":"66.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   6.3M平面","L型钢","L75*6",2,{"v":5660,"d":"5660.00"},75,75,6,6,{"v":3.396,"d":"3.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   2.8M平面","H/工字钢","HM194*150*6*9",6,{"v":2500,"d":"2500.00"},194,150,6,9,14.55,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   2.8M平面","H/工字钢","HW200*200*8*12",12,{"v":2000,"d":"2000.00"},200,200,8,12,{"v":28.224,"d":"28.22"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   2.8M平面","H/工字钢","HW200*200*8*12",1,{"v":3000,"d":"3000.00"},200,200,8,12,{"v":3.528,"d":"3.53"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   2.8M平面","2L型钢","TN200*200*8*13",6,{"v":1440,"d":"1440.00"},200,200,8,13,{"v":6.912,"d":"6.91"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103   2.8M平面","2L型钢","TN200*200*8*13",6,{"v":1730,"d":"1730.00"},200,200,8,13,{"v":8.304,"d":"8.30"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103 E-E面","2L型钢","TN125*125*6*9",8,{"v":4300,"d":"4300.00"},125,125,6,9,{"v":17.2,"d":"17.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103 E-E面","2L型钢","TN125*125*6*9",8,{"v":5300,"d":"5300.00"},125,125,6,9,{"v":21.2,"d":"21.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103 E-E面","2L型钢","TN125*125*6*9",4,{"v":4000,"d":"4000.00"},125,125,6,9,{"v":8,"d":"8.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  D-D面","2L型钢","TN125*125*6*9",8,{"v":4300,"d":"4300.00"},125,125,6,9,{"v":17.2,"d":"17.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  D-D面","2L型钢","TN125*125*6*9",8,{"v":5300,"d":"5300.00"},125,125,6,9,{"v":21.2,"d":"21.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  D-D面","2L型钢","TN125*125*6*9",4,{"v":4000,"d":"4000.00"},125,125,6,9,{"v":8,"d":"8.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  C-C面","2L型钢","TN125*125*6*9",6,{"v":4300,"d":"4300.00"},125,125,6,9,{"v":12.9,"d":"12.90"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  C-C面","2L型钢","TN125*125*6*9",6,{"v":5300,"d":"5300.00"},125,125,6,9,{"v":15.9,"d":"15.90"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  C-C面","2L型钢","TN125*125*6*9",3,{"v":4000,"d":"4000.00"},125,125,6,9,{"v":6,"d":"6.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","H/工字钢","HW150*150*7*10",14,{"v":2100,"d":"2100.00"},150,150,7,10,{"v":25.872,"d":"25.87"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","H/工字钢","HW150*150*7*10",49,{"v":1500,"d":"1500.00"},150,150,7,10,64.68,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","H/工字钢","HW150*150*7*10",4,{"v":2920,"d":"2920.00"},150,150,7,10,{"v":10.2784,"d":"10.28"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","H/工字钢","HW150*150*7*10",10,{"v":1700,"d":"1700.00"},150,150,7,10,14.96,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","H/工字钢","HW200*200*8*12",11,{"v":1700,"d":"1700.00"},200,200,8,12,{"v":21.9912,"d":"21.99"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","H/工字钢","HW200*200*8*12",11,{"v":1500,"d":"1500.00"},200,200,8,12,{"v":19.404,"d":"19.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","H/工字钢","HW200*200*8*12",11,{"v":6000,"d":"6000.00"},200,200,8,12,{"v":77.616,"d":"77.62"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","2L型钢","TN100*100*5.5*8",39,{"v":2100,"d":"2100.00"},100,100,5.5,8,32.76,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","2L型钢","TN100*100*5.5*8",14,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":8.4,"d":"8.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","2L型钢","TN125*125*6*9",4,{"v":5500,"d":"5500.00"},125,125,6,9,{"v":11,"d":"11.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","2L型钢","TN125*125*6*9",2,{"v":4900,"d":"4900.00"},125,125,6,9,{"v":4.9,"d":"4.90"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","2L型钢","TN125*125*6*9",4,{"v":4300,"d":"4300.00"},125,125,6,9,{"v":8.6,"d":"8.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","2L型钢","TN125*125*6*9",4,{"v":3800,"d":"3800.00"},125,125,6,9,{"v":7.6,"d":"7.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","2L型钢","TN125*125*6*9",1,{"v":4000,"d":"4000.00"},125,125,6,9,{"v":2,"d":"2.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","2L型钢","TN125*125*6*9",2,{"v":2500,"d":"2500.00"},125,125,6,9,{"v":2.5,"d":"2.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","2L型钢","TN150*150*6.5*9",4,{"v":2100,"d":"2100.00"},150,150,6.5,9,5.04,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","2L型钢","TN150*150*6.5*9",2,{"v":1500,"d":"1500.00"},150,150,6.5,9,{"v":1.8,"d":"1.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","2L型钢","TN175*175*7*11",2,{"v":2100,"d":"2100.00"},175,175,7,11,2.94,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  B-B面","2L型钢","TN175*175*7*11",4,{"v":2920,"d":"2920.00"},175,175,7,11,{"v":8.176,"d":"8.18"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","H/工字钢","HW150*150*7*10",14,{"v":2100,"d":"2100.00"},150,150,7,10,{"v":25.872,"d":"25.87"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","H/工字钢","HW150*150*7*10",49,{"v":1500,"d":"1500.00"},150,150,7,10,64.68,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","H/工字钢","HW150*150*7*10",4,{"v":2920,"d":"2920.00"},150,150,7,10,{"v":10.2784,"d":"10.28"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","H/工字钢","HW150*150*7*10",10,{"v":1700,"d":"1700.00"},150,150,7,10,14.96,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","H/工字钢","HW200*200*8*12",11,{"v":1700,"d":"1700.00"},200,200,8,12,{"v":21.9912,"d":"21.99"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","H/工字钢","HW200*200*8*12",11,{"v":1500,"d":"1500.00"},200,200,8,12,{"v":19.404,"d":"19.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","H/工字钢","HW200*200*8*12",11,{"v":6000,"d":"6000.00"},200,200,8,12,{"v":77.616,"d":"77.62"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","2L型钢","TN100*100*5.5*8",39,{"v":2100,"d":"2100.00"},100,100,5.5,8,32.76,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","2L型钢","TN100*100*5.5*8",14,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":8.4,"d":"8.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","2L型钢","TN100*100*5.5*8",4,{"v":2920,"d":"2920.00"},100,100,5.5,8,{"v":4.672,"d":"4.67"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","2L型钢","TN125*125*6*9",4,{"v":5500,"d":"5500.00"},125,125,6,9,{"v":11,"d":"11.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","2L型钢","TN125*125*6*9",2,{"v":4900,"d":"4900.00"},125,125,6,9,{"v":4.9,"d":"4.90"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","2L型钢","TN125*125*6*9",4,{"v":4300,"d":"4300.00"},125,125,6,9,{"v":8.6,"d":"8.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","2L型钢","TN125*125*6*9",4,{"v":3800,"d":"3800.00"},125,125,6,9,{"v":7.6,"d":"7.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","2L型钢","TN125*125*6*9",1,{"v":4000,"d":"4000.00"},125,125,6,9,{"v":2,"d":"2.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","2L型钢","TN125*125*6*9",2,{"v":2500,"d":"2500.00"},125,125,6,9,{"v":2.5,"d":"2.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","2L型钢","TN150*150*6.5*9",4,{"v":2100,"d":"2100.00"},150,150,6.5,9,5.04,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","2L型钢","TN150*150*6.5*9",2,{"v":1500,"d":"1500.00"},150,150,6.5,9,{"v":1.8,"d":"1.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K96~GK103  A-A面","2L型钢","TN175*175*7*11",2,{"v":2100,"d":"2100.00"},175,175,7,11,2.94,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110   8.2M平面","H/工字钢","HM194*150*6*9",2,{"v":87000,"d":"87000.00"},194,150,6,9,168.78,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-17","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110   8.2M平面","H/工字钢","HM194*150*6*9",22,{"v":3000,"d":"3000.00"},194,150,6,9,64.02,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-17","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110   8.2M平面","H/工字钢","HM244*175*7*11",13,{"v":3000,"d":"3000.00"},244,175,7,11,{"v":45.474,"d":"45.47"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-17","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110   8.2M平面","L型钢","L75*6",36,{"v":4250,"d":"4250.00"},75,75,6,6,{"v":45.9,"d":"45.90"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-17","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110   6.3M平面","H/工字钢","HM194*150*6*9",2,{"v":87000,"d":"87000.00"},194,150,6,9,168.78,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-17","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110   6.3M平面","H/工字钢","HM194*150*6*9",22,{"v":3000,"d":"3000.00"},194,150,6,9,64.02,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-17","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110   6.3M平面","H/工字钢","HM244*175*7*11",13,{"v":3000,"d":"3000.00"},244,175,7,11,{"v":45.474,"d":"45.47"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-17","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110   6.3M平面","L型钢","L100*10",2,{"v":93000,"d":"93000.00"},100,100,10,10,{"v":55.8,"d":"55.80"},"翼板重合",null,38,null,{"v":130.2,"d":"130.20"},"总图内所有管架、410NC02102-17","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["外线K104~GK110   6.3M平面","L型钢","L75*6",36,{"v":4250,"d":"4250.00"},75,75,6,6,{"v":45.9,"d":"45.90"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-17","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110 B-B面","2L型钢","TN125*125*6*9",36,{"v":4250,"d":"4250.00"},125,125,6,9,{"v":76.5,"d":"76.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110 B-B面","2L型钢","TN125*125*6*9",9,{"v":3000,"d":"3000.00"},125,125,6,9,{"v":13.5,"d":"13.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110 A-A面","H/工字钢","HW150*150*7*10",18,{"v":1900,"d":"1900.00"},150,150,7,10,{"v":30.096,"d":"30.10"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110 A-A面","H/工字钢","HW150*150*7*10",14,{"v":2100,"d":"2100.00"},150,150,7,10,{"v":25.872,"d":"25.87"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110 A-A面","H/工字钢","HW150*150*7*10",36,{"v":1500,"d":"1500.00"},150,150,7,10,47.52,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110 A-A面","H/工字钢","HW200*200*8*12",18,{"v":1900,"d":"1900.00"},200,200,8,12,{"v":40.2192,"d":"40.22"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110 A-A面","H/工字钢","HW200*200*8*12",18,{"v":1500,"d":"1500.00"},200,200,8,12,{"v":31.752,"d":"31.75"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110 A-A面","H/工字钢","HW200*200*8*12",18,{"v":6000,"d":"6000.00"},200,200,8,12,{"v":127.008,"d":"127.01"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110 A-A面","2L型钢","TN100*100*5.5*8",74,{"v":2100,"d":"2100.00"},100,100,5.5,8,62.16,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110 A-A面","2L型钢","TN100*100*5.5*8",26,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":15.6,"d":"15.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110 A-A面","2L型钢","TN125*125*6*9",24,{"v":4250,"d":"4250.00"},125,125,6,9,{"v":51,"d":"51.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110 A-A面","2L型钢","TN125*125*6*9",4,{"v":3000,"d":"3000.00"},125,125,6,9,{"v":6,"d":"6.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110 A-A面","2L型钢","TN150*150*6.5*9",12,{"v":2100,"d":"2100.00"},150,150,6.5,9,15.12,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110 A-A面","2L型钢","TN150*150*6.5*9",4,{"v":1500,"d":"1500.00"},150,150,6.5,9,{"v":3.6,"d":"3.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110   9.7M平面","H/工字钢","HM194*150*6*9",2,{"v":87000,"d":"87000.00"},194,150,6,9,168.78,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110   9.7M平面","H/工字钢","HM194*150*6*9",22,{"v":3000,"d":"3000.00"},194,150,6,9,64.02,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110   9.7M平面","H/工字钢","HM244*175*7*11",13,{"v":3000,"d":"3000.00"},244,175,7,11,{"v":45.474,"d":"45.47"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K104~GK110   9.7M平面","L型钢","L100*10",2,{"v":93000,"d":"93000.00"},100,100,10,10,{"v":55.8,"d":"55.80"},"翼板重合",null,38,null,{"v":130.2,"d":"130.20"},"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["外线K104~GK110   9.7M平面","L型钢","L75*6",36,{"v":4250,"d":"4250.00"},75,75,6,6,{"v":45.9,"d":"45.90"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114   9.7M平面","H/工字钢","HM194*150*6*9",2,{"v":48000,"d":"48000.00"},194,150,6,9,93.12,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114   9.7M平面","H/工字钢","HM194*150*6*9",12,{"v":3000,"d":"3000.00"},194,150,6,9,34.92,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114   9.7M平面","H/工字钢","HM244*175*7*11",6,{"v":3000,"d":"3000.00"},244,175,7,11,{"v":20.988,"d":"20.99"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114   9.7M平面","L型钢","L100*10",2,{"v":42000,"d":"42000.00"},100,100,10,10,{"v":25.2,"d":"25.20"},"翼板重合",null,38,null,{"v":58.8,"d":"58.80"},"总图内所有管架、410NC02102-19","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["外线K111~GK114   9.7M平面","L型钢","L75*6",18,{"v":4250,"d":"4250.00"},75,75,6,6,22.95,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114   9.7M平面","L型钢","L80*8",2,{"v":4250,"d":"4250.00"},80,80,8,8,2.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114   8.2M平面","H/工字钢","HM194*150*6*9",2,{"v":48000,"d":"48000.00"},194,150,6,9,93.12,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114   8.2M平面","H/工字钢","HM194*150*6*9",12,{"v":3000,"d":"3000.00"},194,150,6,9,34.92,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114   8.2M平面","H/工字钢","HM244*175*7*11",6,{"v":3000,"d":"3000.00"},244,175,7,11,{"v":20.988,"d":"20.99"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114   8.2M平面","L型钢","L75*6",32,{"v":4250,"d":"4250.00"},75,75,6,6,{"v":40.8,"d":"40.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114   8.2M平面","L型钢","L80*8",2,{"v":4250,"d":"4250.00"},80,80,8,8,2.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114   6.3M平面","H/工字钢","HM194*150*6*9",2,{"v":48000,"d":"48000.00"},194,150,6,9,93.12,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114   6.3M平面","H/工字钢","HM194*150*6*9",12,{"v":3000,"d":"3000.00"},194,150,6,9,34.92,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114   6.3M平面","H/工字钢","HM244*175*7*11",6,{"v":3000,"d":"3000.00"},244,175,7,11,{"v":20.988,"d":"20.99"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114   6.3M平面","L型钢","L100*10",2,{"v":51000,"d":"51000.00"},100,100,10,10,{"v":30.6,"d":"30.60"},"翼板重合",null,38,null,{"v":71.4,"d":"71.40"},"总图内所有管架、410NC02102-19","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["外线K111~GK114   6.3M平面","L型钢","L75*6",18,{"v":4250,"d":"4250.00"},75,75,6,6,22.95,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114   6.3M平面","L型钢","L80*8",2,{"v":4250,"d":"4250.00"},80,80,8,8,2.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  E-E面","H/工字钢","HW150*150*7*10",8,{"v":2100,"d":"2100.00"},150,150,7,10,{"v":14.784,"d":"14.78"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  E-E面","H/工字钢","HW150*150*7*10",20,{"v":1500,"d":"1500.00"},150,150,7,10,{"v":26.4,"d":"26.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  E-E面","H/工字钢","HW150*150*7*10",4,{"v":1900,"d":"1900.00"},150,150,7,10,{"v":6.688,"d":"6.69"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  E-E面","H/工字钢","HW200*200*8*12",5,{"v":1900,"d":"1900.00"},200,200,8,12,{"v":11.172,"d":"11.17"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  E-E面","H/工字钢","HW200*200*8*12",5,{"v":1500,"d":"1500.00"},200,200,8,12,8.82,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  E-E面","H/工字钢","HW200*200*8*12",5,{"v":6000,"d":"6000.00"},200,200,8,12,35.28,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  E-E面","2L型钢","TN100*100*5.5*8",24,{"v":2100,"d":"2100.00"},100,100,5.5,8,20.16,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  E-E面","2L型钢","TN100*100*5.5*8",8,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":4.8,"d":"4.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  E-E面","2L型钢","TN125*125*6*9",6,{"v":4250,"d":"4250.00"},125,125,6,9,12.75,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  E-E面","2L型钢","TN125*125*6*9",1,{"v":3000,"d":"3000.00"},125,125,6,9,{"v":1.5,"d":"1.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  D-D面","H/工字钢","HW150*150*7*10",8,{"v":2100,"d":"2100.00"},150,150,7,10,{"v":14.784,"d":"14.78"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  D-D面","H/工字钢","HW150*150*7*10",20,{"v":1500,"d":"1500.00"},150,150,7,10,{"v":26.4,"d":"26.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  D-D面","H/工字钢","HW150*150*7*10",4,{"v":1900,"d":"1900.00"},150,150,7,10,{"v":6.688,"d":"6.69"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  D-D面","H/工字钢","HW200*200*8*12",5,{"v":1900,"d":"1900.00"},200,200,8,12,{"v":11.172,"d":"11.17"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  D-D面","H/工字钢","HW200*200*8*12",5,{"v":1500,"d":"1500.00"},200,200,8,12,8.82,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  D-D面","H/工字钢","HW200*200*8*12",5,{"v":6000,"d":"6000.00"},200,200,8,12,35.28,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  D-D面","2L型钢","TN100*100*5.5*8",24,{"v":2100,"d":"2100.00"},100,100,5.5,8,20.16,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  D-D面","2L型钢","TN100*100*5.5*8",8,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":4.8,"d":"4.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  D-D面","2L型钢","TN125*125*6*9",4,{"v":4250,"d":"4250.00"},125,125,6,9,{"v":8.5,"d":"8.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  D-D面","2L型钢","TN125*125*6*9",1,{"v":3000,"d":"3000.00"},125,125,6,9,{"v":1.5,"d":"1.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  AA\\BB\\CC\\A1A1\\A2A2面","2L型钢","TN125*125*6*9",20,{"v":4250,"d":"4250.00"},125,125,6,9,{"v":42.5,"d":"42.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K111~GK114  AA\\BB\\CC\\A1A1\\A2A2面","2L型钢","TN125*125*6*9",5,{"v":3000,"d":"3000.00"},125,125,6,9,{"v":7.5,"d":"7.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123 8.7M平面","H/工字钢","HN350*175*7*11",2,{"v":9500,"d":"9500.00"},350,175,7,11,{"v":26.182,"d":"26.18"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123 8.7M平面","H/工字钢","HM194*150*6*9",2,{"v":19000,"d":"19000.00"},194,150,6,9,36.86,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123 8.7M平面","H/工字钢","HM194*150*6*9",33,{"v":3000,"d":"3000.00"},194,150,6,9,96.03,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123 8.7M平面","H/工字钢","HW450*200*9*14",10,{"v":12000,"d":"12000.00"},450,200,9,14,200.64,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123 8.7M平面","L型钢","L75*6",34,{"v":4250,"d":"4250.00"},75,75,6,6,43.35,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123 8.7M平面","L型钢","L80*8",4,{"v":4250,"d":"4250.00"},80,80,8,8,5.44,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123 6.3M平面","H/工字钢","HN350*175*7*11",2,{"v":9500,"d":"9500.00"},350,175,7,11,{"v":26.182,"d":"26.18"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123 6.3M平面","H/工字钢","HM194*150*6*9",2,{"v":19000,"d":"19000.00"},194,150,6,9,36.86,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123 6.3M平面","H/工字钢","HM194*150*6*9",33,{"v":3000,"d":"3000.00"},194,150,6,9,96.03,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123 6.3M平面","H/工字钢","HW450*200*9*14",10,{"v":12000,"d":"12000.00"},450,200,9,14,200.64,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123 6.3M平面","L型钢","L75*6",34,{"v":4250,"d":"4250.00"},75,75,6,6,43.35,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123 6.3M平面","L型钢","L80*8",4,{"v":4250,"d":"4250.00"},80,80,8,8,5.44,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123  C-C面","2L型钢","TN100*100*5.5*8",9,{"v":3000,"d":"3000.00"},100,100,5.5,8,{"v":10.8,"d":"10.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123  C-C面","2L型钢","TN100*100*5.5*8",36,{"v":4250,"d":"4250.00"},100,100,5.5,8,{"v":61.2,"d":"61.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123   A-A面B-B面总和","H/工字钢","HW150*150*7*10",4,{"v":3100,"d":"3100.00"},150,150,7,10,{"v":10.912,"d":"10.91"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123   A-A面B-B面总和","H/工字钢","HW150*150*7*10",10,{"v":1500,"d":"1500.00"},150,150,7,10,{"v":13.2,"d":"13.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123   A-A面B-B面总和","H/工字钢","HW200*200*8*12",18,{"v":8700,"d":"8700.00"},200,200,8,12,{"v":184.1616,"d":"184.16"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123   A-A面B-B面总和","2L型钢","TN100*100*5.5*8",8,{"v":3100,"d":"3100.00"},100,100,5.5,8,9.92,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123   A-A面B-B面总和","2L型钢","TN100*100*5.5*8",2,{"v":3000,"d":"3000.00"},100,100,5.5,8,{"v":2.4,"d":"2.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123   A-A面B-B面总和","2L型钢","TN100*100*5.5*8",8,{"v":4250,"d":"4250.00"},100,100,5.5,8,{"v":13.6,"d":"13.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 外线K116~GK123   A-A面B-B面总和","2L型钢","TN125*125*6*9",1,{"v":4250,"d":"4250.00"},125,125,6,9,{"v":2.125,"d":"2.13"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  7M层平面","H/工字钢","HN194*150*6*9",76,{"v":4000,"d":"4000.00"},194,150,6,9,294.88,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  7M层平面","H/工字钢","HN194*150*6*9",21,{"v":3000,"d":"3000.00"},194,150,6,9,61.11,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  7M层平面","L型钢","L63*6",14,{"v":5000,"d":"5000.00"},63,63,6,6,17.64,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  7M层平面","L型钢","L63*6",2,{"v":5660,"d":"5660.00"},63,63,6,6,{"v":2.85264,"d":"2.85"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1a-1a面","H/工字钢","HM244*175*7*11",4,{"v":8500,"d":"8500.00"},244,175,7,11,{"v":39.644,"d":"39.64"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1a-1a面","H/工字钢","HW150*150*7*10",53,{"v":3500,"d":"3500.00"},150,150,7,10,163.24,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1a-1a面","H/工字钢","HW150*150*7*10",36,{"v":4610,"d":"4610.00"},150,150,7,10,{"v":146.0448,"d":"146.04"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1a-1a面","H/工字钢","HW200*200*8*12",1,{"v":8500,"d":"8500.00"},200,200,8,12,{"v":9.996,"d":"10.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1a-1a面","H/工字钢","HW250*250*9*14",6,{"v":18770,"d":"18770.00"},250,250,9,14,{"v":165.77664,"d":"165.78"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1a-1a面","H/工字钢","HW300*300*10*15",8,{"v":18770,"d":"18770.00"},300,300,10,15,{"v":265.7832,"d":"265.78"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1a-1a面","H/工字钢","HW340*250*9*14",5,{"v":18770,"d":"18770.00"},340,250,9,14,{"v":155.0402,"d":"155.04"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1a-1a面","H/工字钢","HW390*300*10*16",2,{"v":18770,"d":"18770.00"},390,300,10,16,{"v":73.12792,"d":"73.13"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1a-1a面","2L型钢","TN100*10*5.5*8",20,{"v":4610,"d":"4610.00"},100,100,5.5,8,36.88,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1a-1a面","2L型钢","TN100*100*5.5*8",14,{"v":4610,"d":"4610.00"},100,100,5.5,8,{"v":25.816,"d":"25.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1a-1a面","2L型钢","TN100*100*5.5*8",70,{"v":4000,"d":"4000.00"},100,100,5.5,8,{"v":112,"d":"112.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1a-1a面","2L型钢","TN100*100*5.5*8",28,{"v":4350,"d":"4350.00"},100,100,5.5,8,48.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1a-1a面","2L型钢","TN125*125*6*9",2,{"v":6140,"d":"6140.00"},125,125,6,9,6.14,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1-1面","H/工字钢","HM244*175*7*11",4,{"v":8500,"d":"8500.00"},244,175,7,11,{"v":39.644,"d":"39.64"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1-1面","H/工字钢","HN194*150*6*9",76,{"v":4000,"d":"4000.00"},194,150,6,9,294.88,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1-1面","H/工字钢","HW150*150*7*10",53,{"v":3500,"d":"3500.00"},150,150,7,10,163.24,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1-1面","H/工字钢","HW150*150*7*10",36,{"v":4610,"d":"4610.00"},150,150,7,10,{"v":146.0448,"d":"146.04"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1-1面","H/工字钢","HW200*200*8*12",1,{"v":8500,"d":"8500.00"},200,200,8,12,{"v":9.996,"d":"10.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1-1面","H/工字钢","HW250*250*9*14",6,{"v":18770,"d":"18770.00"},250,250,9,14,{"v":165.77664,"d":"165.78"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1-1面","H/工字钢","HW300*300*10*15",8,{"v":18770,"d":"18770.00"},300,300,10,15,{"v":265.7832,"d":"265.78"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1-1面","H/工字钢","HW340*250*9*14",5,{"v":18770,"d":"18770.00"},340,250,9,14,{"v":155.0402,"d":"155.04"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1-1面","H/工字钢","HW390*300*10*16",2,{"v":18770,"d":"18770.00"},390,300,10,16,{"v":73.12792,"d":"73.13"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1-1面","2L型钢","TN100*10*5.5*8",20,{"v":4610,"d":"4610.00"},100,100,5.5,8,36.88,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1-1面","2L型钢","TN100*100*5.5*8",14,{"v":4610,"d":"4610.00"},100,100,5.5,8,{"v":25.816,"d":"25.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1-1面","2L型钢","TN100*100*5.5*8",70,{"v":4000,"d":"4000.00"},100,100,5.5,8,{"v":112,"d":"112.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1-1面","2L型钢","TN100*100*5.5*8",28,{"v":4350,"d":"4350.00"},100,100,5.5,8,48.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45  1-1面","2L型钢","TN125*125*6*9",2,{"v":6140,"d":"6140.00"},125,125,6,9,6.14,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45   8.5M层平面","H/工字钢","HN194*150*6*9",2,{"v":199000,"d":"199000.00"},194,150,6,9,386.06,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45   8.5M层平面","H/工字钢","HN300*150*6*9",76,{"v":4000,"d":"4000.00"},300,150,6,9,{"v":359.328,"d":"359.33"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45   8.5M层平面","H/工字钢","HN300*150*6*9",7,{"v":3000,"d":"3000.00"},300,150,6,9,{"v":24.822,"d":"24.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45   8.5M层平面","L型钢","L100*10",2,{"v":224000,"d":"224000.00"},100,100,10,10,{"v":134.4,"d":"134.40"},"翼板重合",null,38,null,{"v":313.6,"d":"313.60"},"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["外线 GK63~K45   8.5M层平面","L型钢","L63*6",14,{"v":5000,"d":"5000.00"},63,63,6,6,17.64,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45   8.5M层平面","L型钢","L63*6",2,{"v":5660,"d":"5660.00"},63,63,6,6,{"v":2.85264,"d":"2.85"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45   8.5M层平面","L型钢","L80*6",128,{"v":5150,"d":"5150.00"},80,80,6,6,{"v":210.944,"d":"210.94"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45   5M层平面","H/工字钢","HN194*150*6*9",2,{"v":224000,"d":"224000.00"},194,150,6,9,367.36,"翼板重合",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45   5M层平面","H/工字钢","HN194*150*6*9",74,{"v":4000,"d":"4000.00"},194,150,6,9,287.12,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45   5M层平面","H/工字钢","HN194*150*6*9",7,{"v":3000,"d":"3000.00"},194,150,6,9,20.37,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45   5M层平面","L型钢","L100*10",2,{"v":224000,"d":"224000.00"},100,100,10,10,{"v":179.2,"d":"179.20"},"无重合面",null,38,null,{"v":313.6,"d":"313.60"},"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0.636363636363636,"d":"64%"}]
["外线 GK63~K45   5M层平面","L型钢","L63*6",14,{"v":5000,"d":"5000.00"},63,63,6,6,17.64,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45   5M层平面","L型钢","L63*6",2,{"v":5660,"d":"5660.00"},63,63,6,6,{"v":2.85264,"d":"2.85"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63~K45   5M层平面","L型钢","L80*6",128,{"v":5150,"d":"5150.00"},80,80,6,6,{"v":210.944,"d":"210.94"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1a-1a面","H/工字钢","HW150*150*7*10",43,{"v":3500,"d":"3500.00"},150,150,7,10,132.44,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1a-1a面","H/工字钢","HW150*150*7*10",32,{"v":4610,"d":"4610.00"},150,150,7,10,{"v":129.8176,"d":"129.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1a-1a面","H/工字钢","HW250*250*9*14",7,{"v":17300,"d":"17300.00"},250,250,9,14,{"v":178.2592,"d":"178.26"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1a-1a面","H/工字钢","HW250*250*9*14",5,{"v":21000,"d":"21000.00"},250,250,9,14,154.56,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1a-1a面","H/工字钢","HW300*300*10*15",2,{"v":21000,"d":"21000.00"},300,300,10,15,74.34,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1a-1a面","H/工字钢","HW340*250*9*14",1,{"v":21000,"d":"21000.00"},340,250,9,14,{"v":34.692,"d":"34.69"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1a-1a面","H/工字钢","HW390*300*10*16",3,{"v":17300,"d":"17300.00"},390,300,10,16,{"v":101.1012,"d":"101.10"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1a-1a面","H/工字钢","HW390*300*10*16",8,{"v":21000,"d":"21000.00"},390,300,10,16,{"v":327.264,"d":"327.26"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1a-1a面","2L型钢","TN100*10*5.5*8",22,{"v":4610,"d":"4610.00"},100,100,5.5,8,{"v":40.568,"d":"40.57"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1a-1a面","2L型钢","TN100*100*5.5*8",76,{"v":3900,"d":"3900.00"},100,100,5.5,8,118.56,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1a-1a面","2L型钢","TN100*100*5.5*8",6,{"v":7800,"d":"7800.00"},100,100,5.5,8,18.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1a-1a面","2L型钢","TN100*100*5.5*8",10,{"v":4350,"d":"4350.00"},100,100,5.5,8,{"v":17.4,"d":"17.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1-1面","H/工字钢","HW150*150*7*10",43,{"v":3500,"d":"3500.00"},150,150,7,10,132.44,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1-1面","H/工字钢","HW150*150*7*10",32,{"v":4610,"d":"4610.00"},150,150,7,10,{"v":129.8176,"d":"129.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1-1面","H/工字钢","HW250*250*9*14",7,{"v":17300,"d":"17300.00"},250,250,9,14,{"v":178.2592,"d":"178.26"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1-1面","H/工字钢","HW250*250*9*14",5,{"v":21000,"d":"21000.00"},250,250,9,14,154.56,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1-1面","H/工字钢","HW250*250*9*14",2,{"v":13500,"d":"13500.00"},250,250,9,14,{"v":39.744,"d":"39.74"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1a-1a面","H/工字钢","HW250*250*9*14",2,{"v":13500,"d":"13500.00"},250,250,9,14,{"v":39.744,"d":"39.74"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1-1面","H/工字钢","HW300*300*10*15",2,{"v":21000,"d":"21000.00"},300,300,10,15,74.34,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1-1面","H/工字钢","HW340*250*9*14",1,{"v":21000,"d":"21000.00"},340,250,9,14,{"v":34.692,"d":"34.69"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1-1面","H/工字钢","HW390*300*10*16",3,{"v":17300,"d":"17300.00"},390,300,10,16,{"v":101.1012,"d":"101.10"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1-1面","H/工字钢","HW390*300*10*16",8,{"v":21000,"d":"21000.00"},390,300,10,16,{"v":327.264,"d":"327.26"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1-1面","2L型钢","TN100*10*5.5*8",22,{"v":4610,"d":"4610.00"},100,100,5.5,8,{"v":40.568,"d":"40.57"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1-1面","2L型钢","TN100*100*5.5*8",76,{"v":3900,"d":"3900.00"},100,100,5.5,8,118.56,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1-1面","2L型钢","TN100*100*5.5*8",6,{"v":7800,"d":"7800.00"},100,100,5.5,8,18.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27 1-1面","2L型钢","TN100*100*5.5*8",10,{"v":4350,"d":"4350.00"},100,100,5.5,8,{"v":17.4,"d":"17.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27  7M层平面","H/工字钢","HM294*200*8*12",2,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":10.912,"d":"10.91"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27  7M层平面","H/工字钢","HM294*200*8*12",4,{"v":3500,"d":"3500.00"},294,200,8,12,{"v":19.096,"d":"19.10"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27  7M层平面","H/工字钢","HM294*200*8*12",4,{"v":3800,"d":"3800.00"},294,200,8,12,{"v":20.7328,"d":"20.73"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27  7M层平面","H/工字钢","HN194*150*6*9",58,{"v":4000,"d":"4000.00"},194,150,6,9,225.04,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27  7M层平面","H/工字钢","HN194*150*6*9",8,{"v":3000,"d":"3000.00"},194,150,6,9,23.28,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27  7M层平面","L型钢","L63*6",12,{"v":5000,"d":"5000.00"},63,63,6,6,15.12,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27  7M层平面","L型钢","L63*6",8,{"v":4250,"d":"4250.00"},63,63,6,6,{"v":8.568,"d":"8.57"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   8.5M层平面","H/工字钢","HM294*200*8*12",2,{"v":7680,"d":"7680.00"},294,200,8,12,{"v":20.95104,"d":"20.95"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   8.5M层平面","H/工字钢","HM294*200*8*12",2,{"v":7000,"d":"7000.00"},294,200,8,12,{"v":19.096,"d":"19.10"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   8.5M层平面","H/工字钢","HM294*200*8*12",2,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":10.912,"d":"10.91"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   8.5M层平面","H/工字钢","HN194*150*6*9",2,{"v":203600,"d":"203600.00"},194,150,6,9,{"v":394.984,"d":"394.98"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   8.5M层平面","H/工字钢","HN300*150*6*9",60,{"v":4000,"d":"4000.00"},300,150,6,9,283.68,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   8.5M层平面","H/工字钢","HN300*150*6*9",8,{"v":3000,"d":"3000.00"},300,150,6,9,{"v":28.368,"d":"28.37"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   8.5M层平面","H/工字钢","HN300*150*6*9",10,{"v":5000,"d":"5000.00"},300,150,6,9,{"v":59.1,"d":"59.10"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   8.5M层平面","L型钢","L100*10",2,{"v":218000,"d":"218000.00"},100,100,10,10,{"v":130.8,"d":"130.80"},"翼板重合",null,38,null,{"v":305.2,"d":"305.20"},"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["外线 K45~GK27   8.5M层平面","L型钢","L63*6",12,{"v":5000,"d":"5000.00"},63,63,6,6,15.12,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   8.5M层平面","L型钢","L63*6",8,{"v":4250,"d":"4250.00"},63,63,6,6,{"v":8.568,"d":"8.57"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   8.5M层平面","L型钢","L80*6",118,{"v":5150,"d":"5150.00"},80,80,6,6,{"v":194.464,"d":"194.46"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   8.5M层平面","L型钢","L80*6",6,{"v":7800,"d":"7800.00"},80,80,6,6,{"v":14.976,"d":"14.98"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   5M层平面","H/工字钢","HM294*200*8*12",2,{"v":7680,"d":"7680.00"},294,200,8,12,{"v":20.95104,"d":"20.95"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   5M层平面","H/工字钢","HM294*200*8*12",2,{"v":7000,"d":"7000.00"},294,200,8,12,{"v":19.096,"d":"19.10"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   5M层平面","H/工字钢","HM294*200*8*12",2,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":10.912,"d":"10.91"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   5M层平面","H/工字钢","HN194*150*6*9",2,{"v":203600,"d":"203600.00"},194,150,6,9,{"v":394.984,"d":"394.98"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   5M层平面","H/工字钢","HN194*150*6*9",60,{"v":4000,"d":"4000.00"},194,150,6,9,{"v":232.8,"d":"232.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   5M层平面","H/工字钢","HN194*150*6*9",8,{"v":3000,"d":"3000.00"},194,150,6,9,23.28,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   5M层平面","H/工字钢","HN194*150*6*9",10,{"v":5000,"d":"5000.00"},194,150,6,9,{"v":48.5,"d":"48.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   5M层平面","L型钢","L100*10",2,{"v":218000,"d":"218000.00"},100,100,10,10,{"v":130.8,"d":"130.80"},"翼板重合",null,38,null,{"v":305.2,"d":"305.20"},"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["外线 K45~GK27   5M层平面","L型钢","L63*6",12,{"v":5000,"d":"5000.00"},63,63,6,6,15.12,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   5M层平面","L型钢","L63*6",8,{"v":4250,"d":"4250.00"},63,63,6,6,{"v":8.568,"d":"8.57"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   5M层平面","L型钢","L80*6",118,{"v":5150,"d":"5150.00"},80,80,6,6,{"v":194.464,"d":"194.46"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 K45~GK27   5M层平面","L型钢","L80*6",6,{"v":7800,"d":"7800.00"},80,80,6,6,{"v":14.976,"d":"14.98"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK27~K8  7M层平面","H/工字钢","HM294*200*8*12",2,{"v":5000,"d":"5000.00"},294,200,8,12,13.64,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK27~K8  7M层平面","H/工字钢","HN194*150*6*9",44,{"v":7800,"d":"7800.00"},194,150,6,9,{"v":332.904,"d":"332.90"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK27~K8  7M层平面","H/工字钢","HN194*150*6*9",70,{"v":5000,"d":"5000.00"},194,150,6,9,{"v":339.5,"d":"339.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK27~K8  7M层平面","H/工字钢","HN194*150*6*9",7,{"v":3000,"d":"3000.00"},194,150,6,9,20.37,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK27~K8  7M层平面","H/工字钢","HN300*150*6*9",3,{"v":5000,"d":"5000.00"},300,150,6,9,17.73,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK27~K8  7M层平面","H/工字钢","HW200*200*8*12",2,{"v":3000,"d":"3000.00"},200,200,8,12,{"v":7.056,"d":"7.06"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK27~K8  7M层平面","L型钢","L63*6",14,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":13.7592,"d":"13.76"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1a-1a面","H/工字钢","HW150*150*7*10",45,{"v":3500,"d":"3500.00"},150,150,7,10,{"v":138.6,"d":"138.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1a-1a面","H/工字钢","HW150*150*7*10",34,{"v":4700,"d":"4700.00"},150,150,7,10,{"v":140.624,"d":"140.62"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1a-1a面","H/工字钢","HW250*250*9*14",2,{"v":13500,"d":"13500.00"},250,250,9,14,{"v":39.744,"d":"39.74"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1a-1a面","H/工字钢","HW250*250*9*14",4,{"v":16500,"d":"16500.00"},250,250,9,14,{"v":97.152,"d":"97.15"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1a-1a面","H/工字钢","HW250*250*9*14",2,{"v":19800,"d":"19800.00"},250,250,9,14,{"v":58.2912,"d":"58.29"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1a-1a面","H/工字钢","HW250*250*9*14",8,{"v":17500,"d":"17500.00"},250,250,9,14,206.08,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1a-1a面","H/工字钢","HW300*300*10*15",2,{"v":17500,"d":"17500.00"},300,300,10,15,61.95,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1a-1a面","H/工字钢","HW340*250*9*14",1,{"v":13500,"d":"13500.00"},340,250,9,14,{"v":22.302,"d":"22.30"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1a-1a面","H/工字钢","HW340*250*9*14",5,{"v":16500,"d":"16500.00"},340,250,9,14,136.29,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1a-1a面","H/工字钢","HW340*250*9*14",2,{"v":17500,"d":"17500.00"},340,250,9,14,57.82,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1a-1a面","H/工字钢","HW390*300*10*16",2,{"v":17500,"d":"17500.00"},390,300,10,16,68.18,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1a-1a面","2L型钢","TN100*10*5.5*8",22,{"v":4700,"d":"4700.00"},100,100,5.5,8,41.36,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1a-1a面","2L型钢","TN100*100*5.5*8",96,{"v":3900,"d":"3900.00"},100,100,5.5,8,149.76,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1a-1a面","2L型钢","TN100*100*5.5*8",12,{"v":4700,"d":"4700.00"},100,100,5.5,8,22.56,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1-1面","H/工字钢","HW150*150*7*10",45,{"v":3500,"d":"3500.00"},150,150,7,10,{"v":138.6,"d":"138.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1-1面","H/工字钢","HW150*150*7*10",34,{"v":4700,"d":"4700.00"},150,150,7,10,{"v":140.624,"d":"140.62"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1-1面","H/工字钢","HW250*250*9*14",2,{"v":13500,"d":"13500.00"},250,250,9,14,{"v":39.744,"d":"39.74"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1-1面","H/工字钢","HW250*250*9*14",4,{"v":16500,"d":"16500.00"},250,250,9,14,{"v":97.152,"d":"97.15"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1-1面","H/工字钢","HW250*250*9*14",2,{"v":19800,"d":"19800.00"},250,250,9,14,{"v":58.2912,"d":"58.29"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1-1面","H/工字钢","HW250*250*9*14",8,{"v":17500,"d":"17500.00"},250,250,9,14,206.08,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1-1面","H/工字钢","HW300*300*10*15",2,{"v":17500,"d":"17500.00"},300,300,10,15,61.95,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1-1面","H/工字钢","HW340*250*9*14",1,{"v":13500,"d":"13500.00"},340,250,9,14,{"v":22.302,"d":"22.30"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1-1面","H/工字钢","HW340*250*9*14",5,{"v":16500,"d":"16500.00"},340,250,9,14,136.29,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1-1面","H/工字钢","HW340*250*9*14",2,{"v":17500,"d":"17500.00"},340,250,9,14,57.82,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1-1面","H/工字钢","HW390*300*10*16",2,{"v":17500,"d":"17500.00"},390,300,10,16,68.18,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1-1面","2L型钢","TN100*10*5.5*8",22,{"v":4700,"d":"4700.00"},100,100,5.5,8,41.36,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1-1面","2L型钢","TN100*100*5.5*8",96,{"v":3900,"d":"3900.00"},100,100,5.5,8,149.76,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8   1-1面","2L型钢","TN100*100*5.5*8",12,{"v":4700,"d":"4700.00"},100,100,5.5,8,22.56,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8    8.5M层平面","H/工字钢","HN194*150*6*9",2,{"v":220000,"d":"220000.00"},194,150,6,9,{"v":426.8,"d":"426.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8    8.5M层平面","H/工字钢","HN300*150*6*9",4,{"v":5000,"d":"5000.00"},300,150,6,9,23.64,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8    8.5M层平面","H/工字钢","HN300*150*6*9",74,{"v":5000,"d":"5000.00"},300,150,6,9,437.34,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8    8.5M层平面","H/工字钢","HN300*150*6*9",7,{"v":3000,"d":"3000.00"},300,150,6,9,{"v":24.822,"d":"24.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8    8.5M层平面","L型钢","L100*10",2,{"v":220000,"d":"220000.00"},100,100,10,10,{"v":132,"d":"132.00"},"翼板重合",null,38,null,{"v":308,"d":"308.00"},"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
[" GK27~K8    8.5M层平面","L型钢","L63*6",14,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":13.7592,"d":"13.76"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8    8.5M层平面","L型钢","L80*6",44,{"v":7800,"d":"7800.00"},80,80,6,6,{"v":109.824,"d":"109.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8    8.5M层平面","L型钢","L80*6",38,{"v":6000,"d":"6000.00"},80,80,6,6,72.96,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8    5M层平面","H/工字钢","HN194*150*6*9",2,{"v":220000,"d":"220000.00"},194,150,6,9,{"v":426.8,"d":"426.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8    5M层平面","H/工字钢","HN194*150*6*9",74,{"v":5000,"d":"5000.00"},194,150,6,9,{"v":358.9,"d":"358.90"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8    5M层平面","H/工字钢","HN194*150*6*9",7,{"v":3000,"d":"3000.00"},194,150,6,9,20.37,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8    5M层平面","H/工字钢","HN300*150*6*9",4,{"v":5000,"d":"5000.00"},300,150,6,9,23.64,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8    5M层平面","L型钢","L100*10",2,{"v":220000,"d":"220000.00"},100,100,10,10,{"v":132,"d":"132.00"},"翼板重合",null,38,null,{"v":308,"d":"308.00"},"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
[" GK27~K8    5M层平面","L型钢","L63*6",14,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":13.7592,"d":"13.76"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8    5M层平面","L型钢","L80*6",44,{"v":7800,"d":"7800.00"},80,80,6,6,{"v":109.824,"d":"109.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" GK27~K8    5M层平面","L型钢","L80*6",38,{"v":6000,"d":"6000.00"},80,80,6,6,72.96,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1a-1a面","H/工字钢","HW150*150*7*10",38,{"v":3500,"d":"3500.00"},150,150,7,10,117.04,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1a-1a面","H/工字钢","HW150*150*7*10",30,{"v":4700,"d":"4700.00"},150,150,7,10,124.08,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1a-1a面","H/工字钢","HW200*200*8*12",2,{"v":13500,"d":"13500.00"},200,200,8,12,{"v":31.752,"d":"31.75"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1a-1a面","H/工字钢","HW200*200*8*12",2,{"v":14200,"d":"14200.00"},200,200,8,12,{"v":33.3984,"d":"33.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1a-1a面","H/工字钢","HW250*250*9*14",8,{"v":18400,"d":"18400.00"},250,250,9,14,{"v":216.6784,"d":"216.68"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1a-1a面","H/工字钢","HW340*250*9*14",4,{"v":13500,"d":"13500.00"},340,250,9,14,{"v":89.208,"d":"89.21"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1a-1a面","H/工字钢","HW340*250*9*14",3,{"v":14200,"d":"14200.00"},340,250,9,14,{"v":70.3752,"d":"70.38"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1a-1a面","H/工字钢","HW390*300*10*16",4,{"v":18400,"d":"18400.00"},390,300,10,16,{"v":143.3728,"d":"143.37"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1a-1a面","2L型钢","TN100*10*5.5*8",16,{"v":4700,"d":"4700.00"},100,100,5.5,8,30.08,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1a-1a面","2L型钢","TN100*100*5.5*8",62,{"v":3900,"d":"3900.00"},100,100,5.5,8,96.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1a-1a面","2L型钢","TN100*100*5.5*8",24,{"v":4700,"d":"4700.00"},100,100,5.5,8,45.12,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1-1面","H/工字钢","HW150*150*7*10",38,{"v":3500,"d":"3500.00"},150,150,7,10,117.04,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1-1面","H/工字钢","HW150*150*7*10",30,{"v":4700,"d":"4700.00"},150,150,7,10,124.08,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1-1面","H/工字钢","HW200*200*8*12",2,{"v":13500,"d":"13500.00"},200,200,8,12,{"v":31.752,"d":"31.75"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1-1面","H/工字钢","HW200*200*8*12",2,{"v":14200,"d":"14200.00"},200,200,8,12,{"v":33.3984,"d":"33.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1-1面","H/工字钢","HW250*250*9*14",8,{"v":18400,"d":"18400.00"},250,250,9,14,{"v":216.6784,"d":"216.68"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1-1面","H/工字钢","HW340*250*9*14",4,{"v":13500,"d":"13500.00"},340,250,9,14,{"v":89.208,"d":"89.21"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1-1面","H/工字钢","HW340*250*9*14",3,{"v":14200,"d":"14200.00"},340,250,9,14,{"v":70.3752,"d":"70.38"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1-1面","H/工字钢","HW390*300*10*16",4,{"v":18400,"d":"18400.00"},390,300,10,16,{"v":143.3728,"d":"143.37"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1-1面","2L型钢","TN100*10*5.5*8",16,{"v":4700,"d":"4700.00"},100,100,5.5,8,30.08,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1-1面","2L型钢","TN100*100*5.5*8",62,{"v":3900,"d":"3900.00"},100,100,5.5,8,96.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["K8~GK1、K65~GK73  1-1面","2L型钢","TN100*100*5.5*8",24,{"v":4700,"d":"4700.00"},100,100,5.5,8,45.12,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   8.5米平面","H/工字钢","HM294*200*8*12",3,{"v":7000,"d":"7000.00"},294,200,8,12,{"v":28.644,"d":"28.64"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   8.5米平面","H/工字钢","HN194*150*6*9",2,{"v":182300,"d":"182300.00"},194,150,6,9,{"v":353.662,"d":"353.66"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   8.5米平面","H/工字钢","HN300*150*6*9",61,{"v":5000,"d":"5000.00"},300,150,6,9,360.51,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   8.5米平面","H/工字钢","HN300*150*6*9",5,{"v":3000,"d":"3000.00"},300,150,6,9,17.73,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   8.5米平面","L型钢","L100*10",2,{"v":189300,"d":"189300.00"},100,100,10,10,113.58,"翼板重合",null,38,null,265.02,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
[" K8~GK1、K65~GK73   8.5米平面","L型钢","L63*6",20,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":19.656,"d":"19.66"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   8.5米平面","L型钢","L80*6",32,{"v":7800,"d":"7800.00"},80,80,6,6,{"v":79.872,"d":"79.87"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   8.5米平面","L型钢","L80*6",48,{"v":6000,"d":"6000.00"},80,80,6,6,92.16,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   7米平面","H/工字钢","HM294*200*8*12",3,{"v":5000,"d":"5000.00"},294,200,8,12,20.46,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   7米平面","H/工字钢","HN194*150*6*9",2,{"v":4000,"d":"4000.00"},194,150,6,9,7.76,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   7米平面","H/工字钢","HN194*150*6*9",61,{"v":5000,"d":"5000.00"},194,150,6,9,295.85,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   7米平面","H/工字钢","HN194*150*6*9",15,{"v":3000,"d":"3000.00"},194,150,6,9,43.65,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   7米平面","L型钢","L63*6",20,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":19.656,"d":"19.66"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   7米平面","L型钢","L80*6",2,{"v":6400,"d":"6400.00"},80,80,6,6,{"v":4.096,"d":"4.10"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   5米平面","H/工字钢","HM294*200*8*12",3,{"v":7000,"d":"7000.00"},294,200,8,12,{"v":28.644,"d":"28.64"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   5米平面","H/工字钢","HN194*150*6*9",2,{"v":182300,"d":"182300.00"},194,150,6,9,{"v":353.662,"d":"353.66"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   5米平面","H/工字钢","HN194*150*6*9",61,{"v":5000,"d":"5000.00"},194,150,6,9,295.85,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   5米平面","H/工字钢","HN194*150*6*9",5,{"v":3000,"d":"3000.00"},194,150,6,9,14.55,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   5米平面","L型钢","L100*10",2,{"v":189300,"d":"189300.00"},100,100,10,10,113.58,"翼板重合",null,38,null,265.02,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
[" K8~GK1、K65~GK73   5米平面","L型钢","L63*6",20,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":19.656,"d":"19.66"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   5米平面","L型钢","L80*6",32,{"v":7800,"d":"7800.00"},80,80,6,6,{"v":79.872,"d":"79.87"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" K8~GK1、K65~GK73   5米平面","L型钢","L80*6",48,{"v":6000,"d":"6000.00"},80,80,6,6,92.16,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63支架 ","H/工字钢","HN300*150*6*9",2,{"v":4000,"d":"4000.00"},300,150,6,9,{"v":9.456,"d":"9.46"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63支架 ","2L型钢","TN125*125*6*9",2,{"v":6400,"d":"6400.00"},125,125,6,9,{"v":6.4,"d":"6.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK63支架 ","2L型钢","TN125*125*6*9",2,{"v":6400,"d":"6400.00"},125,125,6,9,{"v":6.4,"d":"6.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架一  K62- K59","H/工字钢","HM294*200*8*12",4,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":21.824,"d":"21.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架一  K62- K59","H/工字钢","HN300*150*6*9",8,{"v":4000,"d":"4000.00"},300,150,6,9,{"v":37.824,"d":"37.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架一  K62- K59","2L型钢","TN125*125*6*9",8,{"v":6400,"d":"6400.00"},125,125,6,9,{"v":25.6,"d":"25.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架五  K37、35-33","H/工字钢","HM294*200*8*12",12,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":65.472,"d":"65.47"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架五  K37、35-33","H/工字钢","HM340*250*9*14",4,{"v":4000,"d":"4000.00"},340,250,9,14,{"v":26.432,"d":"26.43"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架五  K37、35-33","H/工字钢","HN194*150*6*9",2,{"v":1000,"d":"1000.00"},194,150,6,9,1.94,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架五  K37、35-33","H/工字钢","HN300*150*6*9",8,{"v":4000,"d":"4000.00"},300,150,6,9,{"v":37.824,"d":"37.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架五  K37、35-33","H/工字钢","HW200*200*8*12",4,{"v":4000,"d":"4000.00"},200,200,8,12,{"v":18.816,"d":"18.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架五  K37、35-33","L型钢","L63*6",2,{"v":1400,"d":"1400.00"},63,63,6,6,{"v":0.7056,"d":"0.71"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架五  K37、35-33","2L型钢","TN150*150*6*9",8,{"v":6400,"d":"6400.00"},150,150,6,9,30.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架四  K39、38、31、30","H/工字钢","HM294*200*8*12",16,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":87.296,"d":"87.30"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架四  K39、38、31、30","H/工字钢","HM340*250*9*14",4,{"v":4000,"d":"4000.00"},340,250,9,14,{"v":26.432,"d":"26.43"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架四  K39、38、31、30","H/工字钢","HN194*150*6*9",2,{"v":1000,"d":"1000.00"},194,150,6,9,1.94,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架四  K39、38、31、30","H/工字钢","HN300*150*6*9",8,{"v":4000,"d":"4000.00"},300,150,6,9,{"v":37.824,"d":"37.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架四  K39、38、31、30","H/工字钢","HW200*200*8*12",8,{"v":1800,"d":"1800.00"},200,200,8,12,{"v":16.9344,"d":"16.93"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架四  K39、38、31、30","L型钢","L63*6",2,{"v":1400,"d":"1400.00"},63,63,6,6,{"v":0.7056,"d":"0.71"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架四  K39、38、31、30","2L型钢","TN150*150*6*9",8,{"v":6400,"d":"6400.00"},150,150,6,9,30.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架十  K8、6、5、2","H/工字钢","HM294*200*8*12",12,{"v":5000,"d":"5000.00"},294,200,8,12,81.84,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架十  K8、6、5、2","H/工字钢","HM340*250*9*14",12,{"v":5000,"d":"5000.00"},340,250,9,14,99.12,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架十  K8、6、5、2","H/工字钢","HN194*150*6*9",2,{"v":1400,"d":"1400.00"},194,150,6,9,{"v":2.716,"d":"2.72"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架十  K8、6、5、2","H/工字钢","HW200*200*8*12",1,{"v":1900,"d":"1900.00"},200,200,8,12,{"v":2.2344,"d":"2.23"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架十  K8、6、5、2","2L型钢","TN100*100*5.5*8",2,{"v":2870,"d":"2870.00"},100,100,5.5,8,{"v":2.296,"d":"2.30"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架十  K8、6、5、2","2L型钢","TN150*150*6*9",8,{"v":7070,"d":"7070.00"},150,150,6,9,{"v":33.936,"d":"33.94"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架十  K8、6、5、2","2L型钢","TN150*150*6*9",1,{"v":2000,"d":"2000.00"},150,150,6,9,{"v":1.2,"d":"1.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架三  K47,45,44，42","H/工字钢","HM294*200*8*12",16,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":87.296,"d":"87.30"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架三  K47,45,44，42","H/工字钢","HN300*150*6*9",8,{"v":4000,"d":"4000.00"},300,150,6,9,{"v":37.824,"d":"37.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架三  K47,45,44，42","H/工字钢","HW200*200*8*12",8,{"v":1800,"d":"1800.00"},200,200,8,12,{"v":16.9344,"d":"16.93"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架三  K47,45,44，42","2L型钢","TN150*150*6*9",8,{"v":6400,"d":"6400.00"},150,150,6,9,30.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架七  K25、23、19、18、16、15、13","H/工字钢","HM294*200*8*12",32,{"v":5000,"d":"5000.00"},294,200,8,12,218.24,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架七  K25、23、19、18、16、15、13","H/工字钢","HM340*250*9*14",16,{"v":5000,"d":"5000.00"},340,250,9,14,132.16,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架七  K25、23、19、18、16、15、13","H/工字钢","HN194*150*6*9",1,{"v":1000,"d":"1000.00"},194,150,6,9,0.97,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架七  K25、23、19、18、16、15、13","H/工字钢","HN300*150*6*9",1,{"v":1500,"d":"1500.00"},300,150,6,9,{"v":1.773,"d":"1.77"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架七  K25、23、19、18、16、15、13","2L型钢","TN100*100*5.5*8",1,{"v":2700,"d":"2700.00"},100,100,5.5,8,1.08,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架七  K25、23、19、18、16、15、13","2L型钢","TN100*100*5.5*8",1,{"v":2120,"d":"2120.00"},100,100,5.5,8,{"v":0.848,"d":"0.85"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架七  K25、23、19、18、16、15、13","2L型钢","TN150*150*6*9",16,{"v":7070,"d":"7070.00"},150,150,6,9,{"v":67.872,"d":"67.87"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架六  K28、26","H/工字钢","HM294*200*8*12",12,{"v":5000,"d":"5000.00"},294,200,8,12,81.84,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架六  K28、26","H/工字钢","HM390*300*10*16",3,{"v":5000,"d":"5000.00"},390,300,10,16,29.22,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架六  K28、26","2L型钢","TN150*150*6*9",6,{"v":7070,"d":"7070.00"},150,150,6,9,{"v":25.452,"d":"25.45"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架九  K70-72爬梯","H/工字钢","HN194*150*6*9",1,{"v":25000,"d":"25000.00"},194,150,6,9,24.25,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架九  K70-72","H/工字钢","HM294*200*8*12",12,{"v":5000,"d":"5000.00"},294,200,8,12,81.84,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架九  K70-72","H/工字钢","HM340*250*9*14",8,{"v":5000,"d":"5000.00"},340,250,9,14,66.08,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架九  K70-72","H/工字钢","HM340*250*9*14",1,{"v":1000,"d":"1000.00"},340,250,9,14,{"v":1.652,"d":"1.65"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架九  K70-72","H/工字钢","HN194*150*6*9",1,{"v":1000,"d":"1000.00"},194,150,6,9,0.97,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架九  K70-72","H/工字钢","HN300*150*6*9",6,{"v":2000,"d":"2000.00"},300,150,6,9,{"v":14.184,"d":"14.18"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架九  K70-72","2L型钢","TN100*100*5.5*8",1,{"v":2870,"d":"2870.00"},100,100,5.5,8,{"v":1.148,"d":"1.15"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架九  K70-72","2L型钢","TN100*100*5.5*8",1,{"v":1400,"d":"1400.00"},100,100,5.5,8,0.56,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架九  K70-72","2L型钢","TN100*100*5.5*8",6,{"v":2820,"d":"2820.00"},100,100,5.5,8,{"v":6.768,"d":"6.77"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架九  K70-72","2L型钢","TN150*150*6*9",8,{"v":7070,"d":"7070.00"},150,150,6,9,{"v":33.936,"d":"33.94"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架二  K57-53， K51","H/工字钢","HM294*200*8*12",12,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":65.472,"d":"65.47"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架二  K57-53， K51","H/工字钢","HN300*150*6*9",12,{"v":4000,"d":"4000.00"},300,150,6,9,{"v":56.736,"d":"56.74"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架二  K57-53， K51","H/工字钢","HW200*200*8*12",12,{"v":4000,"d":"4000.00"},200,200,8,12,{"v":56.448,"d":"56.45"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架二  K57-53， K51","2L型钢","TN150*150*6*9",12,{"v":6400,"d":"6400.00"},150,150,6,9,46.08,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架八  K68-65","H/工字钢","HM294*200*8*12",12,{"v":5000,"d":"5000.00"},294,200,8,12,81.84,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架八  K68-65","H/工字钢","HM340*250*9*14",8,{"v":5000,"d":"5000.00"},340,250,9,14,66.08,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架八  K68-65","H/工字钢","HN194*150*6*9",1,{"v":1000,"d":"1000.00"},194,150,6,9,0.97,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架八  K68-65","2L型钢","TN100*100*5.5*8",1,{"v":2870,"d":"2870.00"},100,100,5.5,8,{"v":1.148,"d":"1.15"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["单片支架八  K68-65","2L型钢","TN150*150*6*9",8,{"v":7070,"d":"7070.00"},150,150,6,9,{"v":33.936,"d":"33.94"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK58支架 ","H/工字钢","HM294*200*8*12",4,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":21.824,"d":"21.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK58支架 ","H/工字钢","HN194*150*6*9",2,{"v":3000,"d":"3000.00"},194,150,6,9,5.82,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK58支架 ","H/工字钢","HN194*150*6*9",1,{"v":5000,"d":"5000.00"},194,150,6,9,4.85,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK58支架 ","H/工字钢","HN300*150*6*9",10,{"v":4000,"d":"4000.00"},300,150,6,9,47.28,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK58支架 ","H/工字钢","HW200*200*8*12",2,{"v":4000,"d":"4000.00"},200,200,8,12,{"v":9.408,"d":"9.41"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK58支架 ","H/工字钢","HW200*200*8*12",4,{"v":3000,"d":"3000.00"},200,200,8,12,{"v":14.112,"d":"14.11"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK58支架 ","H/工字钢","HW200*200*8*12",4,{"v":4000,"d":"4000.00"},200,200,8,12,{"v":18.816,"d":"18.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK58支架 ","L型钢","L63*6",5,{"v":5000,"d":"5000.00"},63,63,6,6,{"v":6.3,"d":"6.30"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK58支架 ","2L型钢","TN100*100*5.5*8",2,{"v":2400,"d":"2400.00"},100,100,5.5,8,1.92,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK58支架 ","2L型钢","TN125*125*6*9",8,{"v":6400,"d":"6400.00"},125,125,6,9,{"v":25.6,"d":"25.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK55支架 ","H/工字钢","HM294*200*8*12",4,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":21.824,"d":"21.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK55支架 ","H/工字钢","HN194*150*6*9",2,{"v":3000,"d":"3000.00"},194,150,6,9,5.82,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK55支架 ","H/工字钢","HN194*150*6*9",1,{"v":5000,"d":"5000.00"},194,150,6,9,4.85,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK55支架 ","H/工字钢","HN300*150*6*9",10,{"v":4000,"d":"4000.00"},300,150,6,9,47.28,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK55支架 ","H/工字钢","HW200*200*8*12",2,{"v":4000,"d":"4000.00"},200,200,8,12,{"v":9.408,"d":"9.41"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK55支架 ","H/工字钢","HW200*200*8*12",4,{"v":3000,"d":"3000.00"},200,200,8,12,{"v":14.112,"d":"14.11"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK55支架 ","H/工字钢","HW200*200*8*12",4,{"v":4000,"d":"4000.00"},200,200,8,12,{"v":18.816,"d":"18.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK55支架 ","L型钢","L63*6",5,{"v":5000,"d":"5000.00"},63,63,6,6,{"v":6.3,"d":"6.30"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK55支架 ","2L型钢","TN100*100*5.5*8",2,{"v":2400,"d":"2400.00"},100,100,5.5,8,1.92,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK55支架 ","2L型钢","TN125*125*6*9",8,{"v":6400,"d":"6400.00"},125,125,6,9,{"v":25.6,"d":"25.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK52支架 ","H/工字钢","HM294*200*8*12",4,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":21.824,"d":"21.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK52支架 ","H/工字钢","HN194*150*6*9",2,{"v":3000,"d":"3000.00"},194,150,6,9,5.82,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK52支架 ","H/工字钢","HN194*150*6*9",1,{"v":5000,"d":"5000.00"},194,150,6,9,4.85,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK52支架 ","H/工字钢","HN300*150*6*9",10,{"v":4000,"d":"4000.00"},300,150,6,9,47.28,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK52支架 ","H/工字钢","HW200*200*8*12",2,{"v":4000,"d":"4000.00"},200,200,8,12,{"v":9.408,"d":"9.41"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK52支架 ","H/工字钢","HW200*200*8*12",4,{"v":3000,"d":"3000.00"},200,200,8,12,{"v":14.112,"d":"14.11"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK52支架 ","H/工字钢","HW200*200*8*12",4,{"v":4000,"d":"4000.00"},200,200,8,12,{"v":18.816,"d":"18.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK52支架 ","L型钢","L63*6",5,{"v":5000,"d":"5000.00"},63,63,6,6,{"v":6.3,"d":"6.30"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK52支架 ","2L型钢","TN100*100*5.5*8",2,{"v":2400,"d":"2400.00"},100,100,5.5,8,1.92,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK52支架 ","2L型钢","TN125*125*6*9",8,{"v":6400,"d":"6400.00"},125,125,6,9,{"v":25.6,"d":"25.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK50支架 ","H/工字钢","HM294*200*8*12",6,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":32.736,"d":"32.74"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK50支架 ","H/工字钢","HM340*250*9*14",2,{"v":4000,"d":"4000.00"},340,250,9,14,{"v":13.216,"d":"13.22"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK50支架 ","H/工字钢","HN300*150*6*9",4,{"v":4000,"d":"4000.00"},300,150,6,9,{"v":18.912,"d":"18.91"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK50支架 ","2L型钢","TN100*100*5.5*8",6,{"v":2800,"d":"2800.00"},100,100,5.5,8,6.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK50支架 ","2L型钢","TN125*125*6*9",4,{"v":6400,"d":"6400.00"},125,125,6,9,{"v":12.8,"d":"12.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK49支架 ","H/工字钢","HM294*200*8*12",6,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":32.736,"d":"32.74"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK49支架 ","H/工字钢","HM340*250*9*14",2,{"v":4000,"d":"4000.00"},340,250,9,14,{"v":13.216,"d":"13.22"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK49支架 ","H/工字钢","HN300*150*6*9",4,{"v":4000,"d":"4000.00"},300,150,6,9,{"v":18.912,"d":"18.91"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK49支架 ","2L型钢","TN100*100*5.5*8",6,{"v":2800,"d":"2800.00"},100,100,5.5,8,6.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK49支架 ","2L型钢","TN125*125*6*9",4,{"v":6400,"d":"6400.00"},125,125,6,9,{"v":12.8,"d":"12.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK48支架 ","H/工字钢","HM294*200*8*12",6,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":32.736,"d":"32.74"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK48支架 ","H/工字钢","HM390*300*10*16",2,{"v":4000,"d":"4000.00"},390,300,10,16,{"v":15.584,"d":"15.58"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK48支架 ","H/工字钢","HN194*150*6*9",7,{"v":3000,"d":"3000.00"},194,150,6,9,20.37,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK48支架 ","H/工字钢","HN300*150*6*9",4,{"v":4000,"d":"4000.00"},300,150,6,9,{"v":18.912,"d":"18.91"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK48支架 ","H/工字钢","HW200*200*8*12",2,{"v":1700,"d":"1700.00"},200,200,8,12,{"v":3.9984,"d":"4.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK48支架 ","L型钢","L63*6",2,{"v":2500,"d":"2500.00"},63,63,6,6,1.26,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK48支架 ","L型钢","L63*6",4,{"v":4000,"d":"4000.00"},63,63,6,6,{"v":4.032,"d":"4.03"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK48支架 ","L型钢","L63*6",4,{"v":5000,"d":"5000.00"},63,63,6,6,5.04,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK48支架 ","L型钢","L80*6",2,{"v":4000,"d":"4000.00"},80,80,6,6,2.56,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK48支架 ","2L型钢","TN100*100*5.5*8",6,{"v":2800,"d":"2800.00"},100,100,5.5,8,6.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK48支架 ","2L型钢","TN125*125*6*9",6,{"v":1500,"d":"1500.00"},125,125,6,9,{"v":4.5,"d":"4.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK46支架 ","H/工字钢","HM294*200*8*12",6,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":32.736,"d":"32.74"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK46支架 ","H/工字钢","HM390*300*10*16",2,{"v":4000,"d":"4000.00"},390,300,10,16,{"v":15.584,"d":"15.58"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK46支架 ","H/工字钢","HN194*150*6*9",1,{"v":3000,"d":"3000.00"},194,150,6,9,2.91,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK46支架 ","H/工字钢","HN300*150*6*9",13,{"v":4000,"d":"4000.00"},300,150,6,9,{"v":61.464,"d":"61.46"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK46支架 ","H/工字钢","HW200*200*8*12",6,{"v":1700,"d":"1700.00"},200,200,8,12,{"v":11.9952,"d":"12.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK46支架 ","L型钢","L63*6",2,{"v":5000,"d":"5000.00"},63,63,6,6,2.52,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK46支架 ","L型钢","L80*6",7,{"v":5000,"d":"5000.00"},80,80,6,6,{"v":11.2,"d":"11.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK46支架 ","2L型钢","TN100*100*5.5*8",6,{"v":2800,"d":"2800.00"},100,100,5.5,8,6.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK46支架 ","2L型钢","TN125*125*6*9",2,{"v":6400,"d":"6400.00"},125,125,6,9,{"v":6.4,"d":"6.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK43支架 ","H/工字钢","HM294*200*8*12",6,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":32.736,"d":"32.74"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK43支架 ","H/工字钢","HM390*300*10*16",2,{"v":4000,"d":"4000.00"},390,300,10,16,{"v":15.584,"d":"15.58"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK43支架 ","H/工字钢","HN194*150*6*9",1,{"v":3000,"d":"3000.00"},194,150,6,9,2.91,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK43支架 ","H/工字钢","HN300*150*6*9",4,{"v":4000,"d":"4000.00"},300,150,6,9,{"v":18.912,"d":"18.91"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK43支架 ","L型钢","L63*6",2,{"v":5000,"d":"5000.00"},63,63,6,6,2.52,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK43支架 ","2L型钢","TN125*125*6*9",4,{"v":6400,"d":"6400.00"},125,125,6,9,{"v":12.8,"d":"12.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK43支架 ","2L型钢","TN125*125*6*9",5,{"v":1400,"d":"1400.00"},125,125,6,9,{"v":3.5,"d":"3.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK41支架 ","H/工字钢","HM294*200*8*12",6,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":32.736,"d":"32.74"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK41支架 ","H/工字钢","HM390*300*10*16",2,{"v":4000,"d":"4000.00"},390,300,10,16,{"v":15.584,"d":"15.58"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK41支架 ","H/工字钢","HN194*150*6*9",1,{"v":3000,"d":"3000.00"},194,150,6,9,2.91,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK41支架 ","H/工字钢","HN300*150*6*9",13,{"v":4000,"d":"4000.00"},300,150,6,9,{"v":61.464,"d":"61.46"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK41支架 ","H/工字钢","HW200*200*8*12",6,{"v":1700,"d":"1700.00"},200,200,8,12,{"v":11.9952,"d":"12.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK41支架 ","L型钢","L63*6",2,{"v":5000,"d":"5000.00"},63,63,6,6,2.52,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK41支架 ","L型钢","L80*6",7,{"v":5000,"d":"5000.00"},80,80,6,6,{"v":11.2,"d":"11.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK41支架 ","2L型钢","TN100*100*5.5*8",6,{"v":2800,"d":"2800.00"},100,100,5.5,8,6.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK41支架 ","2L型钢","TN125*125*6*9",2,{"v":6400,"d":"6400.00"},125,125,6,9,{"v":6.4,"d":"6.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK40支架 ","H/工字钢","HM294*200*8*12",8,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":43.648,"d":"43.65"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK40支架 ","H/工字钢","HM390*300*10*16",3,{"v":4000,"d":"4000.00"},390,300,10,16,{"v":23.376,"d":"23.38"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK40支架 ","H/工字钢","HN300*150*6*9",5,{"v":4000,"d":"4000.00"},300,150,6,9,23.64,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK40支架 ","L型钢","L63*6",4,{"v":5000,"d":"5000.00"},63,63,6,6,5.04,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK40支架 ","L型钢","L80*6",1,{"v":5000,"d":"5000.00"},80,80,6,6,{"v":1.6,"d":"1.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK40支架 ","2L型钢","TN125*125*6*9",4,{"v":6400,"d":"6400.00"},125,125,6,9,{"v":12.8,"d":"12.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK36\\32支架 ","H/工字钢","HM294*200*8*12",12,{"v":4000,"d":"4000.00"},294,200,8,12,{"v":65.472,"d":"65.47"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK36\\32支架 ","H/工字钢","HM390*300*10*16",4,{"v":4000,"d":"4000.00"},390,300,10,16,{"v":31.168,"d":"31.17"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK36\\32支架 ","H/工字钢","HN194*150*6*9",1,{"v":3000,"d":"3000.00"},194,150,6,9,2.91,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK36\\32支架 ","H/工字钢","HN194*150*6*9",2,{"v":4000,"d":"4000.00"},194,150,6,9,7.76,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK36\\32支架 ","H/工字钢","HN300*150*6*9",8,{"v":4000,"d":"4000.00"},300,150,6,9,{"v":37.824,"d":"37.82"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK36\\32支架 ","H/工字钢","HN300*150*6*9",3,{"v":3000,"d":"3000.00"},300,150,6,9,{"v":10.638,"d":"10.64"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK36\\32支架 ","L型钢","L63*6",10,{"v":5000,"d":"5000.00"},63,63,6,6,{"v":12.6,"d":"12.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK36\\32支架 ","2L型钢","TN100*100*5.5*8",8,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":4.8,"d":"4.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK36\\32支架 ","2L型钢","TN125*125*6*9",8,{"v":6400,"d":"6400.00"},125,125,6,9,{"v":25.6,"d":"25.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK36\\32支架 ","2L型钢","TN125*125*6*9",10,{"v":1400,"d":"1400.00"},125,125,6,9,{"v":7,"d":"7.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK29支架 ","H/工字钢","HM294*200*8*12",12,{"v":5000,"d":"5000.00"},294,200,8,12,81.84,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK29支架 ","H/工字钢","HM340*250*9*14",2,{"v":5000,"d":"5000.00"},340,250,9,14,16.52,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK29支架 ","L型钢","L63*6",8,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":7.8624,"d":"7.86"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK29支架 ","2L型钢","TN125*125*6*9",4,{"v":7000,"d":"7000.00"},125,125,6,9,{"v":14,"d":"14.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK27支架 ","H/工字钢","HM294*200*8*12",8,{"v":5000,"d":"5000.00"},294,200,8,12,54.56,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK27支架 ","H/工字钢","HM340*250*9*14",2,{"v":5000,"d":"5000.00"},340,250,9,14,16.52,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK27支架 ","L型钢","L63*6",8,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":7.8624,"d":"7.86"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK27支架 ","2L型钢","TN125*125*6*9",4,{"v":7000,"d":"7000.00"},125,125,6,9,{"v":14,"d":"14.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK22支架 ","H/工字钢","HM294*200*8*12",14,{"v":5000,"d":"5000.00"},294,200,8,12,95.48,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK22支架 ","L型钢","L63*6",15,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":14.742,"d":"14.74"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK22支架 ","2L型钢","TN125*125*6*9",4,{"v":7000,"d":"7000.00"},125,125,6,9,{"v":14,"d":"14.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK21支架 ","H/工字钢","HM294*200*8*12",12,{"v":5000,"d":"5000.00"},294,200,8,12,81.84,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK21支架 ","H/工字钢","HN194*150*6*9",4,{"v":4000,"d":"4000.00"},194,150,6,9,15.52,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK21支架 ","L型钢","L63*6",4,{"v":6400,"d":"6400.00"},63,63,6,6,{"v":6.4512,"d":"6.45"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK21支架 ","L型钢","L80*6",4,{"v":6400,"d":"6400.00"},80,80,6,6,{"v":8.192,"d":"8.19"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK21支架 ","2L型钢","TN125*125*6*9",4,{"v":7000,"d":"7000.00"},125,125,6,9,{"v":14,"d":"14.00"},"无重合面",null,38,null,{"v":60.8,"d":"60.80"},"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0.812834224598931,"d":"81%"}]
["外线 GK20支架 ","H/工字钢","HM294*200*8*12",10,{"v":5000,"d":"5000.00"},294,200,8,12,{"v":68.2,"d":"68.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK20支架 ","H/工字钢","HM390*300*10*16",4,{"v":5000,"d":"5000.00"},390,300,10,16,38.96,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK20支架 ","H/工字钢","HN194*150*6*9",1,{"v":4000,"d":"4000.00"},194,150,6,9,3.88,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK20支架 ","L型钢","L63*6",8,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":7.8624,"d":"7.86"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK20支架 ","L型钢","L80*6",4,{"v":2900,"d":"2900.00"},80,80,6,6,{"v":3.712,"d":"3.71"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK20支架 ","2L型钢","TN100*100*5.5*8",4,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":2.4,"d":"2.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK20支架 ","2L型钢","TN125*125*6*9",4,{"v":7000,"d":"7000.00"},125,125,6,9,{"v":14,"d":"14.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK17支架 ","H/工字钢","HM294*200*8*12",10,{"v":5000,"d":"5000.00"},294,200,8,12,{"v":68.2,"d":"68.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK17支架 ","H/工字钢","HM390*300*10*16",2,{"v":5000,"d":"5000.00"},390,300,10,16,19.48,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK17支架 ","H/工字钢","HN194*150*6*9",1,{"v":4000,"d":"4000.00"},194,150,6,9,3.88,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK17支架 ","L型钢","L63*6",4,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":3.9312,"d":"3.93"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK17支架 ","L型钢","L80*6",4,{"v":2900,"d":"2900.00"},80,80,6,6,{"v":3.712,"d":"3.71"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK17支架 ","2L型钢","TN100*100*5.5*8",4,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":2.4,"d":"2.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK17支架 ","2L型钢","TN125*125*6*9",4,{"v":7000,"d":"7000.00"},125,125,6,9,{"v":14,"d":"14.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK17支架 ","2L型钢","TN125*125*6*9",4,{"v":1400,"d":"1400.00"},125,125,6,9,{"v":2.8,"d":"2.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK14支架 ","H/工字钢","HM294*200*8*12",10,{"v":5000,"d":"5000.00"},294,200,8,12,{"v":68.2,"d":"68.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK14支架 ","H/工字钢","HM390*300*10*16",4,{"v":5000,"d":"5000.00"},390,300,10,16,38.96,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK14支架 ","H/工字钢","HN194*150*6*9",1,{"v":4000,"d":"4000.00"},194,150,6,9,3.88,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK14支架 ","L型钢","L63*6",4,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":3.9312,"d":"3.93"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK14支架 ","L型钢","L80*6",4,{"v":2900,"d":"2900.00"},80,80,6,6,{"v":3.712,"d":"3.71"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK14支架 ","2L型钢","TN100*100*5.5*8",4,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":2.4,"d":"2.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK14支架 ","2L型钢","TN125*125*6*9",4,{"v":7000,"d":"7000.00"},125,125,6,9,{"v":14,"d":"14.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK14支架 ","2L型钢","TN125*125*6*9",8,{"v":1400,"d":"1400.00"},125,125,6,9,{"v":5.6,"d":"5.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK9支架 ","H/工字钢","HM294*200*8*12",10,{"v":5000,"d":"5000.00"},294,200,8,12,{"v":68.2,"d":"68.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK9支架 ","H/工字钢","HM340*250*9*14",2,{"v":5000,"d":"5000.00"},340,250,9,14,16.52,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK9支架 ","H/工字钢","HN194*150*6*9",1,{"v":4000,"d":"4000.00"},194,150,6,9,3.88,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK9支架 ","H/工字钢","HW200*200*8*12",1,{"v":1700,"d":"1700.00"},200,200,8,12,{"v":1.9992,"d":"2.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK9支架 ","L型钢","L63*6",4,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":3.9312,"d":"3.93"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK9支架 ","L型钢","L80*6",4,{"v":2900,"d":"2900.00"},80,80,6,6,{"v":3.712,"d":"3.71"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK9支架 ","2L型钢","TN100*100*5.5*8",4,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":2.4,"d":"2.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK9支架 ","2L型钢","TN125*125*6*9",4,{"v":7000,"d":"7000.00"},125,125,6,9,{"v":14,"d":"14.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK9支架 ","2L型钢","TN125*125*6*9",8,{"v":1400,"d":"1400.00"},125,125,6,9,{"v":5.6,"d":"5.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK9支架 ","2L型钢","TN125*125*6*9",1,{"v":2100,"d":"2100.00"},125,125,6,9,1.05,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK7支架 ","H/工字钢","HM294*200*8*12",10,{"v":5000,"d":"5000.00"},294,200,8,12,{"v":68.2,"d":"68.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK7支架 ","H/工字钢","HM294*200*8*12",4,{"v":2600,"d":"2600.00"},294,200,8,12,{"v":14.1856,"d":"14.19"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK7支架 ","H/工字钢","HM340*250*9*14",4,{"v":5000,"d":"5000.00"},340,250,9,14,33.04,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK7支架 ","H/工字钢","HN194*150*6*9",1,{"v":4000,"d":"4000.00"},194,150,6,9,3.88,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK7支架 ","H/工字钢","HW200*200*8*12",1,{"v":1700,"d":"1700.00"},200,200,8,12,{"v":1.9992,"d":"2.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK7支架 ","L型钢","L63*6",4,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":3.9312,"d":"3.93"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK7支架 ","L型钢","L80*6",4,{"v":2900,"d":"2900.00"},80,80,6,6,{"v":3.712,"d":"3.71"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK7支架 ","2L型钢","TN100*100*5.5*8",4,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":2.4,"d":"2.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK7支架 ","2L型钢","TN125*125*6*9",4,{"v":7000,"d":"7000.00"},125,125,6,9,{"v":14,"d":"14.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK7支架 ","2L型钢","TN125*125*6*9",8,{"v":1400,"d":"1400.00"},125,125,6,9,{"v":5.6,"d":"5.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK7支架 ","2L型钢","TN125*125*6*9",1,{"v":2100,"d":"2100.00"},125,125,6,9,1.05,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK7支架 ","2L型钢","TN125*125*6*9",2,{"v":3500,"d":"3500.00"},125,125,6,9,{"v":3.5,"d":"3.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK4支架 ","H/工字钢","HM294*200*8*12",12,{"v":5000,"d":"5000.00"},294,200,8,12,81.84,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK4支架 ","H/工字钢","HN194*150*6*9",1,{"v":4000,"d":"4000.00"},194,150,6,9,3.88,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK4支架 ","H/工字钢","HW200*200*8*12",1,{"v":1700,"d":"1700.00"},200,200,8,12,{"v":1.9992,"d":"2.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK4支架 ","L型钢","L63*6",4,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":3.9312,"d":"3.93"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK4支架 ","L型钢","L80*6",4,{"v":2900,"d":"2900.00"},80,80,6,6,{"v":3.712,"d":"3.71"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK4支架 ","2L型钢","TN100*100*5.5*8",4,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":2.4,"d":"2.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK4支架 ","2L型钢","TN125*125*6*9",4,{"v":7000,"d":"7000.00"},125,125,6,9,{"v":14,"d":"14.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK4支架 ","2L型钢","TN125*125*6*9",8,{"v":1400,"d":"1400.00"},125,125,6,9,{"v":5.6,"d":"5.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK4支架 ","2L型钢","TN125*125*6*9",1,{"v":2100,"d":"2100.00"},125,125,6,9,1.05,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK12支架 ","H/工字钢","HM294*200*8*12",10,{"v":5000,"d":"5000.00"},294,200,8,12,{"v":68.2,"d":"68.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK12支架 ","H/工字钢","HM390*300*10*16",2,{"v":5000,"d":"5000.00"},390,300,10,16,19.48,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK12支架 ","H/工字钢","HN194*150*6*9",1,{"v":4000,"d":"4000.00"},194,150,6,9,3.88,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK12支架 ","H/工字钢","HW200*200*8*12",1,{"v":1700,"d":"1700.00"},200,200,8,12,{"v":1.9992,"d":"2.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK12支架 ","L型钢","L63*6",4,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":3.9312,"d":"3.93"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK12支架 ","L型钢","L80*6",4,{"v":2900,"d":"2900.00"},80,80,6,6,{"v":3.712,"d":"3.71"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK12支架 ","2L型钢","TN100*100*5.5*8",4,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":2.4,"d":"2.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK12支架 ","2L型钢","TN125*125*6*9",4,{"v":7000,"d":"7000.00"},125,125,6,9,{"v":14,"d":"14.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK12支架 ","2L型钢","TN125*125*6*9",8,{"v":1400,"d":"1400.00"},125,125,6,9,{"v":5.6,"d":"5.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK12支架 ","2L型钢","TN125*125*6*9",1,{"v":2100,"d":"2100.00"},125,125,6,9,1.05,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK10支架 ","H/工字钢","HM294*200*8*12",12,{"v":5000,"d":"5000.00"},294,200,8,12,81.84,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK10支架 ","H/工字钢","HN194*150*6*9",1,{"v":4000,"d":"4000.00"},194,150,6,9,3.88,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK10支架 ","H/工字钢","HW200*200*8*12",1,{"v":1700,"d":"1700.00"},200,200,8,12,{"v":1.9992,"d":"2.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK10支架 ","L型钢","L63*6",4,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":3.9312,"d":"3.93"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK10支架 ","L型钢","L80*6",4,{"v":2900,"d":"2900.00"},80,80,6,6,{"v":3.712,"d":"3.71"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK10支架 ","2L型钢","TN100*100*5.5*8",4,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":2.4,"d":"2.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK10支架 ","2L型钢","TN125*125*6*9",4,{"v":7000,"d":"7000.00"},125,125,6,9,{"v":14,"d":"14.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK10支架 ","2L型钢","TN125*125*6*9",8,{"v":1400,"d":"1400.00"},125,125,6,9,{"v":5.6,"d":"5.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK10支架 ","2L型钢","TN125*125*6*9",1,{"v":2100,"d":"2100.00"},125,125,6,9,1.05,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK73支架 ","H/工字钢","HM294*200*8*12",10,{"v":5000,"d":"5000.00"},294,200,8,12,{"v":68.2,"d":"68.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK73支架 ","H/工字钢","HM294*200*8*12",15,{"v":2500,"d":"2500.00"},294,200,8,12,51.15,"无重合面",null,38,null,{"v":27,"d":"27.00"},"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0.345489443378119,"d":"35%"}]
["外线 GK73支架 ","H/工字钢","HN194*150*6*9",2,{"v":4000,"d":"4000.00"},194,150,6,9,7.76,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK73支架 ","H/工字钢","HN194*150*6*9",14,{"v":3000,"d":"3000.00"},194,150,6,9,40.74,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK73支架 ","H/工字钢","HN300*150*6*9",1,{"v":3000,"d":"3000.00"},300,150,6,9,{"v":3.546,"d":"3.55"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK73支架 ","H/工字钢","HW200*200*8*12",6,{"v":2000,"d":"2000.00"},200,200,8,12,{"v":14.112,"d":"14.11"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK73支架 ","L型钢","L63*6",8,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":7.8624,"d":"7.86"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK73支架 ","2L型钢","TN125*125*6*9",4,{"v":7000,"d":"7000.00"},125,125,6,9,{"v":14,"d":"14.00"},"无重合面",null,38,null,{"v":54,"d":"54.00"},"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0.794117647058823,"d":"79%"}]
["外线 GK73支架 ","2L型钢","TN125*125*6*9",6,{"v":2900,"d":"2900.00"},125,125,6,9,{"v":8.7,"d":"8.70"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK69支架 ","H/工字钢","HM294*200*8*12",10,{"v":5000,"d":"5000.00"},294,200,8,12,{"v":68.2,"d":"68.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK69支架 ","H/工字钢","HN194*150*6*9",2,{"v":4000,"d":"4000.00"},194,150,6,9,7.76,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK69支架 ","H/工字钢","HN300*150*6*9",1,{"v":3000,"d":"3000.00"},300,150,6,9,{"v":3.546,"d":"3.55"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK69支架 ","L型钢","L63*6",4,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":3.9312,"d":"3.93"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK69支架 ","2L型钢","TN125*125*6*9",4,{"v":7000,"d":"7000.00"},125,125,6,9,{"v":14,"d":"14.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK3支架 ","H/工字钢","HM294*200*8*12",12,{"v":5000,"d":"5000.00"},294,200,8,12,81.84,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK3支架 ","H/工字钢","HN194*150*6*9",2,{"v":4000,"d":"4000.00"},194,150,6,9,7.76,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK3支架 ","L型钢","L80*6",4,{"v":6400,"d":"6400.00"},80,80,6,6,{"v":8.192,"d":"8.19"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK3支架 ","2L型钢","TN125*125*6*9",4,{"v":7000,"d":"7000.00"},125,125,6,9,{"v":14,"d":"14.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK1支架 ","H/工字钢","HM294*200*8*12",13,{"v":5000,"d":"5000.00"},294,200,8,12,88.66,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK1支架 ","H/工字钢","HN194*150*6*9",2,{"v":4000,"d":"4000.00"},194,150,6,9,7.76,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK1支架 ","H/工字钢","HN194*150*6*9",3,{"v":3000,"d":"3000.00"},194,150,6,9,8.73,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK1支架 ","H/工字钢","HW200*200*8*12",1,{"v":1700,"d":"1700.00"},200,200,8,12,{"v":1.9992,"d":"2.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK1支架 ","L型钢","L63*6",8,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":7.8624,"d":"7.86"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK1支架 ","L型钢","L80*6",4,{"v":2900,"d":"2900.00"},80,80,6,6,{"v":3.712,"d":"3.71"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK1支架 ","2L型钢","TN100*100*5.5*8",4,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":2.4,"d":"2.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK1支架 ","2L型钢","TN125*125*6*9",4,{"v":7000,"d":"7000.00"},125,125,6,9,{"v":14,"d":"14.00"},"无重合面",null,38,null,{"v":9,"d":"9.00"},"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0.391304347826087,"d":"39%"}]
["外线 GK1支架 ","2L型钢","TN125*125*6*9",1,{"v":2100,"d":"2100.00"},125,125,6,9,1.05,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架 9m平面","H/工字钢","HM294*200*8*12",1,{"v":4500,"d":"4500.00"},294,200,8,12,{"v":6.138,"d":"6.14"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架 9m平面","H/工字钢","HN194*150*6*9",3,{"v":2000,"d":"2000.00"},194,150,6,9,5.82,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架 9m平面","H/工字钢","HN194*150*6*9",2,{"v":18000,"d":"18000.00"},194,150,6,9,34.92,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架 9m平面","H/工字钢","HN300*150*6*9",2,{"v":4500,"d":"4500.00"},300,150,6,9,{"v":10.638,"d":"10.64"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架 9m平面","H/工字钢","HW200*200*8*12",7,{"v":4500,"d":"4500.00"},200,200,8,12,{"v":37.044,"d":"37.04"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架 9m平面","L型钢","L63*6",4,{"v":3100,"d":"3100.00"},63,63,6,6,{"v":3.1248,"d":"3.12"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架 9m平面","L型钢","L80*6",6,{"v":6430,"d":"6430.00"},80,80,6,6,{"v":12.3456,"d":"12.35"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架 9m平面","L型钢","L80*6",4,{"v":2400,"d":"2400.00"},80,80,6,6,{"v":3.072,"d":"3.07"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架 9m平面","L型钢","L80*8",1.5,{"v":3500,"d":"3500.00"},80,80,8,8,1.68,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架 6.5m平面","H/工字钢","HM294*200*8*12",1,{"v":4500,"d":"4500.00"},294,200,8,12,{"v":6.138,"d":"6.14"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架 6.5m平面","H/工字钢","HN194*150*6*9",3,{"v":2000,"d":"2000.00"},194,150,6,9,5.82,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架 6.5m平面","H/工字钢","HN194*150*6*9",2,{"v":18000,"d":"18000.00"},194,150,6,9,34.92,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架 6.5m平面","H/工字钢","HN300*150*6*9",2,{"v":4500,"d":"4500.00"},300,150,6,9,{"v":10.638,"d":"10.64"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架 6.5m平面","H/工字钢","HW200*200*8*12",7,{"v":4500,"d":"4500.00"},200,200,8,12,{"v":37.044,"d":"37.04"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架 6.5m平面","L型钢","L63*6",4,{"v":3100,"d":"3100.00"},63,63,6,6,{"v":3.1248,"d":"3.12"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架 6.5m平面","L型钢","L80*6",8,{"v":6430,"d":"6430.00"},80,80,6,6,{"v":16.4608,"d":"16.46"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架 6.5m平面","L型钢","L80*6",4,{"v":2400,"d":"2400.00"},80,80,6,6,{"v":3.072,"d":"3.07"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架  HJa","H/工字钢","HN300*200*8*120",2,{"v":11000,"d":"11000.00"},300,200,8,12,{"v":30.272,"d":"30.27"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架  HJa","H/工字钢","HM294*200*8*12",6,{"v":4500,"d":"4500.00"},294,200,8,12,{"v":36.828,"d":"36.83"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架  HJa","H/工字钢","HM340*250*9*14",3,{"v":4500,"d":"4500.00"},340,250,9,14,{"v":22.302,"d":"22.30"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架  HJa","H/工字钢","HW150*150*7*10",7,{"v":2500,"d":"2500.00"},150,150,7,10,{"v":15.4,"d":"15.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架  HJa","H/工字钢","HW150*150*7*10",4,{"v":3500,"d":"3500.00"},150,150,7,10,12.32,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架  HJa","H/工字钢","HW200*200*8*12",4,{"v":11000,"d":"11000.00"},200,200,8,12,{"v":51.744,"d":"51.74"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架  HJa","2L型钢","TN100*10*5.5*8",6,{"v":3500,"d":"3500.00"},100,100,5.5,8,{"v":8.4,"d":"8.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架  HJa","2L型钢","TN125*125*6*9",5,{"v":3500,"d":"3500.00"},125,125,6,9,8.75,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK38a-GK38b支架  HJa","2L型钢","TN125*125*6*9",2,{"v":7700,"d":"7700.00"},125,125,6,9,{"v":7.7,"d":"7.70"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架 9m平面","H/工字钢","HM294*200*8*12",1,{"v":4500,"d":"4500.00"},294,200,8,12,{"v":6.138,"d":"6.14"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架 9m平面","H/工字钢","HN194*150*6*9",3,{"v":2000,"d":"2000.00"},194,150,6,9,5.82,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架 9m平面","H/工字钢","HN194*150*6*9",2,{"v":18000,"d":"18000.00"},194,150,6,9,34.92,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架 9m平面","H/工字钢","HN300*150*6*9",2,{"v":4500,"d":"4500.00"},300,150,6,9,{"v":10.638,"d":"10.64"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架 9m平面","H/工字钢","HW200*200*8*12",7,{"v":4500,"d":"4500.00"},200,200,8,12,{"v":37.044,"d":"37.04"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架 9m平面","L型钢","L63*6",4,{"v":3100,"d":"3100.00"},63,63,6,6,{"v":3.1248,"d":"3.12"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架 9m平面","L型钢","L80*6",6,{"v":6430,"d":"6430.00"},80,80,6,6,{"v":12.3456,"d":"12.35"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架 9m平面","L型钢","L80*6",4,{"v":2400,"d":"2400.00"},80,80,6,6,{"v":3.072,"d":"3.07"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架 9m平面","L型钢","L80*8",1.5,{"v":3500,"d":"3500.00"},80,80,8,8,1.68,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架 6.5m平面","H/工字钢","HM294*200*8*12",1,{"v":4500,"d":"4500.00"},294,200,8,12,{"v":6.138,"d":"6.14"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架 6.5m平面","H/工字钢","HN194*150*6*9",3,{"v":2000,"d":"2000.00"},194,150,6,9,5.82,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架 6.5m平面","H/工字钢","HN194*150*6*9",2,{"v":18000,"d":"18000.00"},194,150,6,9,34.92,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架 6.5m平面","H/工字钢","HN300*150*6*9",2,{"v":4500,"d":"4500.00"},300,150,6,9,{"v":10.638,"d":"10.64"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架 6.5m平面","H/工字钢","HW200*200*8*12",7,{"v":4500,"d":"4500.00"},200,200,8,12,{"v":37.044,"d":"37.04"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架 6.5m平面","L型钢","L63*6",4,{"v":3200,"d":"3200.00"},63,63,6,6,{"v":3.2256,"d":"3.23"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架 6.5m平面","L型钢","L80*6",8,{"v":6430,"d":"6430.00"},80,80,6,6,{"v":16.4608,"d":"16.46"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架 6.5m平面","L型钢","L80*6",4,{"v":2400,"d":"2400.00"},80,80,6,6,{"v":3.072,"d":"3.07"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架  HJa","H/工字钢","HN300*200*8*120",2,{"v":11000,"d":"11000.00"},300,200,8,12,{"v":30.272,"d":"30.27"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架  HJa","H/工字钢","HM294*200*8*12",6,{"v":4500,"d":"4500.00"},294,200,8,12,{"v":36.828,"d":"36.83"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架  HJa","H/工字钢","HM340*250*9*14",3,{"v":4500,"d":"4500.00"},340,250,9,14,{"v":22.302,"d":"22.30"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架  HJa","H/工字钢","HW150*150*7*10",7,{"v":2500,"d":"2500.00"},150,150,7,10,{"v":15.4,"d":"15.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架  HJa","H/工字钢","HW150*150*7*10",4,{"v":3500,"d":"3500.00"},150,150,7,10,12.32,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架  HJa","H/工字钢","HW200*200*8*12",4,{"v":11000,"d":"11000.00"},200,200,8,12,{"v":51.744,"d":"51.74"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架  HJa","2L型钢","TN100*10*5.5*8",6,{"v":3500,"d":"3500.00"},100,100,5.5,8,{"v":8.4,"d":"8.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架  HJa","2L型钢","TN125*125*6*9",5,{"v":3500,"d":"3500.00"},125,125,6,9,8.75,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK34a-GK34b支架  HJa","2L型钢","TN125*125*6*9",2,{"v":7700,"d":"7700.00"},125,125,6,9,{"v":7.7,"d":"7.70"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK31a-GK31b支架","H/工字钢","HM244*175*7*11",4,{"v":11000,"d":"11000.00"},244,175,7,11,{"v":51.304,"d":"51.30"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-39","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK31a-GK31b支架","H/工字钢","HM340*250*9*14",2,{"v":3000,"d":"3000.00"},340,250,9,14,{"v":9.912,"d":"9.91"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-39","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK31a-GK31b支架","2L型钢","TN100*100*5.5*8",16,{"v":4100,"d":"4100.00"},100,100,5.5,8,26.24,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-39","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK31a-GK31b支架","2L型钢","TN100*100*5.5*8",6,{"v":3000,"d":"3000.00"},100,100,5.5,8,{"v":7.2,"d":"7.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-39","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK73-GK73a支架","H/工字钢","HN300*150*6*9",6,{"v":5000,"d":"5000.00"},300,150,6,9,35.46,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK73-GK73a支架","H/工字钢","HN400*200*8*13",2,{"v":16200,"d":"16200.00"},400,200,8,13,{"v":50.9976,"d":"51.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK73-GK73a支架","L型钢","L63*6",4,{"v":3900,"d":"3900.00"},63,63,6,6,{"v":3.9312,"d":"3.93"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK73-GK73a支架","L型钢","L80*8",4,{"v":7800,"d":"7800.00"},80,80,8,8,{"v":9.984,"d":"9.98"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK73-GK73a支架","L型钢","L80*8",1,{"v":16200,"d":"16200.00"},80,80,8,8,{"v":5.184,"d":"5.18"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK28a-GK28b支架","H/工字钢","HM244*175*7*11",4,{"v":8500,"d":"8500.00"},244,175,7,11,{"v":39.644,"d":"39.64"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK28a-GK28b支架","H/工字钢","HN194*150*6*9",2,{"v":2000,"d":"2000.00"},194,150,6,9,3.88,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK28a-GK28b支架","H/工字钢","HW150*150*7*10",10,{"v":2000,"d":"2000.00"},150,150,7,10,{"v":17.6,"d":"17.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK28a-GK28b支架","H/工字钢","HW150*150*7*10",4,{"v":15000,"d":"15000.00"},150,150,7,10,{"v":52.8,"d":"52.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK28a-GK28b支架","H/工字钢","HW150*150*7*10",10,{"v":2000,"d":"2000.00"},150,150,7,10,{"v":17.6,"d":"17.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK28a-GK28b支架","L型钢","L100*10",2,{"v":15000,"d":"15000.00"},100,100,10,10,{"v":9,"d":"9.00"},"翼板重合",null,38,null,{"v":21,"d":"21.00"},"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["外线 GK28a-GK28b支架","L型钢","L80*6",8,{"v":3200,"d":"3200.00"},80,80,6,6,{"v":8.192,"d":"8.19"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK28a-GK28b支架","L型钢","L80*8",4,{"v":3200,"d":"3200.00"},80,80,8,8,{"v":4.096,"d":"4.10"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK28a-GK28b支架","2L型钢","TN100*10*5.5*8",8,{"v":3200,"d":"3200.00"},100,100,5.5,8,10.24,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 GK28a-GK28b支架","2L型钢","TN125*125*6*9",12,{"v":3200,"d":"3200.00"},125,125,6,9,{"v":19.2,"d":"19.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 DJ45-46  立面","H/工字钢","HM244*175*7*11",2,{"v":6300,"d":"6300.00"},244,175,7,11,{"v":14.6916,"d":"14.69"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 DJ45-46  立面","H/工字钢","HW150*150*7*10",18,{"v":2300,"d":"2300.00"},150,150,7,10,{"v":36.432,"d":"36.43"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 DJ45-46  立面","H/工字钢","HW200*200*8*12",4,{"v":6300,"d":"6300.00"},200,200,8,12,{"v":29.6352,"d":"29.64"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 DJ45-46  立面","L型钢","L75*6",10,{"v":2800,"d":"2800.00"},75,75,6,6,{"v":8.4,"d":"8.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 DJ45-46  立面","2L型钢","TN100*10*5.5*8",12,{"v":3200,"d":"3200.00"},100,100,5.5,8,15.36,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 DJ45-46  立面","2L型钢","TN125*125*6*9",8,{"v":3200,"d":"3200.00"},125,125,6,9,{"v":12.8,"d":"12.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 DJ45-46  7-7面","H/工字钢","HM194*150*6*9",2,{"v":20300,"d":"20300.00"},194,150,6,9,{"v":39.382,"d":"39.38"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 DJ45-46  7-7面","H/工字钢","HN194*150*6*9",11,{"v":2000,"d":"2000.00"},194,150,6,9,21.34,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 DJ45-46  7-7面","L型钢","L80*6",6,{"v":2900,"d":"2900.00"},80,80,6,6,{"v":5.568,"d":"5.57"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 DJ45-46  7-7面","L型钢","L80*8",4,{"v":2900,"d":"2900.00"},80,80,8,8,{"v":3.712,"d":"3.71"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 DJ45-46  6-6面","H/工字钢","HM194*150*6*9",2,{"v":20800,"d":"20800.00"},194,150,6,9,{"v":40.352,"d":"40.35"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 DJ45-46  6-6面","H/工字钢","HM224*175*7*11",2,{"v":10000,"d":"10000.00"},224,175,7,11,22.52,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 DJ45-46  6-6面","H/工字钢","HN194*150*6*9",17,{"v":2000,"d":"2000.00"},194,150,6,9,32.98,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 DJ45-46  6-6面","L型钢","L63*6",2,{"v":2820,"d":"2820.00"},63,63,6,6,{"v":1.42128,"d":"1.42"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 DJ45-46  6-6面","L型钢","L75*6",12,{"v":2800,"d":"2800.00"},75,75,6,6,10.08,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 DJ45-46  6-6面","L型钢","L80*6",11,{"v":2900,"d":"2900.00"},80,80,6,6,{"v":10.208,"d":"10.21"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线 DJ45-46  6-6面","L型钢","L80*8",4,{"v":2900,"d":"2900.00"},80,80,8,8,{"v":3.712,"d":"3.71"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K115~GK123  B-B面","2L型钢","TN100*100*5.5*8",4,{"v":4300,"d":"4300.00"},100,100,5.5,8,6.88,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K115~GK123  B-B面","2L型钢","TN100*100*5.5*8",4,{"v":4800,"d":"4800.00"},100,100,5.5,8,7.68,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K115~GK123  A-A面","H/工字钢","HW150*150*7*10",2,{"v":2100,"d":"2100.00"},150,150,7,10,{"v":3.696,"d":"3.70"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K115~GK123  A-A面","H/工字钢","HW150*150*7*10",7,{"v":1500,"d":"1500.00"},150,150,7,10,9.24,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K115~GK123  A-A面","H/工字钢","HW200*200*8*12",4,{"v":7800,"d":"7800.00"},200,200,8,12,{"v":36.6912,"d":"36.69"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K115~GK123  A-A面","2L型钢","TN100*100*5.5*8",18,{"v":2100,"d":"2100.00"},100,100,5.5,8,15.12,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K115~GK123  A-A面","2L型钢","TN100*100*5.5*8",4,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":2.4,"d":"2.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K115~GK123  A-A面","2L型钢","TN100*100*5.5*8",5,{"v":4300,"d":"4300.00"},100,100,5.5,8,{"v":8.6,"d":"8.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K115~GK123  A-A面","2L型钢","TN100*100*5.5*8",4,{"v":4800,"d":"4800.00"},100,100,5.5,8,7.68,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K115~GK123  A-A面","2L型钢","TN125*125*6*9",2,{"v":2300,"d":"2300.00"},125,125,6,9,{"v":2.3,"d":"2.30"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K115~GK123   7.8M平面","H/工字钢","HM194*150*6*9",8,{"v":3000,"d":"3000.00"},194,150,6,9,23.28,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K115~GK123   7.8M平面","H/工字钢","HM244*175*7*11",2,{"v":21000,"d":"21000.00"},244,175,7,11,{"v":48.972,"d":"48.97"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K115~GK123   7.8M平面","L型钢","L75*6",12,{"v":4250,"d":"4250.00"},75,75,6,6,{"v":15.3,"d":"15.30"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K115~GK123   7.8M平面","L型钢","L80*6",2,{"v":4700,"d":"4700.00"},80,80,6,6,{"v":3.008,"d":"3.01"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K115~GK123   6.3M平面","H/工字钢","HM194*150*6*9",8,{"v":3000,"d":"3000.00"},194,150,6,9,23.28,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K115~GK123   6.3M平面","H/工字钢","HM244*175*7*11",2,{"v":21000,"d":"21000.00"},244,175,7,11,{"v":48.972,"d":"48.97"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K115~GK123   6.3M平面","L型钢","L75*6",12,{"v":4250,"d":"4250.00"},75,75,6,6,{"v":15.3,"d":"15.30"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K115~GK123   6.3M平面","L型钢","L80*6",2,{"v":4700,"d":"4700.00"},80,80,6,6,{"v":3.008,"d":"3.01"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209   7.8M平面","H/工字钢","HM194*150*6*9",2,{"v":40000,"d":"40000.00"},194,150,6,9,{"v":77.6,"d":"77.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-42","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209   7.8M平面","H/工字钢","HM244*175*7*11",2,{"v":24000,"d":"24000.00"},244,175,7,11,{"v":55.968,"d":"55.97"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-42","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209   7.8M平面","H/工字钢","HM244*175*7*11",12,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":55.968,"d":"55.97"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-42","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209   7.8M平面","H/工字钢","HW200*200*8*12",9,{"v":4000,"d":"4000.00"},200,200,8,12,{"v":42.336,"d":"42.34"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-42","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209   7.8M平面","L型钢","L75*6",34,{"v":5400,"d":"5400.00"},75,75,6,6,55.08,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-42","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209   7.8M平面","L型钢","L80*6",2,{"v":5660,"d":"5660.00"},80,80,6,6,{"v":3.6224,"d":"3.62"},"无重合面",null,38,null,{"v":28.8,"d":"28.80"},"总图内所有管架、410NC02102-42","一般性腐蚀","环氧富锌漆",{"v":0.888274772996447,"d":"89%"}]
["外线GK63~K209   6.3M平面","H/工字钢","HM194*150*6*9",2,{"v":40000,"d":"40000.00"},194,150,6,9,{"v":77.6,"d":"77.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-42","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209   6.3M平面","H/工字钢","HM244*175*7*11",2,{"v":24000,"d":"24000.00"},244,175,7,11,{"v":55.968,"d":"55.97"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-42","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209   6.3M平面","H/工字钢","HM244*175*7*11",12,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":55.968,"d":"55.97"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-42","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209   6.3M平面","H/工字钢","HW200*200*8*12",9,{"v":4000,"d":"4000.00"},200,200,8,12,{"v":42.336,"d":"42.34"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-42","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209   6.3M平面","L型钢","L75*6",34,{"v":5400,"d":"5400.00"},75,75,6,6,55.08,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-42","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209   6.3M平面","L型钢","L80*6",4,{"v":5660,"d":"5660.00"},80,80,6,6,{"v":7.2448,"d":"7.24"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-42","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208   7.8M平面","H/工字钢","HM194*150*6*9",2,{"v":61000,"d":"61000.00"},194,150,6,9,118.34,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208   7.8M平面","H/工字钢","HM244*175*7*11",7,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":32.648,"d":"32.65"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208   7.8M平面","H/工字钢","HN450*200*9*14",2,{"v":10000,"d":"10000.00"},450,200,9,14,33.44,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208   7.8M平面","H/工字钢","HW200*200*8*12",15,{"v":4000,"d":"4000.00"},200,200,8,12,70.56,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208   7.8M平面","L型钢","L75*6",42,{"v":5400,"d":"5400.00"},75,75,6,6,68.04,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209  B-B面","H/工字钢","HW100*100*6*8",13,{"v":1500,"d":"1500.00"},100,100,6,8,{"v":11.388,"d":"11.39"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209  B-B面","H/工字钢","HW150*150*7*10",8,{"v":2300,"d":"2300.00"},150,150,7,10,{"v":16.192,"d":"16.19"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209  B-B面","H/工字钢","HW150*150*7*10",8,{"v":1500,"d":"1500.00"},150,150,7,10,10.56,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209  B-B面","H/工字钢","HW200*200*8*12",6,{"v":7800,"d":"7800.00"},200,200,8,12,{"v":55.0368,"d":"55.04"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209  B-B面","2L型钢","TN100*100*5.5*8",18,{"v":2300,"d":"2300.00"},100,100,5.5,8,16.56,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209  B-B面","2L型钢","TN100*100*5.5*8",9,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":5.4,"d":"5.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209  B-B面","2L型钢","TN125*125*6*9",8,{"v":2300,"d":"2300.00"},125,125,6,9,{"v":9.2,"d":"9.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209  B-B面","2L型钢","TN125*125*6*9",9,{"v":5000,"d":"5000.00"},125,125,6,9,{"v":22.5,"d":"22.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209  A-A面","H/工字钢","HW100*100*6*8",13,{"v":1500,"d":"1500.00"},100,100,6,8,{"v":11.388,"d":"11.39"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209  A-A面","H/工字钢","HW150*150*7*10",8,{"v":2300,"d":"2300.00"},150,150,7,10,{"v":16.192,"d":"16.19"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209  A-A面","H/工字钢","HW150*150*7*10",8,{"v":1500,"d":"1500.00"},150,150,7,10,10.56,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209  A-A面","H/工字钢","HW200*200*8*12",6,{"v":7800,"d":"7800.00"},200,200,8,12,{"v":55.0368,"d":"55.04"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209  A-A面","2L型钢","TN100*100*5.5*8",18,{"v":2300,"d":"2300.00"},100,100,5.5,8,16.56,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209  A-A面","2L型钢","TN100*100*5.5*8",9,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":5.4,"d":"5.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209  A-A面","2L型钢","TN125*125*6*9",8,{"v":2300,"d":"2300.00"},125,125,6,9,{"v":9.2,"d":"9.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209  A-A面","2L型钢","TN125*125*6*9",10,{"v":5000,"d":"5000.00"},125,125,6,9,{"v":25,"d":"25.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209   C-C面","2L型钢","TN100*100*5.5*8",3,{"v":5000,"d":"5000.00"},100,100,5.5,8,{"v":6,"d":"6.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209   C-C面","2L型钢","TN125*125*6*9",12,{"v":5000,"d":"5000.00"},125,125,6,9,{"v":30,"d":"30.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209   C-C面","2L型钢","TN125*125*6*9",6,{"v":4000,"d":"4000.00"},125,125,6,9,{"v":12,"d":"12.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线GK63~K209   C-C面","2L型钢","TN175*175*7*11",6,{"v":5000,"d":"5000.00"},175,175,7,11,{"v":21,"d":"21.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-43","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208  E-E\\F-F平面","H/工字钢","HW100*100*6*8",15,{"v":1500,"d":"1500.00"},100,100,6,8,13.14,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-44","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208  E-E\\F-F平面","H/工字钢","HW150*150*7*10",8,{"v":2300,"d":"2300.00"},150,150,7,10,{"v":16.192,"d":"16.19"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-44","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208  E-E\\F-F平面","H/工字钢","HW150*150*7*10",8,{"v":1500,"d":"1500.00"},150,150,7,10,10.56,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-44","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208  E-E\\F-F平面","H/工字钢","HW200*200*8*12",10,{"v":7800,"d":"7800.00"},200,200,8,12,{"v":91.728,"d":"91.73"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-44","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208  E-E\\F-F平面","2L型钢","TN100*100*5.5*8",44,{"v":2300,"d":"2300.00"},100,100,5.5,8,40.48,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-44","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208  E-E\\F-F平面","2L型钢","TN100*100*5.5*8",22,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":13.2,"d":"13.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-44","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208  E-E\\F-F平面","2L型钢","TN125*125*6*9",16,{"v":2300,"d":"2300.00"},125,125,6,9,{"v":18.4,"d":"18.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-44","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208  6M平面","H/工字钢","HM194*150*6*9",2,{"v":61000,"d":"61000.00"},194,150,6,9,118.34,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-44","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208  6M平面","H/工字钢","HM244*175*7*11",7,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":32.648,"d":"32.65"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-44","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208  6M平面","H/工字钢","HN450*200*9*14",2,{"v":10000,"d":"10000.00"},450,200,9,14,33.44,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-44","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208  6M平面","H/工字钢","HW200*200*8*12",15,{"v":4000,"d":"4000.00"},200,200,8,12,70.56,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-44","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208  6M平面","L型钢","L75*6",42,{"v":5400,"d":"5400.00"},75,75,6,6,68.04,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-44","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208    C-C面","2L型钢","TN100*100*5.5*8",2.5,{"v":5000,"d":"5000.00"},100,100,5.5,8,{"v":5,"d":"5.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-44","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208    C-C面","2L型钢","TN125*125*6*9",10,{"v":5000,"d":"5000.00"},125,125,6,9,{"v":25,"d":"25.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-44","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208    C-C面","2L型钢","TN125*125*6*9",5,{"v":4000,"d":"4000.00"},125,125,6,9,{"v":10,"d":"10.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-44","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K204~K208    C-C面","2L型钢","TN175*175*7*11",5,{"v":5000,"d":"5000.00"},175,175,7,11,{"v":17.5,"d":"17.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-44","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K220~GK221  6.6M平面","H/工字钢","HM194*150*6*9",8,{"v":2000,"d":"2000.00"},194,150,6,9,15.52,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K220~GK221  6.6M平面","H/工字钢","HM294*200*8*12",2,{"v":16200,"d":"16200.00"},294,200,8,12,{"v":44.1936,"d":"44.19"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K220~GK221  6.6M平面","L型钢","L63*6",8,{"v":3800,"d":"3800.00"},63,63,6,6,{"v":7.6608,"d":"7.66"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K220~GK221  6.6M平面","L型钢","L63*6",2,{"v":2800,"d":"2800.00"},63,63,6,6,{"v":1.4112,"d":"1.41"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K220~GK221   E-E/F-F面","2L型钢","TN100*100*5.5*8",6,{"v":2800,"d":"2800.00"},100,100,5.5,8,6.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K220~GK221   D-D面","H/工字钢","HW150*150*7*10",4,{"v":6600,"d":"6600.00"},150,150,7,10,{"v":23.232,"d":"23.23"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K220~GK221   D-D面","H/工字钢","HW194*150*6*9",2,{"v":6600,"d":"6600.00"},194,150,6,9,{"v":12.804,"d":"12.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K220~GK221   D-D面","2L型钢","TN100*100*5.5*8",6,{"v":2800,"d":"2800.00"},100,100,5.5,8,6.72,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K210~K219  6.6M平面","H/工字钢","HM194*150*6*9",39,{"v":4000,"d":"4000.00"},194,150,6,9,151.32,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K210~K219  6.6M平面","H/工字钢","HM294*200*8*12",2,{"v":113800,"d":"113800.00"},294,200,8,12,{"v":310.4464,"d":"310.45"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K210~K219  6.6M平面","H/工字钢","HN450*200*9*14",null,{"v":10000,"d":"10000.00"},450,200,9,14,{"v":0,"d":"0.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["外线K210~K219  6.6M平面","L型钢","L75*6",40,{"v":5000,"d":"5000.00"},75,75,6,6,{"v":60,"d":"60.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K210~K219  6.6M平面","L型钢","L80*6",2,{"v":5000,"d":"5000.00"},80,80,6,6,{"v":3.2,"d":"3.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K210~K219   B-B\\C-C面","2L型钢","TN100*100*5.5*8",44,{"v":4300,"d":"4300.00"},100,100,5.5,8,75.68,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K210~K219   B-B\\C-C面","2L型钢","TN100*100*5.5*8",11,{"v":3000,"d":"3000.00"},100,100,5.5,8,{"v":13.2,"d":"13.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K210~K219    A-A面","H/工字钢","HW150*150*7*10",4,{"v":7800,"d":"7800.00"},150,150,7,10,{"v":27.456,"d":"27.46"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K210~K219    A-A面","H/工字钢","HW194*150*6*9",18,{"v":7800,"d":"7800.00"},194,150,6,9,{"v":136.188,"d":"136.19"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K210~K219    A-A面","2L型钢","TN100*100*5.5*8",8,{"v":4300,"d":"4300.00"},100,100,5.5,8,13.76,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["外线K210~K219    A-A面","2L型钢","TN100*100*5.5*8",2,{"v":3000,"d":"3000.00"},100,100,5.5,8,{"v":2.4,"d":"2.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-45","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  8、7.5M平面","H/工字钢","HM194*150*6*9",6,{"v":4000,"d":"4000.00"},194,150,6,9,23.28,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  8、7.5M平面","H/工字钢","HM244*175*7*11",10,{"v":4000,"d":"4000.00"},244,175,7,11,46.64,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  8、7.5M平面","H/工字钢","HM244*175*7*11",11,{"v":3000,"d":"3000.00"},244,175,7,11,{"v":38.478,"d":"38.48"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  8、7.5M平面","H/工字钢","HM244*175*7*11",2,{"v":24000,"d":"24000.00"},244,175,7,11,{"v":55.968,"d":"55.97"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  8、7.5M平面","H/工字钢","HM294*200*8*12",2,{"v":13500,"d":"13500.00"},294,200,8,12,{"v":36.828,"d":"36.83"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  8、7.5M平面","H/工字钢","HM294*200*8*12",4,{"v":8000,"d":"8000.00"},294,200,8,12,{"v":43.648,"d":"43.65"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  8、7.5M平面","L型钢","L80*6",2,{"v":5600,"d":"5600.00"},80,80,6,6,{"v":3.584,"d":"3.58"},"无重合面",null,38,null,{"v":68,"d":"68.00"},"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0.9499329459097,"d":"95%"}]
["GK79~K79f  8、7.5M平面","L型钢","L80*6",2,{"v":4720,"d":"4720.00"},80,80,6,6,{"v":3.0208,"d":"3.02"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  6.3、5.5M平面","H/工字钢","HM244*175*7*11",10,{"v":4000,"d":"4000.00"},244,175,7,11,46.64,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  6.3、5.5M平面","H/工字钢","HM244*175*7*11",17,{"v":3000,"d":"3000.00"},244,175,7,11,{"v":59.466,"d":"59.47"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  6.3、5.5M平面","H/工字钢","HM244*175*7*11",2,{"v":24000,"d":"24000.00"},244,175,7,11,{"v":55.968,"d":"55.97"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  6.3、5.5M平面","H/工字钢","HM294*200*8*12",2,{"v":13500,"d":"13500.00"},294,200,8,12,{"v":36.828,"d":"36.83"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  6.3、5.5M平面","H/工字钢","HM294*200*8*12",4,{"v":8000,"d":"8000.00"},294,200,8,12,{"v":43.648,"d":"43.65"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  6.3、5.5M平面","L型钢","L75*6",8,{"v":4250,"d":"4250.00"},75,75,6,6,{"v":10.2,"d":"10.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  6.3、5.5M平面","L型钢","L80*6",2,{"v":5600,"d":"5600.00"},80,80,6,6,{"v":3.584,"d":"3.58"},"无重合面",null,38,null,{"v":68,"d":"68.00"},"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0.9499329459097,"d":"95%"}]
["GK79~K79f  6.3、5.5M平面","L型钢","L80*6",2,{"v":4720,"d":"4720.00"},80,80,6,6,{"v":3.0208,"d":"3.02"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  5.5   B-B\\C-C面","H/工字钢","HW200*200*8*12",6,{"v":10500,"d":"10500.00"},200,200,8,12,{"v":74.088,"d":"74.09"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  5.5   B-B\\C-C面","2L型钢","TN125*125*6*9",20,{"v":5000,"d":"5000.00"},125,125,6,9,{"v":50,"d":"50.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  5.5   B-B\\C-C面","2L型钢","TN125*125*6*9",5,{"v":4000,"d":"4000.00"},125,125,6,9,{"v":10,"d":"10.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  5.5   A-A面","H/工字钢","HM244*175*7*11",10,{"v":1000,"d":"1000.00"},244,175,7,11,11.66,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  5.5   A-A面","H/工字钢","HW200*200*8*12",12,{"v":10500,"d":"10500.00"},200,200,8,12,{"v":148.176,"d":"148.18"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  5.5   A-A面","2L型钢","TN125*125*6*9",24,{"v":4100,"d":"4100.00"},125,125,6,9,{"v":49.2,"d":"49.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  5.5   A-A面","2L型钢","TN125*125*6*9",6,{"v":3000,"d":"3000.00"},125,125,6,9,{"v":9,"d":"9.00"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-48","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  9.5、9M平面","H/工字钢","HM244*175*7*11",10,{"v":4000,"d":"4000.00"},244,175,7,11,46.64,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-49","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  9.5、9M平面","H/工字钢","HM244*175*7*11",17,{"v":3000,"d":"3000.00"},244,175,7,11,{"v":59.466,"d":"59.47"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-49","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  9.5、9M平面","H/工字钢","HM244*175*7*11",2,{"v":24000,"d":"24000.00"},244,175,7,11,{"v":55.968,"d":"55.97"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-49","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  9.5、9M平面","H/工字钢","HM294*200*8*12",2,{"v":13500,"d":"13500.00"},294,200,8,12,{"v":36.828,"d":"36.83"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-49","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  9.5、9M平面","H/工字钢","HM294*200*8*12",4,{"v":8000,"d":"8000.00"},294,200,8,12,{"v":43.648,"d":"43.65"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-49","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  9.5、9M平面","L型钢","L75*6",16,{"v":4250,"d":"4250.00"},75,75,6,6,{"v":20.4,"d":"20.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-49","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  9.5、9M平面","L型钢","L80*6",8,{"v":4720,"d":"4720.00"},80,80,6,6,{"v":12.0832,"d":"12.08"},"无重合面",null,38,null,{"v":68,"d":"68.00"},"总图内所有管架、410NC02102-49","一般性腐蚀","环氧富锌漆",{"v":0.849116918404859,"d":"85%"}]
["GK79~K79f  11、10.5M平面","H/工字钢","HM244*175*7*11",10,{"v":4000,"d":"4000.00"},244,175,7,11,46.64,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-49","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  11、10.5M平面","H/工字钢","HM244*175*7*11",17,{"v":3000,"d":"3000.00"},244,175,7,11,{"v":59.466,"d":"59.47"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-49","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  11、10.5M平面","H/工字钢","HM244*175*7*11",2,{"v":24000,"d":"24000.00"},244,175,7,11,{"v":55.968,"d":"55.97"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-49","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  11、10.5M平面","H/工字钢","HM294*200*8*12",2,{"v":13500,"d":"13500.00"},294,200,8,12,{"v":36.828,"d":"36.83"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-49","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  11、10.5M平面","H/工字钢","HM294*200*8*12",4,{"v":8000,"d":"8000.00"},294,200,8,12,{"v":43.648,"d":"43.65"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-49","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  11、10.5M平面","L型钢","L100*10",2,{"v":61500,"d":"61500.00"},100,100,10,10,{"v":36.9,"d":"36.90"},"翼板重合",null,38,null,{"v":86.1,"d":"86.10"},"总图内所有管架、410NC02102-49","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["GK79~K79f  11、10.5M平面","L型钢","L75*6",16,{"v":4250,"d":"4250.00"},75,75,6,6,{"v":20.4,"d":"20.40"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-49","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f  11、10.5M平面","L型钢","L80*6",8,{"v":4720,"d":"4720.00"},80,80,6,6,{"v":12.0832,"d":"12.08"},"无重合面",null,38,null,{"v":46.4,"d":"46.40"},"总图内所有管架、410NC02102-49","一般性腐蚀","环氧富锌漆",{"v":0.793390238564237,"d":"79%"}]
["GK79~K79f F-F\\G-G面","H/工字钢","HW100*100*6*8",12,{"v":1500,"d":"1500.00"},100,100,6,8,{"v":10.512,"d":"10.51"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-50","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f F-F\\G-G面","H/工字钢","HW100*100*6*8",8,{"v":2100,"d":"2100.00"},100,100,6,8,{"v":9.8112,"d":"9.81"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-50","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f F-F\\G-G面","H/工字钢","HW100*100*6*8",12,{"v":3500,"d":"3500.00"},100,100,6,8,{"v":24.528,"d":"24.53"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-50","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f F-F\\G-G面","2L型钢","TN100*100*5.5*8",16,{"v":2100,"d":"2100.00"},100,100,5.5,8,13.44,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-50","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f F-F\\G-G面","2L型钢","TN100*100*5.5*8",8,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":4.8,"d":"4.80"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-50","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f F-F\\G-G面","2L型钢","TN125*125*6*9",8,{"v":4800,"d":"4800.00"},125,125,6,9,{"v":19.2,"d":"19.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-50","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["GK79~K79f F-F\\G-G面","2L型钢","TN150*150*6.5*9",3,{"v":4800,"d":"4800.00"},150,150,6.5,9,8.64,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-50","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7  A-A\\ B-B面","H/工字钢","HM244*175*7*11",10,{"v":6500,"d":"6500.00"},244,175,7,11,75.79,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-54","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7  A-A\\ B-B面","H/工字钢","HM244*175*7*11",4,{"v":8500,"d":"8500.00"},244,175,7,11,{"v":39.644,"d":"39.64"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-54","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7  A-A\\ B-B面","H/工字钢","HW150*150*7*10",4,{"v":2100,"d":"2100.00"},150,150,7,10,{"v":7.392,"d":"7.39"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-54","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7  A-A\\ B-B面","H/工字钢","HW150*150*7*10",12,{"v":1500,"d":"1500.00"},150,150,7,10,15.84,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-54","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7  A-A\\ B-B面","2L型钢","TN100*100*5.5*8",4,{"v":2100,"d":"2100.00"},100,100,5.5,8,3.36,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-54","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7  A-A\\ B-B面","2L型钢","TN100*100*5.5*8",2,{"v":1500,"d":"1500.00"},100,100,5.5,8,{"v":1.2,"d":"1.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-54","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7  A-A\\ B-B面","2L型钢","TN150*150*6.5*9",8,{"v":8600,"d":"8600.00"},150,150,6.5,9,41.28,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-54","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7  A-A\\ B-B面","2L型钢","TN150*150*6.5*9",5,{"v":6500,"d":"6500.00"},150,150,6.5,9,{"v":19.5,"d":"19.50"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-54","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7  A-A\\ B-B面","2L型钢","TN150*150*6.5*9",12,{"v":2100,"d":"2100.00"},150,150,6.5,9,15.12,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-54","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7  A-A\\ B-B面","2L型钢","TN150*150*6.5*9",4,{"v":1500,"d":"1500.00"},150,150,6.5,9,{"v":3.6,"d":"3.60"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-54","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7    6.5M平面","H/工字钢","HN350*175*7*11",8,{"v":5000,"d":"5000.00"},350,175,7,11,55.12,"无重合面",null,38,null,null,"总图内所有管架、410NC02102-54","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7    6.5M平面","H/工字钢","HN350*175*7*11",2,{"v":6500,"d":"6500.00"},350,175,7,11,{"v":17.914,"d":"17.91"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-54","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7    6.5M平面","H/工字钢","HM244*175*7*11",13,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":60.632,"d":"60.63"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-54","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7    6.5M平面","H/工字钢","HW500*200*10*16",4,{"v":10500,"d":"10500.00"},500,200,10,16,{"v":74.256,"d":"74.26"},"无重合面",null,38,null,{"v":72.6,"d":"72.60"},"总图内所有管架、410NC02102-54","一般性腐蚀","环氧富锌漆",{"v":0.494361823827423,"d":"49%"}]
["洗涤北侧支架NK1~NK7    6.5M平面","L型钢","L100*10",2,{"v":15800,"d":"15800.00"},100,100,10,10,9.48,"翼板重合",null,38,null,22.12,"总图内所有管架、410NC02102-54","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["洗涤北侧支架NK1~NK7    6.5M平面","L型钢","L80*6",12,{"v":5000,"d":"5000.00"},80,80,6,6,{"v":19.2,"d":"19.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-54","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7    6.5M平面","L型钢","L80*6",8,{"v":7500,"d":"7500.00"},80,80,6,6,{"v":19.2,"d":"19.20"},"无重合面",null,38,null,null,"总图内所有管架、410NC02102-54","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤二系南支架 NK9~NK11 6.5M\\8.5M面","H/工字钢","HN350*175*7*11",8,{"v":6500,"d":"6500.00"},350,175,7,11,{"v":71.656,"d":"71.66"},"无重合面",null,39,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系南支架 NK9~NK11 6.5M\\8.5M面","H/工字钢","HM194*150*6*9",4,{"v":2500,"d":"2500.00"},194,150,6,9,{"v":9.7,"d":"9.70"},"无重合面",null,40,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系南支架 NK9~NK11 6.5M\\8.5M面","H/工字钢","HM244*175*7*11",6,{"v":2500,"d":"2500.00"},244,175,7,11,17.49,"无重合面",null,41,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系南支架 NK9~NK11 6.5M\\8.5M面","H/工字钢","HM244*175*7*11",4,{"v":17200,"d":"17200.00"},244,175,7,11,{"v":80.2208,"d":"80.22"},"无重合面",null,42,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系南支架 NK9~NK11 6.5M\\8.5M面","H/工字钢","HW200*200*8*12",14,{"v":2500,"d":"2500.00"},200,200,8,12,41.16,"无重合面",null,43,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系南支架 NK9~NK11 6.5M\\8.5M面","L型钢","L80*6",20,{"v":4300,"d":"4300.00"},80,80,6,6,27.52,"无重合面",null,44,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系南支架 NK9~NK11 6.5M\\8.5M面","L型钢","L80*6",4,{"v":3200,"d":"3200.00"},80,80,6,6,{"v":4.096,"d":"4.10"},"无重合面",null,45,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系南支架NK9~NK11  H-H面","2L型钢","TN100*100*5.5*8",16,{"v":3900,"d":"3900.00"},100,100,5.5,8,24.96,"无重合面",null,46,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系南支架NK9~NK11  H-H面","2L型钢","TN100*100*5.5*8",4,{"v":2500,"d":"2500.00"},100,100,5.5,8,{"v":4,"d":"4.00"},"无重合面",null,47,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系南支架NK9~NK11  F-F\\G-G面","H/工字钢","HW150*150*7*10",4,{"v":3200,"d":"3200.00"},150,150,7,10,{"v":11.264,"d":"11.26"},"无重合面",null,48,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系南支架NK9~NK11  F-F\\G-G面","H/工字钢","HW150*150*7*10",12,{"v":2500,"d":"2500.00"},150,150,7,10,{"v":26.4,"d":"26.40"},"无重合面",null,49,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系南支架NK9~NK11  F-F\\G-G面","H/工字钢","HW200*200*8*12",8,{"v":8500,"d":"8500.00"},200,200,8,12,{"v":79.968,"d":"79.97"},"无重合面",null,50,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系南支架NK9~NK11  F-F\\G-G面","2L型钢","TN100*100*5.5*8",8,{"v":3900,"d":"3900.00"},100,100,5.5,8,12.48,"无重合面",null,51,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系南支架NK9~NK11  F-F\\G-G面","2L型钢","TN100*100*5.5*8",4,{"v":3200,"d":"3200.00"},100,100,5.5,8,5.12,"无重合面",null,52,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系南支架NK9~NK11  F-F\\G-G面","2L型钢","TN100*100*5.5*8",2,{"v":2500,"d":"2500.00"},100,100,5.5,8,{"v":2,"d":"2.00"},"无重合面",null,53,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系南支架NK9~NK11  F-F\\G-G面","2L型钢","TN125*125*6*9",16,{"v":3200,"d":"3200.00"},125,125,6,9,{"v":25.6,"d":"25.60"},"无重合面",null,54,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系南支架NK9~NK11  F-F\\G-G面","2L型钢","TN125*125*6*9",6,{"v":2500,"d":"2500.00"},125,125,6,9,{"v":7.5,"d":"7.50"},"无重合面",null,55,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系南支架NK12~NK14  F-F\\G-G面","H/工字钢","HW150*150*7*10",4,{"v":3200,"d":"3200.00"},150,150,7,10,{"v":11.264,"d":"11.26"},"无重合面",null,56,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系南支架NK12~NK14  F-F\\G-G面","H/工字钢","HW150*150*7*10",12,{"v":2500,"d":"2500.00"},150,150,7,10,{"v":26.4,"d":"26.40"},"无重合面",null,57,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系南支架NK12~NK14  F-F\\G-G面","H/工字钢","HW200*200*8*12",8,{"v":8500,"d":"8500.00"},200,200,8,12,{"v":79.968,"d":"79.97"},"无重合面",null,58,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系南支架NK12~NK14  F-F\\G-G面","2L型钢","TN100*100*5.5*8",8,{"v":3900,"d":"3900.00"},100,100,5.5,8,12.48,"无重合面",null,59,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系南支架NK12~NK14  F-F\\G-G面","2L型钢","TN100*100*5.5*8",4,{"v":3200,"d":"3200.00"},100,100,5.5,8,5.12,"无重合面",null,60,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系南支架NK12~NK14  F-F\\G-G面","2L型钢","TN100*100*5.5*8",2,{"v":2500,"d":"2500.00"},100,100,5.5,8,{"v":2,"d":"2.00"},"无重合面",null,61,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系南支架NK12~NK14  F-F\\G-G面","2L型钢","TN125*125*6*9",16,{"v":3200,"d":"3200.00"},125,125,6,9,{"v":25.6,"d":"25.60"},"无重合面",null,62,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系南支架NK12~NK14  F-F\\G-G面","2L型钢","TN125*125*6*9",6,{"v":2500,"d":"2500.00"},125,125,6,9,{"v":7.5,"d":"7.50"},"无重合面",null,63,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系南支架NK12~NK14   H-H面","2L型钢","TN100*100*5.5*8",16,{"v":3900,"d":"3900.00"},100,100,5.5,8,24.96,"无重合面",null,64,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系南支架NK12~NK14   H-H面","2L型钢","TN100*100*5.5*8",4,{"v":2500,"d":"2500.00"},100,100,5.5,8,{"v":4,"d":"4.00"},"无重合面",null,65,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系南支架NK12~NK14    6.5M\\8.5M面","H/工字钢","HN350*175*7*11",8,{"v":6500,"d":"6500.00"},350,175,7,11,{"v":71.656,"d":"71.66"},"无重合面",null,66,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系南支架NK12~NK14    6.5M\\8.5M面","H/工字钢","HM194*150*6*9",4,{"v":2500,"d":"2500.00"},194,150,6,9,{"v":9.7,"d":"9.70"},"无重合面",null,67,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系南支架NK12~NK14    6.5M\\8.5M面","H/工字钢","HM244*175*7*11",6,{"v":2500,"d":"2500.00"},244,175,7,11,17.49,"无重合面",null,68,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系南支架NK12~NK14    6.5M\\8.5M面","H/工字钢","HM244*175*7*11",4,{"v":17200,"d":"17200.00"},244,175,7,11,{"v":80.2208,"d":"80.22"},"无重合面",null,69,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系南支架NK12~NK14    6.5M\\8.5M面","H/工字钢","HW200*200*8*12",14,{"v":2500,"d":"2500.00"},200,200,8,12,41.16,"无重合面",null,70,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系南支架NK12~NK14    6.5M\\8.5M面","L型钢","L80*6",20,{"v":4300,"d":"4300.00"},80,80,6,6,27.52,"无重合面",null,71,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系南支架NK12~NK14    6.5M\\8.5M面","L型钢","L80*6",4,{"v":3200,"d":"3200.00"},80,80,6,6,{"v":4.096,"d":"4.10"},"无重合面",null,72,null,null,"总图内所有管架、410NC02102-55","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7   8.5M平面","H/工字钢","HM244*175*7*11",17,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":79.288,"d":"79.29"},"无重合面",null,72,null,null,"总图内所有管架、410NC02102-55","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7   8.5M平面","H/工字钢","HN400*200*8*13",2,{"v":18500,"d":"18500.00"},400,200,8,13,{"v":58.238,"d":"58.24"},"无重合面",null,72,null,null,"总图内所有管架、410NC02102-55","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7   8.5M平面","H/工字钢","HW200*200*8*12",2,{"v":15200,"d":"15200.00"},200,200,8,12,{"v":35.7504,"d":"35.75"},"无重合面",null,72,null,{"v":44,"d":"44.00"},"总图内所有管架、410NC02102-55","一般性腐蚀","环氧富锌漆",{"v":0.551721370676511,"d":"55%"}]
["洗涤北侧支架NK1~NK7   8.5M平面","H/工字钢","HW500*200*10*16",2,{"v":10800,"d":"10800.00"},500,200,10,16,{"v":38.1888,"d":"38.19"},"无重合面",null,72,null,null,"总图内所有管架、410NC02102-55","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7   8.5M平面","L型钢","L80*6",30,{"v":5000,"d":"5000.00"},80,80,6,6,{"v":48,"d":"48.00"},"无重合面",null,72,null,null,"总图内所有管架、410NC02102-55","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤北侧支架NK1~NK7   8.5M平面","L型钢","L80*6",4,{"v":5500,"d":"5500.00"},80,80,6,6,7.04,"无重合面",null,72,null,null,"总图内所有管架、410NC02102-55","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 洗涤北侧支架NK1~NK7   10M平面","H/工字钢","HM244*175*7*11",17,{"v":4000,"d":"4000.00"},244,175,7,11,{"v":79.288,"d":"79.29"},"无重合面",null,72,null,null,"总图内所有管架、410NC02102-55","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 洗涤北侧支架NK1~NK7   10M平面","H/工字钢","HN400*200*8*13",2,{"v":18500,"d":"18500.00"},400,200,8,13,{"v":58.238,"d":"58.24"},"无重合面",null,72,null,null,"总图内所有管架、410NC02102-55","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 洗涤北侧支架NK1~NK7   10M平面","H/工字钢","HW200*200*8*12",2,{"v":15200,"d":"15200.00"},200,200,8,12,{"v":35.7504,"d":"35.75"},"无重合面",null,72,null,{"v":22,"d":"22.00"},"总图内所有管架、410NC02102-55","一般性腐蚀","环氧富锌漆",{"v":0.380949742339447,"d":"38%"}]
[" 洗涤北侧支架NK1~NK7   10M平面","H/工字钢","HW500*200*10*16",2,{"v":10800,"d":"10800.00"},500,200,10,16,{"v":38.1888,"d":"38.19"},"无重合面",null,72,null,null,"总图内所有管架、410NC02102-55","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 洗涤北侧支架NK1~NK7   10M平面","L型钢","L100*10",2,{"v":60000,"d":"60000.00"},100,100,10,10,{"v":36,"d":"36.00"},"翼板重合",null,72,null,{"v":84,"d":"84.00"},"总图内所有管架、410NC02102-55","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
[" 洗涤北侧支架NK1~NK7   10M平面","L型钢","L80*6",30,{"v":5000,"d":"5000.00"},80,80,6,6,{"v":48,"d":"48.00"},"无重合面",null,72,null,null,"总图内所有管架、410NC02102-55","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[" 洗涤北侧支架NK1~NK7   10M平面","L型钢","L80*6",4,{"v":5500,"d":"5500.00"},80,80,6,6,7.04,"无重合面",null,72,null,null,"总图内所有管架、410NC02102-55","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["洗涤一系塔与泵房间支架NK18~NK20  S-S\\P-P\\Q-Q面","H/工字钢","HM148*100*6*9",4,{"v":2000,"d":"2000.00"},148,100,6,9,{"v":5.424,"d":"5.42"},"无重合面",null,73,null,null,"总图内所有管架、410NC02102-56","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系塔与泵房间支架NK18~NK21  S-S\\P-P\\Q-Q面","H/工字钢","HM148*100*6*9",5,{"v":2500,"d":"2500.00"},148,100,6,9,{"v":8.475,"d":"8.48"},"无重合面",null,74,null,null,"总图内所有管架、410NC02102-56","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系塔与泵房间支架NK18~NK22  S-S\\P-P\\Q-Q面","H/工字钢","HM194*150*6*9",8,{"v":2000,"d":"2000.00"},194,150,6,9,15.52,"无重合面",null,75,null,null,"总图内所有管架、410NC02102-56","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系塔与泵房间支架NK18~NK23  S-S\\P-P\\Q-Q面","H/工字钢","HM194*150*6*9",4,{"v":6200,"d":"6200.00"},194,150,6,9,{"v":24.056,"d":"24.06"},"无重合面",null,76,null,null,"总图内所有管架、410NC02102-56","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系塔与泵房间支架NK18~NK24  S-S\\P-P\\Q-Q面","L型钢","L63*6",28,{"v":3100,"d":"3100.00"},63,63,6,6,{"v":21.8736,"d":"21.87"},"无重合面",null,77,null,null,"总图内所有管架、410NC02102-56","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系塔与泵房间支架NK18~NK20  A-A面","H/工字钢","HW150*150*7*10",4,{"v":4600,"d":"4600.00"},150,150,7,10,{"v":16.192,"d":"16.19"},"无重合面",null,78,null,null,"总图内所有管架、410NC02102-56","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系塔与泵房间支架NK18~NK20  A-A面","H/工字钢","HW194*150*6*9",4,{"v":4600,"d":"4600.00"},194,150,6,9,{"v":17.848,"d":"17.85"},"无重合面",null,79,null,null,"总图内所有管架、410NC02102-56","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系塔与泵房间支架NK18~NK20  A-A面","L型钢","L63*6",8,{"v":3800,"d":"3800.00"},63,63,6,6,{"v":7.6608,"d":"7.66"},"无重合面",null,80,null,null,"总图内所有管架、410NC02102-56","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系塔与泵房间支架NK18~NK20  A-A面","2L型钢","TN100*100*5.5*8",2,{"v":3900,"d":"3900.00"},100,100,5.5,8,3.12,"无重合面",null,81,null,null,"总图内所有管架、410NC02102-56","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系塔与泵房间支架NK15~NK17  S-S\\P-P\\Q-Q面","H/工字钢","HM148*100*6*9",4,{"v":2000,"d":"2000.00"},148,100,6,9,{"v":5.424,"d":"5.42"},"无重合面",null,82,null,null,"总图内所有管架、410NC02102-56","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系塔与泵房间支架NK15~NK17  S-S\\P-P\\Q-Q面","H/工字钢","HM148*100*6*9",5,{"v":2500,"d":"2500.00"},148,100,6,9,{"v":8.475,"d":"8.48"},"无重合面",null,83,null,null,"总图内所有管架、410NC02102-56","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系塔与泵房间支架NK15~NK17  S-S\\P-P\\Q-Q面","H/工字钢","HM194*150*6*9",8,{"v":2000,"d":"2000.00"},194,150,6,9,15.52,"无重合面",null,84,null,null,"总图内所有管架、410NC02102-56","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系塔与泵房间支架NK15~NK17  S-S\\P-P\\Q-Q面","H/工字钢","HM194*150*6*9",4,{"v":6200,"d":"6200.00"},194,150,6,9,{"v":24.056,"d":"24.06"},"无重合面",null,85,null,null,"总图内所有管架、410NC02102-56","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系塔与泵房间支架NK15~NK17  S-S\\P-P\\Q-Q面","L型钢","L63*6",28,{"v":3100,"d":"3100.00"},63,63,6,6,{"v":21.8736,"d":"21.87"},"无重合面",null,86,null,null,"总图内所有管架、410NC02102-56","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系塔与泵房间支架NK15~NK17  A-A面","H/工字钢","HW150*150*7*10",4,{"v":4600,"d":"4600.00"},150,150,7,10,{"v":16.192,"d":"16.19"},"无重合面",null,87,null,null,"总图内所有管架、410NC02102-56","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系塔与泵房间支架NK15~NK17  A-A面","H/工字钢","HW194*150*6*9",4,{"v":4600,"d":"4600.00"},194,150,6,9,{"v":17.848,"d":"17.85"},"无重合面",null,88,null,null,"总图内所有管架、410NC02102-56","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系塔与泵房间支架NK15~NK17  A-A面","L型钢","L63*6",8,{"v":3800,"d":"3800.00"},63,63,6,6,{"v":7.6608,"d":"7.66"},"无重合面",null,89,null,null,"总图内所有管架、410NC02102-56","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系塔与泵房间支架NK15~NK17  A-A面","2L型钢","TN100*100*5.5*8",2,{"v":3900,"d":"3900.00"},100,100,5.5,8,3.12,"无重合面",null,90,null,null,"总图内所有管架、410NC02102-56","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系PT1平面A-A\\B-B","H/工字钢","HM194*150*6*9",16,{"v":5700,"d":"5700.00"},194,150,6,9,{"v":88.464,"d":"88.46"},"无重合面",null,91,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系PT1平面A-A\\B-B","圆钢","Q68*5",32,{"v":2140,"d":"2140.00"},68,{"$nulls":3},{"v":14.621849600000001,"d":"14.62"},"无重合面",null,92,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系PT1平面A-A\\B-B","圆钢","Q68*5",8,{"v":1700,"d":"1700.00"},68,{"$nulls":3},{"v":2.903872,"d":"2.90"},"无重合面",null,93,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系PT1平面A-A\\B-B","圆钢","Q89*5",6,{"v":7300,"d":"7300.00"},89,{"$nulls":3},{"v":12.240348000000003,"d":"12.24"},"无重合面",null,94,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系PT1平面A-A\\B-B","圆钢","Q89*5",4,{"v":3800,"d":"3800.00"},89,{"$nulls":3},{"v":4.247792000000001,"d":"4.25"},"无重合面",null,95,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系PT1平面","H/工字钢","HM194*150*6*9",2,{"v":38200,"d":"38200.00"},194,150,6,9,{"v":74.108,"d":"74.11"},"无重合面",null,96,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系PT1平面","H/工字钢","HM194*150*6*9",16,{"v":3000,"d":"3000.00"},194,150,6,9,46.56,"无重合面",null,97,null,32.64,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.412121212121212,"d":"41%"}]
["洗涤一系PT1平面","H/工字钢","HM194*150*6*9",28,{"v":1700,"d":"1700.00"},194,150,6,9,{"v":46.172,"d":"46.17"},"无重合面",null,98,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系(1.1米支架，22组)K1\\2\\3\\6\\14\\15\\21\\22\\28\\29\\37等","H/工字钢","H200*250*8*14",7,{"v":1100,"d":"1100.00"},200,250,8,14,{"v":10.5644,"d":"10.56"},"无重合面",null,99,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系(1.1米支架，22组)K1\\2\\3\\6\\14\\15\\21\\22\\28\\29\\37等","H/工字钢","HM194*150*6*9",44,{"v":5900,"d":"5900.00"},194,150,6,9,{"v":251.812,"d":"251.81"},"无重合面",null,100,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系(1.1米支架，22组)K1\\2\\3\\6\\14\\15\\21\\22\\28\\29\\37等","H/工字钢","HM194*150*6*9",2,{"v":1700,"d":"1700.00"},194,150,6,9,{"v":3.298,"d":"3.30"},"无重合面",null,101,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系(1.1米支架，22组)K1\\2\\3\\6\\14\\15\\21\\22\\28\\29\\37等","H/工字钢","HN200*100*5.5*8",4,{"v":1100,"d":"1100.00"},200,100,5.5,8,{"v":3.4496,"d":"3.45"},"无重合面",null,102,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系(1.1米支架，22组)K1\\2\\3\\6\\14\\15\\21\\22\\28\\29\\37等","H/工字钢","HN200*100*5.5*8",4,{"v":1700,"d":"1700.00"},200,100,5.5,8,{"v":5.3312,"d":"5.33"},"无重合面",null,103,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系(1.1米支架，22组)K1\\2\\3\\6\\14\\15\\21\\22\\28\\29\\37等","H/工字钢","HN300*150*6.5*10",2,{"v":1700,"d":"1700.00"},300,150,6.5,10,{"v":4.012,"d":"4.01"},"无重合面",null,104,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系(1.1米支架，22组)K1\\2\\3\\6\\14\\15\\21\\22\\28\\29\\37等","L型钢","L75*6",110,{"v":2600,"d":"2600.00"},75,75,6,6,{"v":85.8,"d":"85.80"},"无重合面",null,105,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤一系(1.1米支架，22组)K1\\2\\3\\6\\14\\15\\21\\22\\28\\29\\37等","L型钢","L75*6",16,{"v":3400,"d":"3400.00"},75,75,6,6,16.32,"无重合面",null,106,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系PT1平面A-A\\B-B","H/工字钢","HM194*150*6*9",16,{"v":5700,"d":"5700.00"},194,150,6,9,{"v":88.464,"d":"88.46"},"无重合面",null,107,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系PT1平面A-A\\B-B","圆钢","Q68*5",32,{"v":2140,"d":"2140.00"},68,{"$nulls":3},{"v":14.621849600000001,"d":"14.62"},"无重合面",null,108,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系PT1平面A-A\\B-B","圆钢","Q68*5",8,{"v":1700,"d":"1700.00"},68,{"$nulls":3},{"v":2.903872,"d":"2.90"},"无重合面",null,109,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系PT1平面A-A\\B-B","圆钢","Q89*5",6,{"v":7300,"d":"7300.00"},89,{"$nulls":3},{"v":12.240348000000003,"d":"12.24"},"无重合面",null,110,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系PT1平面A-A\\B-B","圆钢","Q89*5",4,{"v":3800,"d":"3800.00"},89,{"$nulls":3},{"v":4.247792000000001,"d":"4.25"},"无重合面",null,111,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系PT1平面","H/工字钢","HM194*150*6*9",2,{"v":38200,"d":"38200.00"},194,150,6,9,{"v":74.108,"d":"74.11"},"无重合面",null,112,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系PT1平面","H/工字钢","HM194*150*6*9",16,{"v":3000,"d":"3000.00"},194,150,6,9,46.56,"无重合面",null,113,null,32.64,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.412121212121212,"d":"41%"}]
["洗涤二系PT1平面","H/工字钢","HM194*150*6*9",28,{"v":1700,"d":"1700.00"},194,150,6,9,{"v":46.172,"d":"46.17"},"无重合面",null,114,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系(1.1米支架，22组)K1\\2\\3\\6\\14\\15\\21\\22\\28\\29\\37等","H/工字钢","H200*250*8*14",7,{"v":1100,"d":"1100.00"},200,250,8,14,{"v":10.5644,"d":"10.56"},"无重合面",null,115,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系(1.1米支架，22组)K1\\2\\3\\6\\14\\15\\21\\22\\28\\29\\37等","H/工字钢","HM194*150*6*9",44,{"v":5900,"d":"5900.00"},194,150,6,9,{"v":251.812,"d":"251.81"},"无重合面",null,116,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系(1.1米支架，22组)K1\\2\\3\\6\\14\\15\\21\\22\\28\\29\\37等","H/工字钢","HM194*150*6*9",2,{"v":1700,"d":"1700.00"},194,150,6,9,{"v":3.298,"d":"3.30"},"无重合面",null,117,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系(1.1米支架，22组)K1\\2\\3\\6\\14\\15\\21\\22\\28\\29\\37等","H/工字钢","HN200*100*5.5*8",4,{"v":1100,"d":"1100.00"},200,100,5.5,8,{"v":3.4496,"d":"3.45"},"无重合面",null,118,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系(1.1米支架，22组)K1\\2\\3\\6\\14\\15\\21\\22\\28\\29\\37等","H/工字钢","HN200*100*5.5*8",4,{"v":1700,"d":"1700.00"},200,100,5.5,8,{"v":5.3312,"d":"5.33"},"无重合面",null,119,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系(1.1米支架，22组)K1\\2\\3\\6\\14\\15\\21\\22\\28\\29\\37等","H/工字钢","HN300*150*6.5*10",2,{"v":1700,"d":"1700.00"},300,150,6.5,10,{"v":4.012,"d":"4.01"},"无重合面",null,120,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系(1.1米支架，22组)K1\\2\\3\\6\\14\\15\\21\\22\\28\\29\\37等","L型钢","L75*6",110,{"v":2600,"d":"2600.00"},75,75,6,6,{"v":85.8,"d":"85.80"},"无重合面",null,121,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤二系(1.1米支架，22组)K1\\2\\3\\6\\14\\15\\21\\22\\28\\29\\37等","L型钢","L75*6",16,{"v":3400,"d":"3400.00"},75,75,6,6,16.32,"无重合面",null,122,null,null,"总图内所有管架、410NC02102-59、60、61","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层1","H/工字钢","HM390*300*10*16",2,{"v":11800,"d":"11800.00"},390,300,10,16,{"v":45.9728,"d":"45.97"},"无重合面",null,122,null,null,"总图内所有管架、410NC02102-65","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层1","H/工字钢","HN200*100*5.5*8",6,{"v":1000,"d":"1000.00"},200,100,5.5,8,{"v":4.704,"d":"4.70"},"无重合面",null,122,null,null,"总图内所有管架、410NC02102-65","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层1","H/工字钢","HN200*100*5.5*8",58,{"v":2200,"d":"2200.00"},200,100,5.5,8,{"v":100.0384,"d":"100.04"},"无重合面",null,122,null,null,"总图内所有管架、410NC02102-65","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层1","H/工字钢","HN300*150*6.5*9",2,{"v":24070,"d":"24070.00"},300,150,6.5,9,{"v":56.90148,"d":"56.90"},"无重合面",null,122,null,null,"总图内所有管架、410NC02102-65","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层1","H/工字钢","HN400*200*8*13",2,{"v":101000,"d":"101000.00"},400,200,8,13,{"v":317.948,"d":"317.95"},"无重合面",null,122,null,null,"总图内所有管架、410NC02102-65","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层1","H/工字钢","HW150*150*7*10",20,{"v":2500,"d":"2500.00"},150,150,7,10,{"v":44,"d":"44.00"},"无重合面",null,122,null,null,"总图内所有管架、410NC02102-65","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层1","H/工字钢","HW150*150*7*10",4,{"v":6000,"d":"6000.00"},150,150,7,10,21.12,"无重合面",null,122,null,null,"总图内所有管架、410NC02102-65","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层1","H/工字钢","HW150*150*7*10",4,{"v":2500,"d":"2500.00"},150,150,7,10,{"v":8.8,"d":"8.80"},"无重合面",null,122,null,null,"总图内所有管架、410NC02102-65","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层1","H/工字钢","HW150*150*7*10",12,{"v":6000,"d":"6000.00"},150,150,7,10,63.36,"无重合面",null,122,null,null,"总图内所有管架、410NC02102-65","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层1","H/工字钢","HW194*150*6*9",4,{"v":6000,"d":"6000.00"},194,150,6,9,23.28,"无重合面",null,122,null,null,"总图内所有管架、410NC02102-65","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层1","H/工字钢","HW200*200*8*12",4,{"v":6000,"d":"6000.00"},200,200,8,12,{"v":28.224,"d":"28.22"},"无重合面",null,122,null,null,"总图内所有管架、410NC02102-65","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层1","L型钢","L100*10",2,{"v":155000,"d":"155000.00"},100,100,10,10,{"v":93,"d":"93.00"},"翼板重合",null,122,null,{"v":217,"d":"217.00"},"总图内所有管架、410NC02102-65","一般性腐蚀","环氧富锌漆",{"v":0.7,"d":"70%"}]
["焦油氨水分离单元电缆支架平面层1","L型钢","L56*5",33,{"v":2400,"d":"2400.00"},56,56,5,5,{"v":17.7408,"d":"17.74"},"无重合面",null,122,null,null,"总图内所有管架、410NC02102-65","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层1","L型钢","L56*5",16,{"v":2200,"d":"2200.00"},56,56,5,5,{"v":7.8848,"d":"7.88"},"无重合面",null,122,null,null,"总图内所有管架、410NC02102-65","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层1","L型钢","L56*5",30,{"v":3100,"d":"3100.00"},56,56,5,5,{"v":20.832,"d":"20.83"},"无重合面",null,122,null,null,"总图内所有管架、410NC02102-65","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层1","L型钢","L80*6",90,{"v":3700,"d":"3700.00"},80,80,6,6,106.56,"无重合面",null,122,null,null,"总图内所有管架、410NC02102-65","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层1","2L型钢","TN100*100*5.5*8",18,{"v":2500,"d":"2500.00"},100,100,5.5,8,{"v":18,"d":"18.00"},"无重合面",null,122,null,null,"总图内所有管架、410NC02102-65","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层1","2L型钢","TN125*125*6*9",6,{"v":2800,"d":"2800.00"},125,125,6,9,{"v":8.4,"d":"8.40"},"无重合面",null,122,null,null,"总图内所有管架、410NC02102-65","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层2一系","H/工字钢","HN200*100*5.5*8",20,{"v":1000,"d":"1000.00"},200,100,5.5,8,15.68,"无重合面",null,122,null,null,"总图内所有管架、410NC02102-66","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层2一系","H/工字钢","HN300*150*6.5*9",2,{"v":52500,"d":"52500.00"},300,150,6.5,9,124.11,"无重合面",null,122,null,null,"总图内所有管架、410NC02102-66","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层2一系","H/工字钢","HW100*100*6*10",16,{"v":3500,"d":"3500.00"},100,100,6,10,32.48,"无重合面",null,122,null,null,"总图内所有管架、410NC02102-66","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层2一系","2L型钢","TN100*100*5.5*8",47,{"v":3200,"d":"3200.00"},100,100,5.5,8,60.16,"无重合面",null,122,null,null,"总图内所有管架、410NC02102-66","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层2一系","L型钢","L56*5",30,{"v":1400,"d":"1400.00"},56,56,5,5,{"v":9.408,"d":"9.41"},"无重合面",null,122,null,null,"总图内所有管架、410NC02102-66","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层2二系","H/工字钢","HN200*100*5.5*8",20,{"v":1000,"d":"1000.00"},200,100,5.5,8,15.68,"无重合面",null,122,null,null,"总图内所有管架、410NC02102-66","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层2二系","H/工字钢","HN300*150*6.5*9",2,{"v":52500,"d":"52500.00"},300,150,6.5,9,124.11,"无重合面",null,122,null,null,"总图内所有管架、410NC02102-66","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层2二系","H/工字钢","HW100*100*6*9",16,{"v":3500,"d":"3500.00"},100,100,6,9,{"v":32.592,"d":"32.59"},"无重合面",null,122,null,null,"总图内所有管架、410NC02102-66","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层2二系","2L型钢","TN100*100*5.5*8",47,{"v":3200,"d":"3200.00"},100,100,5.5,8,60.16,"无重合面",null,122,null,null,"总图内所有管架、410NC02102-66","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离单元电缆支架平面层2二系","L型钢","L56*5",30,{"v":1400,"d":"1400.00"},56,56,5,5,{"v":9.408,"d":"9.41"},"无重合面",null,122,null,null,"总图内所有管架、410NC02102-75\\76\\77","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构电捕前","H/工字钢","HM294*200*8*12",10,{"v":1500,"d":"1500.00"},294,200,8,12,20.46,"无重合面",null,123,null,{"v":92.4,"d":"92.40"},"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.818713450292398,"d":"82%"}]
["初冷电捕区域钢结构电捕前","H/工字钢","HN300*150*6.5*9",8,{"v":7700,"d":"7700.00"},300,150,6.5,9,{"v":72.8112,"d":"72.81"},"无重合面",null,124,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构电捕前","H/工字钢","HW150*150*7*10",12,{"v":2770,"d":"2770.00"},150,150,7,10,{"v":29.2512,"d":"29.25"},"无重合面",null,125,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构电捕前","H/工字钢","HW200*200*8*12",8,{"v":1500,"d":"1500.00"},200,200,8,12,{"v":14.112,"d":"14.11"},"无重合面",null,126,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构电捕前","2L型钢","TM97*150*6*9",16,{"v":3000,"d":"3000.00"},97,150,6,9,{"v":23.712,"d":"23.71"},"无重合面",null,127,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构电捕前","2L型钢","TN100*100*5.5*8",6,{"v":3300,"d":"3300.00"},100,100,5.5,8,7.92,"无重合面",null,128,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构电捕后","[槽钢","[16a（160*63*6.5）",4,{"v":7700,"d":"7700.00"},160,63,6.5,6.5,{"v":17.2172,"d":"17.22"},"无重合面",null,129,null,135.52,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.887275660415406,"d":"89%"}]
["初冷电捕区域钢结构电捕后","H/工字钢","HM294*200*8*12",10,{"v":2200,"d":"2200.00"},294,200,8,12,{"v":30.008,"d":"30.01"},"无重合面",null,130,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构电捕后","H/工字钢","HN300*150*6.5*9",8,{"v":7700,"d":"7700.00"},300,150,6.5,9,{"v":72.8112,"d":"72.81"},"无重合面",null,131,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构电捕后","H/工字钢","HW150*150*7*10",12,{"v":2770,"d":"2770.00"},150,150,7,10,{"v":29.2512,"d":"29.25"},"无重合面",null,132,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构电捕后","H/工字钢","HW200*200*8*12",8,{"v":2200,"d":"2200.00"},200,200,8,12,{"v":20.6976,"d":"20.70"},"无重合面",null,133,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构电捕后","2L型钢","TM97*150*6*9",16,{"v":3200,"d":"3200.00"},97,150,6,9,{"v":25.2928,"d":"25.29"},"无重合面",null,134,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构电捕后","2L型钢","TN100*100*5.5*8",6,{"v":3300,"d":"3300.00"},100,100,5.5,8,7.92,"无重合面",null,135,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构初冷前","[槽钢","[16a（160*63*6.5）",1,{"v":53400,"d":"53400.00"},160,63,6.5,6.5,{"v":29.8506,"d":"29.85"},"无重合面",null,136,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构初冷前","[槽钢","[16b（160*63*6.5）",1,{"v":72160,"d":"72160.00"},160,63,6.5,6.5,{"v":40.33744,"d":"40.34"},"无重合面",null,137,null,{"v":57.728,"d":"57.73"},"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.588668138337013,"d":"59%"}]
["初冷电捕区域钢结构初冷前","H/工字钢","HM294*200*8*12",22,{"v":2000,"d":"2000.00"},294,200,8,12,{"v":60.016,"d":"60.02"},"无重合面",null,138,null,{"v":213.6,"d":"213.60"},"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.78065610198234,"d":"78%"}]
["初冷电捕区域钢结构初冷前","H/工字钢","HN300*150*6.5*9",2,{"v":53400,"d":"53400.00"},300,150,6.5,9,{"v":126.2376,"d":"126.24"},"无重合面",null,139,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构初冷前","H/工字钢","HW150*150*7*10",16,{"v":6800,"d":"6800.00"},150,150,7,10,{"v":95.744,"d":"95.74"},"无重合面",null,140,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构初冷前","2L型钢","TM97*150*6*9",4,{"v":10400,"d":"10400.00"},97,150,6,9,{"v":20.5504,"d":"20.55"},"无重合面",null,141,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构初冷前","2L型钢","TN100*100*5.5*8",24,{"v":2900,"d":"2900.00"},100,100,5.5,8,27.84,"无重合面",null,142,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构初冷后","[槽钢","[16a（160*63*6.5）",2,{"v":5600,"d":"5600.00"},160,63,6.5,6.5,{"v":6.2608,"d":"6.26"},"无重合面",null,143,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构初冷后","[槽钢","[16a（160*63*6.5）",5,{"v":4000,"d":"4000.00"},160,63,6.5,6.5,11.18,"无重合面",null,144,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构初冷后","H/工字钢","HM294*200*8*12",14,{"v":1900,"d":"1900.00"},294,200,8,12,{"v":36.2824,"d":"36.28"},"无重合面",null,145,null,126.16,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.776644521381117,"d":"78%"}]
["初冷电捕区域钢结构初冷后","H/工字钢","HM294*200*8*12",42,{"v":1200,"d":"1200.00"},294,200,8,12,{"v":68.7456,"d":"68.75"},"无重合面",null,146,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构初冷后","H/工字钢","HN300*150*6.5*9",10,{"v":4000,"d":"4000.00"},300,150,6.5,9,47.28,"无重合面",null,147,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构初冷后","H/工字钢","HN300*150*6.5*9",4,{"v":5600,"d":"5600.00"},300,150,6.5,9,{"v":26.4768,"d":"26.48"},"无重合面",null,148,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构初冷后","H/工字钢","HN300*150*6.5*9",2,{"v":5600,"d":"5600.00"},300,150,6.5,9,{"v":13.2384,"d":"13.24"},"无重合面",null,149,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构初冷后","H/工字钢","HW150*150*7*10",28,{"v":7450,"d":"7450.00"},150,150,7,10,{"v":183.568,"d":"183.57"},"无重合面",null,150,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构初冷后","H/工字钢","HW200*200*8*12",10,{"v":4000,"d":"4000.00"},200,200,8,12,47.04,"无重合面",null,151,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构初冷后","H/工字钢","HW200*200*8*12",2,{"v":5600,"d":"5600.00"},200,200,8,12,{"v":13.1712,"d":"13.17"},"无重合面",null,152,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构初冷后","L型钢","L75*6",40,{"v":5200,"d":"5200.00"},75,75,6,6,{"v":62.4,"d":"62.40"},"无重合面",null,153,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构初冷后","L型钢","L75*6",8,{"v":6700,"d":"6700.00"},75,75,6,6,16.08,"无重合面",null,154,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构初冷后","2L型钢","TN100*100*5.5*8",4,{"v":2100,"d":"2100.00"},100,100,5.5,8,3.36,"无重合面",null,155,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷电捕区域钢结构初冷后","2L型钢","TN125*125*6*9",84,{"v":1500,"d":"1500.00"},125,125,6,9,{"v":63,"d":"63.00"},"无重合面",null,156,null,null,"总图内所有管架、410NC02102-75\\76\\77","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["硫回收钢结构PT4*3","[槽钢","[16b（160*63*6.5）",18,{"v":2220,"d":"2220.00"},160,63,6.5,6.5,{"v":22.33764,"d":"22.34"},"无重合面",null,156,null,{"v":45.675,"d":"45.68"},"总图内所有管架、410NC34101-10","一般性腐蚀","环氧富锌漆",{"v":0.671566344138384,"d":"67%"}]
["硫回收钢结构PT4*3","H/工字钢","HM148*100*6*9",3,{"v":2500,"d":"2500.00"},148,100,6,9,{"v":5.085,"d":"5.09"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PT4*3","H/工字钢","HM194*150*6*9",3,{"v":1000,"d":"1000.00"},194,150,6,9,2.91,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PT4*3","H/工字钢","HM194*150*6*9",15,{"v":2500,"d":"2500.00"},194,150,6,9,{"v":36.375,"d":"36.38"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PT4*3","H/工字钢","HM194*150*6*9",12,{"v":3300,"d":"3300.00"},194,150,6,9,{"v":38.412,"d":"38.41"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PT4*3","H/工字钢","HW150*150*7*10",12,{"v":3360,"d":"3360.00"},150,150,7,10,{"v":35.4816,"d":"35.48"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构酸气管道支架","[槽钢","[16b（160*63*6.5）",4,{"v":3500,"d":"3500.00"},160,63,6.5,6.5,{"v":7.826,"d":"7.83"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构酸气管道支架","H/工字钢","H200*170*6*10",1,{"v":1600,"d":"1600.00"},200,170,6,10,{"v":1.696,"d":"1.70"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构酸气管道支架","H/工字钢","HM194*150*6*9",6,{"v":1700,"d":"1700.00"},194,150,6,9,{"v":9.894,"d":"9.89"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构酸气管道支架","H/工字钢","HM194*150*6*9",8,{"v":3000,"d":"3000.00"},194,150,6,9,23.28,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构酸气管道支架","H/工字钢","HM194*150*6*9",4,{"v":4000,"d":"4000.00"},194,150,6,9,15.52,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构酸气管道支架","H/工字钢","HM194*150*6*9",2,{"v":7000,"d":"7000.00"},194,150,6,9,13.58,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构酸气管道支架","H/工字钢","HW150*150*7*10",12,{"v":4500,"d":"4500.00"},150,150,7,10,47.52,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构酸气管道支架","L型钢","L80*6",4,{"v":2200,"d":"2200.00"},80,80,6,6,{"v":2.816,"d":"2.82"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构酸气管道支架","2L型钢","TN100*10*5.5*8",12,{"v":2500,"d":"2500.00"},100,100,5.5,8,{"v":12,"d":"12.00"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构酸气管道支架","2L型钢","TN100*10*5.5*8",6,{"v":1700,"d":"1700.00"},100,100,5.5,8,4.08,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构管道支架ZJab","H/工字钢","HM194*150*6*9",6,{"v":6000,"d":"6000.00"},194,150,6,9,34.92,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构管道支架ZJab","H/工字钢","HM224*175*7*11",6,{"v":2850,"d":"2850.00"},224,175,7,11,{"v":19.2546,"d":"19.25"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构管道支架ZJab","H/工字钢","HW200*200*8*12",8,{"v":6000,"d":"6000.00"},200,200,8,12,{"v":46.848,"d":"46.85"},"翼板重合",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构管道支架ZJab","H/工字钢","HW200*200*8*12",8,{"v":2850,"d":"2850.00"},200,200,8,12,{"v":26.8128,"d":"26.81"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构管道支架ZJab","L型钢","L80*6",6,{"v":4600,"d":"4600.00"},80,80,6,6,{"v":8.832,"d":"8.83"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构管道支架ZJab","L型钢","L80*6",8,{"v":4600,"d":"4600.00"},80,80,6,6,{"v":11.776,"d":"11.78"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PTb1\\2*3","H/工字钢","HM194*150*6*9",2,{"v":3000,"d":"3000.00"},194,150,6,9,5.82,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PTb1\\2*3","H/工字钢","HM194*150*6*9",5,{"v":2150,"d":"2150.00"},194,150,6,9,{"v":10.4275,"d":"10.43"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PTb1\\2*3","H/工字钢","HW150*150*7*10",4,{"v":3500,"d":"3500.00"},150,150,7,10,12.32,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PTb1\\2*3","L型钢","L63*6",4,{"v":4800,"d":"4800.00"},63,63,6,6,{"v":4.8384,"d":"4.84"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PTb1\\2*3","2L型钢","TN100*10*5.5*8",4,{"v":2800,"d":"2800.00"},100,100,5.5,8,4.48,"无重合面",null,156,null,41.58,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0.90273556231003,"d":"90%"}]
["硫回收钢结构PTb1\\2*3","2L型钢","TN100*10*5.5*8",2,{"v":2150,"d":"2150.00"},100,100,5.5,8,1.72,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构DJ1*3","H/工字钢","HW150*150*7*10",6,{"v":2270,"d":"2270.00"},150,150,7,10,{"v":11.9856,"d":"11.99"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构DJ1*3","H/工字钢","HW200*200*8*12",3,{"v":1750,"d":"1750.00"},200,200,8,12,{"v":6.174,"d":"6.17"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构DJ1*3","L型钢","L63*6",3,{"v":3400,"d":"3400.00"},63,63,6,6,{"v":2.5704,"d":"2.57"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PTC4","H/工字钢","HW100*100*6*8",4,{"v":1940,"d":"1940.00"},100,100,6,8,{"v":4.53184,"d":"4.53"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PTC4","H/工字钢","HW100*100*6*8",2,{"v":900,"d":"900.00"},100,100,6,8,{"v":1.0512,"d":"1.05"},"无重合面",null,156,null,3.88,"总图内所有管架、410NC34101-12","一般性腐蚀","环氧富锌漆",{"v":0.786826735885788,"d":"79%"}]
["硫回收钢结构PTC4","H/工字钢","HW100*100*6*8",4,{"v":2700,"d":"2700.00"},100,100,6,8,{"v":6.3072,"d":"6.31"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PTC3","H/工字钢","HW100*100*6*8",4,{"v":2250,"d":"2250.00"},100,100,6,8,{"v":5.256,"d":"5.26"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PTC3","H/工字钢","HW100*100*6*8",2,{"v":900,"d":"900.00"},100,100,6,8,{"v":1.0512,"d":"1.05"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PTC3","H/工字钢","HW100*100*6*8",4,{"v":2700,"d":"2700.00"},100,100,6,8,{"v":6.3072,"d":"6.31"},"无重合面",null,156,null,{"v":6,"d":"6.00"},"总图内所有管架、410NC34101-12","一般性腐蚀","环氧富锌漆",{"v":0.487519500780031,"d":"49%"}]
["硫回收钢结构PTC2","H/工字钢","HW100*100*6*8",6,{"v":2700,"d":"2700.00"},100,100,6,8,{"v":9.4608,"d":"9.46"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PTC2","H/工字钢","HW100*100*6*8",12,{"v":900,"d":"900.00"},100,100,6,8,{"v":6.3072,"d":"6.31"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PTC2","H/工字钢","HW100*100*6*8",2,{"v":6500,"d":"6500.00"},100,100,6,8,{"v":7.592,"d":"7.59"},"无重合面",null,156,null,{"v":13,"d":"13.00"},"总图内所有管架、410NC34101-12","一般性腐蚀","环氧富锌漆",{"v":0.631313131313131,"d":"63%"}]
["硫回收钢结构PTC1","H/工字钢","HW100*100*6*8",6,{"v":2700,"d":"2700.00"},100,100,6,8,{"v":9.4608,"d":"9.46"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PTC1","H/工字钢","HW100*100*6*8",12,{"v":900,"d":"900.00"},100,100,6,8,{"v":6.3072,"d":"6.31"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PTC1","H/工字钢","HW100*100*6*8",2,{"v":7100,"d":"7100.00"},100,100,6,8,{"v":8.2928,"d":"8.29"},"无重合面",null,156,null,{"v":14.2,"d":"14.20"},"总图内所有管架、410NC34101-12","一般性腐蚀","环氧富锌漆",{"v":0.631313131313131,"d":"63%"}]
["硫回收钢结构E","H/工字钢","HM294*200*8*12",8,{"v":800,"d":"800.00"},294,200,8,12,{"v":8.7296,"d":"8.73"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构E","H/工字钢","HM294*200*8*12",6,{"v":5500,"d":"5500.00"},294,200,8,12,{"v":45.012,"d":"45.01"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构E","H/工字钢","HW250*250*9*14",5,{"v":11500,"d":"11500.00"},250,250,9,14,84.64,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构E","2L型钢","TN100*100*5.5*8",4,{"v":7300,"d":"7300.00"},100,100,5.5,8,11.68,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构E","2L型钢","TN100*100*5.5*8",4,{"v":8500,"d":"8500.00"},100,100,5.5,8,{"v":13.6,"d":"13.60"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构CD","H/工字钢","H500*250*10*20",3,{"v":5500,"d":"5500.00"},500,250,10,20,32.34,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构CD","H/工字钢","HN400*200*8*13",3,{"v":5500,"d":"5500.00"},400,200,8,13,{"v":25.971,"d":"25.97"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构CD","H/工字钢","HW200*200*8*12",8,{"v":800,"d":"800.00"},200,200,8,12,{"v":7.5264,"d":"7.53"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构CD","H/工字钢","HW250*250*9*14",5,{"v":11500,"d":"11500.00"},250,250,9,14,84.64,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构B","H/工字钢","H500*250*10*20",3,{"v":5500,"d":"5500.00"},500,250,10,20,32.34,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构B","H/工字钢","HM294*200*8*12",3,{"v":6000,"d":"6000.00"},294,200,8,12,{"v":24.552,"d":"24.55"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构B","H/工字钢","HN400*200*8*13",3,{"v":5500,"d":"5500.00"},400,200,8,13,{"v":25.971,"d":"25.97"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构B","H/工字钢","HN400*200*8*13",1,{"v":6000,"d":"6000.00"},400,200,8,13,{"v":9.444,"d":"9.44"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构B","H/工字钢","HW250*250*9*14",5,{"v":11500,"d":"11500.00"},250,250,9,14,84.64,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构B","H/工字钢","HW250*250*9*14",2,{"v":5000,"d":"5000.00"},250,250,9,14,14.72,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构A","H/工字钢","HM294*200*8*12",6,{"v":5500,"d":"5500.00"},294,200,8,12,{"v":45.012,"d":"45.01"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构A","H/工字钢","HM294*200*8*12",4,{"v":6000,"d":"6000.00"},294,200,8,12,{"v":32.736,"d":"32.74"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构A","H/工字钢","HN400*200*8*13",1,{"v":6000,"d":"6000.00"},400,200,8,13,{"v":9.444,"d":"9.44"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构A","H/工字钢","HW250*250*9*14",5,{"v":11500,"d":"11500.00"},250,250,9,14,84.64,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构A","H/工字钢","HW250*250*9*14",2,{"v":5000,"d":"5000.00"},250,250,9,14,14.72,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构A","2L型钢","TN100*100*5.5*8",4,{"v":7300,"d":"7300.00"},100,100,5.5,8,11.68,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构A","2L型钢","TN100*100*5.5*8",4,{"v":8500,"d":"8500.00"},100,100,5.5,8,{"v":13.6,"d":"13.60"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构2-6","H/工字钢","HM294*200*8*12",3,{"v":1200,"d":"1200.00"},294,200,8,12,{"v":4.9104,"d":"4.91"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构2-6","H/工字钢","HM294*200*8*12",5,{"v":1000,"d":"1000.00"},294,200,8,12,6.82,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构2-6","H/工字钢","HM294*200*8*12",5,{"v":1500,"d":"1500.00"},294,200,8,12,10.23,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构2-6","H/工字钢","HM294*200*8*12",10,{"v":20000,"d":"20000.00"},294,200,8,12,{"v":272.8,"d":"272.80"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构2-6","2L型钢","TN100*100*5.5*8",10,{"v":7300,"d":"7300.00"},100,100,5.5,8,{"v":29.2,"d":"29.20"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构2-6","2L型钢","TN100*100*5.5*8",10,{"v":8500,"d":"8500.00"},100,100,5.5,8,{"v":34,"d":"34.00"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构1.7","H/工字钢","HM294*200*8*12",2,{"v":5600,"d":"5600.00"},294,200,8,12,{"v":15.2768,"d":"15.28"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构ZJ4","H/工字钢","H200*170*6*10",12,{"v":2000,"d":"2000.00"},200,170,6,10,25.44,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构ZJ4","H/工字钢","H200*170*6*10",12,{"v":700,"d":"700.00"},200,170,6,10,{"v":8.904,"d":"8.90"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构ZJ4","H/工字钢","HW150*150*7*10",12,{"v":2860,"d":"2860.00"},150,150,7,10,{"v":30.2016,"d":"30.20"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构ZJ4","L型钢","L63*6",24,{"v":3500,"d":"3500.00"},63,63,6,6,{"v":21.168,"d":"21.17"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构ZJ3","H/工字钢","H200*170*6*10",12,{"v":1200,"d":"1200.00"},200,170,6,10,{"v":15.264,"d":"15.26"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构ZJ3","H/工字钢","HW150*150*7*10",6,{"v":1580,"d":"1580.00"},150,150,7,10,{"v":8.3424,"d":"8.34"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构ZJ3","L型钢","L63*6",6,{"v":2200,"d":"2200.00"},63,63,6,6,{"v":3.3264,"d":"3.33"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构ZJ2","H/工字钢","H200*170*6*10",12,{"v":1200,"d":"1200.00"},200,170,6,10,{"v":15.264,"d":"15.26"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构ZJ2","H/工字钢","HW150*150*7*10",12,{"v":1400,"d":"1400.00"},150,150,7,10,{"v":14.784,"d":"14.78"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构ZJ2","L型钢","L63*6",12,{"v":1500,"d":"1500.00"},63,63,6,6,{"v":4.536,"d":"4.54"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构ZJ1","H/工字钢","H200*170*6*10",12,{"v":1200,"d":"1200.00"},200,170,6,10,{"v":15.264,"d":"15.26"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构ZJ1","H/工字钢","HW150*150*7*10",12,{"v":2050,"d":"2050.00"},150,150,7,10,{"v":21.648,"d":"21.65"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构ZJ1","L型钢","L63*6",24,{"v":1500,"d":"1500.00"},63,63,6,6,{"v":9.072,"d":"9.07"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构5M平面","H/工字钢","H400*200*8*13",8,{"v":5000,"d":"5000.00"},400,200,8,13,54.96,"翼板重合",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构5M平面","H/工字钢","HM194*150*6*9",33,{"v":5000,"d":"5000.00"},194,150,6,9,{"v":135.3,"d":"135.30"},"翼板重合",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构5M平面","H/工字钢","HN200*100*5.5*8",12,{"v":5000,"d":"5000.00"},200,100,5.5,8,41.04,"翼板重合",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构5M平面","H/工字钢","HN200*100*5.5*9",1,{"v":19700,"d":"19700.00"},200,100,5.5,9,{"v":13.4354,"d":"13.44"},"翼板重合",null,156,null,1024.24,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0.987052405790867,"d":"99%"}]
["硫回收钢结构5M平面","H/工字钢","HW200*200*8*12",9,{"v":5000,"d":"5000.00"},200,200,8,12,43.92,"翼板重合",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构11M平面","[槽钢","[16a（160*63*6.5）",12,{"v":1200,"d":"1200.00"},160,63,6.5,6.5,{"v":5.7456,"d":"5.75"},"腹板重合",null,156,null,{"v":769.5,"d":"769.50"},"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0.992588671254632,"d":"99%"}]
["硫回收钢结构11M平面","[槽钢","[16a（160*63*6.5）",3,{"v":3100,"d":"3100.00"},160,63,6.5,6.5,{"v":4.6128,"d":"4.61"},"翼板重合",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构11M平面","[槽钢","[16a（160*63*6.5）",8,{"v":1500,"d":"1500.00"},160,63,6.5,6.5,{"v":5.952,"d":"5.95"},"翼板重合",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构11M平面","H/工字钢","H500*250*10*20",12,{"v":5000,"d":"5000.00"},500,250,10,20,{"v":102.6,"d":"102.60"},"翼板重合",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构11M平面","H/工字钢","HM194*150*6*9",14,{"v":5000,"d":"5000.00"},194,150,6,9,{"v":57.4,"d":"57.40"},"翼板重合",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构11M平面","H/工字钢","HM194*150*6*9",6,{"v":2000,"d":"2000.00"},194,150,6,9,9.84,"翼板重合",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构11M平面","H/工字钢","HM194*150*6*9",11,{"v":1750,"d":"1750.00"},194,150,6,9,{"v":15.785,"d":"15.79"},"翼板重合",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构11M平面","H/工字钢","HW200*200*8*12",9,{"v":3400,"d":"3400.00"},200,200,8,12,{"v":29.8656,"d":"29.87"},"翼板重合",null,156,null,null,"总图内所有管架、410NC34101-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PT1a","H/工字钢","HM148*100*6*9",8,{"v":5000,"d":"5000.00"},148,100,6,9,27.12,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PT1a","H/工字钢","HM148*100*6*9",4,{"v":800,"d":"800.00"},148,100,6,9,{"v":2.1696,"d":"2.17"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PT1a","H/工字钢","HM148*100*6*9",4,{"v":1300,"d":"1300.00"},148,100,6,9,{"v":3.5256,"d":"3.53"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PT1a","H/工字钢","HM148*100*6*9",5,{"v":12950,"d":"12950.00"},148,100,6,9,{"v":43.9005,"d":"43.90"},"无重合面",null,156,null,28.49,"总图内所有管架、410NC34101-8","一般性腐蚀","环氧富锌漆",{"v":0.393559928443649,"d":"39%"}]
["硫回收钢结构PT1a","L型钢","L50*5",16,{"v":1450,"d":"1450.00"},50,50,5,5,4.64,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PT1","H/工字钢","HM148*100*6*9",8,{"v":5000,"d":"5000.00"},148,100,6,9,27.12,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PT1","H/工字钢","HM148*100*6*9",4,{"v":800,"d":"800.00"},148,100,6,9,{"v":2.1696,"d":"2.17"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PT1","H/工字钢","HM148*100*6*9",4,{"v":1300,"d":"1300.00"},148,100,6,9,{"v":3.5256,"d":"3.53"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PT1","H/工字钢","HM148*100*6*9",5,{"v":12950,"d":"12950.00"},148,100,6,9,{"v":43.9005,"d":"43.90"},"无重合面",null,156,null,28.49,"总图内所有管架、410NC34101-8","一般性腐蚀","环氧富锌漆",{"v":0.393559928443649,"d":"39%"}]
["硫回收钢结构PT1","L型钢","L50*5",16,{"v":1450,"d":"1450.00"},50,50,5,5,4.64,"无重合面",null,156,null,null,"总图内所有管架、410NC34101-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PT3*3","H/工字钢","HM148*100*6*9",6,{"v":3000,"d":"3000.00"},148,100,6,9,{"v":12.204,"d":"12.20"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PT3*3","H/工字钢","HM148*100*6*9",12,{"v":1800,"d":"1800.00"},148,100,6,9,{"v":14.6448,"d":"14.64"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PT3*3","H/工字钢","HM148*100*6*9",6,{"v":2250,"d":"2250.00"},148,100,6,9,{"v":9.153,"d":"9.15"},"无重合面",null,156,null,21.87,"总图内所有管架、410NC34101-9","一般性腐蚀","环氧富锌漆",{"v":0.704960835509138,"d":"70%"}]
["硫回收钢结构PT2*3","H/工字钢","HM125*125*6.5*9",12,{"v":5100,"d":"5100.00"},125,125,6.5,9,{"v":44.7984,"d":"44.80"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PT2*3","H/工字钢","HM125*125*6.5*9",18,{"v":2000,"d":"2000.00"},125,125,6.5,9,{"v":26.352,"d":"26.35"},"无重合面",null,156,null,null,"总图内所有管架、410NC34101-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收钢结构PT2*3","H/工字钢","HM125*125*6.5*9",21,{"v":1700,"d":"1700.00"},125,125,6.5,9,{"v":26.1324,"d":"26.13"},"无重合面",null,156,null,{"v":17.625,"d":"17.63"},"总图内所有管架、410NC34101-9","一般性腐蚀","环氧富锌漆",{"v":0.402789013972494,"d":"40%"}]
["精脱硫一系K101-108","[槽钢","[16b（160*63*6.5）",4,{"v":5500,"d":"5500.00"},160,63,6.5,6.5,{"v":12.298,"d":"12.30"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","H/工字钢","HM244*175*7*11",16,{"v":5900,"d":"5900.00"},244,175,7,11,{"v":110.0704,"d":"110.07"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","H/工字钢","HM244*175*7*11",4,{"v":5500,"d":"5500.00"},244,175,7,11,{"v":25.652,"d":"25.65"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","H/工字钢","HM294*200*8*12",8,{"v":2600,"d":"2600.00"},294,200,8,12,{"v":28.3712,"d":"28.37"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","H/工字钢","HM294*200*8*12",2,{"v":1300,"d":"1300.00"},294,200,8,12,{"v":3.5464,"d":"3.55"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","H/工字钢","HM294*200*8*12",9,{"v":3000,"d":"3000.00"},294,200,8,12,{"v":36.828,"d":"36.83"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","H/工字钢","HN200*100*5.5*8",4,{"v":4500,"d":"4500.00"},200,100,5.5,8,{"v":14.112,"d":"14.11"},"无重合面",null,156,null,{"v":60.5,"d":"60.50"},"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0.810861523615504,"d":"81%"}]
["精脱硫一系K101-108","H/工字钢","HN250*250*9*14",6,{"v":4000,"d":"4000.00"},250,250,9,14,{"v":35.328,"d":"35.33"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","H/工字钢","HN300*150*6.5*9",1,{"v":36400,"d":"36400.00"},300,150,6.5,9,{"v":43.0248,"d":"43.02"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","H/工字钢","HN350*175*7*11",1,{"v":36400,"d":"36400.00"},350,175,7,11,{"v":50.1592,"d":"50.16"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","H/工字钢","HN350*175*7*11",14,{"v":4600,"d":"4600.00"},350,175,7,11,{"v":88.7432,"d":"88.74"},"无重合面",null,156,null,351.44,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0.798394850144213,"d":"80%"}]
["精脱硫一系K101-108","H/工字钢","HN350*175*7*11",2,{"v":7000,"d":"7000.00"},350,175,7,11,{"v":19.292,"d":"19.29"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","H/工字钢","HW150*150*7*10",14,{"v":3300,"d":"3300.00"},150,150,7,10,{"v":40.656,"d":"40.66"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","H/工字钢","HW200*200*8*12",8,{"v":2600,"d":"2600.00"},200,200,8,12,{"v":24.4608,"d":"24.46"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","H/工字钢","HW200*200*8*12",2,{"v":1000,"d":"1000.00"},200,200,8,12,{"v":2.352,"d":"2.35"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","L型钢","L100*6",4,{"v":2800,"d":"2800.00"},100,100,6,6,4.48,"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","L型钢","L100*6",2,{"v":3600,"d":"3600.00"},100,100,6,6,2.88,"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","L型钢","L75*6",8,{"v":4300,"d":"4300.00"},75,75,6,6,10.32,"无重合面",null,156,null,{"v":22.8,"d":"22.80"},"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0.688405797101449,"d":"69%"}]
["精脱硫一系K101-108","L型钢","L75*6",2,{"v":5000,"d":"5000.00"},75,75,6,6,{"v":3,"d":"3.00"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","L型钢","L75*6",2,{"v":3800,"d":"3800.00"},75,75,6,6,2.28,"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","L型钢","L75*6",2,{"v":4100,"d":"4100.00"},75,75,6,6,2.46,"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","圆钢","Q102*6",14,{"v":4300,"d":"4300.00"},102,{"$nulls":3},{"v":19.280856,"d":"19.28"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","圆钢","Q140*6",7,{"v":4300,"d":"4300.00"},140,{"$nulls":3},{"v":13.23196,"d":"13.23"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系K101-108","圆钢","Q140*6",7,{"v":3400,"d":"3400.00"},140,{"$nulls":3},{"v":10.46248,"d":"10.46"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","[槽钢","[16b（160*63*6.5）",4,{"v":5500,"d":"5500.00"},160,63,6.5,6.5,{"v":12.298,"d":"12.30"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","H/工字钢","HM244*175*7*11",16,{"v":5900,"d":"5900.00"},244,175,7,11,{"v":110.0704,"d":"110.07"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","H/工字钢","HM244*175*7*11",4,{"v":5500,"d":"5500.00"},244,175,7,11,{"v":25.652,"d":"25.65"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","H/工字钢","HM294*200*8*12",8,{"v":2600,"d":"2600.00"},294,200,8,12,{"v":28.3712,"d":"28.37"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","H/工字钢","HM294*200*8*12",2,{"v":1300,"d":"1300.00"},294,200,8,12,{"v":3.5464,"d":"3.55"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","H/工字钢","HM294*200*8*12",9,{"v":3000,"d":"3000.00"},294,200,8,12,{"v":36.828,"d":"36.83"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","H/工字钢","HN200*100*5.5*8",4,{"v":4500,"d":"4500.00"},200,100,5.5,8,{"v":14.112,"d":"14.11"},"无重合面",null,156,null,{"v":60.5,"d":"60.50"},"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0.810861523615504,"d":"81%"}]
["精脱硫二系K201-208","H/工字钢","HN250*250*9*14",6,{"v":4000,"d":"4000.00"},250,250,9,14,{"v":35.328,"d":"35.33"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","H/工字钢","HN300*150*6.5*9",1,{"v":36400,"d":"36400.00"},300,150,6.5,9,{"v":43.0248,"d":"43.02"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","H/工字钢","HN350*175*7*11",1,{"v":36400,"d":"36400.00"},350,175,7,11,{"v":50.1592,"d":"50.16"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","H/工字钢","HN350*175*7*11",14,{"v":4600,"d":"4600.00"},350,175,7,11,{"v":88.7432,"d":"88.74"},"无重合面",null,156,null,351.44,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0.798394850144213,"d":"80%"}]
["精脱硫二系K201-208","H/工字钢","HN350*175*7*11",2,{"v":7000,"d":"7000.00"},350,175,7,11,{"v":19.292,"d":"19.29"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","H/工字钢","HW150*150*7*10",14,{"v":3300,"d":"3300.00"},150,150,7,10,{"v":40.656,"d":"40.66"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","H/工字钢","HW200*200*8*12",8,{"v":2600,"d":"2600.00"},200,200,8,12,{"v":24.4608,"d":"24.46"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","H/工字钢","HW200*200*8*12",2,{"v":1000,"d":"1000.00"},200,200,8,12,{"v":2.352,"d":"2.35"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","L型钢","L100*6",4,{"v":2800,"d":"2800.00"},100,100,6,6,4.48,"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","L型钢","L100*6",2,{"v":3600,"d":"3600.00"},100,100,6,6,2.88,"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","L型钢","L75*6",8,{"v":4300,"d":"4300.00"},75,75,6,6,10.32,"无重合面",null,156,null,{"v":22.8,"d":"22.80"},"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0.688405797101449,"d":"69%"}]
["精脱硫二系K201-208","L型钢","L75*6",2,{"v":5000,"d":"5000.00"},75,75,6,6,{"v":3,"d":"3.00"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","L型钢","L75*6",2,{"v":3800,"d":"3800.00"},75,75,6,6,2.28,"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","L型钢","L75*6",2,{"v":4100,"d":"4100.00"},75,75,6,6,2.46,"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","圆钢","Q102*6",14,{"v":4300,"d":"4300.00"},102,{"$nulls":3},{"v":19.280856,"d":"19.28"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","圆钢","Q140*6",7,{"v":4300,"d":"4300.00"},140,{"$nulls":3},{"v":13.23196,"d":"13.23"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系K201-208","圆钢","Q140*6",7,{"v":3400,"d":"3400.00"},140,{"$nulls":3},{"v":10.46248,"d":"10.46"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0003\\4\\5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫管架   ZJ-1平面","H/工字钢","H250*250*10*16",4,{"v":2800,"d":"2800.00"},250,250,10,16,{"v":16.4416,"d":"16.44"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0007","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫管架   ZJ-1平面","H/工字钢","HM194*150*6*9",26,{"v":4500,"d":"4500.00"},194,150,6,9,113.49,"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0007","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫管架   ZJ-1平面","H/工字钢","HM224*175*7*11",16,{"v":11000,"d":"11000.00"},224,175,7,11,{"v":198.176,"d":"198.18"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0007","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫管架   ZJ-1平面","H/工字钢","HM224*175*7*11",4,{"v":5700,"d":"5700.00"},224,175,7,11,{"v":25.6728,"d":"25.67"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0007","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫管架   ZJ-1平面","H/工字钢","HM340*250*9*14",8,{"v":4500,"d":"4500.00"},340,250,9,14,{"v":59.472,"d":"59.47"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0007","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫管架   ZJ-1平面","H/工字钢","HW200*200*8*12",8,{"v":4500,"d":"4500.00"},200,200,8,12,{"v":42.336,"d":"42.34"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0007","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫管架   ZJ-1平面","H/工字钢","HW200*200*8*12",4,{"v":2800,"d":"2800.00"},200,200,8,12,{"v":13.1712,"d":"13.17"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0007","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫管架   ZJ-1平面","圆钢","Q102*6",20,{"v":7300,"d":"7300.00"},102,{"$nulls":3},{"v":46.76088000000001,"d":"46.76"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0007","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫管架   8.5平面","[槽钢","[5（50*37*4.5）",1,{"v":25300,"d":"25300.00"},160,63,6.5,6.5,{"v":14.1427,"d":"14.14"},"无重合面",null,156,null,27.67,"总图内所有管架、410NC34105-0007","一般性腐蚀","环氧富锌漆",{"v":0.661760661234505,"d":"66%"}]
["精脱硫管架   8.5平面","H/工字钢","HM194*150*6*9",10,{"v":4500,"d":"4500.00"},194,150,6,9,43.65,"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0007","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫管架   8.5平面","H/工字钢","HN200*100*5.5*8",2,{"v":4000,"d":"4000.00"},200,100,5.5,8,{"v":6.272,"d":"6.27"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0007","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫管架   8.5平面","H/工字钢","HN300*150*6.5*10",2,{"v":8500,"d":"8500.00"},300,150,6.5,10,20.06,"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0007","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫管架   8.5平面","H/工字钢","HN300*150*6.5*10",2,{"v":10500,"d":"10500.00"},300,150,6.5,10,24.78,"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0007","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫管架   8.5平面","H/工字钢","HN400*200*8*13",2,{"v":11300,"d":"11300.00"},400,200,8,13,{"v":35.5724,"d":"35.57"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0007","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫管架   8.5平面","H/工字钢","HN400*200*8*13",2,{"v":12000,"d":"12000.00"},400,200,8,13,{"v":37.776,"d":"37.78"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0007","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫管架   8.5平面","H/工字钢","HN600*200*11*17",2,{"v":15000,"d":"15000.00"},600,200,11,17,58.98,"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0007","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫管架   8.5平面","H/工字钢","HW200*200*8*12",8,{"v":4500,"d":"4500.00"},200,200,8,12,{"v":42.336,"d":"42.34"},"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0007","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫管架   8.5平面","L型钢","L75*6",32,{"v":5900,"d":"5900.00"},75,75,6,6,56.64,"无重合面",null,156,null,null,"总图内所有管架、410NC34105-0007","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8   2-2面","H/工字钢","HM194*150*6*9",6,{"v":5600,"d":"5600.00"},194,150,6,9,{"v":32.592,"d":"32.59"},"无重合面",null,156,null,null,"总图内所有管架、","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8   2-2面","H/工字钢","HW200*200*8*12",4,{"v":5600,"d":"5600.00"},200,200,8,12,{"v":26.3424,"d":"26.34"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8   2-2面","2L型钢","2L80*6",4,{"v":4800,"d":"4800.00"},160,80,6,0,{"v":9.216,"d":"9.22"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8   2-2面","2L型钢","2L80*6",4,{"v":2100,"d":"2100.00"},160,80,6,0,{"v":4.032,"d":"4.03"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8   1-1面","H/工字钢","HM194*150*6*9",10,{"v":5600,"d":"5600.00"},194,150,6,9,54.32,"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8   1-1面","2L型钢","2L80*6",4,{"v":4800,"d":"4800.00"},160,80,6,0,{"v":9.216,"d":"9.22"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8   3-3面","L型钢","L80*6",14,{"v":4800,"d":"4800.00"},80,80,6,6,{"v":21.504,"d":"21.50"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17    5-5面","L型钢","L80*6",8,{"v":4200,"d":"4200.00"},80,80,6,6,{"v":10.752,"d":"10.75"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17    5-5面","2L型钢","2L80*6",2,{"v":3000,"d":"3000.00"},160,80,6,0,2.88,"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17    5-5面","2L型钢","2L80*6",2,{"v":3200,"d":"3200.00"},160,80,6,0,{"v":3.072,"d":"3.07"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  4-4面","2L型钢","2L90*6",8,{"v":4100,"d":"4100.00"},180,90,6,0,{"v":17.712,"d":"17.71"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  4-4面","2L型钢","2L90*6",2,{"v":3000,"d":"3000.00"},180,90,6,0,3.24,"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17   6-6面","2L型钢","2L90*6",8,{"v":4100,"d":"4100.00"},180,90,6,0,{"v":17.712,"d":"17.71"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17   6-6面","2L型钢","2L90*6",2,{"v":3000,"d":"3000.00"},180,90,6,0,3.24,"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  7-7面","L型钢","L80*6",32,{"v":4200,"d":"4200.00"},80,80,6,6,{"v":43.008,"d":"43.01"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  7-7面","2L型钢","2L80*6",8,{"v":3000,"d":"3000.00"},160,80,6,0,11.52,"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17立柱","H/工字钢","HM194*150*6*9",16,{"v":7500,"d":"7500.00"},194,150,6,9,{"v":116.4,"d":"116.40"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17立柱","H/工字钢","HW200*200*8*12",8,{"v":7500,"d":"7500.00"},200,200,8,12,70.56,"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSDZJ1","H/工字钢","HM194*150*6*9",2,{"v":5900,"d":"5900.00"},194,150,6,9,{"v":11.446,"d":"11.45"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSDZJ1","L型钢","L80*6",4,{"v":4200,"d":"4200.00"},80,80,6,6,{"v":5.376,"d":"5.38"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSDZJ1","2L型钢","2L80*6",1,{"v":3000,"d":"3000.00"},160,80,6,0,1.44,"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8  +5.9M","圆钢","Q20圆钢",30,{"v":5000,"d":"5000.00"},20,{"$nulls":3},9.42,"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8  +5.9M","圆钢","Q20圆钢",8,{"v":4250,"d":"4250.00"},20,{"$nulls":3},{"v":2.1352,"d":"2.14"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8  +5.9M","圆钢","Q20圆钢",2,{"v":3900,"d":"3900.00"},20,{"$nulls":3},{"v":0.48984000000000005,"d":"0.49"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8  +5.9M","圆钢","Q20圆钢",4,{"v":4700,"d":"4700.00"},20,{"$nulls":3},{"v":1.18064,"d":"1.18"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8  +5.9M","H/工字钢","HN300*150*6.5*9",2,{"v":12000,"d":"12000.00"},300,150,6.5,9,{"v":28.368,"d":"28.37"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8  +5.9M","H/工字钢","HN300*150*6.5*9",2,{"v":58000,"d":"58000.00"},300,150,6.5,9,{"v":137.112,"d":"137.11"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8  +5.9M","H/工字钢","HN250*125*6*9",2,{"v":6150,"d":"6150.00"},250,125,6,9,{"v":12.0786,"d":"12.08"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8  +5.9M","H/工字钢","HM194*150*6*9",27,{"v":3000,"d":"3000.00"},194,150,6,9,78.57,"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +5.9M","圆钢","Q20圆钢",4,{"v":3500,"d":"3500.00"},20,{"$nulls":3},{"v":0.8792000000000001,"d":"0.88"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +5.9M","圆钢","Q20圆钢",38,{"v":5000,"d":"5000.00"},20,{"$nulls":3},{"v":11.932,"d":"11.93"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +5.9M","圆钢","Q20圆钢",12,{"v":4750,"d":"4750.00"},20,{"$nulls":3},{"v":3.5796000000000006,"d":"3.58"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +5.9M","H/工字钢","HN350*175*7*11",2,{"v":14400,"d":"14400.00"},350,175,7,11,{"v":39.6864,"d":"39.69"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +5.9M","H/工字钢","HN350*175*7*11",2,{"v":12000,"d":"12000.00"},350,175,7,11,{"v":33.072,"d":"33.07"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +5.9M","H/工字钢","HN300*150*6.5*9",2,{"v":5000,"d":"5000.00"},300,150,6.5,9,11.82,"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +5.9M","H/工字钢","HN300*150*6.5*9",2,{"v":8000,"d":"8000.00"},300,150,6.5,9,{"v":18.912,"d":"18.91"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +5.9M","H/工字钢","HN300*150*6.5*9",6,{"v":12000,"d":"12000.00"},300,150,6.5,9,{"v":85.104,"d":"85.10"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +5.9M","H/工字钢","HN250*125*6*9",2,{"v":8000,"d":"8000.00"},250,125,6,9,{"v":15.712,"d":"15.71"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +5.9M","H/工字钢","HN250*125*6*9",2,{"v":12000,"d":"12000.00"},250,125,6,9,{"v":23.568,"d":"23.57"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +5.9M","H/工字钢","HM194*150*6*9",3,{"v":28000,"d":"28000.00"},194,150,6,9,81.48,"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8  +7.5M","圆钢","Q20圆钢",30,{"v":4500,"d":"4500.00"},20,{"$nulls":3},{"v":8.478,"d":"8.48"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8  +7.5M","圆钢","Q20圆钢",8,{"v":3700,"d":"3700.00"},20,{"$nulls":3},{"v":1.8588800000000003,"d":"1.86"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8  +7.5M","圆钢","Q20圆钢",4,{"v":4100,"d":"4100.00"},20,{"$nulls":3},{"v":1.0299200000000002,"d":"1.03"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8  +7.5M","H/工字钢","HN300*150*6.5*9",2,{"v":12000,"d":"12000.00"},300,150,6.5,9,{"v":28.368,"d":"28.37"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8  +7.5M","H/工字钢","HN300*150*6.5*9",2,{"v":58000,"d":"58000.00"},300,150,6.5,9,{"v":137.112,"d":"137.11"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8  +7.5M","H/工字钢","HN250*125*6*9",2,{"v":6150,"d":"6150.00"},250,125,6,9,{"v":12.0786,"d":"12.08"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8  +7.5M","H/工字钢","HM194*150*6*9",27,{"v":3000,"d":"3000.00"},194,150,6,9,78.57,"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ1-8  +7.5M","[槽钢","[126*53*5.5",1,{"v":84600,"d":"84600.00"},126,53,5.5,5.5,{"v":27.6642,"d":"27.66"},"腹板重合",null,156,null,118.44,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0.810654313839027,"d":"81%"}]
["水处理管架FSZJ8-17  +7.5M","圆钢","Q20圆钢",4,{"v":3200,"d":"3200.00"},20,{"$nulls":3},{"v":0.80384,"d":"0.80"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +7.5M","圆钢","Q20圆钢",38,{"v":4500,"d":"4500.00"},20,{"$nulls":3},{"v":10.7388,"d":"10.74"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +7.5M","圆钢","Q20圆钢",12,{"v":4100,"d":"4100.00"},20,{"$nulls":3},{"v":3.08976,"d":"3.09"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +7.5M","H/工字钢","HN350*175*7*11",2,{"v":14400,"d":"14400.00"},350,175,7,11,{"v":39.6864,"d":"39.69"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +7.5M","H/工字钢","HN350*175*7*11",2,{"v":12000,"d":"12000.00"},350,175,7,11,{"v":33.072,"d":"33.07"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +7.5M","H/工字钢","HN300*150*6.5*9",2,{"v":5000,"d":"5000.00"},300,150,6.5,9,11.82,"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +7.5M","H/工字钢","HN300*150*6.5*9",2,{"v":8000,"d":"8000.00"},300,150,6.5,9,{"v":18.912,"d":"18.91"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +7.5M","H/工字钢","HN300*150*6.5*9",6,{"v":12000,"d":"12000.00"},300,150,6.5,9,{"v":85.104,"d":"85.10"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +7.5M","H/工字钢","HN250*125*6*9",2,{"v":8000,"d":"8000.00"},250,125,6,9,{"v":15.712,"d":"15.71"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +7.5M","H/工字钢","HN250*125*6*9",2,{"v":12000,"d":"12000.00"},250,125,6,9,{"v":23.568,"d":"23.57"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +7.5M","H/工字钢","HM194*150*6*9",3,{"v":28000,"d":"28000.00"},194,150,6,9,81.48,"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架FSZJ8-17  +7.5M","[槽钢","[12.6*53*5.5",1,{"v":106000,"d":"106000.00"},126,53,5.5,5.5,{"v":34.662,"d":"34.66"},"腹板重合",null,156,null,{"v":148.4,"d":"148.40"},"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0.810654313839027,"d":"81%"}]
["水处理管架FSZJ1-8  +5.5M  ZD1","[槽钢","[12.6*53*5.5",2,{"v":3100,"d":"3100.00"},126,53,5.5,5.5,{"v":2.0274,"d":"2.03"},"腹板重合",null,156,null,4.34,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0.68159688412853,"d":"68%"}]
["水处理管架FSZJ8-17  +7.5M  ST1","[槽钢","[12.6*53*5.5",2,{"v":3000,"d":"3000.00"},126,53,5.5,5.5,{"v":1.962,"d":"1.96"},"腹板重合",null,156,null,{"v":4.2,"d":"4.20"},"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0.68159688412853,"d":"68%"}]
["水处理管架FSZJ8-17  +7.5M  ST2","[槽钢","[12.6*53*5.5",2,{"v":4500,"d":"4500.00"},126,53,5.5,5.5,{"v":2.943,"d":"2.94"},"腹板重合",null,156,null,{"v":6.3,"d":"6.30"},"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0.68159688412853,"d":"68%"}]
["水处理管架FSZJ8-17  +7.5M  ST3","[槽钢","[12.6*53*5.5",2,{"v":3400,"d":"3400.00"},126,53,5.5,5.5,{"v":2.2236,"d":"2.22"},"腹板重合",null,156,null,4.76,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0.68159688412853,"d":"68%"}]
["水处理重力除油池护栏支撑杆","圆钢","圆钢Q48*3",2,{"v":116000,"d":"116000.00"},48,{"$nulls":3},{"v":34.96704,"d":"34.97"},"无重合面",null,156,null,null,"总图内所有管架、FG110204-SS-JG06.05-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理重力除油池护栏扁铁","方（扁）钢","扁铁50*4",2,{"v":116000,"d":"116000.00"},50,4,null,null,{"v":25.056,"d":"25.06"},"无重合面",null,156,null,null,"总图内所有管架、总平面图","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理重力除油池护栏踢腿板","方（扁）钢","踢腿板100*4",1,{"v":116000,"d":"116000.00"},100,4,null,null,{"v":24.128,"d":"24.13"},"无重合面",null,156,null,null,"总图内所有管架、总平面图","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理事故池调节池护栏支撑杆","圆钢","圆钢Q48*3",2,{"v":170000,"d":"170000.00"},48,{"$nulls":3},{"v":51.2448,"d":"51.24"},"无重合面",null,156,null,null,"总图内所有管架、总平面图","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理事故池调节池护栏扁铁","方（扁）钢","扁铁50*4",2,{"v":170000,"d":"170000.00"},50,4,null,null,36.72,"无重合面",null,156,null,null,"总图内所有管架、总平面图","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理事故池调节池护栏踢腿板","方（扁）钢","踢腿板100*4",1,{"v":170000,"d":"170000.00"},100,4,null,null,35.36,"无重合面",null,156,null,null,"总图内所有管架、总平面图","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理一级生化护栏支撑杆","圆钢","圆钢Q48*3",2,{"v":586000,"d":"586000.00"},48,{"$nulls":3},{"v":176.64384,"d":"176.64"},"无重合面",null,156,null,null,"总图内所有管架、总平面图","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理一级生化护栏扁铁","方（扁）钢","扁铁50*4",2,{"v":586000,"d":"586000.00"},50,4,null,null,{"v":126.576,"d":"126.58"},"无重合面",null,156,null,null,"总图内所有管架、总平面图","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理一级生化护栏踢腿板","方（扁）钢","踢腿板100*4",1,{"v":586000,"d":"586000.00"},100,4,null,null,{"v":121.888,"d":"121.89"},"无重合面",null,156,null,null,"总图内所有管架、总平面图","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理一级生化过道",null,null,2,{"v":18000,"d":"18000.00"},{"$nulls":4},"",null,null,156,null,{"v":36,"d":"36.00"},"总图内所有管架、总平面图","一般性腐蚀","环氧富锌漆",""]
["水处理二级生化护栏支撑杆","圆钢","圆钢Q48*3",2,{"v":725000,"d":"725000.00"},48,{"$nulls":3},{"v":218.544,"d":"218.54"},"无重合面",null,156,null,null,"总图内所有管架、总平面图","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理二级生化护栏扁铁","方（扁）钢","扁铁50*4",2,{"v":725000,"d":"725000.00"},50,4,null,null,{"v":156.6,"d":"156.60"},"无重合面",null,156,null,null,"总图内所有管架、总平面图","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理二级生化护栏踢腿板","方（扁）钢","踢腿板100*4",1,{"v":725000,"d":"725000.00"},100,4,null,null,{"v":150.8,"d":"150.80"},"无重合面",null,156,null,null,"总图内所有管架、总平面图","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理二级生化过道",null,null,2,{"v":43000,"d":"43000.00"},{"$nulls":4},"",null,null,156,null,{"v":86,"d":"86.00"},"总图内所有管架、总平面图","一般性腐蚀","环氧富锌漆",""]
["水处理管架过道护栏支撑杆","圆钢","圆钢Q48*3",2,{"v":190000,"d":"190000.00"},48,{"$nulls":3},{"v":57.2736,"d":"57.27"},"无重合面",null,156,null,null,"总图内所有管架、总平面图","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架过道护栏扁铁","方（扁）钢","扁铁50*4",2,{"v":190000,"d":"190000.00"},50,4,null,null,41.04,"无重合面",null,156,null,null,"总图内所有管架、总平面图","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["水处理管架过道护栏踢腿板","方（扁）钢","踢腿板100*4",1,{"v":190000,"d":"190000.00"},100,4,null,null,39.52,"无重合面",null,156,null,null,"总图内所有管架、总平面图","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台悬臂一","[槽钢","[126*53*5.5",1,900,{"v":126,"d":"126.00"},{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.4077,"d":"0.41"},"无重合面",null,156,null,null,"34NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台三脚架七","[槽钢","[148*48*5",1,1300,148,48,5,5,{"v":0.6214,"d":"0.62"},"无重合面",null,156,null,null,"34NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台三脚架七","[槽钢","[126*53*5.5",1,1500,{"v":126,"d":"126.00"},{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.6795,"d":"0.68"},"无重合面",null,156,null,null,"34NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台悬臂三","[槽钢","[126*53*5.5",81,930,{"v":126,"d":"126.00"},{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":34.12449,"d":"34.12"},"无重合面",null,156,null,null,"34NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台平台一+5.5m","[槽钢","[100*48*5.3",1,18200,100,48,5.3,5.3,{"v":6.06788,"d":"6.07"},"翼板重合",null,156,null,{"v":16.1264,"d":"16.13"},"34NM057-2","一般性腐蚀","环氧富锌漆",{"v":0.726601628888164,"d":"73%"}]
["精脱硫一系吸附塔联合操作台平台一+5.5m","方（扁）钢","加强筋40*4",10,1000,"40",4,null,null,0.88,"无重合面",null,156,null,null,"34NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台平台二+5.5m","[槽钢","[100*48*5.3",2,26000,100,48,5.3,5.3,{"v":17.3368,"d":"17.34"},"翼板重合",null,156,null,{"v":22.352,"d":"22.35"},"34NM057-3","一般性腐蚀","环氧富锌漆",{"v":0.563181552478281,"d":"56%"}]
["精脱硫一系吸附塔联合操作台平台二+5.5m","方（扁）钢","加强筋40*4",28,1000,"40",4,null,null,{"v":2.464,"d":"2.46"},"无重合面",null,156,null,null,"34NM057-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台平台三+5.5m","[槽钢","[100*48*5.3",1,21800,100,48,5.3,5.3,{"v":7.268119999999999,"d":"7.27"},"翼板重合",null,156,null,{"v":18.0096,"d":"18.01"},"34NM057-3","一般性腐蚀","环氧富锌漆",{"v":0.712469320808997,"d":"71%"}]
["精脱硫一系吸附塔联合操作台平台三+5.5m","方（扁）钢","加强筋40*4",11,1000,"40",4,null,null,{"v":0.968,"d":"0.97"},"无重合面",null,156,null,null,"34NM057-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台平台五+11.6m","[槽钢","[100*48*5.3",2,33500,100,48,5.3,5.3,{"v":22.3378,"d":"22.34"},"翼板重合",null,156,null,{"v":29.392,"d":"29.39"},"34NM057-3","一般性腐蚀","环氧富锌漆",{"v":0.568183136219355,"d":"57%"}]
["精脱硫一系吸附塔联合操作台平台五+11.6m","方（扁）钢","加强筋40*4",38,1000,"40",4,null,null,{"v":3.344,"d":"3.34"},"无重合面",null,156,null,null,"34NM057-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台平台四+5.5m","[槽钢","[100*48*5.3",1,29000,100,48,5.3,5.3,{"v":9.6686,"d":"9.67"},"翼板重合",null,156,null,{"v":23.208,"d":"23.21"},"34NM057-4","一般性腐蚀","环氧富锌漆",{"v":0.705912411867407,"d":"71%"}]
["精脱硫一系吸附塔联合操作台平台四+5.5m","方（扁）钢","加强筋40*4",26,1000,"40",4,null,null,{"v":2.288,"d":"2.29"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台三脚架一","[槽钢","[100*48*5.3",1,3200,100,48,5.3,5.3,{"v":1.22048,"d":"1.22"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台三脚架一","[槽钢","[126*53*5.5",1,2590,{"v":126,"d":"126.00"},{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.17327,"d":"1.17"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台三脚架二","[槽钢","[100*48*5.3",1,3200,100,48,5.3,5.3,{"v":1.22048,"d":"1.22"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台三脚架二","[槽钢","[126*53*5.5",1,2290,{"v":126,"d":"126.00"},{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.03737,"d":"1.04"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台盘梯6.6m","方（扁）钢","外侧板160*8",2,10800,"160",8,null,null,{"v":7.2576,"d":"7.26"},"无重合面",null,156,null,null,"34NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台盘梯6.6m","方（扁）钢","内侧板160*8",2,9330,"160",8,null,null,{"v":6.26976,"d":"6.27"},"无重合面",null,156,null,null,"34NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台盘梯6.6m","L型钢","L63*63*6",6,2000,63,63,6,6,{"v":3.024,"d":"3.02"},"无重合面",null,156,null,null,"34NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台盘梯6.6m","方（扁）钢","踏板",76,800,380,{"$nulls":3},{"v":46.208,"d":"46.21"},"无重合面",null,156,null,null,"34NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台平台六+11.6m","[槽钢","[100*48*5.3",2,21500,100,48,5.3,5.3,{"v":14.336199999999998,"d":"14.34"},"翼板重合",null,156,null,{"v":34.336,"d":"34.34"},"34NM057-6","一般性腐蚀","环氧富锌漆",{"v":0.705454037417663,"d":"71%"}]
["精脱硫一系吸附塔联合操作台平台六+11.6m","方（扁）钢","加强筋40*4",22,1000,"40",4,null,null,{"v":1.936,"d":"1.94"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台平台七+11.6m","[槽钢","[100*48*5.3",1,21500,100,48,5.3,5.3,{"v":7.168099999999999,"d":"7.17"},"翼板重合",null,156,null,{"v":17.168,"d":"17.17"},"34NM057-6","一般性腐蚀","环氧富锌漆",{"v":0.705454037417663,"d":"71%"}]
["精脱硫一系吸附塔联合操作台平台七+11.6m","方（扁）钢","加强筋40*4",11,1000,"40",4,null,null,{"v":0.968,"d":"0.97"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台平台八+21.5m","[槽钢","[100*48*5.3",2,12200,100,48,5.3,5.3,{"v":8.13496,"d":"8.13"},"翼板重合",null,156,null,{"v":22.4288,"d":"22.43"},"34NM057-6","一般性腐蚀","环氧富锌漆",{"v":0.733836412797378,"d":"73%"}]
["精脱硫一系吸附塔联合操作台平台八+21.5m","方（扁）钢","加强筋40*4",10,1000,"40",4,null,null,0.88,"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台三脚架三+21.5m","[槽钢","[100*48*5.3",17,1200,100,48,5.3,5.3,{"v":7.78056,"d":"7.78"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台盘梯9.9m","方（扁）钢","外侧板160*8",2,16200,"160",8,null,null,{"v":10.8864,"d":"10.89"},"无重合面",null,156,null,null,"34NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台盘梯9.9m","方（扁）钢","内侧板160*8",2,14000,"160",8,null,null,{"v":9.408,"d":"9.41"},"无重合面",null,156,null,null,"34NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台盘梯9.9m","L型钢","L63*63*6",8,2000,63,63,6,6,{"v":4.032,"d":"4.03"},"无重合面",null,156,null,null,"34NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台盘梯9.9m","方（扁）钢","踏板",90,800,380,{"$nulls":3},54.72,"无重合面",null,156,null,null,"34NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台三脚架四+21.5m","[槽钢","[100*48*5.3",4,4500,100,48,5.3,5.3,{"v":6.8652,"d":"6.87"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台三脚架五+21.5m","[槽钢","[100*48*5.3",4,4300,100,48,5.3,5.3,{"v":6.56008,"d":"6.56"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台三脚架六+21.5m","[槽钢","[100*48*5.3",8,4350,100,48,5.3,5.3,{"v":13.27272,"d":"13.27"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台平台九+21.5m","[槽钢","[100*48*5.3",2,20000,100,48,5.3,5.3,{"v":13.336,"d":"13.34"},"翼板重合",null,156,null,28.08,"34NM057-8","一般性腐蚀","环氧富锌漆",{"v":0.677998841027622,"d":"68%"}]
["精脱硫一系吸附塔联合操作台平台九+21.5m","方（扁）钢","加强筋40*4",14,1000,"40",4,null,null,{"v":1.232,"d":"1.23"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台管道支架一","[槽钢","[80*43*5",5,900,80,43,5,5,{"v":1.449,"d":"1.45"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台管道支架二","[槽钢","[80*43*5",5,900,80,43,5,5,{"v":1.449,"d":"1.45"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台平台十+21.5m","[槽钢","[100*48*5.3",1,20200,100,48,5.3,5.3,{"v":6.73468,"d":"6.73"},"翼板重合",null,156,null,{"v":14.2304,"d":"14.23"},"34NM057-9","一般性腐蚀","环氧富锌漆",{"v":0.678766787438922,"d":"68%"}]
["精脱硫一系吸附塔联合操作台平台十+21.5m","方（扁）钢","加强筋40*4",7,1000,"40",4,null,null,{"v":0.616,"d":"0.62"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台平台十一+23.4m","方（扁）钢","花纹板4",1,1000,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":10,"d":"10.00"},"34NM057-9","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["精脱硫一系吸附塔联合操作台悬臂四","[槽钢","[126*53*5.5",6,810,{"v":126,"d":"126.00"},{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":2.20158,"d":"2.20"},"无重合面",null,156,null,null,"34NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台悬臂五","[槽钢","[126*53*5.5",4,970,{"v":126,"d":"126.00"},{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.75764,"d":"1.76"},"无重合面",null,156,null,null,"34NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台平直梯+23.4m","L型钢","L63*63*6",10,3000,63,63,6,6,7.56,"无重合面",null,156,null,null,"34NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台平直梯+23.4m","方（扁）钢","扁铁40*4",20,3200,"40",4,null,null,{"v":5.632,"d":"5.63"},"无重合面",null,156,null,null,"34NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台平直梯+23.4m","圆钢","圆钢Q18",50,500,18,{"$nulls":3},{"v":1.413,"d":"1.41"},"无重合面",null,156,null,null,"34NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台平台栏杆230m","圆钢","圆钢 Q50*3",2,230000,50,{"$nulls":3},72.22,"无重合面",null,156,null,null,"34NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台平台栏杆230m","方（扁）钢","扁铁50*4",2,230000,"50",4,null,null,49.68,"无重合面",null,156,null,null,"34NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台平台栏杆230m","方（扁）钢","踢腿板100*4",1,230000,"100",4,null,null,47.84,"无重合面",null,156,null,null,"34NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台盘梯栏杆70m","圆钢","圆钢 Q50*3",2,70000,50,{"$nulls":3},21.98,"无重合面",null,156,null,null,"34NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系吸附塔联合操作台盘梯栏杆70m","方（扁）钢","扁铁50*4",2,70000,"50",4,null,null,15.12,"无重合面",null,156,null,null,"34NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台悬臂一","[槽钢","[126*53*5.5",1,900,{"v":126,"d":"126.00"},{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.4077,"d":"0.41"},"无重合面",null,156,null,null,"34NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台三脚架七","[槽钢","[148*48*5",1,1300,148,48,5,5,{"v":0.6214,"d":"0.62"},"无重合面",null,156,null,null,"34NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台三脚架七","[槽钢","[126*53*5.5",1,1500,{"v":126,"d":"126.00"},{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.6795,"d":"0.68"},"无重合面",null,156,null,null,"34NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台悬臂三","[槽钢","[126*53*5.5",81,930,{"v":126,"d":"126.00"},{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":34.12449,"d":"34.12"},"无重合面",null,156,null,null,"34NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台平台一+5.5m","[槽钢","[100*48*5.3",1,18200,100,48,5.3,5.3,{"v":6.06788,"d":"6.07"},"翼板重合",null,156,null,{"v":16.1264,"d":"16.13"},"34NM057-2","一般性腐蚀","环氧富锌漆",{"v":0.726601628888164,"d":"73%"}]
["精脱硫二系吸附塔联合操作台平台一+5.5m","方（扁）钢","加强筋40*4",10,1000,"40",4,null,null,0.88,"无重合面",null,156,null,null,"34NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台平台二+5.5m","[槽钢","[100*48*5.3",2,26000,100,48,5.3,5.3,{"v":17.3368,"d":"17.34"},"翼板重合",null,156,null,{"v":22.352,"d":"22.35"},"34NM057-3","一般性腐蚀","环氧富锌漆",{"v":0.563181552478281,"d":"56%"}]
["精脱硫二系吸附塔联合操作台平台二+5.5m","方（扁）钢","加强筋40*4",28,1000,"40",4,null,null,{"v":2.464,"d":"2.46"},"无重合面",null,156,null,null,"34NM057-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台平台三+5.5m","[槽钢","[100*48*5.3",1,21800,100,48,5.3,5.3,{"v":7.268119999999999,"d":"7.27"},"翼板重合",null,156,null,{"v":18.0096,"d":"18.01"},"34NM057-3","一般性腐蚀","环氧富锌漆",{"v":0.712469320808997,"d":"71%"}]
["精脱硫二系吸附塔联合操作台平台三+5.5m","方（扁）钢","加强筋40*4",11,1000,"40",4,null,null,{"v":0.968,"d":"0.97"},"无重合面",null,156,null,null,"34NM057-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台平台五+11.6m","[槽钢","[100*48*5.3",2,33500,100,48,5.3,5.3,{"v":22.3378,"d":"22.34"},"翼板重合",null,156,null,{"v":29.392,"d":"29.39"},"34NM057-3","一般性腐蚀","环氧富锌漆",{"v":0.568183136219355,"d":"57%"}]
["精脱硫二系吸附塔联合操作台平台五+11.6m","方（扁）钢","加强筋40*4",38,1000,"40",4,null,null,{"v":3.344,"d":"3.34"},"无重合面",null,156,null,null,"34NM057-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台平台四+5.5m","[槽钢","[100*48*5.3",1,29000,100,48,5.3,5.3,{"v":9.6686,"d":"9.67"},"翼板重合",null,156,null,{"v":23.208,"d":"23.21"},"34NM057-4","一般性腐蚀","环氧富锌漆",{"v":0.705912411867407,"d":"71%"}]
["精脱硫二系吸附塔联合操作台平台四+5.5m","方（扁）钢","加强筋40*4",26,1000,"40",4,null,null,{"v":2.288,"d":"2.29"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台三脚架一","[槽钢","[100*48*5.3",1,3200,100,48,5.3,5.3,{"v":1.22048,"d":"1.22"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台三脚架一","[槽钢","[126*53*5.5",1,2590,{"v":126,"d":"126.00"},{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.17327,"d":"1.17"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台三脚架二","[槽钢","[100*48*5.3",1,3200,100,48,5.3,5.3,{"v":1.22048,"d":"1.22"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台三脚架二","[槽钢","[126*53*5.5",1,2290,{"v":126,"d":"126.00"},{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.03737,"d":"1.04"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台盘梯6.6m","方（扁）钢","外侧板160*8",2,10800,"160",8,null,null,{"v":7.2576,"d":"7.26"},"无重合面",null,156,null,null,"34NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台盘梯6.6m","方（扁）钢","内侧板160*8",2,9330,"160",8,null,null,{"v":6.26976,"d":"6.27"},"无重合面",null,156,null,null,"34NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台盘梯6.6m","L型钢","L63*63*6",6,2000,63,63,6,6,{"v":3.024,"d":"3.02"},"无重合面",null,156,null,null,"34NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台盘梯6.6m","方（扁）钢","踏板",76,800,380,{"$nulls":3},{"v":46.208,"d":"46.21"},"无重合面",null,156,null,null,"34NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台平台六+11.6m","[槽钢","[100*48*5.3",2,21500,100,48,5.3,5.3,{"v":14.336199999999998,"d":"14.34"},"翼板重合",null,156,null,{"v":34.336,"d":"34.34"},"34NM057-6","一般性腐蚀","环氧富锌漆",{"v":0.705454037417663,"d":"71%"}]
["精脱硫二系吸附塔联合操作台平台六+11.6m","方（扁）钢","加强筋40*4",22,1000,"40",4,null,null,{"v":1.936,"d":"1.94"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台平台七+11.6m","[槽钢","[100*48*5.3",1,21500,100,48,5.3,5.3,{"v":7.168099999999999,"d":"7.17"},"翼板重合",null,156,null,{"v":17.168,"d":"17.17"},"34NM057-6","一般性腐蚀","环氧富锌漆",{"v":0.705454037417663,"d":"71%"}]
["精脱硫二系吸附塔联合操作台平台七+11.6m","方（扁）钢","加强筋40*4",11,1000,"40",4,null,null,{"v":0.968,"d":"0.97"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台平台八+21.5m","[槽钢","[100*48*5.3",2,12200,100,48,5.3,5.3,{"v":8.13496,"d":"8.13"},"翼板重合",null,156,null,{"v":22.4288,"d":"22.43"},"34NM057-6","一般性腐蚀","环氧富锌漆",{"v":0.733836412797378,"d":"73%"}]
["精脱硫二系吸附塔联合操作台平台八+21.5m","方（扁）钢","加强筋40*4",10,1000,"40",4,null,null,0.88,"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台三脚架三+21.5m","[槽钢","[100*48*5.3",17,1200,100,48,5.3,5.3,{"v":7.78056,"d":"7.78"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台盘梯9.9m","方（扁）钢","外侧板160*8",2,16200,"160",8,null,null,{"v":10.8864,"d":"10.89"},"无重合面",null,156,null,null,"34NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台盘梯9.9m","方（扁）钢","内侧板160*8",2,14000,"160",8,null,null,{"v":9.408,"d":"9.41"},"无重合面",null,156,null,null,"34NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台盘梯9.9m","L型钢","L63*63*6",8,2000,63,63,6,6,{"v":4.032,"d":"4.03"},"无重合面",null,156,null,null,"34NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台盘梯9.9m","方（扁）钢","踏板",90,800,380,{"$nulls":3},54.72,"无重合面",null,156,null,null,"34NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台三脚架四+21.5m","[槽钢","[100*48*5.3",4,4500,100,48,5.3,5.3,{"v":6.8652,"d":"6.87"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台三脚架五+21.5m","[槽钢","[100*48*5.3",4,4300,100,48,5.3,5.3,{"v":6.56008,"d":"6.56"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台三脚架六+21.5m","[槽钢","[100*48*5.3",8,4350,100,48,5.3,5.3,{"v":13.27272,"d":"13.27"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台平台九+21.5m","[槽钢","[100*48*5.3",2,20000,100,48,5.3,5.3,{"v":13.336,"d":"13.34"},"翼板重合",null,156,null,28.08,"34NM057-8","一般性腐蚀","环氧富锌漆",{"v":0.677998841027622,"d":"68%"}]
["精脱硫二系吸附塔联合操作台平台九+21.5m","方（扁）钢","加强筋40*4",14,1000,"40",4,null,null,{"v":1.232,"d":"1.23"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台管道支架一","[槽钢","[80*43*5",5,900,80,43,5,5,{"v":1.449,"d":"1.45"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台管道支架二","[槽钢","[80*43*5",5,900,80,43,5,5,{"v":1.449,"d":"1.45"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台平台十+21.5m","[槽钢","[100*48*5.3",1,20200,100,48,5.3,5.3,{"v":6.73468,"d":"6.73"},"翼板重合",null,156,null,{"v":14.2304,"d":"14.23"},"34NM057-9","一般性腐蚀","环氧富锌漆",{"v":0.678766787438922,"d":"68%"}]
["精脱硫二系吸附塔联合操作台平台十+21.5m","方（扁）钢","加强筋40*4",7,1000,"40",4,null,null,{"v":0.616,"d":"0.62"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台平台十一+23.4m","方（扁）钢","花纹板4",1,1000,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":10,"d":"10.00"},"34NM057-9","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["精脱硫二系吸附塔联合操作台悬臂四","[槽钢","[126*53*5.5",6,810,{"v":126,"d":"126.00"},{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":2.20158,"d":"2.20"},"无重合面",null,156,null,null,"34NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台悬臂五","[槽钢","[126*53*5.5",4,970,{"v":126,"d":"126.00"},{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.75764,"d":"1.76"},"无重合面",null,156,null,null,"34NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台平直梯+23.4m","L型钢","L63*63*6",10,3000,63,63,6,6,7.56,"无重合面",null,156,null,null,"34NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台平直梯+23.4m","方（扁）钢","扁铁40*4",20,3200,"40",4,null,null,{"v":5.632,"d":"5.63"},"无重合面",null,156,null,null,"34NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台平直梯+23.4m","圆钢","圆钢Q18",50,500,18,{"$nulls":3},{"v":1.413,"d":"1.41"},"无重合面",null,156,null,null,"34NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台平台栏杆230m","圆钢","圆钢 Q50*3",2,230000,50,{"$nulls":3},72.22,"无重合面",null,156,null,null,"34NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台平台栏杆230m","方（扁）钢","扁铁50*4",2,230000,"50",4,null,null,49.68,"无重合面",null,156,null,null,"34NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台平台栏杆230m","方（扁）钢","踢腿板100*4",1,230000,"100",4,null,null,47.84,"无重合面",null,156,null,null,"34NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系吸附塔联合操作台盘梯栏杆70m","圆钢","圆钢 Q50*3",2,70000,50,{"$nulls":3},21.98,"无重合面",null,156,null,21.98,"34NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["精脱硫二系吸附塔联合操作台盘梯栏杆70m","方（扁）钢","扁铁50*4",2,70000,"50",4,null,null,15.12,"无重合面",null,156,null,null,"34NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系1V4610 2V4610操作台及爬梯栏杆4.5m","圆钢","圆钢 Q50*3",2,4500,50,{"$nulls":3},{"v":1.413,"d":"1.41"},"无重合面",null,156,null,{"v":1.413,"d":"1.41"},"34NM058-2","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["精脱硫一系1V4610 2V4610操作台及爬梯栏杆4.5m","方（扁）钢","扁铁50*4",6,4500,"50",4,null,null,{"v":2.916,"d":"2.92"},"无重合面",null,156,null,null,"34NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系1V4610 2V4610操作台及爬梯栏杆4.5m","方（扁）钢","踢腿板100*4",1,4500,"100",4,null,null,{"v":0.936,"d":"0.94"},"无重合面",null,156,null,null,"34NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系1V4610 2V4610操作台及爬梯栏杆4.5m","[槽钢","[80*43*5",4,700,80,43,5,5,{"v":0.9016,"d":"0.90"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系1V4610 2V4610操作台及爬梯栏杆4.5m","[槽钢","[100*48*5.3",4,2400,100,48,5.3,5.3,{"v":3.66144,"d":"3.66"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系1V4610 2V4610操作台及爬梯栏杆4.5m","[槽钢","[100*48*5.3",2,1500,100,48,5.3,5.3,{"v":1.0002,"d":"1.00"},"翼板重合",null,156,null,null,"34NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系1V4610 2V4610操作台及爬梯栏杆4.5m","[槽钢","[126*53*5.5",2,4800,{"v":126,"d":"126.00"},{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":4.3488,"d":"4.35"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM058-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系1V4610 2V4610操作台及爬梯栏杆4.5m","圆钢","圆钢 Q50*2.5",1,13900,50,{"$nulls":3},{"v":2.1823,"d":"2.18"},"无重合面",null,156,null,{"v":2.1823,"d":"2.18"},"34NM058-3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["精脱硫一系1V4610 2V4610操作台及爬梯栏杆4.5m","圆钢","圆钢 Q33.5",1,4050,33.5,{"$nulls":3},{"v":0.4260195,"d":"0.43"},"无重合面",null,156,null,{"v":0.63585,"d":"0.64"},"34NM058-3","一般性腐蚀","环氧富锌漆",{"v":0.598802395209581,"d":"60%"}]
["精脱硫一系1V4610 2V4610操作台及爬梯栏杆4.5m","方（扁）钢","花纹板4",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":3,"d":"3.00"},"34NM058-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["精脱硫二系1V4610 2V4610操作台及爬梯栏杆4.5m","圆钢","圆钢 Q50*3",2,4500,50,{"$nulls":3},{"v":1.413,"d":"1.41"},"无重合面",null,156,null,{"v":1.413,"d":"1.41"},"34NM058-2","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["精脱硫二系1V4610 2V4610操作台及爬梯栏杆4.5m","方（扁）钢","扁铁50*4",6,4500,50,4,null,null,{"v":2.916,"d":"2.92"},"无重合面",null,156,null,null,"34NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系1V4610 2V4610操作台及爬梯栏杆4.5m","方（扁）钢","踢腿板100*4",1,4500,100,4,null,null,{"v":0.936,"d":"0.94"},"无重合面",null,156,null,null,"34NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系1V4610 2V4610操作台及爬梯栏杆4.5m","[槽钢","[80*43*5",4,700,null,43,5,5,{"v":0.4536,"d":"0.45"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系1V4610 2V4610操作台及爬梯栏杆4.5m","[槽钢","[100*48*5.3",4,2400,null,48,5.3,5.3,{"v":1.74144,"d":"1.74"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系1V4610 2V4610操作台及爬梯栏杆4.5m","[槽钢","[100*48*5.3",2,1500,null,48,5.3,5.3,{"v":0.4002,"d":"0.40"},"翼板重合",null,156,null,null,"34NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系1V4610 2V4610操作台及爬梯栏杆4.5m","[槽钢","[126*53*5.5",2,4800,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.9296,"d":"1.93"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM058-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系1V4610 2V4610操作台及爬梯栏杆4.5m","圆钢","圆钢 Q50*2.5",1,13900,50,{"$nulls":3},{"v":2.1823,"d":"2.18"},"无重合面",null,156,null,{"v":2.1823,"d":"2.18"},"34NM058-3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["精脱硫二系1V4610 2V4610操作台及爬梯栏杆4.5m","圆钢","圆钢 Q33.5",1,4050,33.5,{"$nulls":3},{"v":0.4260195,"d":"0.43"},"无重合面",null,156,null,{"v":0.63585,"d":"0.64"},"34NM058-3","一般性腐蚀","环氧富锌漆",{"v":0.598802395209581,"d":"60%"}]
["精脱硫二系1V4610 2V4610操作台及爬梯栏杆4.5m","方（扁）钢","花纹板4",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":3,"d":"3.00"},"34NM058-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["精脱硫一系放散管操作台及爬梯","圆钢","圆钢 Q50*3",2,4000,50,{"$nulls":3},{"v":1.256,"d":"1.26"},"无重合面",null,156,null,{"v":1.256,"d":"1.26"},"34NM059-2.3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["精脱硫一系放散管操作台及爬梯","方（扁）钢","扁铁50*4",6,4000,50,4,null,null,{"v":2.592,"d":"2.59"},"无重合面",null,156,null,null,"34NM059-2.3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系放散管操作台及爬梯","方（扁）钢","踢腿板100*4",1,4000,100,4,null,null,{"v":0.832,"d":"0.83"},"无重合面",null,156,null,null,"34NM059-2.3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系放散管操作台及爬梯","[槽钢","[100*48*5.3",4,300,null,48,5.3,5.3,{"v":0.21768,"d":"0.22"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM059-2.3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系放散管操作台及爬梯","[槽钢","[100*48*5.3",2,1500,null,48,5.3,5.3,{"v":0.4002,"d":"0.40"},"翼板重合",null,156,null,null,"34NM059-2.3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系放散管操作台及爬梯","[槽钢","[126*53*5.5",2,4800,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.9296,"d":"1.93"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM059-2.3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系放散管操作台及爬梯","圆钢","圆钢 Q50*2.5",1,14200,50,{"$nulls":3},{"v":2.2294,"d":"2.23"},"无重合面",null,156,null,{"v":2.2294,"d":"2.23"},"34NM059-2.3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["精脱硫一系放散管操作台及爬梯","圆钢","圆钢 Q33.5",1,3900,33.5,{"$nulls":3},{"v":0.410241,"d":"0.41"},"无重合面",null,156,null,{"v":0.6123,"d":"0.61"},"34NM059-2.3","一般性腐蚀","环氧富锌漆",{"v":0.598802395209581,"d":"60%"}]
["精脱硫一系放散管操作台及爬梯","方（扁）钢","花纹板4",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":2.4,"d":"2.40"},"34NM059-2.3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["精脱硫二系放散管操作台及爬梯","圆钢","圆钢 Q50*3",2,4000,50,{"$nulls":3},{"v":1.256,"d":"1.26"},"无重合面",null,156,null,{"v":1.256,"d":"1.26"},"34NM059-2.3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["精脱硫二系放散管操作台及爬梯","方（扁）钢","扁铁50*4",6,4000,50,4,null,null,{"v":2.592,"d":"2.59"},"无重合面",null,156,null,null,"34NM059-2.3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系放散管操作台及爬梯","方（扁）钢","踢腿板100*4",1,4000,100,4,null,null,{"v":0.832,"d":"0.83"},"无重合面",null,156,null,null,"34NM059-2.3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系放散管操作台及爬梯","[槽钢","[100*48*5.3",4,300,null,48,5.3,5.3,{"v":0.21768,"d":"0.22"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM059-2.3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系放散管操作台及爬梯","[槽钢","[100*48*5.3",2,1500,null,48,5.3,5.3,{"v":0.4002,"d":"0.40"},"翼板重合",null,156,null,null,"34NM059-2.3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系放散管操作台及爬梯","[槽钢","[126*53*5.5",2,4800,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.9296,"d":"1.93"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"34NM059-2.3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系放散管操作台及爬梯","圆钢","圆钢 Q50*2.5",1,14200,50,{"$nulls":3},{"v":2.2294,"d":"2.23"},"无重合面",null,156,null,{"v":2.2294,"d":"2.23"},"34NM059-2.3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["精脱硫二系放散管操作台及爬梯","圆钢","圆钢 Q33.5",1,3900,33.5,{"$nulls":3},{"v":0.410241,"d":"0.41"},"无重合面",null,156,null,{"v":0.6123,"d":"0.61"},"34NM059-2.3","一般性腐蚀","环氧富锌漆",{"v":0.598802395209581,"d":"60%"}]
["精脱硫二系放散管操作台及爬梯","方（扁）钢","花纹板4",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":2.4,"d":"2.40"},"34NM059-2.3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["精脱硫一系1V4609、1V4611联合操作台及爬梯","L型钢","L63*63*6",2,10020,null,63,6,6,{"v":2.52504,"d":"2.53"},"无重合面",null,156,null,null,"34NM060-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系1V4609、1V4611联合操作台及爬梯","圆钢","圆钢Q18",34,500,18,{"$nulls":3},{"v":0.96084,"d":"0.96"},"无重合面",null,156,null,{"v":0.96084,"d":"0.96"},"34NM060-2","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["精脱硫一系1V4609、1V4611联合操作台及爬梯","方（扁）钢","扁铁40*4",4,7000,40,4,null,null,{"v":2.464,"d":"2.46"},"无重合面",null,156,null,null,"34NM060-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系1V4609、1V4611联合操作台及爬梯","圆钢","圆钢 Q50*3",2,12300,50,{"$nulls":3},{"v":3.8622,"d":"3.86"},"无重合面",null,156,null,{"v":3.8622,"d":"3.86"},"34NM060-2","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["精脱硫一系1V4609、1V4611联合操作台及爬梯","方（扁）钢","扁铁40*4",2,12300,40,4,null,null,{"v":2.1648,"d":"2.16"},"无重合面",null,156,null,null,"34NM060-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系1V4609、1V4611联合操作台及爬梯","方（扁）钢","踢腿板100*4",1,12300,100,4,null,null,{"v":2.5584,"d":"2.56"},"无重合面",null,156,null,null,"34NM060-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系1V4609、1V4611联合操作台及爬梯","方（扁）钢","花纹板4",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,3.59,"34NM060-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["精脱硫一系1V4609、1V4611联合操作台及爬梯","[槽钢","[100*48*5.3",1,15400,null,48,5.3,5.3,{"v":2.05436,"d":"2.05"},"翼板重合",null,156,null,null,"34NM060-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系1V4609、1V4611联合操作台及爬梯","[槽钢","[126*53*5.5",2,1030,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.41406,"d":"0.41"},"无重合面",null,156,null,null,"34NM060-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系1V4609、1V4611联合操作台及爬梯","[槽钢","[100*48*5.3",4,2900,null,48,5.3,5.3,{"v":2.10424,"d":"2.10"},"无重合面",null,156,null,null,"34NM060-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系1V4609、1V4611联合操作台及爬梯","[槽钢","[100*48*5.3",1,4400,null,48,5.3,5.3,{"v":0.79816,"d":"0.80"},"无重合面",null,156,null,null,"34NM060-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系1V4609、1V4611联合操作台及爬梯","L型钢","L50*50*5",1,13100,null,50,5,5,1.31,"无重合面",null,156,null,null,"34NM060-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系1V4609、1V4611联合操作台及爬梯","[槽钢","[100*48*5.3",4,2600,null,48,5.3,5.3,{"v":1.88656,"d":"1.89"},"无重合面",null,156,null,null,"34NM060-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系1V4609、1V4611联合操作台及爬梯","[槽钢","[100*48*5.3",1,4040,null,48,5.3,5.3,{"v":0.732856,"d":"0.73"},"无重合面",null,156,null,null,"34NM060-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系1V4609、1V4611联合操作台及爬梯","L型钢","L50*50*5",1,12400,null,50,5,5,1.24,"无重合面",null,156,null,null,"34NM060-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系2V4609、2V4611联合操作台及爬梯+4.425m平台","[槽钢","[100*48*5.3",1,9400,null,48,5.3,5.3,{"v":1.70516,"d":"1.71"},"无重合面",null,156,null,null,"34NM061-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系2V4609、2V4611联合操作台及爬梯+4.425m平台","方（扁）钢","花纹板4.5",1,{"$nulls":5},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":7.4,"d":"7.40"},"34NM061-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["精脱硫二系2V4609、2V4611联合操作台及爬梯+4.425m平台","方（扁）钢","加强筋50*4",3,1000,50,4,null,null,{"v":0.324,"d":"0.32"},"无重合面",null,156,null,null,"34NM061-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系2V4609、2V4611联合操作台及爬梯直梯*3","L型钢","L63*63*6",2,13300,null,63,6,6,{"v":3.3516,"d":"3.35"},"无重合面",null,156,null,null,"34NM061-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系2V4609、2V4611联合操作台及爬梯","圆钢","圆钢Q18",44,500,18,{"$nulls":3},{"v":1.24344,"d":"1.24"},"无重合面",null,156,null,{"v":1.24344,"d":"1.24"},"34NM061-2","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["精脱硫二系2V4609、2V4611联合操作台及爬梯","方（扁）钢","扁铁40*4",5,10000,40,4,null,null,{"v":4.4,"d":"4.40"},"无重合面",null,156,null,null,"34NM061-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系2V4609、2V4611联合操作台及爬梯","圆钢","圆钢 Q50*3",2,12600,50,{"$nulls":3},{"v":3.9564,"d":"3.96"},"翼板重合",null,156,null,{"v":3.3516,"d":"3.35"},"34NM061-2","一般性腐蚀","环氧富锌漆",{"v":0.458620689655172,"d":"46%"}]
["精脱硫二系2V4609、2V4611联合操作台及爬梯","方（扁）钢","扁铁40*4",2,12600,40,4,null,null,{"v":2.2176,"d":"2.22"},"无重合面",null,156,null,null,"34NM061-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系2V4609、2V4611联合操作台及爬梯","方（扁）钢","踢腿板100*4",1,12600,100,4,null,null,{"v":2.6208,"d":"2.62"},"无重合面",null,156,null,null,"34NM061-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系2V4609、2V4611联合操作台及爬梯","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,4.16,"34NM061-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["精脱硫二系2V4609、2V4611联合操作台及爬梯","[槽钢","[126*53*5.5",3,1030,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.62109,"d":"0.62"},"无重合面",null,156,null,null,"34NM061-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系2V4609、2V4611联合操作台及爬梯","[槽钢","[100*48*5.3",4,2400,null,48,5.3,5.3,{"v":1.74144,"d":"1.74"},"无重合面",null,156,null,null,"34NM061-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系2V4609、2V4611联合操作台及爬梯","[槽钢","[100*48*5.3",2,1500,null,48,5.3,5.3,{"v":0.5442,"d":"0.54"},"无重合面",null,156,null,null,"34NM061-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系2V4609、2V4611联合操作台及爬梯","[槽钢","[80*43*5",2,700,null,43,5,5,{"v":0.2268,"d":"0.23"},"无重合面",null,156,null,null,"34NM061-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系2V4609、2V4611联合操作台及爬梯","[槽钢","[100*48*5.3",4,2700,null,48,5.3,5.3,{"v":1.95912,"d":"1.96"},"无重合面",null,156,null,null,"34NM061-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系2V4609、2V4611联合操作台及爬梯","[槽钢","[100*48*5.3",2,1540,null,48,5.3,5.3,{"v":0.558712,"d":"0.56"},"无重合面",null,156,null,null,"34NM061-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系2V4609、2V4611联合操作台及爬梯","[槽钢","[80*43*5",2,700,null,43,5,5,{"v":0.2268,"d":"0.23"},"无重合面",null,156,null,null,"34NM061-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系管道过桥","方（扁）钢","扁铁60*8",11,3980,60,8,null,null,{"v":5.95408,"d":"5.95"},"无重合面",null,156,null,null,"34NM062-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系管道过桥","圆钢","圆钢Q18",44,500,18,{"$nulls":3},{"v":1.24344,"d":"1.24"},"无重合面",null,156,null,{"v":1.24344,"d":"1.24"},"34NM062-2\\3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["精脱硫一系管道过桥","L型钢","L75*75*6",40,265,null,75,6,6,1.59,"无重合面",null,156,null,null,"34NM062-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系管道过桥","L型钢","L75*75*6",20,740,null,75,6,6,2.22,"无重合面",null,156,null,null,"34NM062-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系管道过桥","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":45,"d":"45.00"},"34NM062-2\\3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["精脱硫一系管道过桥","方（扁）钢","加强筋50*4",26,660,50,4,null,null,{"v":1.85328,"d":"1.85"},"无重合面",null,156,null,null,"34NM062-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系管道过桥","[槽钢","[126*53*5.5",1,65800,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":9.7384,"d":"9.74"},"翼板重合",null,156,null,null,"34NM062-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系管道过桥","圆钢","圆钢 Q50*3",2,60300,50,{"$nulls":3},{"v":18.9342,"d":"18.93"},"无重合面",null,156,null,{"v":18.9342,"d":"18.93"},"34NM062-2\\3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["精脱硫一系管道过桥","方（扁）钢","扁铁40*4",2,60300,40,4,null,null,{"v":10.6128,"d":"10.61"},"无重合面",null,156,null,null,"34NM062-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫一系管道过桥","方（扁）钢","踢腿板100*4",1,60300,100,4,null,null,{"v":12.5424,"d":"12.54"},"无重合面",null,156,null,null,"34NM062-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系管道过桥","方（扁）钢","扁铁60*8",11,3980,60,8,null,null,{"v":5.95408,"d":"5.95"},"无重合面",null,156,null,null,"34NM062-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系管道过桥","圆钢","圆钢Q18",44,500,18,{"$nulls":3},{"v":1.24344,"d":"1.24"},"无重合面",null,156,null,{"v":1.24344,"d":"1.24"},"34NM062-2\\3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["精脱硫二系管道过桥","L型钢","L75*75*6",40,265,null,75,6,6,1.59,"无重合面",null,156,null,null,"34NM062-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系管道过桥","L型钢","L75*75*6",20,740,null,75,6,6,2.22,"无重合面",null,156,null,null,"34NM062-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系管道过桥","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":45,"d":"45.00"},"34NM062-2\\3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["精脱硫二系管道过桥","方（扁）钢","加强筋50*4",26,660,50,4,null,null,{"v":1.85328,"d":"1.85"},"无重合面",null,156,null,null,"34NM062-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系管道过桥","[槽钢","[126*53*5.5",1,65800,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":9.7384,"d":"9.74"},"翼板重合",null,156,null,null,"34NM062-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系管道过桥","圆钢","圆钢 Q50*3",2,60300,50,{"$nulls":3},{"v":18.9342,"d":"18.93"},"无重合面",null,156,null,{"v":18.9342,"d":"18.93"},"34NM062-2\\3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["精脱硫二系管道过桥","方（扁）钢","扁铁40*4",2,60300,40,4,null,null,{"v":10.6128,"d":"10.61"},"无重合面",null,156,null,null,"34NM062-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["精脱硫二系管道过桥","方（扁）钢","踢腿板100*4",1,60300,100,4,null,null,{"v":12.5424,"d":"12.54"},"无重合面",null,156,null,null,"34NM062-2\\3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台45斜梯","圆钢","圆钢 Q50*3",2,8200,50,{"$nulls":3},{"v":2.5748,"d":"2.57"},"无重合面",null,156,null,null,"33NM128-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台45斜梯","方（扁）钢","扁铁40*4",2,8200,40,4,null,null,{"v":1.4432,"d":"1.44"},"无重合面",null,156,null,null,"33NM128-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台45斜梯","[槽钢","[16b（160*63*6.5）",1,8200,null,63,6.5,6.5,{"v":1.9598,"d":"1.96"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"33NM128-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台45斜梯","方（扁）钢","踏板a3",15,600,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,5.94,"33NM128-1-1图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台平台护栏46.5m","圆钢","圆钢 Q50*3",2,46500,50,{"$nulls":3},{"v":14.601,"d":"14.60"},"无重合面",null,156,null,null,"33NM128-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台平台护栏46.5m","方（扁）钢","扁铁40*4",2,46500,40,4,null,null,{"v":8.184,"d":"8.18"},"无重合面",null,156,null,null,"33NM128-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台平台护栏46.5m","方（扁）钢","踢腿板100*4",1,46500,100,4,null,null,{"v":9.672,"d":"9.67"},"无重合面",null,156,null,null,"33NM128-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台平台护栏支架一","[槽钢","[100*48*5.3",6,2210,null,48,5.3,5.3,{"v":2.405364,"d":"2.41"},"无重合面",null,156,null,null,"33NM128-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台平台护栏支架一","L型钢","L80*50*6",12,120,null,50,6,6,{"v":0.144,"d":"0.14"},"无重合面",null,156,null,null,"33NM128-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台平台护栏支架二","[槽钢","[100*48*5.3",2,3700,null,48,5.3,5.3,{"v":1.34236,"d":"1.34"},"无重合面",null,156,null,null,"33NM128-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台平台护栏支架二","L型钢","L80*50*6",4,120,null,50,6,6,{"v":0.048,"d":"0.05"},"无重合面",null,156,null,null,"33NM128-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台平台护栏平台二","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":28.4,"d":"28.40"},"33NM128-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台平台护栏平台二","[槽钢","[100*48*5.3",1,29100,null,48,5.3,5.3,{"v":3.88194,"d":"3.88"},"翼板重合",null,156,null,null,"33NM128-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台平台护栏平台二","方（扁）钢","加强筋50*4",11,1100,50,4,null,null,{"v":1.3068,"d":"1.31"},"无重合面",null,156,{"$nulls":3},"一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台平台护栏直梯","L型钢","L63*63*6",2,2950,null,63,6,6,{"v":0.7434,"d":"0.74"},"无重合面",null,156,null,null,"33NM128-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台平台护栏直梯","圆钢","圆钢Q18",5,500,18,{"$nulls":3},{"v":0.1413,"d":"0.14"},"无重合面",null,156,null,null,"33NM128-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台平台护栏直梯","方（扁）钢","扁铁40*4",7,1500,40,4,null,null,{"v":0.924,"d":"0.92"},"无重合面",null,156,null,null,"33NM128-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台平台护栏平台一","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":13.6,"d":"13.60"},"33NM128-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台平台护栏平台一","[槽钢","[100*48*5.3",1,18600,null,48,5.3,5.3,{"v":2.48124,"d":"2.48"},"翼板重合",null,156,null,null,"33NM128-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台平台护栏平台一","方（扁）钢","加强筋50*4",6,800,50,4,null,null,{"v":0.5184,"d":"0.52"},"无重合面",null,156,null,null,"33NM128-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉A和废热锅炉A操作平台平台护栏支架三","[槽钢","[100*48*5.3",7,5300,null,48,5.3,5.3,{"v":6.72994,"d":"6.73"},"无重合面",null,156,null,null,"33NM128-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台45斜梯","圆钢","圆钢 Q50*3",2,8200,50,{"$nulls":3},{"v":2.5748,"d":"2.57"},"无重合面",null,156,null,null,"33NM128-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台45斜梯","方（扁）钢","扁铁40*4",2,8200,40,4,null,null,{"v":1.4432,"d":"1.44"},"无重合面",null,156,null,null,"33NM128-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台45斜梯","[槽钢","[16b（160*63*6.5）",1,8200,null,63,6.5,6.5,{"v":1.9598,"d":"1.96"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"33NM128-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台45斜梯","方（扁）钢","踏板B3",15,600,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,5.94,"33NM128-1-1图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台平台护栏46.5m","圆钢","圆钢 Q50*3",2,46500,50,{"$nulls":3},{"v":14.601,"d":"14.60"},"无重合面",null,156,null,null,"33NM128-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台平台护栏46.5m","方（扁）钢","扁铁40*4",2,46500,40,4,null,null,{"v":8.184,"d":"8.18"},"无重合面",null,156,null,null,"33NM128-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台平台护栏46.5m","方（扁）钢","踢腿板100*4",1,46500,100,4,null,null,{"v":9.672,"d":"9.67"},"无重合面",null,156,null,null,"33NM128-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台平台护栏支架一","[槽钢","[100*48*5.3",6,2210,null,48,5.3,5.3,{"v":2.405364,"d":"2.41"},"无重合面",null,156,null,null,"33NM128-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台平台护栏支架一","L型钢","L80*50*6",12,120,null,50,6,6,{"v":0.144,"d":"0.14"},"无重合面",null,156,null,null,"33NM128-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台平台护栏支架二","[槽钢","[100*48*5.3",2,3700,null,48,5.3,5.3,{"v":1.34236,"d":"1.34"},"无重合面",null,156,null,null,"33NM128-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台平台护栏支架二","L型钢","L80*50*6",4,120,null,50,6,6,{"v":0.048,"d":"0.05"},"无重合面",null,156,null,null,"33NM128-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台平台护栏平台二","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":28.4,"d":"28.40"},"33NM128-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台平台护栏平台二","[槽钢","[100*48*5.3",1,29100,null,48,5.3,5.3,{"v":3.88194,"d":"3.88"},"翼板重合",null,156,null,null,"33NM128-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台平台护栏平台二","方（扁）钢","加强筋50*4",11,1100,50,4,null,null,{"v":1.3068,"d":"1.31"},"无重合面",null,156,{"$nulls":3},"一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台平台护栏直梯","L型钢","L63*63*6",2,2950,null,63,6,6,{"v":0.7434,"d":"0.74"},"无重合面",null,156,null,null,"33NM128-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台平台护栏直梯","圆钢","圆钢Q18",5,500,18,{"$nulls":3},{"v":0.1413,"d":"0.14"},"无重合面",null,156,null,null,"33NM128-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台平台护栏直梯","方（扁）钢","扁铁40*4",7,1500,40,4,null,null,{"v":0.924,"d":"0.92"},"无重合面",null,156,null,null,"33NM128-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台平台护栏平台一","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":13.6,"d":"13.60"},"33NM128-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台平台护栏平台一","[槽钢","[100*48*5.3",1,18600,null,48,5.3,5.3,{"v":2.48124,"d":"2.48"},"翼板重合",null,156,null,null,"33NM128-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台平台护栏平台一","方（扁）钢","加强筋50*4",6,800,50,4,null,null,{"v":0.5184,"d":"0.52"},"无重合面",null,156,null,null,"33NM128-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉B和废热锅炉B操作平台平台护栏支架三","[槽钢","[100*48*5.3",7,5300,null,48,5.3,5.3,{"v":6.72994,"d":"6.73"},"无重合面",null,156,null,null,"33NM128-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台45斜梯","圆钢","圆钢 Q50*3",2,8200,50,{"$nulls":3},{"v":2.5748,"d":"2.57"},"无重合面",null,156,null,null,"33NM129-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台45斜梯","方（扁）钢","扁铁40*4",2,8200,40,4,null,null,{"v":1.4432,"d":"1.44"},"无重合面",null,156,null,null,"33NM129-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台45斜梯","[槽钢","[16b（160*63*6.5）",1,8200,null,63,6.5,6.5,{"v":1.9598,"d":"1.96"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"33NM129-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台45斜梯","方（扁）钢","踏板a3",15,600,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,5.94,"33NM129-1-1图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台平台护栏49m","圆钢","圆钢 Q50*3",2,49000,50,{"$nulls":3},{"v":15.386,"d":"15.39"},"无重合面",null,156,null,null,"33NM129-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台平台护栏49m","方（扁）钢","扁铁40*4",2,49000,40,4,null,null,{"v":8.624,"d":"8.62"},"无重合面",null,156,null,null,"33NM129-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台平台护栏49m","方（扁）钢","踢腿板100*4",1,49000,100,4,null,null,{"v":10.192,"d":"10.19"},"无重合面",null,156,null,null,"33NM129-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台平台护栏支架二","[槽钢","[100*48*5.3",7,2210,null,48,5.3,5.3,{"v":2.806258,"d":"2.81"},"无重合面",null,156,null,null,"33NM129-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台平台护栏支架二","L型钢","L80*50*6",14,120,null,50,6,6,{"v":0.168,"d":"0.17"},"无重合面",null,156,null,null,"33NM129-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台平台护栏支架一","[槽钢","[100*48*5.3",2,5870,null,48,5.3,5.3,{"v":2.129636,"d":"2.13"},"无重合面",null,156,null,null,"33NM129-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台平台护栏支架一","L型钢","L80*50*6",4,120,null,50,6,6,{"v":0.048,"d":"0.05"},"无重合面",null,156,null,null,"33NM129-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台平台护栏平台二","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":32.4,"d":"32.40"},"33NM129-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台平台护栏平台二","[槽钢","[100*48*5.3",1,33600,null,48,5.3,5.3,{"v":4.48224,"d":"4.48"},"翼板重合",null,156,null,null,"33NM129-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台平台护栏平台二","方（扁）钢","加强筋50*4",12,1060,50,4,null,null,{"v":1.37376,"d":"1.37"},"无重合面",null,156,null,null,"33NM129-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台平台护栏直梯","L型钢","L63*63*6",2,2950,null,63,6,6,{"v":0.7434,"d":"0.74"},"无重合面",null,156,null,null,"33NM129-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台平台护栏直梯","圆钢","圆钢Q18",5,500,18,{"$nulls":3},{"v":0.1413,"d":"0.14"},"无重合面",null,156,null,null,"33NM129-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台平台护栏直梯","方（扁）钢","扁铁40*4",7,1500,40,4,null,null,{"v":0.924,"d":"0.92"},"无重合面",null,156,null,null,"33NM129-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台平台护栏平台二","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":13.6,"d":"13.60"},"33NM129-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台平台护栏平台二","[槽钢","[100*48*5.3",1,18600,null,48,5.3,5.3,{"v":2.48124,"d":"2.48"},"翼板重合",null,156,null,null,"33NM129-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台平台护栏平台二","方（扁）钢","加强筋50*4",6,780,50,4,null,null,{"v":0.50544,"d":"0.51"},"无重合面",null,156,null,null,"33NM129-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收氨分解克劳斯炉C和废热锅炉C操作平台平台护栏支架三","[槽钢","[100*48*5.3",2,5310,null,48,5.3,5.3,{"v":1.926468,"d":"1.93"},"无重合面",null,156,null,null,"33NM129-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收锅炉供水除氧槽操作平台45斜梯","圆钢","圆钢 Q50*3",2,2000,50,{"$nulls":3},{"v":0.628,"d":"0.63"},"无重合面",null,156,null,null,"33NM134-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收锅炉供水除氧槽操作平台45斜梯","方（扁）钢","扁铁40*4",2,2000,40,4,null,null,{"v":0.352,"d":"0.35"},"无重合面",null,156,null,null,"33NM134-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收锅炉供水除氧槽操作平台45斜梯","[槽钢","[16b（160*63*6.5）",1,2000,null,63,6.5,6.5,{"v":0.478,"d":"0.48"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"33NM134-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收锅炉供水除氧槽操作平台45斜梯","方（扁）钢","踏板a3",3,600,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":1.188,"d":"1.19"},"33NM134-1图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收锅炉供水除氧槽操作平台平台护栏9m","圆钢","圆钢 Q50*3",2,9000,50,{"$nulls":3},{"v":2.826,"d":"2.83"},"无重合面",null,156,null,null,"33NM134-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收锅炉供水除氧槽操作平台平台护栏9m","方（扁）钢","扁铁40*4",2,9000,40,4,null,null,{"v":1.584,"d":"1.58"},"无重合面",null,156,null,null,"33NM134-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收锅炉供水除氧槽操作平台平台护栏9m","方（扁）钢","踢腿板100*4",1,9000,100,4,null,null,{"v":1.872,"d":"1.87"},"无重合面",null,156,null,null,"33NM134-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收锅炉供水除氧槽操作平台平台","方（扁）钢","加强筋40*4",4,850,40,4,null,null,{"v":0.2992,"d":"0.30"},"无重合面",null,156,null,null,"33NM134-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收锅炉供水除氧槽操作平台平台","[槽钢","[100*48*5.3",1,9560,null,48,5.3,5.3,{"v":1.275304,"d":"1.28"},"翼板重合",null,156,null,null,"33NM134-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收锅炉供水除氧槽操作平台平台","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":6.4,"d":"6.40"},"33NM134-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收锅炉供水除氧槽操作平台护栏支架","[槽钢","[100*48*5.3",3,1840,null,48,5.3,5.3,{"v":1.001328,"d":"1.00"},"无重合面",null,156,null,null,"33NM134-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收克劳斯反应器AB操作平台","方（扁）钢","加强筋50*4",27,1400,50,4,null,null,{"v":4.0824,"d":"4.08"},"无重合面",null,156,null,null,"33NM132-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收克劳斯反应器AB操作平台","[槽钢","[100*48*5.3",1,42400,null,48,5.3,5.3,{"v":5.65616,"d":"5.66"},"翼板重合",null,156,null,null,"33NM132-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收克劳斯反应器AB操作平台","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":74.4,"d":"74.40"},"33NM132-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收克劳斯反应器AB操作平台护栏支架","[槽钢","[100*48*5.3",5,7120,null,48,5.3,5.3,{"v":6.45784,"d":"6.46"},"无重合面",null,156,null,null,"33NM132-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收克劳斯反应器AB操作平台护栏支架","L型钢","L80*50*6",10,120,null,50,6,6,0.12,"无重合面",null,156,null,null,"33NM132-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收克劳斯反应器AB操作平台59斜梯","圆钢","圆钢 Q50*3",2,8700,50,{"$nulls":3},{"v":2.7318,"d":"2.73"},"无重合面",null,156,null,null,"33NM132-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收克劳斯反应器AB操作平台59斜梯","方（扁）钢","扁铁40*4",2,8700,40,4,null,null,{"v":1.5312,"d":"1.53"},"无重合面",null,156,null,null,"33NM132-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收克劳斯反应器AB操作平台59斜梯","[槽钢","[16b（160*63*6.5）",1,8700,null,63,6.5,6.5,{"v":2.0793,"d":"2.08"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"33NM132-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收克劳斯反应器AB操作平台59斜梯","方（扁）钢","踏板a3",9,600,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":3.564,"d":"3.56"},"33NM132-1图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收克劳斯反应器AB操作平台平台护栏24.5m","圆钢","圆钢 Q50*3",2,24500,50,{"$nulls":3},{"v":7.693,"d":"7.69"},"无重合面",null,156,null,{"v":2.826,"d":"2.83"},"33NM132-1","一般性腐蚀","环氧富锌漆",{"v":0.26865671641791,"d":"27%"}]
["硫回收克劳斯反应器AB操作平台平台护栏24.5m","方（扁）钢","扁铁40*4",2,24500,40,4,null,null,{"v":4.312,"d":"4.31"},"无重合面",null,156,null,null,"33NM132-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收克劳斯反应器AB操作平台平台护栏24.5m","方（扁）钢","踢腿板100*4",1,24500,100,4,null,null,{"v":5.096,"d":"5.10"},"无重合面",null,156,null,null,"33NM132-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收克劳斯反应器C操作平台","方（扁）钢","加强筋50*4",8,980,50,4,null,null,{"v":0.84672,"d":"0.85"},"无重合面",null,156,null,null,"33NM133-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收克劳斯反应器C操作平台","[槽钢","[100*48*5.3",1,18900,null,48,5.3,5.3,{"v":2.52126,"d":"2.52"},"翼板重合",null,156,null,null,"33NM133-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收克劳斯反应器C操作平台","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":16.9,"d":"16.90"},"33NM133-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收克劳斯反应器C操作平台护栏支架","[槽钢","[100*48*5.3",5,2230,null,48,5.3,5.3,{"v":2.02261,"d":"2.02"},"无重合面",null,156,null,null,"33NM133-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收克劳斯反应器C操作平台护栏支架","L型钢","L80*50*6",10,120,null,50,6,6,0.12,"无重合面",null,156,null,null,"33NM133-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收克劳斯反应器C操作平台59斜梯","圆钢","圆钢 Q50*3",2,8700,50,{"$nulls":3},{"v":2.7318,"d":"2.73"},"无重合面",null,156,null,null,"33NM133-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收克劳斯反应器C操作平台59斜梯","方（扁）钢","扁铁40*4",2,8700,40,4,null,null,{"v":1.5312,"d":"1.53"},"无重合面",null,156,null,null,"33NM133-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收克劳斯反应器C操作平台59斜梯","[槽钢","[16b（160*63*6.5）",1,8700,null,63,6.5,6.5,{"v":2.0793,"d":"2.08"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"33NM133-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收克劳斯反应器C操作平台59斜梯","方（扁）钢","踏板a3",9,600,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":3.564,"d":"3.56"},"33NM133-1图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收克劳斯反应器C操作平台平台护栏17.7m","圆钢","圆钢 Q50*3",2,17700,50,{"$nulls":3},{"v":5.5578,"d":"5.56"},"无重合面",null,156,null,{"v":2.826,"d":"2.83"},"33NM133-1","一般性腐蚀","环氧富锌漆",{"v":0.337078651685393,"d":"34%"}]
["硫回收克劳斯反应器C操作平台平台护栏17.7m","方（扁）钢","扁铁40*4",2,17700,40,4,null,null,{"v":3.1152,"d":"3.12"},"无重合面",null,156,null,null,"33NM133-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收克劳斯反应器C操作平台平台护栏17.7m","方（扁）钢","踢腿板100*4",1,17700,100,4,null,null,{"v":3.6816,"d":"3.68"},"无重合面",null,156,null,null,"33NM133-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器AB操作平台45斜梯","圆钢","圆钢 Q50*3",2,11100,50,{"$nulls":3},{"v":3.4854,"d":"3.49"},"无重合面",null,156,null,null,"33NM134-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器AB操作平台45斜梯","方（扁）钢","扁铁40*4",2,11100,40,4,null,null,{"v":1.9536,"d":"1.95"},"无重合面",null,156,null,null,"33NM134-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器AB操作平台45斜梯","[槽钢","[16b（160*63*6.5）",1,11100,null,63,6.5,6.5,{"v":2.6529,"d":"2.65"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"33NM134-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器AB操作平台45斜梯","方（扁）钢","踏板a3",11,600,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":4.356,"d":"4.36"},"33NM134-1图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收硫冷凝器AB操作平台平台护栏11m","圆钢","圆钢 Q50*3",2,11000,50,{"$nulls":3},{"v":3.454,"d":"3.45"},"无重合面",null,156,null,null,"33NM134-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器AB操作平台平台护栏11m","方（扁）钢","扁铁40*4",2,11000,40,4,null,null,{"v":1.936,"d":"1.94"},"无重合面",null,156,null,null,"33NM134-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器AB操作平台平台护栏11m","方（扁）钢","踢腿板100*4",1,11000,100,4,null,null,{"v":2.288,"d":"2.29"},"无重合面",null,156,null,null,"33NM134-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器AB操作平台支架","[槽钢","[140*58*6",4,500,null,58,6,6,0.44,"无重合面",null,156,null,null,"33NM134-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器AB操作平台支架","[槽钢","[140*58*6",4,300,null,58,6,6,{"v":0.264,"d":"0.26"},"无重合面",null,156,null,null,"33NM134-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器AB操作平台","方（扁）钢","加强筋50*4",4,1200,50,4,null,null,{"v":0.5184,"d":"0.52"},"无重合面",null,156,null,null,"33NM134-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器AB操作平台","方（扁）钢","加强筋50*4",4,600,50,4,null,null,{"v":0.2592,"d":"0.26"},"无重合面",null,156,null,null,"33NM134-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器AB操作平台","[槽钢","[140*58*6",1,15500,null,58,6,6,{"v":2.511,"d":"2.51"},"翼板重合",null,156,null,null,"33NM134-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器AB操作平台","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":18.4,"d":"18.40"},"33NM134-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收硫冷凝器C操作平台45斜梯","圆钢","圆钢 Q50*3",2,11100,50,{"$nulls":3},{"v":3.4854,"d":"3.49"},"无重合面",null,156,null,null,"33NM131-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器C操作平台45斜梯","方（扁）钢","扁铁40*4",2,11100,40,4,null,null,{"v":1.9536,"d":"1.95"},"无重合面",null,156,null,null,"33NM131-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器C操作平台45斜梯","[槽钢","[16b（160*63*6.5）",1,11100,null,63,6.5,6.5,{"v":2.6529,"d":"2.65"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"33NM131-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器C操作平台45斜梯","方（扁）钢","踏板a3",11,600,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":4.356,"d":"4.36"},"33NM131-1图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收硫冷凝器C操作平台平台护栏7m","圆钢","圆钢 Q50*3",2,7000,50,{"$nulls":3},{"v":2.198,"d":"2.20"},"无重合面",null,156,null,null,"33NM131-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器C操作平台平台护栏7m","方（扁）钢","扁铁40*4",2,7000,40,4,null,null,{"v":1.232,"d":"1.23"},"无重合面",null,156,null,null,"33NM134-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器C操作平台平台护栏7m","方（扁）钢","踢腿板100*4",1,7000,100,4,null,null,{"v":1.456,"d":"1.46"},"无重合面",null,156,null,null,"33NM134-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器C操作平台支架","[槽钢","[100*48*5.3",2,3330,null,48,5.3,5.3,{"v":1.208124,"d":"1.21"},"无重合面",null,156,null,null,"33NM134-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器C操作平台","方（扁）钢","加强筋50*4",2,920,50,4,null,null,{"v":0.19872,"d":"0.20"},"无重合面",null,156,null,null,"33NM134-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器C操作平台","[槽钢","[100*48*5.3",1,12840,null,48,5.3,5.3,{"v":1.712856,"d":"1.71"},"翼板重合",null,156,null,null,"33NM134-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收硫冷凝器C操作平台","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":8.4,"d":"8.40"},"33NM134-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收液硫储槽AB操作平台45斜梯","圆钢","圆钢 Q50*3",2,10000,50,{"$nulls":3},3.14,"无重合面",null,156,null,null,"33NM135-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收液硫储槽AB操作平台45斜梯","方（扁）钢","扁铁40*4",2,10000,40,4,null,null,1.76,"无重合面",null,156,null,null,"33NM135-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收液硫储槽AB操作平台45斜梯","[槽钢","[16b（160*63*6.5）",1,10000,null,63,6.5,6.5,2.39,"无重合面",null,156,null,{"v":0,"d":"0.00"},"33NM135-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收液硫储槽AB操作平台45斜梯","方（扁）钢","踏板a3",11,600,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":4.356,"d":"4.36"},"33NM135-1图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收液硫储槽AB操作平台平台护栏19m","圆钢","圆钢 Q50*3",2,19000,50,{"$nulls":3},{"v":5.966,"d":"5.97"},"无重合面",null,156,null,{"v":3.454,"d":"3.45"},"33NM135-1","一般性腐蚀","环氧富锌漆",{"v":0.366666666666667,"d":"37%"}]
["硫回收液硫储槽AB操作平台平台护栏19m","方（扁）钢","扁铁40*4",2,19000,40,4,null,null,{"v":3.344,"d":"3.34"},"无重合面",null,156,null,null,"33NM135-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收液硫储槽AB操作平台平台护栏19m","方（扁）钢","踢腿板100*4",1,19000,100,4,null,null,{"v":3.952,"d":"3.95"},"无重合面",null,156,null,null,"33NM135-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收液硫储槽AB操作平台","[槽钢","[100*48*5.3",1,38400,null,48,5.3,5.3,{"v":5.12256,"d":"5.12"},"翼板重合",null,156,null,null,"33NM135-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收液硫储槽AB操作平台","方（扁）钢","加强筋50*4",3,3000,50,4,null,null,{"v":0.972,"d":"0.97"},"无重合面",null,156,null,null,"33NM135-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["硫回收液硫储槽AB操作平台","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":39.4,"d":"39.40"},"33NM135-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["硫回收液硫储槽AB操作平台支架","[槽钢","[100*48*5.3",10,1950,null,48,5.3,5.3,{"v":3.5373,"d":"3.54"},"无重合面",null,156,null,null,"33NM135-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台","其他",{"$nulls":7},"需手动计算","无重合面",null,156,null,null,"33NM120-2","一般性腐蚀","环氧富锌漆",{"$error":"#VALUE!"}]
["脱酸蒸氨固定氨塔联合操作台平台一*3","方（扁）钢","加强筋40*4",6,866,40,4,null,null,{"v":0.457248,"d":"0.46"},"无重合面",null,156,null,null,"33NM120-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台一*3","方（扁）钢","加强筋40*4",6,986,40,4,null,null,{"v":0.520608,"d":"0.52"},"无重合面",null,156,null,null,"33NM120-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台一*3","[槽钢","[100*48*5.3",3,10600,null,48,5.3,5.3,{"v":4.24212,"d":"4.24"},"翼板重合",null,156,null,null,"33NM120-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台一*3","方（扁）钢","加强筋60*6",3,1437,60,6,null,null,{"v":0.569052,"d":"0.57"},"无重合面",null,156,null,null,"33NM120-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台一*3","方（扁）钢","花纹板4.5",3,{"$nulls":5},{"v":0,"d":"0.00"},"无重合面",null,156,null,24.48,"33NM120-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨固定氨塔联合操作台平台二*3","方（扁）钢","加强筋40*4",18,986,40,4,null,null,{"v":1.561824,"d":"1.56"},"无重合面",null,156,null,null,"33NM120-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台二*3","[槽钢","[100*48*5.3",3,12400,null,48,5.3,5.3,{"v":4.96248,"d":"4.96"},"翼板重合",null,156,null,null,"33NM120-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台二*3","方（扁）钢","花纹板4.5",3,{"$nulls":5},{"v":0,"d":"0.00"},"无重合面",null,156,null,31.08,"33NM120-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨固定氨塔联合操作台平台三*2","方（扁）钢","加强筋40*4",4,986,40,4,null,null,{"v":0.347072,"d":"0.35"},"无重合面",null,156,null,null,"33NM120-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台三*2","[槽钢","[100*48*5.3",2,9000,null,48,5.3,5.3,{"v":2.4012,"d":"2.40"},"翼板重合",null,156,null,null,"33NM120-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台三*2","方（扁）钢","花纹板4.5",2,{"$nulls":5},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":14,"d":"14.00"},"33NM120-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨固定氨塔联合操作台平台四*1","方（扁）钢","加强筋40*4",2,772,40,4,null,null,{"v":0.135872,"d":"0.14"},"无重合面",null,156,null,null,"33NM120-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台四*1","[槽钢","[100*48*5.3",1,5900,null,48,5.3,5.3,{"v":0.78706,"d":"0.79"},"翼板重合",null,156,null,null,"33NM120-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台四*1","方（扁）钢","加强筋60*6",1,1450,60,6,null,null,{"v":0.1914,"d":"0.19"},"无重合面",null,156,null,null,"33NM120-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台四*1","方（扁）钢","花纹板4.5",1,{"$nulls":5},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":4.1,"d":"4.10"},"33NM120-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨固定氨塔联合操作台平台五*2","方（扁）钢","加强筋40*4",18,800,40,4,null,null,{"v":1.2672,"d":"1.27"},"无重合面",null,156,null,null,"33NM120-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台五*2","方（扁）钢","加强筋40*4",2,1060,40,4,null,null,{"v":0.18656,"d":"0.19"},"无重合面",null,156,null,null,"33NM120-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台五*2","[槽钢","[100*48*5.3",2,18000,null,48,5.3,5.3,{"v":4.8024,"d":"4.80"},"翼板重合",null,156,null,null,"33NM120-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台五*2","方（扁）钢","加强筋60*6",16,1316,60,6,null,null,{"v":2.779392,"d":"2.78"},"无重合面",null,156,null,null,"33NM120-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台五*2","方（扁）钢","花纹板4.5",1,{"$nulls":5},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":20.2,"d":"20.20"},"33NM120-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨固定氨塔联合操作台平台六*1","方（扁）钢","加强筋40*4",10,800,40,4,null,null,{"v":0.704,"d":"0.70"},"无重合面",null,156,null,null,"33NM120-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台六*1","[槽钢","[100*48*5.3",1,18820,null,48,5.3,5.3,{"v":2.510588,"d":"2.51"},"翼板重合",null,156,null,null,"33NM120-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台六*1","方（扁）钢","加强筋60*6",9,1316,60,6,null,null,{"v":1.563408,"d":"1.56"},"无重合面",null,156,null,null,"33NM120-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台六*1","方（扁）钢","花纹板4.5",1,{"$nulls":5},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":21.5,"d":"21.50"},"33NM120-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨固定氨塔联合操作台平台七*3","方（扁）钢","加强筋40*4",12,800,40,4,null,null,{"v":0.8448,"d":"0.84"},"无重合面",null,156,null,null,"33NM120-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台七*3","方（扁）钢","加强筋60*6",9,1486,60,6,null,null,{"v":1.765368,"d":"1.77"},"无重合面",null,156,null,null,"33NM120-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台七*3","[槽钢","[100*48*5.3",3,9300,null,48,5.3,5.3,{"v":3.72186,"d":"3.72"},"翼板重合",null,156,null,null,"33NM120-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台七*3","方（扁）钢","花纹板4.5",3,{"$nulls":5},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":28.2,"d":"28.20"},"33NM120-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨固定氨塔联合操作台平台八*3","方（扁）钢","加强筋40*4",12,986,40,4,null,null,{"v":1.041216,"d":"1.04"},"无重合面",null,156,null,null,"33NM120-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台八*3","[槽钢","[100*48*5.3",3,8900,null,48,5.3,5.3,{"v":3.56178,"d":"3.56"},"翼板重合",null,156,null,null,"33NM120-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台八*3","方（扁）钢","花纹板4.5",3,{"$nulls":5},{"v":0,"d":"0.00"},"无重合面",null,156,null,20.64,"33NM120-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨固定氨塔联合操作台平台九*3","方（扁）钢","加强筋40*4",18,800,40,4,null,null,{"v":1.2672,"d":"1.27"},"无重合面",null,156,null,null,"33NM120-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台九*3","方（扁）钢","加强筋60*6",15,1486,60,6,null,null,{"v":2.94228,"d":"2.94"},"无重合面",null,156,null,null,"33NM120-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台九*3","[槽钢","[100*48*5.3",3,12630,null,48,5.3,5.3,{"v":5.054526,"d":"5.05"},"翼板重合",null,156,null,null,"33NM120-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台九*3","方（扁）钢","花纹板4.5",3,{"$nulls":5},{"v":0,"d":"0.00"},"无重合面",null,156,null,43.38,"33NM120-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨固定氨塔联合操作台平台十*3","方（扁）钢","加强筋40*4",6,986,40,4,null,null,{"v":0.520608,"d":"0.52"},"无重合面",null,156,null,null,"33NM120-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台十*3","[槽钢","[100*48*5.3",3,5680,null,48,5.3,5.3,{"v":2.273136,"d":"2.27"},"翼板重合",null,156,null,null,"33NM120-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台十*3","方（扁）钢","花纹板4.5",3,{"$nulls":5},{"v":0,"d":"0.00"},"无重合面",null,156,null,11.04,"33NM120-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨固定氨塔联合操作台平台十一*3","方（扁）钢","加强筋40*4",18,986,40,4,null,null,{"v":1.561824,"d":"1.56"},"无重合面",null,156,null,null,"33NM120-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台十一*3","[槽钢","[100*48*5.3",3,12430,null,48,5.3,5.3,{"v":4.974486,"d":"4.97"},"翼板重合",null,156,null,null,"33NM120-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台十一*3","方（扁）钢","花纹板4.5",3,{"$nulls":5},{"v":0,"d":"0.00"},"无重合面",null,156,null,31.32,"33NM120-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨固定氨塔联合操作台平台十二*3","方（扁）钢","加强筋40*4",12,986,40,4,null,null,{"v":1.041216,"d":"1.04"},"无重合面",null,156,null,null,"33NM120-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台十二*3","[槽钢","[100*48*5.3",3,9600,null,48,5.3,5.3,{"v":3.84192,"d":"3.84"},"翼板重合",null,156,null,null,"33NM120-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台十二*3","方（扁）钢","花纹板4.5",3,{"$nulls":5},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":22.8,"d":"22.80"},"33NM120-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨固定氨塔联合操作台平台十三*3","方（扁）钢","加强筋40*4",6,986,40,4,null,null,{"v":0.520608,"d":"0.52"},"无重合面",null,156,null,null,"33NM120-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台十三*3","[槽钢","[100*48*5.3",3,5180,null,48,5.3,5.3,{"v":2.073036,"d":"2.07"},"翼板重合",null,156,null,null,"33NM120-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台十三*3","方（扁）钢","花纹板4.5",3,{"$nulls":5},{"v":0,"d":"0.00"},"无重合面",null,156,null,9.54,"33NM120-5图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨固定氨塔联合操作台平台十四*3","方（扁）钢","加强筋40*4",9,986,40,4,null,null,{"v":0.780912,"d":"0.78"},"无重合面",null,156,null,null,"33NM120-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台十四*3","[槽钢","[100*48*5.3",3,6540,null,48,5.3,5.3,{"v":2.617308,"d":"2.62"},"翼板重合",null,156,null,null,"33NM120-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台平台十四*3","方（扁）钢","花纹板4.5",3,{"$nulls":5},{"v":0,"d":"0.00"},"无重合面",null,156,null,13.62,"33NM120-5图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨固定氨塔联合操作台悬臂梁一*15","[槽钢","[126*53*5.5",15,1100,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":3.3165,"d":"3.32"},"无重合面",null,156,null,null,"33NM120-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台悬臂梁二*21","[槽钢","[126*53*5.5",21,1040,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":4.38984,"d":"4.39"},"无重合面",null,156,null,null,"33NM120-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台悬臂梁L=1191*3","[槽钢","[126*53*5.5",3,1191,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.718173,"d":"0.72"},"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台悬臂梁L=1132*74","[槽钢","[126*53*5.5",74,1132,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":16.837368,"d":"16.84"},"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台悬臂梁L=957*3","[槽钢","[126*53*5.5",3,957,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.577071,"d":"0.58"},"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台悬臂梁L=703*5","[槽钢","[126*53*5.5",5,703,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.706515,"d":"0.71"},"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台悬臂梁L=1138*3","[槽钢","[126*53*5.5",3,1138,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.686214,"d":"0.69"},"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台三角架L=1332*3","[槽钢","[100*48*5.3",3,1332,null,48,5.3,5.3,{"v":0.7248744,"d":"0.72"},"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台三角架L=1332*3","[槽钢","[126*53*5.5",3,1655,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.997965,"d":"1.00"},"无重合面",null,156,{"$nulls":3},"一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台三角架L=1463*3","[槽钢","[100*48*5.3",3,1463,null,48,5.3,5.3,{"v":0.7961646,"d":"0.80"},"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台三角架L=1463*3","[槽钢","[126*53*5.5",3,1655,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.997965,"d":"1.00"},"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台三角架L=1784*3","[槽钢","[100*48*5.3",3,1784,null,48,5.3,5.3,{"v":0.9708528000000001,"d":"0.97"},"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台三角架L=1784*3","[槽钢","[126*53*5.5",3,1655,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.997965,"d":"1.00"},"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台三角架L=1462*27","[槽钢","[100*48*5.3",27,1462,null,48,5.3,5.3,{"v":7.160583600000001,"d":"7.16"},"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台三角架L=1462*27","[槽钢","[126*53*5.5",27,1655,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":8.981685,"d":"8.98"},"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台三角架L=1634*30","[槽钢","[100*48*5.3",30,1634,null,48,5.3,5.3,{"v":8.892228,"d":"8.89"},"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台三角架L=1634*30","[槽钢","[126*53*5.5",30,1655,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":9.97965,"d":"9.98"},"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台梯子入口*15","方（扁）钢","扁铁50*4",60,1400,50,4,null,null,{"v":9.072,"d":"9.07"},"无重合面",null,156,null,null,"33NM120-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台梯子入口*15","方（扁）钢","扁铁30*4",60,1240,30,4,null,null,{"v":5.0592,"d":"5.06"},"无重合面",null,156,null,null,"33NM120-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台FH1=4800直梯*3","方（扁）钢","钢板60*8",6,6060,60,8,null,null,{"v":4.94496,"d":"4.94"},"无重合面",null,156,null,null,"33NM120-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台FH1=4800直梯*3","圆钢","圆钢Q18",60,500,18,{"$nulls":3},{"v":1.6956,"d":"1.70"},"无重合面",null,156,null,{"v":1.6956,"d":"1.70"},"33NM120-7","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨固定氨塔联合操作台FH1=4800直梯*3","方（扁）钢","扁铁40*4",12,1800,40,4,null,null,{"v":1.9008,"d":"1.90"},"无重合面",null,156,null,null,"33NM120-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台FH1=4800直梯*3","方（扁）钢","扁铁25*4",15,2700,25,4,null,null,{"v":2.349,"d":"2.35"},"无重合面",null,156,null,null,"33NM120-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台FH1=2460直梯*3","方（扁）钢","钢板60*8",6,3800,60,8,null,null,{"v":3.1008,"d":"3.10"},"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台FH1=2460直梯*3","圆钢","圆钢Q18",36,500,18,{"$nulls":3},{"v":1.01736,"d":"1.02"},"无重合面",null,156,null,{"v":1.01736,"d":"1.02"},"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨固定氨塔联合操作台FH1=2460直梯*3","方（扁）钢","扁铁40*4",9,1800,40,4,null,null,{"v":1.4256,"d":"1.43"},"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台FH1=2460直梯*3","方（扁）钢","扁铁25*4",15,1000,25,4,null,null,0.87,"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台FH1=4100直梯*3","方（扁）钢","钢板60*8",6,5200,60,8,null,null,{"v":4.2432,"d":"4.24"},"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台FH1=4100直梯*3","圆钢","圆钢Q18",57,500,18,{"$nulls":3},{"v":1.61082,"d":"1.61"},"无重合面",null,156,null,{"v":1.61082,"d":"1.61"},"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨固定氨塔联合操作台FH1=4100直梯*3","方（扁）钢","扁铁40*4",12,1800,40,4,null,null,{"v":1.9008,"d":"1.90"},"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台FH1=4100直梯*3","方（扁）钢","扁铁25*4",15,2000,25,4,null,null,1.74,"无重合面",null,156,null,null,"33NM120-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台AD=1900直梯*3","方（扁）钢","钢板60*8",6,4628,60,8,null,null,{"v":3.776448,"d":"3.78"},"无重合面",null,156,null,null,"33NM120-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台AD=1900直梯*3","圆钢","圆钢Q18",18,500,18,{"$nulls":3},{"v":0.50868,"d":"0.51"},"无重合面",null,156,null,{"v":0.50868,"d":"0.51"},"33NM120-8","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨固定氨塔联合操作台AD=1300直梯*3","方（扁）钢","钢板60*8",6,4028,60,8,null,null,{"v":3.286848,"d":"3.29"},"无重合面",null,156,null,null,"33NM120-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台AD=1300直梯*3","圆钢","圆钢Q18",12,500,18,{"$nulls":3},{"v":0.33912,"d":"0.34"},"无重合面",null,156,null,{"v":0.33912,"d":"0.34"},"33NM120-8","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨固定氨塔联合操作台AD=1000直梯*2","方（扁）钢","钢板60*8",4,3728,60,8,null,null,{"v":2.028032,"d":"2.03"},"无重合面",null,156,null,null,"33NM120-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台AD=1000直梯*2","圆钢","圆钢Q18",6,500,18,{"$nulls":3},{"v":0.16956,"d":"0.17"},"无重合面",null,156,null,{"v":0.16956,"d":"0.17"},"33NM120-8","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨固定氨塔联合操作台AD=800直梯*2","方（扁）钢","钢板60*8",4,3528,60,8,null,null,{"v":1.919232,"d":"1.92"},"无重合面",null,156,null,null,"33NM120-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台AD=800直梯*2","圆钢","圆钢Q18",6,500,18,{"$nulls":3},{"v":0.16956,"d":"0.17"},"无重合面",null,156,null,{"v":0.16956,"d":"0.17"},"33NM120-8","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨固定氨塔联合操作台KH1=2700直梯*3","L型钢","L63*63*6",6,3984,null,63,6,6,{"v":3.011904,"d":"3.01"},"无重合面",null,156,null,null,"33NM120-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台KH1=2700直梯*3","方（扁）钢","扁铁40*4",9,1840,40,4,null,null,{"v":1.45728,"d":"1.46"},"无重合面",null,156,null,null,"33NM120-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台KH1=2700直梯*3","方（扁）钢","扁铁25*4",15,1970,25,4,null,null,{"v":1.7139,"d":"1.71"},"无重合面",null,156,null,null,"33NM120-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台KH1=2700直梯*3","圆钢","圆钢Q18",27,480,18,{"$nulls":3},{"v":0.7324992,"d":"0.73"},"无重合面",null,156,null,{"v":0.7324992,"d":"0.73"},"33NM120-8","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨固定氨塔联合操作台KH1=2700直梯*3","圆钢","圆钢Q18",6,1366,18,{"$nulls":3},{"v":0.46323792,"d":"0.46"},"无重合面",null,156,null,{"v":0.46323792,"d":"0.46"},"33NM120-8","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨固定氨塔联合操作台斜梯-17*3","[槽钢","[16b（160*63*6.5）",6,2400,null,63,6.5,6.5,{"v":3.4416,"d":"3.44"},"无重合面",null,156,null,null,"33NM120-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台斜梯-17*3","圆钢","圆钢 Q50*2.5",6,4400,50,{"$nulls":3},{"v":4.1448,"d":"4.14"},"无重合面",null,156,null,{"v":4.1448,"d":"4.14"},"33NM120-1","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨固定氨塔联合操作台斜梯-17*3","圆钢","圆钢 Q20*2.5",42,1000,20,{"$nulls":3},{"v":2.6376,"d":"2.64"},"无重合面",null,156,null,0.84,"33NM120-1","一般性腐蚀","环氧富锌漆",{"v":0.241545893719807,"d":"24%"}]
["脱酸蒸氨固定氨塔联合操作台斜梯-17*3","方（扁）钢","踏板a3",21,600,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":8.316,"d":"8.32"},"33NM120-1图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨固定氨塔联合操作台斜梯-25*3","[槽钢","[16b（160*63*6.5）",6,3500,null,63,6.5,6.5,{"v":5.019,"d":"5.02"},"无重合面",null,156,null,null,"33NM120-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨固定氨塔联合操作台斜梯-25*3","圆钢","圆钢 Q50*2.5",6,5500,50,{"$nulls":3},{"v":5.181,"d":"5.18"},"无重合面",null,156,null,{"v":5.181,"d":"5.18"},"33NM120-1","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨固定氨塔联合操作台斜梯-25*3","圆钢","圆钢 Q20*2.5",60,1000,20,{"$nulls":3},{"v":3.7680000000000007,"d":"3.77"},"无重合面",null,156,null,{"v":1.2,"d":"1.20"},"33NM120-1","一般性腐蚀","环氧富锌漆",{"v":0.241545893719807,"d":"24%"}]
["脱酸蒸氨固定氨塔联合操作台斜梯-25*3","方（扁）钢","踏板a3",30,600,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,11.88,"33NM120-1图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨氨水中间槽操作台斜梯","[槽钢","[16b（160*63*6.5）",2,4500,null,63,6.5,6.5,{"v":2.151,"d":"2.15"},"无重合面",null,156,null,null,"33NM123-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨氨水中间槽操作台斜梯","圆钢","圆钢 Q50*2.5",2,6500,50,{"$nulls":3},{"v":2.041,"d":"2.04"},"无重合面",null,156,null,{"v":2.041,"d":"2.04"},"33NM123-1","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨氨水中间槽操作台斜梯","圆钢","圆钢 Q20*2.5",15,1000,20,{"$nulls":3},{"v":0.9420000000000002,"d":"0.94"},"无重合面",null,156,null,{"v":0.3,"d":"0.30"},"33NM123-1","一般性腐蚀","环氧富锌漆",{"v":0.241545893719807,"d":"24%"}]
["脱酸蒸氨氨水中间槽操作台斜梯","方（扁）钢","踏板a3",15,600,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,5.94,"33NM123-1图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨氨水中间槽操作台斜梯护栏10m","圆钢","圆钢 Q50*3",2,10000,50,{"$nulls":3},3.14,"无重合面",null,156,null,3.14,"33NM123-1","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨氨水中间槽操作台斜梯护栏10m","方（扁）钢","扁铁40*4",2,10000,40,4,null,null,1.76,"无重合面",null,156,null,null,"33NM123-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨氨水中间槽操作台护栏17m","圆钢","圆钢 Q50*3",2,17000,50,{"$nulls":3},{"v":5.338,"d":"5.34"},"无重合面",null,156,null,{"v":2.198,"d":"2.20"},"33NM123-1","一般性腐蚀","环氧富锌漆",{"v":0.291666666666667,"d":"29%"}]
["脱酸蒸氨氨水中间槽操作台护栏17m","方（扁）钢","扁铁40*4",2,17000,40,4,null,null,{"v":2.992,"d":"2.99"},"无重合面",null,156,null,null,"33NM123-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨氨水中间槽操作台护栏17m","方（扁）钢","踢腿板100*4",1,17000,100,4,null,null,{"v":3.536,"d":"3.54"},"无重合面",null,156,null,null,"33NM123-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨氨水中间槽操作台平台","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":12,"d":"12.00"},"33NM123-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨氨水中间槽操作台平台","[槽钢","[100*48*5.3",6,800,null,48,5.3,5.3,{"v":0.64032,"d":"0.64"},"翼板重合",null,156,null,null,"33NM123-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨氨水中间槽操作台平台","[槽钢","[100*48*5.3",4,3300,null,48,5.3,5.3,{"v":1.76088,"d":"1.76"},"翼板重合",null,156,null,null,"33NM123-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨氨水中间槽操作台平台","方（扁）钢","加强筋40*4",6,800,40,4,null,null,{"v":0.4224,"d":"0.42"},"无重合面",null,156,null,null,"33NM123-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨氨水中间槽操作台平台支架","[槽钢","[100*48*5.3",6,1340,null,48,5.3,5.3,{"v":1.072536,"d":"1.07"},"翼板重合",null,156,null,null,"33NM123-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨陶瓷过滤器联合操作台","其他",{"$nulls":7},"需手动计算","无重合面",null,156,null,null,"33NM127-1","一般性腐蚀","环氧富锌漆",{"$error":"#VALUE!"}]
["脱酸蒸氨陶瓷过滤器联合操作台45斜梯","圆钢","圆钢 Q50*3",2,14000,50,{"$nulls":3},{"v":4.396,"d":"4.40"},"无重合面",null,156,null,{"v":4.396,"d":"4.40"},"33NM127-1","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨陶瓷过滤器联合操作台45斜梯","方（扁）钢","扁铁40*4",2,14000,40,4,null,null,{"v":2.464,"d":"2.46"},"无重合面",null,156,null,null,"33NM127-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨陶瓷过滤器联合操作台45斜梯","[槽钢","[16b（160*63*6.5）",1,14000,null,63,6.5,6.5,{"v":3.346,"d":"3.35"},"无重合面",null,156,null,{"v":0,"d":"0.00"},"33NM127-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨陶瓷过滤器联合操作台45斜梯","方（扁）钢","踏板a3",24,600,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":9.504,"d":"9.50"},"33NM127-1图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨陶瓷过滤器联合操作台平台护栏140m","圆钢","圆钢 Q50*3",2,140000,50,{"$nulls":3},43.96,"无重合面",null,156,null,{"v":3.454,"d":"3.45"},"33NM127-1","一般性腐蚀","环氧富锌漆",{"v":0.0728476821192053,"d":"7%"}]
["脱酸蒸氨陶瓷过滤器联合操作台平台护栏140m","方（扁）钢","扁铁40*4",2,140000,40,4,null,null,24.64,"无重合面",null,156,null,null,"33NM127-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨陶瓷过滤器联合操作台平台护栏140m","方（扁）钢","踢腿板100*4",1,140000,100,4,null,null,29.12,"无重合面",null,156,null,null,"33NM127-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨陶瓷过滤器联合操作台悬梁一","[槽钢","[126*53*5.5",23,1180,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":5.45514,"d":"5.46"},"无重合面",null,156,null,null,"33NM127-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨陶瓷过滤器联合操作台悬梁二","[槽钢","[126*53*5.5",3,1100,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.6633,"d":"0.66"},"无重合面",null,156,null,null,"33NM127-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨陶瓷过滤器联合操作台支架","[槽钢","[100*48*5.3",40,840,null,48,5.3,5.3,{"v":6.09504,"d":"6.10"},"无重合面",null,156,null,null,"33NM127-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨陶瓷过滤器联合操作台支架","[槽钢","[100*48*5.3",40,800,null,48,5.3,5.3,{"v":5.8048,"d":"5.80"},"无重合面",null,156,null,null,"33NM127-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨陶瓷过滤器联合操作台平台一","[槽钢","[100*48*5.3",1,66000,null,48,5.3,5.3,{"v":8.8044,"d":"8.80"},"翼板重合",null,156,null,null,"33NM127-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨陶瓷过滤器联合操作台平台一","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":61.2,"d":"61.20"},"33NM127-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨陶瓷过滤器联合操作台平台一","方（扁）钢","加强筋40*4",30,1086,40,4,null,null,{"v":2.86704,"d":"2.87"},"无重合面",null,156,null,null,"33NM127-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨陶瓷过滤器联合操作台平台二","[槽钢","[100*48*5.3",1,117000,null,48,5.3,5.3,{"v":15.6078,"d":"15.61"},"翼板重合",null,156,null,null,"33NM127-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨陶瓷过滤器联合操作台平台二","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":86.4,"d":"86.40"},"33NM127-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨陶瓷过滤器联合操作台平台二","方（扁）钢","加强筋40*4",5,586,40,4,null,null,{"v":0.25784,"d":"0.26"},"无重合面",null,156,null,null,"33NM127-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨陶瓷过滤器联合操作台平台二","方（扁）钢","加强筋40*4",65,786,40,4,null,null,{"v":4.49592,"d":"4.50"},"无重合面",null,156,null,null,"33NM127-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨陶瓷过滤器联合操作台KH1=4100直梯*3","L型钢","L63*63*6",6,5384,null,63,6,6,{"v":4.070304,"d":"4.07"},"无重合面",null,156,null,null,"33NM127-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨陶瓷过滤器联合操作台KH1=4100直梯*3","方（扁）钢","扁铁40*4",15,1840,40,4,null,null,{"v":2.4288,"d":"2.43"},"无重合面",null,156,null,null,"33NM127-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨陶瓷过滤器联合操作台KH1=4100直梯*3","方（扁）钢","扁铁25*4",15,3350,25,4,null,null,{"v":2.9145,"d":"2.91"},"无重合面",null,156,null,null,"33NM127-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨陶瓷过滤器联合操作台KH1=4100直梯*3","圆钢","圆钢Q18",42,480,18,{"$nulls":3},{"v":1.1394431999999999,"d":"1.14"},"无重合面",null,156,null,{"v":1.1394432,"d":"1.14"},"33NM127-2","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨陶瓷过滤器联合操作台KH1=4100直梯*3","圆钢","圆钢Q18",6,1366,18,{"$nulls":3},{"v":0.46323792,"d":"0.46"},"无重合面",null,156,null,{"v":0.46323792,"d":"0.46"},"33NM127-2","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨气液分离器操作台平台护栏29m","圆钢","圆钢 Q50*3",2,29000,50,{"$nulls":3},{"v":9.106,"d":"9.11"},"无重合面",null,156,null,{"v":3.454,"d":"3.45"},"33NM124-1-1","一般性腐蚀","环氧富锌漆",{"v":0.275,"d":"28%"}]
["脱酸蒸氨气液分离器操作台平台护栏29m","方（扁）钢","扁铁40*4",2,30000,40,4,null,null,5.28,"无重合面",null,156,null,null,"33NM124-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨气液分离器操作台平台护栏29m","方（扁）钢","踢腿板100*4",1,31000,100,4,null,null,{"v":6.448,"d":"6.45"},"无重合面",null,156,null,null,"33NM124-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨气液分离器操作台KH1=2975直梯*1","方（扁）钢","扁铁40*4",2,2110,40,4,null,null,{"v":0.37136,"d":"0.37"},"无重合面",null,156,null,null,"33NM124-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨气液分离器操作台KH1=2975直梯*1","方（扁）钢","扁铁25*4",5,2170,25,4,null,null,{"v":0.6293,"d":"0.63"},"无重合面",null,156,null,null,"33NM124-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨气液分离器操作台KH1=2975直梯*1","圆钢","圆钢Q18",9,480,18,{"$nulls":3},{"v":0.24416640000000003,"d":"0.24"},"无重合面",null,156,null,{"v":0.2441664,"d":"0.24"},"33NM124-2","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨气液分离器操作台KH1=2975直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,156,null,{"v":0.15441264,"d":"0.15"},"33NM124-2","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨气液分离器操作台KH1=2975直梯*1","L型钢","L63*63*6",2,4200,null,63,6,6,{"v":1.0584,"d":"1.06"},"无重合面",null,156,null,null,"33NM124-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨气液分离器操作台KH1=3500直梯*1","L型钢","L63*63*6",2,4784,null,63,6,6,{"v":1.205568,"d":"1.21"},"无重合面",null,156,null,null,"33NM124-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨气液分离器操作台KH1=3500直梯*1","方（扁）钢","扁铁40*4",4,1840,40,4,null,null,{"v":0.64768,"d":"0.65"},"无重合面",null,156,null,null,"33NM124-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨气液分离器操作台KH1=3500直梯*1","方（扁）钢","扁铁25*4",5,2780,25,4,null,null,{"v":0.8062,"d":"0.81"},"无重合面",null,156,null,null,"33NM124-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨气液分离器操作台KH1=3500直梯*1","圆钢","圆钢Q18",10,480,18,{"$nulls":3},{"v":0.271296,"d":"0.27"},"无重合面",null,156,null,{"v":0.271296,"d":"0.27"},"33NM124-2","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨气液分离器操作台KH1=3500直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,156,null,{"v":0.15441264,"d":"0.15"},"33NM124-2","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨气液分离器操作台平台一*2","[槽钢","[100*48*5.3",2,8300,null,48,5.3,5.3,{"v":2.21444,"d":"2.21"},"翼板重合",null,156,null,null,"33NM124-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨气液分离器操作台平台一*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":11.6,"d":"11.60"},"33NM124-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨气液分离器操作台平台一*2","方（扁）钢","加强筋40*4",2,900,40,4,null,null,{"v":0.1584,"d":"0.16"},"无重合面",null,156,null,null,"33NM124-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨气液分离器操作台平台一*2","方（扁）钢","加强筋40*4",6,990,40,4,null,null,{"v":0.52272,"d":"0.52"},"无重合面",null,156,null,null,"33NM124-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨气液分离器操作台悬臂梁一*4","[槽钢","[126*53*5.5",4,1180,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.94872,"d":"0.95"},"无重合面",null,156,null,null,"33NM124-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨气液分离器操作台悬臂梁二*2","[槽钢","[126*53*5.5",2,1010,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.40602,"d":"0.41"},"无重合面",null,156,null,null,"33NM124-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨气液分离器操作台平台二*2","[槽钢","[100*48*5.3",2,12350,null,48,5.3,5.3,{"v":3.29498,"d":"3.29"},"翼板重合",null,156,null,null,"33NM124-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨气液分离器操作台平台二*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":18,"d":"18.00"},"33NM124-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨气液分离器操作台平台二*2","方（扁）钢","加强筋40*4",18,800,40,4,null,null,{"v":1.2672,"d":"1.27"},"无重合面",null,156,null,null,"33NM124-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨气液分离器操作台支架一*10","[槽钢","[100*48*5.3",10,1390,null,48,5.3,5.3,{"v":2.52146,"d":"2.52"},"无重合面",null,156,null,null,"33NM124-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨气液分离器操作台支架二*4","[槽钢","[100*48*5.3",4,2620,null,48,5.3,5.3,{"v":1.901072,"d":"1.90"},"无重合面",null,156,null,null,"33NM124-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台护栏90m","圆钢","圆钢 Q50*3",2,90000,50,{"$nulls":3},28.26,"无重合面",null,156,null,{"v":3.454,"d":"3.45"},"33NM113-1-3","一般性腐蚀","环氧富锌漆",{"v":0.108910891089109,"d":"11%"}]
["脱酸蒸氨脱氰塔联合操作台平台护栏90m","方（扁）钢","扁铁40*4",2,90000,40,4,null,null,15.84,"无重合面",null,156,null,null,"33NM113-1-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台护栏90m","方（扁）钢","踢腿板100*4",1,90000,100,4,null,null,18.72,"无重合面",null,156,null,null,"33NM113-1-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台盘梯护栏19m","圆钢","圆钢 Q50*3",2,19000,50,{"$nulls":3},{"v":5.966,"d":"5.97"},"无重合面",null,156,null,{"v":5.966,"d":"5.97"},"33NM113-1-3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱氰塔联合操作台盘梯护栏19m","方（扁）钢","扁铁40*4",2,19000,40,4,null,null,{"v":3.344,"d":"3.34"},"无重合面",null,156,null,null,"33NM113-1-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台一*2","[槽钢","[100*48*5.3",2,9900,null,48,5.3,5.3,{"v":2.64132,"d":"2.64"},"翼板重合",null,156,null,null,"33NM113-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台一*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,15.76,"33NM113-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱氰塔联合操作台平台一*2","方（扁）钢","加强筋40*4",4,621,40,4,null,null,{"v":0.218592,"d":"0.22"},"无重合面",null,156,null,null,"33NM113-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台一*2","方（扁）钢","加强筋40*4",6,986,40,4,null,null,{"v":0.520608,"d":"0.52"},"无重合面",null,156,null,null,"33NM113-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台一*2","方（扁）钢","加强筋60*6",2,1300,60,6,null,null,{"v":0.3432,"d":"0.34"},"无重合面",null,156,null,null,"33NM113-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台二*2","[槽钢","[100*48*5.3",2,5700,null,48,5.3,5.3,{"v":1.52076,"d":"1.52"},"翼板重合",null,156,null,null,"33NM113-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台二*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,6.44,"33NM113-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱氰塔联合操作台平台二*2","方（扁）钢","加强筋40*4",2,816,40,4,null,null,{"v":0.143616,"d":"0.14"},"无重合面",null,156,null,null,"33NM113-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台三*1","[槽钢","[100*48*5.3",1,6200,null,48,5.3,5.3,{"v":0.82708,"d":"0.83"},"翼板重合",null,156,null,null,"33NM113-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台三*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,4.62,"33NM113-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱氰塔联合操作台平台三*1","方（扁）钢","加强筋40*4",2,1186,40,4,null,null,{"v":0.208736,"d":"0.21"},"无重合面",null,156,null,null,"33NM113-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台四*2","[槽钢","[100*48*5.3",2,6840,null,48,5.3,5.3,{"v":1.824912,"d":"1.82"},"翼板重合",null,156,null,null,"33NM113-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台四*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":8.6,"d":"8.60"},"33NM113-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱氰塔联合操作台平台四*2","方（扁）钢","加强筋40*4",2,816,40,4,null,null,{"v":0.143616,"d":"0.14"},"无重合面",null,156,null,null,"33NM113-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台四*2","方（扁）钢","加强筋40*4",2,920,40,4,null,null,{"v":0.16192,"d":"0.16"},"无重合面",null,156,null,null,"33NM113-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台五*1","[槽钢","[100*48*5.3",1,6400,null,48,5.3,5.3,{"v":0.85376,"d":"0.85"},"翼板重合",null,156,null,null,"33NM113-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台五*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":4.4,"d":"4.40"},"33NM113-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱氰塔联合操作台平台五*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM113-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台六*1","[槽钢","[100*48*5.3",1,14700,null,48,5.3,5.3,{"v":1.96098,"d":"1.96"},"翼板重合",null,156,null,null,"33NM113-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台六*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,13.68,"33NM113-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱氰塔联合操作台平台六*1","方（扁）钢","加强筋40*4",1,816,40,4,null,null,{"v":0.071808,"d":"0.07"},"无重合面",null,156,null,null,"33NM113-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台六*1","方（扁）钢","加强筋40*4",2,970,40,4,null,null,{"v":0.17072,"d":"0.17"},"无重合面",null,156,null,null,"33NM113-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台六*1","方（扁）钢","加强筋60*6",3,1286,60,6,null,null,{"v":0.509256,"d":"0.51"},"无重合面",null,156,null,null,"33NM113-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台七*1","[槽钢","[100*48*5.3",1,10240,null,48,5.3,5.3,{"v":1.366016,"d":"1.37"},"翼板重合",null,156,null,null,"33NM113-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台七*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,7.96,"33NM113-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱氰塔联合操作台平台七*1","方（扁）钢","加强筋40*4",1,816,40,4,null,null,{"v":0.071808,"d":"0.07"},"无重合面",null,156,null,null,"33NM113-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台七*1","方（扁）钢","加强筋40*4",2,970,40,4,null,null,{"v":0.17072,"d":"0.17"},"无重合面",null,156,null,null,"33NM113-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台七*1","方（扁）钢","加强筋60*6",1,1286,60,6,null,null,{"v":0.169752,"d":"0.17"},"无重合面",null,156,null,null,"33NM113-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台八*2","[槽钢","[100*48*5.3",2,5700,null,48,5.3,5.3,{"v":1.52076,"d":"1.52"},"翼板重合",null,156,null,null,"33NM113-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台八*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":7.4,"d":"7.40"},"33NM113-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱氰塔联合操作台平台八*2","方（扁）钢","加强筋40*4",4,986,40,4,null,null,{"v":0.347072,"d":"0.35"},"无重合面",null,156,null,null,"33NM113-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台九*2","[槽钢","[100*48*5.3",2,20100,null,48,5.3,5.3,{"v":5.36268,"d":"5.36"},"翼板重合",null,156,null,null,"33NM113-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台平台九*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":40,"d":"40.00"},"33NM113-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱氰塔联合操作台平台九*2","方（扁）钢","加强筋40*4",32,1086,40,4,null,null,{"v":3.058176,"d":"3.06"},"无重合面",null,156,null,null,"33NM113-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台罐顶平台支架*20","[槽钢","[100*48*5.3",20,1780,null,48,5.3,5.3,{"v":6.45784,"d":"6.46"},"无重合面",null,156,null,null,"33NM113-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台盘梯DN4000  H2500","方（扁）钢","外侧板160*8",1,4230,160,8,null,null,{"v":1.42128,"d":"1.42"},"无重合面",null,156,null,null,"33NM113-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台盘梯DN4000  H2500","方（扁）钢","内侧板160*8",1,3530,160,8,null,null,{"v":1.18608,"d":"1.19"},"无重合面",null,156,null,null,"33NM113-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台盘梯DN4000  H2500","L型钢","L63*63*6",1,2600,null,63,6,6,{"v":0.3276,"d":"0.33"},"无重合面",null,156,null,null,"33NM113-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台盘梯DN4000  H2500","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,156,null,null,"33NM113-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台盘梯DN4000  H2500","方（扁）钢","踏板",11,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":5.808,"d":"5.81"},"33NM113-5图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱氰塔联合操作台盘梯DN4000  H4200","方（扁）钢","外侧板160*8",1,7110,160,8,null,null,{"v":2.38896,"d":"2.39"},"无重合面",null,156,null,null,"33NM113-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台盘梯DN4000  H4200","方（扁）钢","内侧板160*8",1,5940,160,8,null,null,{"v":1.99584,"d":"2.00"},"无重合面",null,156,null,null,"33NM113-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台盘梯DN4000  H4200","L型钢","L63*63*6",2,2600,null,63,6,6,{"v":0.6552,"d":"0.66"},"无重合面",null,156,null,null,"33NM113-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台盘梯DN4000  H4200","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,156,null,null,"33NM113-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台盘梯DN4000  H4200","方（扁）钢","踏板",20,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,10.56,"33NM113-6图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱氰塔联合操作台盘梯DN4000  H4200","方（扁）钢","外侧板160*8",1,7110,160,8,null,null,{"v":2.38896,"d":"2.39"},"无重合面",null,156,null,null,"33NM113-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台盘梯DN4000  H4200","方（扁）钢","内侧板160*8",1,5940,160,8,null,null,{"v":1.99584,"d":"2.00"},"无重合面",null,156,null,null,"33NM113-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台盘梯DN4000  H4200","L型钢","L63*63*6",2,2600,null,63,6,6,{"v":0.6552,"d":"0.66"},"无重合面",null,156,null,null,"33NM113-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台盘梯DN4000  H4200","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,156,null,null,"33NM113-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台盘梯DN4000  H4200","方（扁）钢","踏板",20,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,10.56,"33NM113-7图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱氰塔联合操作台悬壁梁L=1134*14","[槽钢","[126*53*5.5",4,14000,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":11.256,"d":"11.26"},"无重合面",null,156,null,null,"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台悬壁梁L=1154*8","[槽钢","[126*53*5.5",8,8000,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":12.864,"d":"12.86"},"无重合面",null,156,null,null,"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台悬壁梁L=1134*14","[槽钢","[126*53*5.5",14,14000,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":39.396,"d":"39.40"},"无重合面",null,156,null,null,"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台悬壁梁L=964*4","[槽钢","[126*53*5.5",4,940,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.75576,"d":"0.76"},"无重合面",null,156,null,null,"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台悬壁梁L=1069*2","[槽钢","[126*53*5.5",2,1069,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.429738,"d":"0.43"},"无重合面",null,156,null,null,"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台悬壁梁L=1031*2","[槽钢","[126*53*5.5",2,1031,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.414462,"d":"0.41"},"无重合面",null,156,null,null,"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台悬壁梁L=994*2","[槽钢","[126*53*5.5",2,994,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.399588,"d":"0.40"},"无重合面",null,156,null,null,"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台悬壁梁L=884*1","[槽钢","[126*53*5.5",1,884,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.177684,"d":"0.18"},"无重合面",null,156,null,null,"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台三角架L=1381*2","[槽钢","[100*48*5.3",2,1605,null,48,5.3,5.3,{"v":0.582294,"d":"0.58"},"无重合面",null,156,null,null,"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台三角架L=1381*2","[槽钢","[126*53*5.5",2,1400,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.5628,"d":"0.56"},"无重合面",null,156,{"$nulls":3},"一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台三角架L=1325*2","[槽钢","[100*48*5.3",2,1605,null,48,5.3,5.3,{"v":0.582294,"d":"0.58"},"无重合面",null,156,null,null,"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台三角架L=1325*2","[槽钢","[126*53*5.5",2,1340,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.53868,"d":"0.54"},"无重合面",null,156,{"$nulls":3},"一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台三角架L=1334*2","[槽钢","[100*48*5.3",2,1605,null,48,5.3,5.3,{"v":0.582294,"d":"0.58"},"无重合面",null,156,null,null,"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台三角架L=1334*2","[槽钢","[126*53*5.5",2,1350,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.5427,"d":"0.54"},"无重合面",null,156,{"$nulls":3},"一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台三角架L=1434*5","[槽钢","[100*48*5.3",5,1605,null,48,5.3,5.3,{"v":1.455735,"d":"1.46"},"无重合面",null,156,{"$nulls":3},"一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台三角架L=1434*5","[槽钢","[126*53*5.5",5,1450,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.45725,"d":"1.46"},"无重合面",null,156,{"$nulls":3},"一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台三角架L=1424*2","[槽钢","[100*48*5.3",2,1605,null,48,5.3,5.3,{"v":0.582294,"d":"0.58"},"无重合面",null,156,{"$nulls":3},"一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台三角架L=1424*2","[槽钢","[126*53*5.5",2,1440,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.57888,"d":"0.58"},"无重合面",null,156,null,null,"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台三角架L=1359*1","[槽钢","[100*48*5.3",1,1605,null,48,5.3,5.3,{"v":0.291147,"d":"0.29"},"无重合面",null,156,null,null,"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台三角架L=1359*1","[槽钢","[126*53*5.5",1,1380,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.27738,"d":"0.28"},"无重合面",null,156,null,null,"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台KH1=2600直梯*1","L型钢","L63*63*6",2,3884,null,63,6,6,{"v":0.978768,"d":"0.98"},"无重合面",null,156,null,null,"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台KH1=2600直梯*1","方（扁）钢","扁铁40*4",3,1840,40,4,null,null,{"v":0.48576,"d":"0.49"},"无重合面",null,156,null,null,"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台KH1=2600直梯*1","方（扁）钢","扁铁25*4",5,1870,25,4,null,null,{"v":0.5423,"d":"0.54"},"无重合面",null,156,null,null,"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台KH1=2600直梯*1","圆钢","圆钢Q18",9,480,18,{"$nulls":3},{"v":0.24416640000000003,"d":"0.24"},"无重合面",null,156,null,{"v":0.2441664,"d":"0.24"},"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱氰塔联合操作台KH1=2600直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,156,null,{"v":0.15441264,"d":"0.15"},"33NM113-8","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱氰塔联合操作台梯子入口","方（扁）钢","扁铁50*4",4,1400,50,4,null,null,{"v":0.6048,"d":"0.60"},"无重合面",null,156,null,null,"33NM113-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台梯子入口","方（扁）钢","扁铁30*4",4,1240,30,4,null,null,{"v":0.33728,"d":"0.34"},"无重合面",null,156,null,null,"33NM113-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台KH1=3700直梯*2","L型钢","L63*63*6",4,4984,null,63,6,6,{"v":2.511936,"d":"2.51"},"无重合面",null,156,null,null,"33NM113-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台KH1=3700直梯*2","方（扁）钢","扁铁40*4",8,1840,40,4,null,null,{"v":1.29536,"d":"1.30"},"无重合面",null,156,null,null,"33NM113-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台KH1=3700直梯*2","方（扁）钢","扁铁25*4",10,2980,25,4,null,null,{"v":1.7284,"d":"1.73"},"无重合面",null,156,null,null,"33NM113-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台KH1=3700直梯*2","圆钢","圆钢Q18",20,480,18,{"$nulls":3},{"v":0.542592,"d":"0.54"},"无重合面",null,156,null,{"v":0.542592,"d":"0.54"},"33NM113-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱氰塔联合操作台KH1=3700直梯*2","圆钢","圆钢Q18",4,1366,18,{"$nulls":3},{"v":0.30882528000000004,"d":"0.31"},"无重合面",null,156,null,{"v":0.30882528,"d":"0.31"},"33NM113-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱氰塔联合操作台FH1=4600直梯*1","方（扁）钢","钢板60*8",2,5760,60,8,null,null,{"v":1.56672,"d":"1.57"},"无重合面",null,156,null,null,"33NM113-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台FH1=4600直梯*1","圆钢","圆钢Q18",50,500,18,{"$nulls":3},{"v":1.413,"d":"1.41"},"无重合面",null,156,null,{"v":1.413,"d":"1.41"},"33NM113-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱氰塔联合操作台FH1=4600直梯*1","方（扁）钢","扁铁40*4",4,1800,40,4,null,null,{"v":0.6336,"d":"0.63"},"无重合面",null,156,null,null,"33NM113-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台FH1=4600直梯*1","方（扁）钢","扁铁25*4",5,2500,25,4,null,null,{"v":0.725,"d":"0.73"},"无重合面",null,156,null,null,"33NM113-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台AD=650直梯*1","方（扁）钢","钢板60*8",2,3350,60,8,null,null,{"v":0.9112,"d":"0.91"},"无重合面",null,156,null,null,"33NM113-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台AD=650直梯*2","圆钢","圆钢Q18",2,500,18,{"$nulls":3},{"v":0.05652,"d":"0.06"},"无重合面",null,156,null,{"v":0.05652,"d":"0.06"},"33NM113-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱氰塔联合操作台KH1=3200直梯*1","L型钢","L63*63*6",2,4484,null,63,6,6,{"v":1.129968,"d":"1.13"},"无重合面",null,156,null,null,"33NM113-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台KH1=3200直梯*1","方（扁）钢","扁铁40*4",4,1840,40,4,null,null,{"v":0.64768,"d":"0.65"},"无重合面",null,156,null,null,"33NM113-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台KH1=3200直梯*1","方（扁）钢","扁铁25*4",5,2460,25,4,null,null,{"v":0.7134,"d":"0.71"},"无重合面",null,156,null,null,"33NM113-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱氰塔联合操作台KH1=3200直梯*1","圆钢","圆钢Q18",11,480,18,{"$nulls":3},{"v":0.2984256,"d":"0.30"},"无重合面",null,156,null,{"v":0.2984256,"d":"0.30"},"33NM113-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱氰塔联合操作台KH1=3200直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,156,null,{"v":0.15441264,"d":"0.15"},"33NM113-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台一*1","[槽钢","[100*48*5.3",1,9550,null,48,5.3,5.3,{"v":1.27397,"d":"1.27"},"翼板重合",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台一*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":6.4,"d":"6.40"},"33NM114-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台一*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台一*1","方（扁）钢","加强筋40*4",1,886,40,4,null,null,{"v":0.077968,"d":"0.08"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台二*1","[槽钢","[100*48*5.3",1,10500,null,48,5.3,5.3,{"v":1.4007,"d":"1.40"},"翼板重合",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台二*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":8.2,"d":"8.20"},"33NM114-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台二*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台二*1","方（扁）钢","加强筋40*4",2,886,40,4,null,null,{"v":0.155936,"d":"0.16"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台二*1","方（扁）钢","加强筋60*6",1,1436,60,6,null,null,{"v":0.189552,"d":"0.19"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台三*1","[槽钢","[100*48*5.3",1,5580,null,48,5.3,5.3,{"v":0.744372,"d":"0.74"},"翼板重合",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台三*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,3.58,"33NM114-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台三*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台四*1","方（扁）钢","加强筋40*4",4,986,40,4,null,null,{"v":0.347072,"d":"0.35"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台四*1","方（扁）钢","加强筋60*6",1,1136,60,6,null,null,{"v":0.149952,"d":"0.15"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台四*1","[槽钢","[100*48*5.3",1,8360,null,48,5.3,5.3,{"v":1.115224,"d":"1.12"},"翼板重合",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台四*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":6.4,"d":"6.40"},"33NM114-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台五*1","[槽钢","[100*48*5.3",1,9500,null,48,5.3,5.3,{"v":1.2673,"d":"1.27"},"翼板重合",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台五*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,7.66,"33NM114-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台五*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台五*1","方（扁）钢","加强筋40*4",2,886,40,4,null,null,{"v":0.155936,"d":"0.16"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台五*1","方（扁）钢","加强筋60*6",1,1236,60,6,null,null,{"v":0.163152,"d":"0.16"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台六*1","[槽钢","[100*48*5.3",1,6250,null,48,5.3,5.3,{"v":0.83375,"d":"0.83"},"翼板重合",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台六*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,4.26,"33NM114-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台六*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台七*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,7.68,"33NM114-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台七*1","方（扁）钢","加强筋60*6",4,1386,60,6,null,null,{"v":0.731808,"d":"0.73"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台七*1","[槽钢","[100*48*5.3",1,8300,null,48,5.3,5.3,{"v":1.10722,"d":"1.11"},"翼板重合",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台八*1","方（扁）钢","加强筋40*4",7,986,40,4,null,null,{"v":0.607376,"d":"0.61"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台八*1","方（扁）钢","加强筋60*6",2,1386,60,6,null,null,{"v":0.365904,"d":"0.37"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台八*1","[槽钢","[100*48*5.3",1,18600,null,48,5.3,5.3,{"v":2.48124,"d":"2.48"},"翼板重合",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台八*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,16.34,"33NM114-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台九*1","[槽钢","[100*48*5.3",1,5150,null,48,5.3,5.3,{"v":0.68701,"d":"0.69"},"翼板重合",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台九*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,3.14,"33NM114-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台九*1","方（扁）钢","加强筋40*4",1,986,40,4,null,null,{"v":0.086768,"d":"0.09"},"无重合面",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台十*1","[槽钢","[100*48*5.3",1,10630,null,48,5.3,5.3,{"v":1.418042,"d":"1.42"},"翼板重合",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台十*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":8.6,"d":"8.60"},"33NM114-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台十*1","方（扁）钢","加强筋40*4",5,986,40,4,null,null,{"v":0.43384,"d":"0.43"},"无重合面",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台十二*1","[槽钢","[100*48*5.3",1,5150,null,48,5.3,5.3,{"v":0.68701,"d":"0.69"},"翼板重合",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台十二*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,2.54,"33NM114-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台十二*1","方（扁）钢","加强筋40*4",1,986,40,4,null,null,{"v":0.086768,"d":"0.09"},"无重合面",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台十四*1","[槽钢","[100*48*5.3",1,6220,null,48,5.3,5.3,{"v":0.829748,"d":"0.83"},"翼板重合",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台十四*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,4.22,"33NM114-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台十四*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台十一*1","[槽钢","[100*48*5.3",1,12840,null,48,5.3,5.3,{"v":1.712856,"d":"1.71"},"翼板重合",null,156,null,null,"33NM114-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台十二*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":9,"d":"9.00"},"33NM114-5图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台十二*1","方（扁）钢","加强筋40*4",9,786,40,4,null,null,{"v":0.622512,"d":"0.62"},"无重合面",null,156,null,null,"33NM114-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台十三*1","[槽钢","[100*48*5.3",1,12100,null,48,5.3,5.3,{"v":1.61414,"d":"1.61"},"翼板重合",null,156,null,null,"33NM114-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台十三*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":9,"d":"9.00"},"33NM114-5图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台十三*1","方（扁）钢","加强筋40*4",9,786,40,4,null,null,{"v":0.622512,"d":"0.62"},"无重合面",null,156,null,null,"33NM114-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台罐顶平台支架一*7","[槽钢","[100*48*5.3",7,1500,null,48,5.3,5.3,{"v":1.9047,"d":"1.90"},"无重合面",null,156,null,null,"33NM114-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台罐顶平台支架二*7","[槽钢","[100*48*5.3",7,1500,null,48,5.3,5.3,{"v":1.9047,"d":"1.90"},"无重合面",null,156,null,null,"33NM114-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台FH1=2600直梯*1","方（扁）钢","钢板60*8",2,3960,60,8,null,null,{"v":1.07712,"d":"1.08"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台FH1=2600直梯*1","圆钢","圆钢Q18",14,500,18,{"$nulls":3},{"v":0.39564,"d":"0.40"},"无重合面",null,156,null,{"v":0.39564,"d":"0.40"},"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台FH1=2600直梯*1","方（扁）钢","扁铁40*4",2,1870,40,4,null,null,{"v":0.32912,"d":"0.33"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台FH1=2600直梯*1","方（扁）钢","扁铁25*4",5,530,25,4,null,null,{"v":0.1537,"d":"0.15"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台悬壁梁L=1190*1","[槽钢","[126*53*5.5",1,1210,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.24321,"d":"0.24"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台悬壁梁L=1135*38","[槽钢","[126*53*5.5",38,1150,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":8.7837,"d":"8.78"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台悬壁梁L=1035*2","[槽钢","[126*53*5.5",2,1050,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.4221,"d":"0.42"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台悬壁梁L=672*1","[槽钢","[126*53*5.5",1,690,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.13869,"d":"0.14"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台悬壁梁L=959*1","[槽钢","[126*53*5.5",1,980,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.19698,"d":"0.20"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台悬壁梁L=814*1","[槽钢","[126*53*5.5",1,830,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.16683,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台悬壁梁L=705*1","[槽钢","[126*53*5.5",1,720,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.14472,"d":"0.14"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台三角架L=1535*7","[槽钢","[100*48*5.3",2,1605,null,48,5.3,5.3,{"v":0.582294,"d":"0.58"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台三角架L=1535*7","[槽钢","[126*53*5.5",2,1535,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.61707,"d":"0.62"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台三角架L=1334*1","[槽钢","[100*48*5.3",2,1605,null,48,5.3,5.3,{"v":0.582294,"d":"0.58"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台三角架L=1334*1","[槽钢","[126*53*5.5",2,1334,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.536268,"d":"0.54"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台三角架L=1465*1","[槽钢","[100*48*5.3",2,1605,null,48,5.3,5.3,{"v":0.582294,"d":"0.58"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台三角架L=1465*1","[槽钢","[126*53*5.5",2,1465,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.58893,"d":"0.59"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台三角架L=1786*1","[槽钢","[100*48*5.3",5,1605,null,48,5.3,5.3,{"v":1.455735,"d":"1.46"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台三角架L=1786*1","[槽钢","[126*53*5.5",5,1786,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.79493,"d":"1.79"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台三角架L=1380*1","[槽钢","[100*48*5.3",2,1605,null,48,5.3,5.3,{"v":0.582294,"d":"0.58"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台三角架L=1380*1","[槽钢","[126*53*5.5",2,1380,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.55476,"d":"0.55"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台三角架L=1609*1","[槽钢","[100*48*5.3",1,1605,null,48,5.3,5.3,{"v":0.291147,"d":"0.29"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台三角架L=1609*1","[槽钢","[126*53*5.5",1,1609,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.323409,"d":"0.32"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台盘梯DN2800  H3200","方（扁）钢","外侧板160*8",1,5782,160,8,null,null,{"v":1.942752,"d":"1.94"},"无重合面",null,156,null,null,"33NM114-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台盘梯DN2800  H3200","方（扁）钢","内侧板160*8",1,4585,160,8,null,null,{"v":1.54056,"d":"1.54"},"无重合面",null,156,null,null,"33NM114-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台盘梯DN2800  H3200","L型钢","L63*63*6",1,2500,null,63,6,6,{"v":0.315,"d":"0.32"},"无重合面",null,156,null,null,"33NM114-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台盘梯DN2800  H3200","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,156,null,null,"33NM114-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台盘梯DN2800  H3200","方（扁）钢","踏板",14,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":7.392,"d":"7.39"},"33NM114-7图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台盘梯DN2800  H3000","方（扁）钢","外侧板160*8",1,5420,160,8,null,null,{"v":1.82112,"d":"1.82"},"无重合面",null,156,null,null,"33NM114-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台盘梯DN2800  H3000","方（扁）钢","内侧板160*8",1,4240,160,8,null,null,{"v":1.42464,"d":"1.42"},"无重合面",null,156,null,null,"33NM114-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台盘梯DN2800  H3000","L型钢","L63*63*6",1,2500,null,63,6,6,{"v":0.315,"d":"0.32"},"无重合面",null,156,null,null,"33NM114-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台盘梯DN2800  H3000","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,156,null,null,"33NM114-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台盘梯DN2800  H3000","方（扁）钢","踏板",13,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":6.864,"d":"6.86"},"33NM114-8图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台AD=1300直梯*1","方（扁）钢","钢板60*8",2,4028,60,8,null,null,{"v":1.095616,"d":"1.10"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台AD=1300直梯*1","圆钢","圆钢Q18",4,500,18,{"$nulls":3},{"v":0.11304,"d":"0.11"},"无重合面",null,156,null,{"v":0.11304,"d":"0.11"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台AD=1100直梯*1","方（扁）钢","钢板60*8",2,3828,60,8,null,null,{"v":1.041216,"d":"1.04"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台AD=1100直梯*1","圆钢","圆钢Q18",3,500,18,{"$nulls":3},{"v":0.08478,"d":"0.08"},"无重合面",null,156,null,{"v":0.08478,"d":"0.08"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台KH1=2800直梯*1","L型钢","L63*63*6",2,4080,null,63,6,6,{"v":1.02816,"d":"1.03"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台KH1=2800直梯*1","方（扁）钢","扁铁40*4",3,1840,40,4,null,null,{"v":0.48576,"d":"0.49"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台KH1=2800直梯*1","方（扁）钢","扁铁25*4",5,2090,25,4,null,null,{"v":0.6061,"d":"0.61"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台KH1=2800直梯*1","圆钢","圆钢Q18",9,480,18,{"$nulls":3},{"v":0.24416640000000003,"d":"0.24"},"无重合面",null,156,null,{"v":0.2441664,"d":"0.24"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台KH1=2800直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,156,null,{"v":0.15441264,"d":"0.15"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台KH1=2400直梯*1","L型钢","L63*63*6",2,3680,null,63,6,6,{"v":0.92736,"d":"0.93"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台KH1=2400直梯*1","方（扁）钢","扁铁40*4",3,1840,40,4,null,null,{"v":0.48576,"d":"0.49"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台KH1=2400直梯*1","方（扁）钢","扁铁25*4",5,1670,25,4,null,null,{"v":0.4843,"d":"0.48"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台KH1=2400直梯*1","圆钢","圆钢Q18",8,480,18,{"$nulls":3},{"v":0.21703680000000003,"d":"0.22"},"无重合面",null,156,null,{"v":0.2170368,"d":"0.22"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台KH1=2400直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,156,null,{"v":0.15441264,"d":"0.15"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台FH1=3200直梯*1","方（扁）钢","钢板60*8",2,4560,60,8,null,null,{"v":1.24032,"d":"1.24"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台FH1=3200直梯*1","圆钢","圆钢Q18",16,500,18,{"$nulls":3},{"v":0.45216,"d":"0.45"},"无重合面",null,156,null,{"v":0.45216,"d":"0.45"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台FH1=3200直梯*1","方（扁）钢","扁铁40*4",3,1870,40,4,null,null,{"v":0.49368,"d":"0.49"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台FH1=3200直梯*1","方（扁）钢","扁铁25*4",5,1130,25,4,null,null,{"v":0.3277,"d":"0.33"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台梯子入口*3","方（扁）钢","扁铁50*4",12,1400,50,4,null,null,{"v":1.8144,"d":"1.81"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台梯子入口*3","方（扁）钢","扁铁30*4",12,1240,30,4,null,null,{"v":1.01184,"d":"1.01"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台KH1=2500直梯*1","L型钢","L63*63*6",2,3780,null,63,6,6,{"v":0.95256,"d":"0.95"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台KH1=2500直梯*1","方（扁）钢","扁铁40*4",3,1840,40,4,null,null,{"v":0.48576,"d":"0.49"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台KH1=2500直梯*1","方（扁）钢","扁铁25*4",5,1770,25,4,null,null,{"v":0.5133,"d":"0.51"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台KH1=2500直梯*1","圆钢","圆钢Q18",8,480,18,{"$nulls":3},{"v":0.21703680000000003,"d":"0.22"},"无重合面",null,156,null,{"v":0.2170368,"d":"0.22"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台KH1=2500直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,156,null,{"v":0.15441264,"d":"0.15"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台护栏84m","圆钢","圆钢 Q50*3",2,84000,50,{"$nulls":3},{"v":26.376,"d":"26.38"},"无重合面",null,156,null,{"v":3.454,"d":"3.45"},"33NM114-1-3","一般性腐蚀","环氧富锌漆",{"v":0.115789473684211,"d":"12%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台护栏84m","方（扁）钢","扁铁40*4",2,84000,40,4,null,null,{"v":14.784,"d":"14.78"},"无重合面",null,156,null,null,"33NM114-1-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台平台护栏84m","方（扁）钢","踢腿板100*4",1,84000,100,4,null,null,{"v":17.472,"d":"17.47"},"无重合面",null,156,null,null,"33NM114-1-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台盘梯护栏18.3m","圆钢","圆钢 Q50*3",2,18300,50,{"$nulls":3},{"v":5.7462,"d":"5.75"},"无重合面",null,156,null,{"v":5.7462,"d":"5.75"},"33NM114-1-3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔1#联合操作台盘梯护栏18.3m","方（扁）钢","扁铁40*4",2,18300,40,4,null,null,{"v":3.2208,"d":"3.22"},"无重合面",null,156,null,null,"33NM114-1-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台一*1","[槽钢","[100*48*5.3",1,9550,null,48,5.3,5.3,{"v":1.27397,"d":"1.27"},"翼板重合",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台一*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":6.4,"d":"6.40"},"33NM114-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台一*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台一*1","方（扁）钢","加强筋40*4",1,886,40,4,null,null,{"v":0.077968,"d":"0.08"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台二*1","[槽钢","[100*48*5.3",1,10500,null,48,5.3,5.3,{"v":1.4007,"d":"1.40"},"翼板重合",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台二*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":8.2,"d":"8.20"},"33NM114-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台二*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台二*1","方（扁）钢","加强筋40*4",2,886,40,4,null,null,{"v":0.155936,"d":"0.16"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台二*1","方（扁）钢","加强筋60*6",1,1436,60,6,null,null,{"v":0.189552,"d":"0.19"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台三*1","[槽钢","[100*48*5.3",1,5580,null,48,5.3,5.3,{"v":0.744372,"d":"0.74"},"翼板重合",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台三*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,3.58,"33NM114-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台三*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台四*1","方（扁）钢","加强筋40*4",4,986,40,4,null,null,{"v":0.347072,"d":"0.35"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台四*1","方（扁）钢","加强筋60*6",1,1136,60,6,null,null,{"v":0.149952,"d":"0.15"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台四*1","[槽钢","[100*48*5.3",1,8360,null,48,5.3,5.3,{"v":1.115224,"d":"1.12"},"翼板重合",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台四*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":6.4,"d":"6.40"},"33NM114-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台五*1","[槽钢","[100*48*5.3",1,9500,null,48,5.3,5.3,{"v":1.2673,"d":"1.27"},"翼板重合",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台五*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,7.66,"33NM114-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台五*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台五*1","方（扁）钢","加强筋40*4",2,886,40,4,null,null,{"v":0.155936,"d":"0.16"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台五*1","方（扁）钢","加强筋60*6",1,1236,60,6,null,null,{"v":0.163152,"d":"0.16"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台六*1","[槽钢","[100*48*5.3",1,6250,null,48,5.3,5.3,{"v":0.83375,"d":"0.83"},"翼板重合",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台六*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,4.26,"33NM114-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台六*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台七*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,7.68,"33NM114-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台七*1","方（扁）钢","加强筋60*6",4,1386,60,6,null,null,{"v":0.731808,"d":"0.73"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台七*1","[槽钢","[100*48*5.3",1,8300,null,48,5.3,5.3,{"v":1.10722,"d":"1.11"},"翼板重合",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台八*1","方（扁）钢","加强筋40*4",7,986,40,4,null,null,{"v":0.607376,"d":"0.61"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台八*1","方（扁）钢","加强筋60*6",2,1386,60,6,null,null,{"v":0.365904,"d":"0.37"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台八*1","[槽钢","[100*48*5.3",1,18600,null,48,5.3,5.3,{"v":2.48124,"d":"2.48"},"翼板重合",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台八*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,16.34,"33NM114-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台九*1","[槽钢","[100*48*5.3",1,5150,null,48,5.3,5.3,{"v":0.68701,"d":"0.69"},"翼板重合",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台九*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,3.14,"33NM114-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台九*1","方（扁）钢","加强筋40*4",1,986,40,4,null,null,{"v":0.086768,"d":"0.09"},"无重合面",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台十*1","[槽钢","[100*48*5.3",1,10630,null,48,5.3,5.3,{"v":1.418042,"d":"1.42"},"翼板重合",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台十*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":8.6,"d":"8.60"},"33NM114-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台十*1","方（扁）钢","加强筋40*4",5,986,40,4,null,null,{"v":0.43384,"d":"0.43"},"无重合面",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台十二*1","[槽钢","[100*48*5.3",1,5150,null,48,5.3,5.3,{"v":0.68701,"d":"0.69"},"翼板重合",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台十二*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,2.54,"33NM114-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台十二*1","方（扁）钢","加强筋40*4",1,986,40,4,null,null,{"v":0.086768,"d":"0.09"},"无重合面",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台十四*1","[槽钢","[100*48*5.3",1,6220,null,48,5.3,5.3,{"v":0.829748,"d":"0.83"},"翼板重合",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台十四*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,4.22,"33NM114-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台十四*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台十一*1","[槽钢","[100*48*5.3",1,12840,null,48,5.3,5.3,{"v":1.712856,"d":"1.71"},"翼板重合",null,156,null,null,"33NM114-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台十二*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":9,"d":"9.00"},"33NM114-5图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台十二*1","方（扁）钢","加强筋40*4",9,786,40,4,null,null,{"v":0.622512,"d":"0.62"},"无重合面",null,156,null,null,"33NM114-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台十三*1","[槽钢","[100*48*5.3",1,12100,null,48,5.3,5.3,{"v":1.61414,"d":"1.61"},"翼板重合",null,156,null,null,"33NM114-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台十三*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":9,"d":"9.00"},"33NM114-5图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台十三*1","方（扁）钢","加强筋40*4",9,786,40,4,null,null,{"v":0.622512,"d":"0.62"},"无重合面",null,156,null,null,"33NM114-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台罐顶平台支架一*7","[槽钢","[100*48*5.3",7,1500,null,48,5.3,5.3,{"v":1.9047,"d":"1.90"},"无重合面",null,156,null,null,"33NM114-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台罐顶平台支架二*7","[槽钢","[100*48*5.3",7,1500,null,48,5.3,5.3,{"v":1.9047,"d":"1.90"},"无重合面",null,156,null,null,"33NM114-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台FH1=2600直梯*1","方（扁）钢","钢板60*8",2,3960,60,8,null,null,{"v":1.07712,"d":"1.08"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台FH1=2600直梯*1","圆钢","圆钢Q18",14,500,18,{"$nulls":3},{"v":0.39564,"d":"0.40"},"无重合面",null,156,null,{"v":0.39564,"d":"0.40"},"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台FH1=2600直梯*1","方（扁）钢","扁铁40*4",2,1870,40,4,null,null,{"v":0.32912,"d":"0.33"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台FH1=2600直梯*1","方（扁）钢","扁铁25*4",5,530,25,4,null,null,{"v":0.1537,"d":"0.15"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台悬壁梁L=1190*1","[槽钢","[126*53*5.5",1,1210,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.24321,"d":"0.24"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台悬壁梁L=1135*38","[槽钢","[126*53*5.5",38,1150,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":8.7837,"d":"8.78"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台悬壁梁L=1035*2","[槽钢","[126*53*5.5",2,1050,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.4221,"d":"0.42"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台悬壁梁L=672*1","[槽钢","[126*53*5.5",1,690,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.13869,"d":"0.14"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台悬壁梁L=959*1","[槽钢","[126*53*5.5",1,980,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.19698,"d":"0.20"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台悬壁梁L=814*1","[槽钢","[126*53*5.5",1,830,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.16683,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台悬壁梁L=705*1","[槽钢","[126*53*5.5",1,720,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.14472,"d":"0.14"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台三角架L=1535*7","[槽钢","[100*48*5.3",2,1605,null,48,5.3,5.3,{"v":0.582294,"d":"0.58"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台三角架L=1535*7","[槽钢","[126*53*5.5",2,1535,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.61707,"d":"0.62"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台三角架L=1334*1","[槽钢","[100*48*5.3",2,1605,null,48,5.3,5.3,{"v":0.582294,"d":"0.58"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台三角架L=1334*1","[槽钢","[126*53*5.5",2,1334,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.536268,"d":"0.54"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台三角架L=1465*1","[槽钢","[100*48*5.3",2,1605,null,48,5.3,5.3,{"v":0.582294,"d":"0.58"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台三角架L=1465*1","[槽钢","[126*53*5.5",2,1465,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.58893,"d":"0.59"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台三角架L=1786*1","[槽钢","[100*48*5.3",5,1605,null,48,5.3,5.3,{"v":1.455735,"d":"1.46"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台三角架L=1786*1","[槽钢","[126*53*5.5",5,1786,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.79493,"d":"1.79"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台三角架L=1380*1","[槽钢","[100*48*5.3",2,1605,null,48,5.3,5.3,{"v":0.582294,"d":"0.58"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台三角架L=1380*1","[槽钢","[126*53*5.5",2,1380,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.55476,"d":"0.55"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台三角架L=1609*1","[槽钢","[100*48*5.3",1,1605,null,48,5.3,5.3,{"v":0.291147,"d":"0.29"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台三角架L=1609*1","[槽钢","[126*53*5.5",1,1609,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.323409,"d":"0.32"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台盘梯DN2800  H3200","方（扁）钢","外侧板160*8",1,5782,160,8,null,null,{"v":1.942752,"d":"1.94"},"无重合面",null,156,null,null,"33NM114-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台盘梯DN2800  H3200","方（扁）钢","内侧板160*8",1,4585,160,8,null,null,{"v":1.54056,"d":"1.54"},"无重合面",null,156,null,null,"33NM114-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台盘梯DN2800  H3200","L型钢","L63*63*6",1,2500,null,63,6,6,{"v":0.315,"d":"0.32"},"无重合面",null,156,null,null,"33NM114-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台盘梯DN2800  H3200","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,156,null,null,"33NM114-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台盘梯DN2800  H3200","方（扁）钢","踏板",14,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":7.392,"d":"7.39"},"33NM114-7图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台盘梯DN2800  H3000","方（扁）钢","外侧板160*8",1,5420,160,8,null,null,{"v":1.82112,"d":"1.82"},"无重合面",null,156,null,null,"33NM114-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台盘梯DN2800  H3000","方（扁）钢","内侧板160*8",1,4240,160,8,null,null,{"v":1.42464,"d":"1.42"},"无重合面",null,156,null,null,"33NM114-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台盘梯DN2800  H3000","L型钢","L63*63*6",1,2500,null,63,6,6,{"v":0.315,"d":"0.32"},"无重合面",null,156,null,null,"33NM114-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台盘梯DN2800  H3000","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,156,null,null,"33NM114-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台盘梯DN2800  H3000","方（扁）钢","踏板",13,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":6.864,"d":"6.86"},"33NM114-8图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台AD=1300直梯*1","方（扁）钢","钢板60*8",2,4028,60,8,null,null,{"v":1.095616,"d":"1.10"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台AD=1300直梯*1","圆钢","圆钢Q18",4,500,18,{"$nulls":3},{"v":0.11304,"d":"0.11"},"无重合面",null,156,null,{"v":0.11304,"d":"0.11"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台AD=1100直梯*1","方（扁）钢","钢板60*8",2,3828,60,8,null,null,{"v":1.041216,"d":"1.04"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台AD=1100直梯*1","圆钢","圆钢Q18",3,500,18,{"$nulls":3},{"v":0.08478,"d":"0.08"},"无重合面",null,156,null,{"v":0.08478,"d":"0.08"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台KH1=2800直梯*1","L型钢","L63*63*6",2,4080,null,63,6,6,{"v":1.02816,"d":"1.03"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台KH1=2800直梯*1","方（扁）钢","扁铁40*4",3,1840,40,4,null,null,{"v":0.48576,"d":"0.49"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台KH1=2800直梯*1","方（扁）钢","扁铁25*4",5,2090,25,4,null,null,{"v":0.6061,"d":"0.61"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台KH1=2800直梯*1","圆钢","圆钢Q18",9,480,18,{"$nulls":3},{"v":0.24416640000000003,"d":"0.24"},"无重合面",null,156,null,{"v":0.2441664,"d":"0.24"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台KH1=2800直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,156,null,{"v":0.15441264,"d":"0.15"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台KH1=2400直梯*1","L型钢","L63*63*6",2,3680,null,63,6,6,{"v":0.92736,"d":"0.93"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台KH1=2400直梯*1","方（扁）钢","扁铁40*4",3,1840,40,4,null,null,{"v":0.48576,"d":"0.49"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台KH1=2400直梯*1","方（扁）钢","扁铁25*4",5,1670,25,4,null,null,{"v":0.4843,"d":"0.48"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台KH1=2400直梯*1","圆钢","圆钢Q18",8,480,18,{"$nulls":3},{"v":0.21703680000000003,"d":"0.22"},"无重合面",null,156,null,{"v":0.2170368,"d":"0.22"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台KH1=2400直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,156,null,{"v":0.15441264,"d":"0.15"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台FH1=3200直梯*1","方（扁）钢","钢板60*8",2,4560,60,8,null,null,{"v":1.24032,"d":"1.24"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台FH1=3200直梯*1","圆钢","圆钢Q18",16,500,18,{"$nulls":3},{"v":0.45216,"d":"0.45"},"无重合面",null,156,null,{"v":0.45216,"d":"0.45"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台FH1=3200直梯*1","方（扁）钢","扁铁40*4",3,1870,40,4,null,null,{"v":0.49368,"d":"0.49"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台FH1=3200直梯*1","方（扁）钢","扁铁25*4",5,1130,25,4,null,null,{"v":0.3277,"d":"0.33"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台梯子入口*3","方（扁）钢","扁铁50*4",12,1400,50,4,null,null,{"v":1.8144,"d":"1.81"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台梯子入口*3","方（扁）钢","扁铁30*4",12,1240,30,4,null,null,{"v":1.01184,"d":"1.01"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台KH1=2500直梯*1","L型钢","L63*63*6",2,3780,null,63,6,6,{"v":0.95256,"d":"0.95"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台KH1=2500直梯*1","方（扁）钢","扁铁40*4",3,1840,40,4,null,null,{"v":0.48576,"d":"0.49"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台KH1=2500直梯*1","方（扁）钢","扁铁25*4",5,1770,25,4,null,null,{"v":0.5133,"d":"0.51"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台KH1=2500直梯*1","圆钢","圆钢Q18",8,480,18,{"$nulls":3},{"v":0.21703680000000003,"d":"0.22"},"无重合面",null,156,null,{"v":0.2170368,"d":"0.22"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台KH1=2500直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,156,null,{"v":0.15441264,"d":"0.15"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台护栏84m","圆钢","圆钢 Q50*3",2,84000,50,{"$nulls":3},{"v":26.376,"d":"26.38"},"无重合面",null,156,null,{"v":3.454,"d":"3.45"},"33NM114-1-3","一般性腐蚀","环氧富锌漆",{"v":0.115789473684211,"d":"12%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台护栏84m","方（扁）钢","扁铁40*4",2,84000,40,4,null,null,{"v":14.784,"d":"14.78"},"无重合面",null,156,null,null,"33NM114-1-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台平台护栏84m","方（扁）钢","踢腿板100*4",1,84000,100,4,null,null,{"v":17.472,"d":"17.47"},"无重合面",null,156,null,null,"33NM114-1-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台盘梯护栏18.3m","圆钢","圆钢 Q50*3",2,18300,50,{"$nulls":3},{"v":5.7462,"d":"5.75"},"无重合面",null,156,null,{"v":5.7462,"d":"5.75"},"33NM114-1-3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔2#联合操作台盘梯护栏18.3m","方（扁）钢","扁铁40*4",2,18300,40,4,null,null,{"v":3.2208,"d":"3.22"},"无重合面",null,156,null,null,"33NM114-1-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台一*1","[槽钢","[100*48*5.3",1,9550,null,48,5.3,5.3,{"v":1.27397,"d":"1.27"},"翼板重合",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台一*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":6.4,"d":"6.40"},"33NM114-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台一*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台一*1","方（扁）钢","加强筋40*4",1,886,40,4,null,null,{"v":0.077968,"d":"0.08"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台二*1","[槽钢","[100*48*5.3",1,10500,null,48,5.3,5.3,{"v":1.4007,"d":"1.40"},"翼板重合",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台二*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":8.2,"d":"8.20"},"33NM114-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台二*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台二*1","方（扁）钢","加强筋40*4",2,886,40,4,null,null,{"v":0.155936,"d":"0.16"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台二*1","方（扁）钢","加强筋60*6",1,1436,60,6,null,null,{"v":0.189552,"d":"0.19"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台三*1","[槽钢","[100*48*5.3",1,5580,null,48,5.3,5.3,{"v":0.744372,"d":"0.74"},"翼板重合",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台三*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,3.58,"33NM114-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台三*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台四*1","方（扁）钢","加强筋40*4",4,986,40,4,null,null,{"v":0.347072,"d":"0.35"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台四*1","方（扁）钢","加强筋60*6",1,1136,60,6,null,null,{"v":0.149952,"d":"0.15"},"无重合面",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台四*1","[槽钢","[100*48*5.3",1,8360,null,48,5.3,5.3,{"v":1.115224,"d":"1.12"},"翼板重合",null,156,null,null,"33NM114-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台四*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":6.4,"d":"6.40"},"33NM114-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台五*1","[槽钢","[100*48*5.3",1,9500,null,48,5.3,5.3,{"v":1.2673,"d":"1.27"},"翼板重合",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台五*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,7.66,"33NM114-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台五*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台五*1","方（扁）钢","加强筋40*4",2,886,40,4,null,null,{"v":0.155936,"d":"0.16"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台五*1","方（扁）钢","加强筋60*6",1,1236,60,6,null,null,{"v":0.163152,"d":"0.16"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台六*1","[槽钢","[100*48*5.3",1,6250,null,48,5.3,5.3,{"v":0.83375,"d":"0.83"},"翼板重合",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台六*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,4.26,"33NM114-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台六*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台七*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,7.68,"33NM114-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台七*1","方（扁）钢","加强筋60*6",4,1386,60,6,null,null,{"v":0.731808,"d":"0.73"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台七*1","[槽钢","[100*48*5.3",1,8300,null,48,5.3,5.3,{"v":1.10722,"d":"1.11"},"翼板重合",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台八*1","方（扁）钢","加强筋40*4",7,986,40,4,null,null,{"v":0.607376,"d":"0.61"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台八*1","方（扁）钢","加强筋60*6",2,1386,60,6,null,null,{"v":0.365904,"d":"0.37"},"无重合面",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台八*1","[槽钢","[100*48*5.3",1,18600,null,48,5.3,5.3,{"v":2.48124,"d":"2.48"},"翼板重合",null,156,null,null,"33NM114-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台八*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,16.34,"33NM114-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台九*1","[槽钢","[100*48*5.3",1,5150,null,48,5.3,5.3,{"v":0.68701,"d":"0.69"},"翼板重合",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台九*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,3.14,"33NM114-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台九*1","方（扁）钢","加强筋40*4",1,986,40,4,null,null,{"v":0.086768,"d":"0.09"},"无重合面",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台十*1","[槽钢","[100*48*5.3",1,10630,null,48,5.3,5.3,{"v":1.418042,"d":"1.42"},"翼板重合",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台十*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":8.6,"d":"8.60"},"33NM114-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台十*1","方（扁）钢","加强筋40*4",5,986,40,4,null,null,{"v":0.43384,"d":"0.43"},"无重合面",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台十二*1","[槽钢","[100*48*5.3",1,5150,null,48,5.3,5.3,{"v":0.68701,"d":"0.69"},"翼板重合",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台十二*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,2.54,"33NM114-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台十二*1","方（扁）钢","加强筋40*4",1,986,40,4,null,null,{"v":0.086768,"d":"0.09"},"无重合面",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台十四*1","[槽钢","[100*48*5.3",1,6220,null,48,5.3,5.3,{"v":0.829748,"d":"0.83"},"翼板重合",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台十四*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,4.22,"33NM114-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台十四*1","方（扁）钢","加强筋40*4",2,986,40,4,null,null,{"v":0.173536,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台十一*1","[槽钢","[100*48*5.3",1,12840,null,48,5.3,5.3,{"v":1.712856,"d":"1.71"},"翼板重合",null,156,null,null,"33NM114-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台十二*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":9,"d":"9.00"},"33NM114-5图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台十二*1","方（扁）钢","加强筋40*4",9,786,40,4,null,null,{"v":0.622512,"d":"0.62"},"无重合面",null,156,null,null,"33NM114-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台十三*1","[槽钢","[100*48*5.3",1,12100,null,48,5.3,5.3,{"v":1.61414,"d":"1.61"},"翼板重合",null,156,null,null,"33NM114-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台十三*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":9,"d":"9.00"},"33NM114-5图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台十三*1","方（扁）钢","加强筋40*4",9,786,40,4,null,null,{"v":0.622512,"d":"0.62"},"无重合面",null,156,null,null,"33NM114-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台罐顶平台支架一*7","[槽钢","[100*48*5.3",7,1500,null,48,5.3,5.3,{"v":1.9047,"d":"1.90"},"无重合面",null,156,null,null,"33NM114-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台罐顶平台支架二*7","[槽钢","[100*48*5.3",7,1500,null,48,5.3,5.3,{"v":1.9047,"d":"1.90"},"无重合面",null,156,null,null,"33NM114-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台FH1=2600直梯*1","方（扁）钢","钢板60*8",2,3960,60,8,null,null,{"v":1.07712,"d":"1.08"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台FH1=2600直梯*1","圆钢","圆钢Q18",14,500,18,{"$nulls":3},{"v":0.39564,"d":"0.40"},"无重合面",null,156,null,{"v":0.39564,"d":"0.40"},"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台FH1=2600直梯*1","方（扁）钢","扁铁40*4",2,1870,40,4,null,null,{"v":0.32912,"d":"0.33"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台FH1=2600直梯*1","方（扁）钢","扁铁25*4",5,530,25,4,null,null,{"v":0.1537,"d":"0.15"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台悬壁梁L=1190*1","[槽钢","[126*53*5.5",1,1210,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.24321,"d":"0.24"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台悬壁梁L=1135*38","[槽钢","[126*53*5.5",38,1150,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":8.7837,"d":"8.78"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台悬壁梁L=1035*2","[槽钢","[126*53*5.5",2,1050,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.4221,"d":"0.42"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台悬壁梁L=672*1","[槽钢","[126*53*5.5",1,690,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.13869,"d":"0.14"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台悬壁梁L=959*1","[槽钢","[126*53*5.5",1,980,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.19698,"d":"0.20"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台悬壁梁L=814*1","[槽钢","[126*53*5.5",1,830,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.16683,"d":"0.17"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台悬壁梁L=705*1","[槽钢","[126*53*5.5",1,720,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.14472,"d":"0.14"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台三角架L=1535*7","[槽钢","[100*48*5.3",2,1605,null,48,5.3,5.3,{"v":0.582294,"d":"0.58"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台三角架L=1535*7","[槽钢","[126*53*5.5",2,1535,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.61707,"d":"0.62"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台三角架L=1334*1","[槽钢","[100*48*5.3",2,1605,null,48,5.3,5.3,{"v":0.582294,"d":"0.58"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台三角架L=1334*1","[槽钢","[126*53*5.5",2,1334,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.536268,"d":"0.54"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台三角架L=1465*1","[槽钢","[100*48*5.3",2,1605,null,48,5.3,5.3,{"v":0.582294,"d":"0.58"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台三角架L=1465*1","[槽钢","[126*53*5.5",2,1465,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.58893,"d":"0.59"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台三角架L=1786*1","[槽钢","[100*48*5.3",5,1605,null,48,5.3,5.3,{"v":1.455735,"d":"1.46"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台三角架L=1786*1","[槽钢","[126*53*5.5",5,1786,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.79493,"d":"1.79"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台三角架L=1380*1","[槽钢","[100*48*5.3",2,1605,null,48,5.3,5.3,{"v":0.582294,"d":"0.58"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台三角架L=1380*1","[槽钢","[126*53*5.5",2,1380,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.55476,"d":"0.55"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台三角架L=1609*1","[槽钢","[100*48*5.3",1,1605,null,48,5.3,5.3,{"v":0.291147,"d":"0.29"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台三角架L=1609*1","[槽钢","[126*53*5.5",1,1609,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.323409,"d":"0.32"},"无重合面",null,156,null,null,"33NM114-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台盘梯DN2800  H3200","方（扁）钢","外侧板160*8",1,5782,160,8,null,null,{"v":1.942752,"d":"1.94"},"无重合面",null,156,null,null,"33NM114-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台盘梯DN2800  H3200","方（扁）钢","内侧板160*8",1,4585,160,8,null,null,{"v":1.54056,"d":"1.54"},"无重合面",null,156,null,null,"33NM114-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台盘梯DN2800  H3200","L型钢","L63*63*6",1,2500,null,63,6,6,{"v":0.315,"d":"0.32"},"无重合面",null,156,null,null,"33NM114-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台盘梯DN2800  H3200","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,156,null,null,"33NM114-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台盘梯DN2800  H3200","方（扁）钢","踏板",14,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":7.392,"d":"7.39"},"33NM114-7图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台盘梯DN2800  H3000","方（扁）钢","外侧板160*8",1,5420,160,8,null,null,{"v":1.82112,"d":"1.82"},"无重合面",null,156,null,null,"33NM114-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台盘梯DN2800  H3000","方（扁）钢","内侧板160*8",1,4240,160,8,null,null,{"v":1.42464,"d":"1.42"},"无重合面",null,156,null,null,"33NM114-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台盘梯DN2800  H3000","L型钢","L63*63*6",1,2500,null,63,6,6,{"v":0.315,"d":"0.32"},"无重合面",null,156,null,null,"33NM114-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台盘梯DN2800  H3000","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,156,null,null,"33NM114-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台盘梯DN2800  H3000","方（扁）钢","踏板",13,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,156,null,{"v":6.864,"d":"6.86"},"33NM114-8图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台AD=1300直梯*1","方（扁）钢","钢板60*8",2,4028,60,8,null,null,{"v":1.095616,"d":"1.10"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台AD=1300直梯*1","圆钢","圆钢Q18",4,500,18,{"$nulls":3},{"v":0.11304,"d":"0.11"},"无重合面",null,156,null,{"v":0.11304,"d":"0.11"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台AD=1100直梯*1","方（扁）钢","钢板60*8",2,3828,60,8,null,null,{"v":1.041216,"d":"1.04"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台AD=1100直梯*1","圆钢","圆钢Q18",3,500,18,{"$nulls":3},{"v":0.08478,"d":"0.08"},"无重合面",null,156,null,{"v":0.08478,"d":"0.08"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台KH1=2800直梯*1","L型钢","L63*63*6",2,4080,null,63,6,6,{"v":1.02816,"d":"1.03"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台KH1=2800直梯*1","方（扁）钢","扁铁40*4",3,1840,40,4,null,null,{"v":0.48576,"d":"0.49"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台KH1=2800直梯*1","方（扁）钢","扁铁25*4",5,2090,25,4,null,null,{"v":0.6061,"d":"0.61"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台KH1=2800直梯*1","圆钢","圆钢Q18",9,480,18,{"$nulls":3},{"v":0.24416640000000003,"d":"0.24"},"无重合面",null,156,null,{"v":0.2441664,"d":"0.24"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台KH1=2800直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,156,null,{"v":0.15441264,"d":"0.15"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台KH1=2400直梯*1","L型钢","L63*63*6",2,3680,null,63,6,6,{"v":0.92736,"d":"0.93"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台KH1=2400直梯*1","方（扁）钢","扁铁40*4",3,1840,40,4,null,null,{"v":0.48576,"d":"0.49"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台KH1=2400直梯*1","方（扁）钢","扁铁25*4",5,1670,25,4,null,null,{"v":0.4843,"d":"0.48"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台KH1=2400直梯*1","圆钢","圆钢Q18",8,480,18,{"$nulls":3},{"v":0.21703680000000003,"d":"0.22"},"无重合面",null,156,null,{"v":0.2170368,"d":"0.22"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台KH1=2400直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,156,null,{"v":0.15441264,"d":"0.15"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台FH1=3200直梯*1","方（扁）钢","钢板60*8",2,4560,60,8,null,null,{"v":1.24032,"d":"1.24"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台FH1=3200直梯*1","圆钢","圆钢Q18",16,500,18,{"$nulls":3},{"v":0.45216,"d":"0.45"},"无重合面",null,156,null,{"v":0.45216,"d":"0.45"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台FH1=3200直梯*1","方（扁）钢","扁铁40*4",3,1870,40,4,null,null,{"v":0.49368,"d":"0.49"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台FH1=3200直梯*1","方（扁）钢","扁铁25*4",5,1130,25,4,null,null,{"v":0.3277,"d":"0.33"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台梯子入口*3","方（扁）钢","扁铁50*4",12,1400,50,4,null,null,{"v":1.8144,"d":"1.81"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台梯子入口*3","方（扁）钢","扁铁50*4",12,1240,50,4,null,null,{"v":1.60704,"d":"1.61"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台KH1=2500直梯*1","L型钢","L63*63*6",2,3780,null,63,6,6,{"v":0.95256,"d":"0.95"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台KH1=2500直梯*1","方（扁）钢","扁铁40*4",3,1840,40,4,null,null,{"v":0.48576,"d":"0.49"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台KH1=2500直梯*1","方（扁）钢","扁铁25*4",5,1770,25,4,null,null,{"v":0.5133,"d":"0.51"},"无重合面",null,156,null,null,"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台KH1=2500直梯*1","圆钢","圆钢Q18",8,480,18,{"$nulls":3},{"v":0.21703680000000003,"d":"0.22"},"无重合面",null,156,null,{"v":0.2170368,"d":"0.22"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台KH1=2500直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,156,null,{"v":0.15441264,"d":"0.15"},"33NM114-9","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台护栏84m","圆钢","圆钢 Q50*3",2,84000,50,{"$nulls":3},{"v":26.376,"d":"26.38"},"无重合面",null,156,null,{"v":3.454,"d":"3.45"},"33NM114-1-3","一般性腐蚀","环氧富锌漆",{"v":0.115789473684211,"d":"12%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台护栏84m","方（扁）钢","扁铁40*4",2,84000,40,4,null,null,{"v":14.784,"d":"14.78"},"无重合面",null,156,null,null,"33NM114-1-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台平台护栏84m","方（扁）钢","踢腿板100*4",1,84000,100,4,null,null,{"v":17.472,"d":"17.47"},"无重合面",null,156,null,null,"33NM114-1-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台盘梯护栏18.3m","圆钢","圆钢 Q50*3",2,18300,50,{"$nulls":3},{"v":5.7462,"d":"5.75"},"无重合面",null,156,null,{"v":5.7462,"d":"5.75"},"33NM114-1-3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["脱酸蒸氨脱酸塔、挥发氨塔3#联合操作台盘梯护栏18.3m","方（扁）钢","扁铁40*4",2,18300,40,4,null,null,{"v":3.2208,"d":"3.22"},"无重合面",null,156,null,null,"33NM114-1-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=3000直梯*2","L型钢","L63*63*6",4,4284,null,63,6,6,{"v":2.159136,"d":"2.16"},"无重合面",null,157,null,null,"31NM056-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=3000直梯*2","方（扁）钢","扁铁40*4",8,1840,40,4,null,null,{"v":1.29536,"d":"1.30"},"无重合面",null,158,null,null,"31NM056-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=3000直梯*2","方（扁）钢","扁铁25*4",10,2280,25,4,null,null,{"v":1.3224,"d":"1.32"},"无重合面",null,159,null,null,"31NM056-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=3000直梯*2","圆钢","圆钢Q18",20,480,18,{"$nulls":3},{"v":0.542592,"d":"0.54"},"无重合面",null,160,null,null,"31NM056-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=3000直梯*2","圆钢","圆钢Q18",4,1366,18,{"$nulls":3},{"v":0.30882528000000004,"d":"0.31"},"无重合面",null,161,null,null,"31NM056-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=3900直梯*4","L型钢","L63*63*6",8,5184,null,63,6,6,{"v":5.225472,"d":"5.23"},"无重合面",null,162,null,null,"31NM056-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=3900直梯*4","方（扁）钢","扁铁40*4",20,1840,40,4,null,null,{"v":3.2384,"d":"3.24"},"无重合面",null,163,null,null,"31NM056-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=3900直梯*4","方（扁）钢","扁铁25*4",20,3150,25,4,null,null,{"v":3.654,"d":"3.65"},"无重合面",null,164,null,null,"31NM056-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=3900直梯*4","圆钢","圆钢Q18",42,480,18,{"$nulls":3},{"v":1.1394431999999999,"d":"1.14"},"无重合面",null,165,null,null,"31NM056-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=3900直梯*4","圆钢","圆钢Q18",8,1366,18,{"$nulls":3},{"v":0.6176505600000001,"d":"0.62"},"无重合面",null,166,null,null,"31NM056-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台支架一","[槽钢","[100*48*5.3",52,2018,null,48,5.3,5.3,{"v":19.0353904,"d":"19.04"},"无重合面",null,167,null,null,"31NM056-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+3400-8800-11900*6","[槽钢","[100*48*5.3",6,12500,null,48,5.3,5.3,{"v":10.005,"d":"10.01"},"翼板重合",null,168,null,null,"31NM056-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+3400-8800-11900*6","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,169,null,55.92,"31NM056-3图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["电捕煤气管道联合平台+3400-8800-11900*6","方（扁）钢","加强筋50*4",30,986,50,4,null,null,{"v":3.19464,"d":"3.19"},"无重合面",null,170,null,null,"31NM056-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+15000*2","[槽钢","[100*48*5.3",2,80000,null,48,5.3,5.3,{"v":21.344,"d":"21.34"},"翼板重合",null,171,null,null,"31NM056-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+15000*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,172,null,{"v":127.2,"d":"127.20"},"31NM056-4图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["电捕煤气管道联合平台+15000*2","方（扁）钢","加强筋50*4",8,980,50,4,null,null,{"v":0.84672,"d":"0.85"},"无重合面",null,173,null,null,"31NM056-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+15000*2","方（扁）钢","加强筋50*4",72,686,50,4,null,null,{"v":5.334336,"d":"5.33"},"无重合面",null,174,null,null,"31NM056-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+15000*2","[槽钢","[200*75*9",2,3900,null,75,9,9,{"v":1.6146,"d":"1.61"},"翼板重合",null,175,null,null,"31NM056-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+15000*2","[槽钢","[200*75*9",2,5800,null,75,9,9,{"v":2.4012,"d":"2.40"},"翼板重合",null,176,null,null,"31NM056-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台走台*2","L型钢","L50*50*5",6,780,null,50,5,5,{"v":0.468,"d":"0.47"},"无重合面",null,177,null,null,"31NM056-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台走台*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,178,null,{"v":16,"d":"16.00"},"31NM056-5图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["电捕煤气管道联合平台走台*2","[槽钢","[200*75*9",4,5110,null,75,9,9,{"v":4.23108,"d":"4.23"},"翼板重合",null,179,null,null,"31NM056-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+19600*4","[槽钢","[100*48*5.3",4,5920,null,48,5.3,5.3,{"v":3.158912,"d":"3.16"},"翼板重合",null,180,null,null,"31NM056-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+19600*4","[槽钢","[100*48*5.3",8,308,null,48,5.3,5.3,{"v":0.4469696,"d":"0.45"},"无重合面",null,181,null,null,"31NM056-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+19600*4","[槽钢","[100*48*5.3",8,746,null,48,5.3,5.3,{"v":1.0825951999999999,"d":"1.08"},"无重合面",null,182,null,null,"31NM056-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+19600*4","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,183,null,{"v":12.8,"d":"12.80"},"31NM056-5图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["电捕煤气管道联合平台支座一*20","[槽钢","[100*48*5.3",20,180,null,48,5.3,5.3,{"v":0.65304,"d":"0.65"},"无重合面",null,184,null,null,"31NM056-6","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台支座二*20","[槽钢","[100*48*5.3",20,180,null,48,5.3,5.3,{"v":0.65304,"d":"0.65"},"无重合面",null,185,null,null,"31NM056-6","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台悬壁梁一*4","[槽钢","[126*53*5.5",4,825,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.6633,"d":"0.66"},"无重合面",null,186,null,null,"31NM056-6","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台悬壁梁二*4","[槽钢","[126*53*5.5",4,550,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.4422,"d":"0.44"},"无重合面",null,187,null,null,"31NM056-6","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+2800*4","[槽钢","[100*48*5.3",4,4610,null,48,5.3,5.3,{"v":2.459896,"d":"2.46"},"翼板重合",null,188,null,null,"31NM056-7","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+2800*4","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,189,null,{"v":8,"d":"8.00"},"31NM056-7图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["电捕煤气管道联合平台+2800*4","方（扁）钢","加强筋50*4",4,582,50,4,null,null,{"v":0.251424,"d":"0.25"},"无重合面",null,190,null,null,"31NM056-7","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台支架三*8","L型钢","L75*75*6",16,840,null,75,6,6,{"v":2.016,"d":"2.02"},"无重合面",null,191,null,null,"31NM056-7","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台支架三*8","[槽钢","[100*48*5.3",16,3135,null,48,5.3,5.3,{"v":9.099024,"d":"9.10"},"无重合面",null,192,null,null,"31NM056-7","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台AD=600直梯*4","方（扁）钢","钢板60*8",8,3320,60,8,null,null,{"v":3.61216,"d":"3.61"},"无重合面",null,193,null,null,"31NM056-8","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台AD=600直梯*4","圆钢","圆钢Q18",8,500,18,{"$nulls":3},{"v":0.22608,"d":"0.23"},"无重合面",null,194,null,null,"31NM056-8","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台支座三四*4","[槽钢","[100*48*5.3",8,150,null,48,5.3,5.3,{"v":0.21768,"d":"0.22"},"无重合面",null,195,null,null,"31NM056-9","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台支座三四*4","L型钢","L75*75*6",8,840,null,75,6,6,{"v":1.008,"d":"1.01"},"无重合面",null,196,null,null,"31NM056-9","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台支架四*4","L型钢","L75*75*6",8,840,null,75,6,6,{"v":1.008,"d":"1.01"},"无重合面",null,197,null,null,"31NM056-9","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台支架四*4","[槽钢","[100*48*5.3",8,150,null,48,5.3,5.3,{"v":0.21768,"d":"0.22"},"无重合面",null,198,null,null,"31NM056-9","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+5400*2","[槽钢","[100*48*5.3",2,4800,null,48,5.3,5.3,{"v":1.28064,"d":"1.28"},"翼板重合",null,199,null,null,"31NM056-9","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+5400*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,200,null,5.12,"31NM056-9图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["电捕煤气管道联合平台+5400*2","方（扁）钢","加强筋50*4",2,786,50,4,null,null,{"v":0.169776,"d":"0.17"},"无重合面",null,201,null,null,"31NM056-9","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台支架二*4","[槽钢","[100*48*5.3",8,3010,null,48,5.3,5.3,{"v":4.368112,"d":"4.37"},"无重合面",null,202,null,null,"31NM056-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台支架二*4","[槽钢","[80*43*5",4,6773,null,43,5,5,{"v":4.388904,"d":"4.39"},"无重合面",null,203,null,null,"31NM056-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台支架二*4","[槽钢","[100*48*5.3",16,3135,null,48,5.3,5.3,{"v":9.099024,"d":"9.10"},"无重合面",null,204,null,null,"31NM056-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+8400*2","[槽钢","[100*48*5.3",2,30100,null,48,5.3,5.3,{"v":8.03068,"d":"8.03"},"翼板重合",null,205,null,null,"31NM056-11","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+8400*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,206,null,{"v":45.2,"d":"45.20"},"31NM056-11图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["电捕煤气管道联合平台+8400*2","方（扁）钢","加强筋50*4",24,786,50,4,null,null,{"v":2.037312,"d":"2.04"},"无重合面",null,207,null,null,"31NM056-11","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+5700*2","[槽钢","[100*48*5.3",2,31800,null,48,5.3,5.3,{"v":8.48424,"d":"8.48"},"翼板重合",null,208,null,null,"31NM056-11","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台+5700*3","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,209,null,{"v":50.4,"d":"50.40"},"31NM056-11图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["电捕煤气管道联合平台+5700*4","方（扁）钢","加强筋50*4",1,12000,50,4,null,null,{"v":1.296,"d":"1.30"},"无重合面",null,210,null,null,"31NM056-11","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台27*28","L型钢","L75*75*6",28,800,null,75,6,6,3.36,"无重合面",null,211,null,null,"31NM056-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台25*152m","[槽钢","[200*75*9",1,152000,null,75,9,9,{"v":42.864,"d":"42.86"},"无重合面",null,212,null,null,"31NM056-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台25.9°斜梯T1B08a-27*2","[槽钢","[16b（160*63*6.5）",4,5200,null,63,6.5,6.5,{"v":4.9712,"d":"4.97"},"无重合面",null,213,null,null,"31NM056-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台25.9°斜梯T1B08a-27*2","方（扁）钢","花纹板4.5",40,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,214,null,21.12,"31NM056-1-1图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["电捕煤气管道联合平台45°斜梯T2B08a-32*2","[槽钢","[16b（160*63*6.5）",4,4500,null,63,6.5,6.5,{"v":4.302,"d":"4.30"},"无重合面",null,215,null,null,"31NM056-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台45°斜梯T2B08a-32*2","方（扁）钢","花纹板4.5",30,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,216,null,15.84,"31NM056-1-1图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["电捕煤气管道联合平台36.3°斜梯T1B08a-23*2","[槽钢","[16b（160*63*6.5）",4,4300,null,63,6.5,6.5,{"v":4.1108,"d":"4.11"},"无重合面",null,217,null,null,"31NM056-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台36.3°斜梯T1B08a-23*2","方（扁）钢","花纹板4.5",36,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,218,null,{"v":19.008,"d":"19.01"},"31NM056-1-1图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["电捕煤气管道联合平台45°斜梯T2B08a-31*6","[槽钢","[16b（160*63*6.5）",12,4500,null,63,6.5,6.5,{"v":12.906,"d":"12.91"},"无重合面",null,219,null,null,"31NM056-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台45°斜梯T2B08a-31*6","方（扁）钢","花纹板4.5",90,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,220,null,47.52,"31NM056-1-1图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["电捕煤气管道联合平台栏杆398m","圆钢","圆钢 Q50*3",2,398000,50,{"$nulls":3},{"v":124.972,"d":"124.97"},"无重合面",null,221,null,null,"31NM056-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台栏杆398m","方（扁）钢","扁铁40*4",2,398000,40,4,null,null,{"v":70.048,"d":"70.05"},"无重合面",null,222,null,null,"31NM056-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台栏杆398m","方（扁）钢","踢腿板100*4",1,398000,100,4,null,null,{"v":82.784,"d":"82.78"},"无重合面",null,223,null,null,"31NM056-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台斜梯护栏43m","圆钢","圆钢 Q50*3",2,43000,50,{"$nulls":3},{"v":13.502,"d":"13.50"},"无重合面",null,224,null,null,"31NM056-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台斜梯护栏43m","方（扁）钢","扁铁40*4",2,43000,40,4,null,null,{"v":7.568,"d":"7.57"},"无重合面",null,225,null,null,"31NM056-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台斜梯护栏71m","圆钢","圆钢 Q50*3",2,71000,50,{"$nulls":3},{"v":22.294,"d":"22.29"},"无重合面",null,226,null,null,"31NM056-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台斜梯护栏71m","方（扁）钢","扁铁40*4",2,71000,40,4,null,null,{"v":12.496,"d":"12.50"},"无重合面",null,227,null,null,"31NM056-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台栏杆48m","圆钢","圆钢 Q50*3",2,48000,50,{"$nulls":3},{"v":15.072,"d":"15.07"},"无重合面",null,228,null,null,"31NM061-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台栏杆48m","方（扁）钢","扁铁40*4",2,48000,40,4,null,null,{"v":8.448,"d":"8.45"},"无重合面",null,229,null,null,"31NM061-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台栏杆48m","方（扁）钢","踢腿板100*4",1,48000,100,4,null,null,{"v":9.984,"d":"9.98"},"无重合面",null,230,null,null,"31NM061-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台一*5","[槽钢","[100*48*5.3",10,1200,null,48,5.3,5.3,{"v":1.6008,"d":"1.60"},"翼板重合",null,231,null,null,"31NM061-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台一*5","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,232,null,{"v":10,"d":"10.00"},"31NM061-2图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["电捕后风机前煤气阀门操作平台一*5","方（扁）钢","加强筋50*4",5,800,50,4,null,null,{"v":0.432,"d":"0.43"},"无重合面",null,233,null,null,"31NM061-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台一*5","[槽钢","[100*48*5.3",10,800,null,48,5.3,5.3,{"v":1.0672,"d":"1.07"},"翼板重合",null,234,null,null,"31NM061-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台支架一*5","L型钢","L75*75*6",2,1240,null,75,6,6,{"v":0.372,"d":"0.37"},"无重合面",null,235,null,null,"31NM061-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台支架一*5","[槽钢","[100*48*5.3",4,2540,null,48,5.3,5.3,{"v":1.843024,"d":"1.84"},"无重合面",null,236,null,null,"31NM061-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台支架一*5","[槽钢","[80*43*5",2,350,null,43,5,5,{"v":0.1134,"d":"0.11"},"无重合面",null,237,null,null,"31NM061-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台支架二*4","[槽钢","[100*48*5.3",8,610,null,48,5.3,5.3,{"v":0.885232,"d":"0.89"},"无重合面",null,238,null,null,"31NM061-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台支架二*4","[槽钢","[100*48*5.3",4,1640,null,48,5.3,5.3,{"v":1.189984,"d":"1.19"},"无重合面",null,239,null,null,"31NM061-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台二*1","[槽钢","[100*48*5.3",2,1200,null,48,5.3,5.3,{"v":0.32016,"d":"0.32"},"翼板重合",null,240,null,null,"31NM061-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台二*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,241,null,{"v":3.8,"d":"3.80"},"31NM061-3图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["电捕后风机前煤气阀门操作平台二*1","方（扁）钢","加强筋60*6",1,2800,60,6,null,null,{"v":0.3696,"d":"0.37"},"无重合面",null,242,null,null,"31NM061-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台二*1","[槽钢","[100*48*5.3",2,1600,null,48,5.3,5.3,{"v":0.42688,"d":"0.43"},"翼板重合",null,243,null,null,"31NM061-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=5300直梯*3","L型钢","L63*63*6",6,6580,null,63,6,6,{"v":4.97448,"d":"4.97"},"无重合面",null,244,null,null,"31NM061-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=5300直梯*3","方（扁）钢","扁铁40*4",18,1840,40,4,null,null,{"v":2.91456,"d":"2.91"},"无重合面",null,245,null,null,"31NM061-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=5300直梯*3","方（扁）钢","扁铁25*4",15,4570,25,4,null,null,{"v":3.9759,"d":"3.98"},"无重合面",null,246,null,null,"31NM061-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=5300直梯*3","圆钢","圆钢Q18",54,480,18,{"$nulls":3},{"v":1.4649984,"d":"1.46"},"无重合面",null,247,null,null,"31NM061-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=5300直梯*3","圆钢","圆钢Q18",6,1366,18,{"$nulls":3},{"v":0.46323792,"d":"0.46"},"无重合面",null,248,null,null,"31NM061-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台三*1","[槽钢","[100*48*5.3",3,1600,null,48,5.3,5.3,{"v":0.64032,"d":"0.64"},"翼板重合",null,249,null,null,"31NM061-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台三*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,250,null,{"v":6.4,"d":"6.40"},"31NM061-4图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["电捕后风机前煤气阀门操作平台三*1","方（扁）钢","加强筋40*4",2,1000,40,4,null,null,{"v":0.176,"d":"0.18"},"无重合面",null,251,null,null,"31NM061-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台三*1","[槽钢","[100*48*5.3",2,2000,null,48,5.3,5.3,{"v":0.5336,"d":"0.53"},"翼板重合",null,252,null,null,"31NM061-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=2500直梯*5","L型钢","L63*63*6",10,3780,null,63,6,6,{"v":4.7628,"d":"4.76"},"无重合面",null,253,null,null,"31NM061-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=2500直梯*5","方（扁）钢","扁铁40*4",15,1840,40,4,null,null,{"v":2.4288,"d":"2.43"},"无重合面",null,254,null,null,"31NM061-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=2500直梯*5","方（扁）钢","扁铁25*4",25,1770,25,4,null,null,{"v":2.5665,"d":"2.57"},"无重合面",null,255,null,null,"31NM061-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=2500直梯*5","圆钢","圆钢Q18",40,480,18,{"$nulls":3},{"v":1.085184,"d":"1.09"},"无重合面",null,256,null,null,"31NM061-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台KH1=2500直梯*5","圆钢","圆钢Q18",10,1366,18,{"$nulls":3},{"v":0.7720632000000001,"d":"0.77"},"无重合面",null,257,null,null,"31NM061-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台四*1","[槽钢","[100*48*5.3",2,1200,null,48,5.3,5.3,{"v":0.32016,"d":"0.32"},"翼板重合",null,258,null,null,"31NM061-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台四*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,259,null,{"v":10,"d":"10.00"},"31NM061-5图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["电捕后风机前煤气阀门操作平台四*1","方（扁）钢","加强筋40*4",1,4200,40,4,null,null,{"v":0.3696,"d":"0.37"},"无重合面",null,260,null,null,"31NM061-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台四*1","方（扁）钢","加强筋40*4",8,600,40,4,null,null,{"v":0.4224,"d":"0.42"},"无重合面",null,261,null,null,"31NM061-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台四*1","[槽钢","[100*48*5.3",2,4200,null,48,5.3,5.3,{"v":1.12056,"d":"1.12"},"翼板重合",null,262,null,null,"31NM061-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台五*1","[槽钢","[100*48*5.3",2,1200,null,48,5.3,5.3,{"v":0.32016,"d":"0.32"},"翼板重合",null,263,null,null,"31NM061-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台五*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,264,null,7.68,"31NM061-5图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["电捕后风机前煤气阀门操作平台五*1","方（扁）钢","加强筋40*4",2,1186,40,4,null,null,{"v":0.208736,"d":"0.21"},"无重合面",null,265,null,null,"31NM061-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台五*1","方（扁）钢","加强筋40*4",3,990,40,4,null,null,{"v":0.26136,"d":"0.26"},"无重合面",null,266,null,null,"31NM061-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台五*1","[槽钢","[100*48*5.3",2,3000,null,48,5.3,5.3,{"v":0.8004,"d":"0.80"},"翼板重合",null,267,null,null,"31NM061-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台五*1","[槽钢","[100*48*5.3",1,1400,null,48,5.3,5.3,{"v":0.18676,"d":"0.19"},"翼板重合",null,268,null,null,"31NM061-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台支架三*4","[槽钢","[100*48*5.3",8,600,null,48,5.3,5.3,{"v":0.87072,"d":"0.87"},"无重合面",null,269,null,null,"31NM061-6","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台支架三*4","[槽钢","[100*48*5.3",4,1640,null,48,5.3,5.3,{"v":1.189984,"d":"1.19"},"无重合面",null,270,null,null,"31NM061-6","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台支架四*2","[槽钢","[100*48*5.3",4,350,null,48,5.3,5.3,{"v":0.25396,"d":"0.25"},"无重合面",null,271,null,null,"31NM061-6","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台支架四*2","[槽钢","[100*48*5.3",8,2540,null,48,5.3,5.3,{"v":3.686048,"d":"3.69"},"无重合面",null,272,null,null,"31NM061-6","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕后风机前煤气阀门操作平台支架四*2","L型钢","L75*75*6",4,1240,null,75,6,6,{"v":0.744,"d":"0.74"},"无重合面",null,273,null,null,"31NM061-6","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台AD=1100直梯*1","方（扁）钢","钢板60*8",2,3670,60,8,null,null,{"v":0.99824,"d":"1.00"},"无重合面",null,274,null,null,"31NM061-6","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["电捕煤气管道联合平台AD=1100直梯*1","圆钢","圆钢Q18",4,500,18,{"$nulls":3},{"v":0.11304,"d":"0.11"},"无重合面",null,275,null,null,"31NM061-6","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台45°斜梯T2B08a-41.5*2","[槽钢","[16b（160*63*6.5）",4,5860,null,63,6.5,6.5,{"v":5.60216,"d":"5.60"},"无重合面",null,276,null,null,"31NM062-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台45°斜梯T2B08a-41.5*2","方（扁）钢","花纹板4.5",40,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,277,null,21.12,"31NM062-1图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["冷凝液槽初冷器水封槽联合平台斜梯护栏11.8m*2","圆钢","圆钢 Q50*3",2,23600,50,{"$nulls":3},{"v":7.4104,"d":"7.41"},"无重合面",null,278,null,null,"31NM062-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台斜梯护栏11.8m*2","方（扁）钢","扁铁40*4",2,23600,40,4,null,null,{"v":4.1536,"d":"4.15"},"无重合面",null,279,null,null,"31NM062-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台栏杆57.9m","圆钢","圆钢 Q50*3",2,57900,50,{"$nulls":3},{"v":18.1806,"d":"18.18"},"无重合面",null,280,null,null,"31NM062-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台栏杆57.9m","方（扁）钢","扁铁40*4",2,57900,40,4,null,null,{"v":10.1904,"d":"10.19"},"无重合面",null,281,null,null,"31NM062-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台栏杆57.9m","方（扁）钢","踢腿板100*4",1,57900,100,4,null,null,{"v":12.0432,"d":"12.04"},"无重合面",null,282,null,null,"31NM062-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台立柱*6","圆钢","圆钢Q219",6,3800,219,{"$nulls":3},{"v":15.678648000000003,"d":"15.68"},"无重合面",null,283,null,null,"31NM061-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台立柱*6","[槽钢","[100*48*5.3",6,1040,null,48,5.3,5.3,{"v":1.131936,"d":"1.13"},"无重合面",null,284,null,null,"31NM061-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台平台*1","[槽钢","[140*60*8",1,50400,null,60,8,8,{"v":8.2656,"d":"8.27"},"翼板重合",null,285,null,null,"31NM061-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台平台*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,286,null,{"v":48.4,"d":"48.40"},"31NM061-2图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["冷凝液槽初冷器水封槽联合平台平台*1","方（扁）钢","加强筋40*4",29,986,40,4,null,null,{"v":2.516272,"d":"2.52"},"无重合面",null,287,null,null,"31NM061-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台AD=1100直梯*2","方（扁）钢","钢板60*8",4,3820,60,8,null,null,{"v":2.07808,"d":"2.08"},"无重合面",null,288,null,null,"31NM061-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台AD=1100直梯*2","圆钢","圆钢Q18",8,500,18,{"$nulls":3},{"v":0.22608,"d":"0.23"},"无重合面",null,289,null,null,"31NM061-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台三脚架*4","[槽钢","[100*48*5.3",4,780,null,48,5.3,5.3,{"v":0.565968,"d":"0.57"},"无重合面",null,290,null,null,"31NM061-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台三脚架*4","[槽钢","[100*48*5.3",4,890,null,48,5.3,5.3,{"v":0.645784,"d":"0.65"},"无重合面",null,291,null,null,"31NM061-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台二*2","[槽钢","[100*48*5.3",2,4900,null,48,5.3,5.3,{"v":1.30732,"d":"1.31"},"翼板重合",null,292,null,null,"31NM061-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台二*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,293,null,5.44,"31NM061-3图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["冷凝液槽初冷器水封槽联合平台二*2","方（扁）钢","加强筋40*4",2,836,40,4,null,null,{"v":0.147136,"d":"0.15"},"无重合面",null,294,null,null,"31NM061-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台31°斜梯T1B08a-39.1*2","[槽钢","[16b（160*63*6.5）",4,7700,null,63,6.5,6.5,{"v":7.3612,"d":"7.36"},"无重合面",null,295,null,null,"31NM055-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台31°斜梯T1B08a-39.1*2","方（扁）钢","花纹板4.5",66,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,296,null,{"v":34.848,"d":"34.85"},"31NM055-1-1图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["初冷器煤气管道联合平台43.5°斜梯T2B08a-58.1*2","[槽钢","[16b（160*63*6.5）",4,8400,null,63,6.5,6.5,{"v":8.0304,"d":"8.03"},"无重合面",null,297,null,null,"31NM055-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台43.5°斜梯T2B08a-58.1*2","方（扁）钢","花纹板4.5",60,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,298,null,31.68,"31NM055-1-1图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["初冷器煤气管道联合平台45°斜梯T2B08a-25.1*2","[槽钢","[16b（160*63*6.5）",4,3500,null,63,6.5,6.5,{"v":3.346,"d":"3.35"},"无重合面",null,299,null,null,"31NM055-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台45°斜梯T2B08a-25.1*2","方（扁）钢","花纹板4.5",24,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,300,null,{"v":12.672,"d":"12.67"},"31NM055-1-1图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["冷凝液槽初冷器水封槽联合平台AD=1000直梯*4","方（扁）钢","钢板60*8",8,3720,60,8,null,null,{"v":4.04736,"d":"4.05"},"无重合面",null,301,null,null,"31NM055-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台AD=1000直梯*4","圆钢","圆钢Q18",12,500,18,{"$nulls":3},{"v":0.33912,"d":"0.34"},"无重合面",null,302,null,null,"31NM055-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台AD=1200直梯*8","方（扁）钢","钢板60*8",16,3920,60,8,null,null,{"v":8.52992,"d":"8.53"},"无重合面",null,303,null,null,"31NM055-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["冷凝液槽初冷器水封槽联合平台AD=1200直梯*8","圆钢","圆钢Q18",32,500,18,{"$nulls":3},{"v":0.90432,"d":"0.90"},"无重合面",null,304,null,null,"31NM055-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台KH1=2200直梯*2","L型钢","L63*63*6",4,3480,null,63,6,6,{"v":1.75392,"d":"1.75"},"无重合面",null,305,null,null,"31NM055-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台KH1=2200直梯*2","方（扁）钢","扁铁40*4",15,1840,40,4,null,null,{"v":2.4288,"d":"2.43"},"无重合面",null,306,null,null,"31NM055-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台KH1=2200直梯*2","方（扁）钢","扁铁25*4",15,1470,25,4,null,null,{"v":1.2789,"d":"1.28"},"无重合面",null,307,null,null,"31NM055-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台KH1=2200直梯*2","圆钢","圆钢Q18",14,480,18,{"$nulls":3},{"v":0.3798144,"d":"0.38"},"无重合面",null,308,null,null,"31NM055-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台KH1=2200直梯*2","圆钢","圆钢Q18",4,1366,18,{"$nulls":3},{"v":0.30882528000000004,"d":"0.31"},"无重合面",null,309,null,null,"31NM055-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支座*108","[槽钢","[100*48*5.3",108,140,null,48,5.3,5.3,{"v":2.742768,"d":"2.74"},"无重合面",null,310,null,null,"31NM055-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台三脚架*12","[槽钢","[100*48*5.3",12,1390,null,48,5.3,5.3,{"v":3.025752,"d":"3.03"},"无重合面",null,311,null,null,"31NM055-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台三脚架*12","[槽钢","[100*48*5.3",12,1679,null,48,5.3,5.3,{"v":3.6548472000000003,"d":"3.65"},"无重合面",null,312,null,null,"31NM055-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台45°斜梯T2B08a-28.9*6","[槽钢","[16b（160*63*6.5）",12,4100,null,63,6.5,6.5,{"v":11.7588,"d":"11.76"},"无重合面",null,313,null,null,"31NM055-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台45°斜梯T2B08a-28.9*6","方（扁）钢","花纹板4.5",84,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,314,null,{"v":44.352,"d":"44.35"},"31NM055-1-1图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["初冷器煤气管道联合平台54.2°斜梯T3B06a-41.1*4","[槽钢","[16b（160*63*6.5）",8,5070,null,63,6.5,6.5,{"v":9.69384,"d":"9.69"},"无重合面",null,315,null,null,"31NM055-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台54.2°斜梯T3B06a-41.1*4","方（扁）钢","花纹板4.5",60,600,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,316,null,23.76,"31NM055-1-1图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["初冷器煤气管道联合平台60.6°斜梯T3B06a-51.4*2","[槽钢","[16b（160*63*6.5）",4,8300,null,63,6.5,6.5,{"v":7.9348,"d":"7.93"},"无重合面",null,317,null,null,"31NM055-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台60.6°斜梯T3B06a-51.4*2","方（扁）钢","花纹板4.5",30,600,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,318,null,11.88,"31NM055-1-1图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["初冷器煤气管道联合平台40°斜梯T1B06a-18.9*2","[槽钢","[16b（160*63*6.5）",4,2950,null,63,6.5,6.5,{"v":2.8202,"d":"2.82"},"无重合面",null,319,null,null,"31NM055-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台40°斜梯T1B06a-18.9*2","方（扁）钢","花纹板4.5",22,600,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,320,null,{"v":8.712,"d":"8.71"},"31NM055-1-1图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["初冷器煤气管道联合平台45°斜梯T2B08a-17*2","[槽钢","[16b（160*63*6.5）",4,2400,null,63,6.5,6.5,{"v":2.2944,"d":"2.29"},"无重合面",null,321,null,null,"31NM055-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台45°斜梯T2B08a-17*2","方（扁）钢","花纹板4.5",16,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,322,null,{"v":8.448,"d":"8.45"},"31NM055-1-1图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["初冷器煤气管道联合平台槽钢梁37-0*54","[槽钢","[140*60*8",54,4990,null,60,8,8,{"v":60.35904,"d":"60.36"},"无重合面",null,323,null,null,"31NM055-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台45°斜梯T2B08a-28.9*4","[槽钢","[16b（160*63*6.5）",8,4100,null,63,6.5,6.5,{"v":7.8392,"d":"7.84"},"无重合面",null,324,null,null,"31NM055-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台45°斜梯T2B08a-28.9*4","方（扁）钢","花纹板4.5",56,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,325,null,{"v":29.568,"d":"29.57"},"31NM055-1-1图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["初冷器煤气管道联合平台栏杆1200m","圆钢","圆钢 Q50*3",2,1200000,50,{"$nulls":3},{"v":376.8,"d":"376.80"},"无重合面",null,326,null,null,"31NM062-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台栏杆1200m","方（扁）钢","扁铁40*4",2,1200000,40,4,null,null,{"v":211.2,"d":"211.20"},"无重合面",null,327,null,null,"31NM062-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台栏杆1200m","方（扁）钢","踢腿板100*4",1,1200000,100,4,null,null,{"v":249.6,"d":"249.60"},"无重合面",null,328,null,null,"31NM062-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台45斜梯护栏142m","圆钢","圆钢 Q50*3",2,142000,50,{"$nulls":3},{"v":44.588,"d":"44.59"},"无重合面",null,329,null,null,"31NM056-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台45斜梯护栏142m","方（扁）钢","扁铁40*4",2,142000,40,4,null,null,{"v":24.992,"d":"24.99"},"无重合面",null,330,null,null,"31NM056-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台35.5斜梯护栏38m","圆钢","圆钢 Q50*3",2,38000,50,{"$nulls":3},{"v":11.932,"d":"11.93"},"无重合面",null,331,null,null,"31NM056-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台35.5斜梯护栏38m","方（扁）钢","扁铁40*4",2,38000,40,4,null,null,{"v":6.688,"d":"6.69"},"无重合面",null,332,null,null,"31NM056-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台59斜梯护栏65m","圆钢","圆钢 Q50*3",1,65000,50,{"$nulls":3},{"v":10.205,"d":"10.21"},"无重合面",null,333,null,null,"31NM055-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台59斜梯护栏65m","圆钢","圆钢 Q33.5",108,558,33.5,{"$nulls":3},{"v":6.33917016,"d":"6.34"},"无重合面",null,334,null,null,"31NM055-1-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台KH1=3200直梯*7","L型钢","L63*63*6",14,4480,null,63,6,6,{"v":7.90272,"d":"7.90"},"无重合面",null,335,null,null,"31NM055-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台KH1=3200直梯*7","方（扁）钢","扁铁40*4",28,1840,40,4,null,null,{"v":4.53376,"d":"4.53"},"无重合面",null,336,null,null,"31NM055-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台KH1=3200直梯*7","方（扁）钢","扁铁25*4",35,2460,25,4,null,null,{"v":4.9938,"d":"4.99"},"无重合面",null,337,null,null,"31NM055-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台KH1=3200直梯*7","圆钢","圆钢Q18",77,480,18,{"$nulls":3},{"v":2.0889792000000003,"d":"2.09"},"无重合面",null,338,null,null,"31NM055-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台KH1=3200直梯*7","圆钢","圆钢Q18",14,1366,18,{"$nulls":3},{"v":1.08088848,"d":"1.08"},"无重合面",null,339,null,null,"31NM055-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台KH1=3700直梯*2","L型钢","L63*63*6",4,4984,null,63,6,6,{"v":2.511936,"d":"2.51"},"无重合面",null,340,null,null,"31NM055-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台KH1=3700直梯*2","方（扁）钢","扁铁40*4",8,1840,40,4,null,null,{"v":1.29536,"d":"1.30"},"无重合面",null,341,null,null,"31NM055-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台KH1=3700直梯*2","方（扁）钢","扁铁25*4",35,2970,25,4,null,null,{"v":6.0291,"d":"6.03"},"无重合面",null,342,null,null,"31NM055-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台KH1=3700直梯*2","圆钢","圆钢Q18",24,480,18,{"$nulls":3},{"v":0.6511104,"d":"0.65"},"无重合面",null,343,null,null,"31NM055-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台KH1=3700直梯*2","圆钢","圆钢Q18",4,1366,18,{"$nulls":3},{"v":0.30882528000000004,"d":"0.31"},"无重合面",null,344,null,null,"31NM055-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台矩形平台二*6","[槽钢","[100*48*5.3",6,11200,null,48,5.3,5.3,{"v":8.96448,"d":"8.96"},"翼板重合",null,345,null,null,"31NM055-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台矩形平台二*6","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,346,null,46.08,"31NM055-3图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["初冷器煤气管道联合平台矩形平台二*6","方（扁）钢","加强筋50*4",12,786,50,4,null,null,{"v":1.018656,"d":"1.02"},"无重合面",null,347,null,null,"31NM055-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架一*2","L型钢","L75*75*6",4,840,null,75,6,6,{"v":0.504,"d":"0.50"},"无重合面",null,348,null,null,"31NM055-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架一*2","[槽钢","[80*43*5",4,150,null,43,5,5,{"v":0.0972,"d":"0.10"},"无重合面",null,349,null,null,"31NM055-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架四*23","L型钢","L75*75*6",46,840,null,75,6,6,{"v":5.796,"d":"5.80"},"无重合面",null,350,null,null,"31NM055-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架四*23","[槽钢","[80*43*5",46,2135,null,43,5,5,{"v":15.91002,"d":"15.91"},"无重合面",null,351,null,null,"31NM055-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十七*24","L型钢","L75*75*6",48,840,null,75,6,6,{"v":6.048,"d":"6.05"},"无重合面",null,352,null,null,"31NM055-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十七*24","[槽钢","[80*43*5",48,350,null,43,5,5,{"v":2.7216,"d":"2.72"},"无重合面",null,353,null,null,"31NM055-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架二*4","L型钢","L75*75*6",4,840,null,75,6,6,{"v":0.504,"d":"0.50"},"无重合面",null,354,null,null,"31NM055-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架二*4","[槽钢","[80*43*5",4,7184,null,43,5,5,{"v":4.655232,"d":"4.66"},"无重合面",null,355,null,null,"31NM055-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架二*4","[槽钢","[100*48*5.3",8,2840,null,48,5.3,5.3,{"v":4.121408,"d":"4.12"},"无重合面",null,356,null,null,"31NM055-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架二*4","[槽钢","[100*48*5.3",16,1835,null,48,5.3,5.3,{"v":5.325904,"d":"5.33"},"无重合面",null,357,null,null,"31NM055-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架三*4","[槽钢","[80*43*5",8,650,null,43,5,5,{"v":0.8424,"d":"0.84"},"无重合面",null,358,null,null,"31NM055-6","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架三*4","[槽钢","[100*48*5.3",8,3835,null,48,5.3,5.3,{"v":5.565352,"d":"5.57"},"无重合面",null,359,null,null,"31NM055-6","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架三*4","[槽钢","[100*48*5.3",8,1980,null,48,5.3,5.3,{"v":2.873376,"d":"2.87"},"无重合面",null,360,null,null,"31NM055-6","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架三*4","[槽钢","[100*48*5.3",8,4086,null,48,5.3,5.3,{"v":5.9296032,"d":"5.93"},"无重合面",null,361,null,null,"31NM055-6","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架五*7","[槽钢","[100*48*5.3",14,2150,null,48,5.3,5.3,{"v":5.46014,"d":"5.46"},"无重合面",null,362,null,null,"31NM055-7","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架五*7","[槽钢","[100*48*5.3",14,2405,null,48,5.3,5.3,{"v":6.107738,"d":"6.11"},"无重合面",null,363,null,null,"31NM055-7","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架五*7","[槽钢","[100*48*5.3",14,2435,null,48,5.3,5.3,{"v":6.183926,"d":"6.18"},"无重合面",null,364,null,null,"31NM055-7","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架六*2","[槽钢","[100*48*5.3",4,1540,null,48,5.3,5.3,{"v":1.117424,"d":"1.12"},"无重合面",null,365,null,null,"31NM055-8","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架六*2","[槽钢","[100*48*5.3",4,2610,null,48,5.3,5.3,{"v":1.893816,"d":"1.89"},"无重合面",null,366,null,null,"31NM055-8","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架六*2","[槽钢","[100*48*5.3",4,2440,null,48,5.3,5.3,{"v":1.770464,"d":"1.77"},"无重合面",null,367,null,null,"31NM055-8","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架六*2","[槽钢","[80*43*5",4,400,null,43,5,5,{"v":0.2592,"d":"0.26"},"无重合面",null,368,null,null,"31NM055-8","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架七*1","[槽钢","[100*48*5.3",2,1440,null,48,5.3,5.3,{"v":0.522432,"d":"0.52"},"无重合面",null,369,null,null,"31NM055-8","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架七*1","[槽钢","[100*48*5.3",2,2435,null,48,5.3,5.3,{"v":0.883418,"d":"0.88"},"无重合面",null,370,null,null,"31NM055-8","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架七*1","[槽钢","[80*43*5",2,750,null,43,5,5,{"v":0.243,"d":"0.24"},"无重合面",null,371,null,null,"31NM055-8","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架八*1","L型钢","L75*75*6",2,840,null,75,6,6,{"v":0.252,"d":"0.25"},"无重合面",null,372,null,null,"31NM055-9","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架八*1","[槽钢","[100*48*5.3",2,2190,null,48,5.3,5.3,{"v":0.794532,"d":"0.79"},"无重合面",null,373,null,null,"31NM055-9","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架九*1","L型钢","L75*75*6",2,840,null,75,6,6,{"v":0.252,"d":"0.25"},"无重合面",null,374,null,null,"31NM055-9","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架九*1","[槽钢","[100*48*5.3",2,2025,null,48,5.3,5.3,{"v":0.73467,"d":"0.73"},"无重合面",null,375,null,null,"31NM055-9","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十*7","[槽钢","[100*48*5.3",7,4640,null,48,5.3,5.3,{"v":5.891872,"d":"5.89"},"无重合面",null,376,null,null,"31NM055-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十*7","[槽钢","[100*48*5.3",28,4330,null,48,5.3,5.3,{"v":21.992936,"d":"21.99"},"无重合面",null,377,null,null,"31NM055-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十*7","L型钢","L50*50*5",7,28600,null,50,5,5,20.02,"无重合面",null,378,null,null,"31NM055-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十一*17","L型钢","L75*75*6",34,840,null,75,6,6,{"v":4.284,"d":"4.28"},"无重合面",null,379,null,null,"31NM055-11","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十一*17","[槽钢","[100*48*5.3",34,4135,null,48,5.3,5.3,{"v":25.503026,"d":"25.50"},"无重合面",null,380,null,null,"31NM055-11","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十六*4","L型钢","L75*75*6",8,840,null,75,6,6,{"v":1.008,"d":"1.01"},"无重合面",null,381,null,null,"31NM055-12","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十六*4","[槽钢","[100*48*5.3",8,1535,null,48,5.3,5.3,{"v":2.227592,"d":"2.23"},"无重合面",null,382,null,null,"31NM055-12","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十二*16","L型钢","L50*50*5",16,19400,null,50,5,5,31.04,"无重合面",null,383,null,null,"31NM055-12","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十二*16","[槽钢","[100*48*5.3",16,4640,null,48,5.3,5.3,{"v":13.467136,"d":"13.47"},"无重合面",null,384,null,null,"31NM055-12","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十二*16","[槽钢","[100*48*5.3",64,3330,null,48,5.3,5.3,{"v":38.659968,"d":"38.66"},"无重合面",null,385,null,null,"31NM055-12","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十三*2","L型钢","L75*75*6",4,840,null,75,6,6,{"v":0.504,"d":"0.50"},"无重合面",null,386,null,null,"31NM055-13","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十三*2","[槽钢","[100*48*5.3",4,4238,null,48,5.3,5.3,{"v":3.0750928,"d":"3.08"},"无重合面",null,387,null,null,"31NM055-13","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十四*4","[槽钢","[100*48*5.3",8,1535,null,48,5.3,5.3,{"v":2.227592,"d":"2.23"},"无重合面",null,388,null,null,"31NM055-14","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十四*4","L型钢","L75*75*6",8,1540,null,75,6,6,{"v":1.848,"d":"1.85"},"无重合面",null,389,null,null,"31NM055-14","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十四*4","[槽钢","[100*48*5.3",4,1034,null,48,5.3,5.3,{"v":0.7502704,"d":"0.75"},"无重合面",null,390,null,null,"31NM055-14","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十五*2","[槽钢","[100*48*5.3",4,2235,null,48,5.3,5.3,{"v":1.621716,"d":"1.62"},"无重合面",null,391,null,null,"31NM055-14","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台支架十五*2","L型钢","L75*75*6",4,840,null,75,6,6,{"v":0.504,"d":"0.50"},"无重合面",null,392,null,null,"31NM055-14","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台矩形平台一*21","[槽钢","[100*48*5.3",21,10000,null,48,5.3,5.3,{"v":28.014,"d":"28.01"},"翼板重合",null,393,null,null,"31NM055-15","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台矩形平台一*21","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,394,null,{"v":142.8,"d":"142.80"},"31NM055-15图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["初冷器煤气管道联合平台矩形平台一*21","方（扁）钢","加强筋50*4",42,786,50,4,null,null,{"v":3.565296,"d":"3.57"},"无重合面",null,395,null,null,"31NM055-15","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台+40900*7","[槽钢","[100*48*5.3",7,5600,null,48,5.3,5.3,{"v":5.22928,"d":"5.23"},"翼板重合",null,396,null,null,"31NM055-15","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台+40900*7","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,397,null,22.68,"31NM055-15图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["初冷器煤气管道联合平台+40900*7","[槽钢","[100*48*5.3",14,939,null,48,5.3,5.3,{"v":2.3846844,"d":"2.38"},"无重合面",null,398,null,null,"31NM055-15","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台悬臂架*23","[槽钢","[126*53*5.5",23,1525,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":7.050075,"d":"7.05"},"无重合面",null,399,null,null,"31NM055-15","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台+7200-9400-11300-13000","[槽钢","[100*48*5.3",1,470000,null,48,5.3,5.3,{"v":62.698,"d":"62.70"},"翼板重合",null,400,null,null,"31NM055-16","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台+7200-9400-11300-13000","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,401,null,{"v":224,"d":"224.00"},"31NM055-16图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["初冷器煤气管道联合平台+7200-9400-11300-13000","方（扁）钢","加强筋50*4",1,112000,50,4,null,null,{"v":12.096,"d":"12.10"},"无重合面",null,402,null,null,"31NM055-16","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台+15000-28800-35800","[槽钢","[100*48*5.3",1,161000,null,48,5.3,5.3,{"v":21.4774,"d":"21.48"},"翼板重合",null,403,null,null,"31NM055-17","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["初冷器煤气管道联合平台+15000-28800-35800","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,404,null,{"v":156,"d":"156.00"},"31NM055-17图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["初冷器煤气管道联合平台+15000-28800-35800","方（扁）钢","加强筋50*4",1,63000,50,4,null,null,{"v":6.804,"d":"6.80"},"无重合面",null,405,null,null,"31NM055-17","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台","其他",{"$nulls":7},"需手动计算","无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"$error":"#VALUE!"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台栏杆206m","圆钢","圆钢 Q50*3",2,206000,50,{"$nulls":3},{"v":64.684,"d":"64.68"},"无重合面",null,405,null,{"v":64.684,"d":"64.68"},"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台栏杆206m","方（扁）钢","扁铁40*4",2,206000,40,4,null,null,{"v":36.256,"d":"36.26"},"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台栏杆206m","方（扁）钢","踢腿板100*4",1,206000,100,4,null,null,{"v":42.848,"d":"42.85"},"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台45°斜梯T2B08a-10*2","[槽钢","[16b（160*63*6.5）",4,1400,null,63,6.5,6.5,{"v":1.3384,"d":"1.34"},"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台45°斜梯T2B08a-10*2","方（扁）钢","花纹板4.5",10,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,405,null,5.28,"31NM057-1-1图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台45斜梯护栏5.7m","圆钢","圆钢 Q50*3",2,5700,50,{"$nulls":3},{"v":1.7898,"d":"1.79"},"无重合面",null,405,null,{"v":1.7898,"d":"1.79"},"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台45斜梯护栏5.7m","方（扁）钢","扁铁40*4",2,5700,40,4,null,null,{"v":1.0032,"d":"1.00"},"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台45°斜梯T2B08a-14*1","[槽钢","[16b（160*63*6.5）",2,2000,null,63,6.5,6.5,{"v":0.956,"d":"0.96"},"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台45°斜梯T2B08a-14*1","方（扁）钢","花纹板4.5",14,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":7.392,"d":"7.39"},"31NM057-1-1图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台45斜梯护栏4m","圆钢","圆钢 Q50*3",2,4000,50,{"$nulls":3},{"v":1.256,"d":"1.26"},"无重合面",null,405,null,{"v":1.256,"d":"1.26"},"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台45斜梯护栏4m","方（扁）钢","扁铁40*4",2,4000,40,4,null,null,{"v":0.704,"d":"0.70"},"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台罐顶平台护栏246m","圆钢","圆钢 Q50*3",2,246000,50,{"$nulls":3},{"v":77.244,"d":"77.24"},"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台罐顶平台护栏246m","方（扁）钢","扁铁40*4",2,246000,40,4,null,null,{"v":43.296,"d":"43.30"},"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台罐顶平台护栏246m","方（扁）钢","踢腿板100*4",1,246000,100,4,null,null,{"v":51.168,"d":"51.17"},"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台盘梯护栏40m","圆钢","圆钢 Q50*3",2,40000,50,{"$nulls":3},12.56,"无重合面",null,405,null,12.56,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台盘梯护栏40m","方（扁）钢","扁铁40*4",2,40000,40,4,null,null,7.04,"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","方（扁）钢","外侧板160*8",2,6050,160,8,null,null,{"v":4.0656,"d":"4.07"},"无重合面",null,405,null,null,"31NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","方（扁）钢","内侧板160*8",2,5670,160,8,null,null,{"v":3.81024,"d":"3.81"},"无重合面",null,405,null,null,"31NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","L型钢","L63*63*6",2,2500,null,63,6,6,0.63,"无重合面",null,405,null,null,"31NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,405,null,null,"31NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","方（扁）钢","踏板",36,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":19.008,"d":"19.01"},"31NM057-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","方（扁）钢","外侧板160*8",2,6643,160,8,null,null,{"v":4.464096,"d":"4.46"},"无重合面",null,405,null,null,"31NM057-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","方（扁）钢","内侧板160*8",2,6220,160,8,null,null,{"v":4.17984,"d":"4.18"},"无重合面",null,405,null,null,"31NM057-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","L型钢","L63*63*6",2,2500,null,63,6,6,0.63,"无重合面",null,405,null,null,"31NM057-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,405,null,null,"31NM057-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","方（扁）钢","踏板",40,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,405,null,21.12,"31NM057-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台罐顶支架一*72","L型钢","L75*75*6",72,1740,null,75,6,6,{"v":18.792,"d":"18.79"},"无重合面",null,405,null,null,"31NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台罐顶支架二*4","L型钢","L100*100*6",4,840,null,100,6,6,{"v":0.672,"d":"0.67"},"无重合面",null,405,null,null,"31NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台罐顶支架二*4","[槽钢","[100*48*5.3",8,925,null,48,5.3,5.3,{"v":1.34236,"d":"1.34"},"无重合面",null,405,null,null,"31NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台罐顶支架三*2","L型钢","L100*100*6",2,840,null,100,6,6,{"v":0.336,"d":"0.34"},"无重合面",null,405,null,null,"31NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台罐顶支架三*2","[槽钢","[100*48*5.3",4,1125,null,48,5.3,5.3,{"v":0.8163,"d":"0.82"},"无重合面",null,405,null,null,"31NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台罐顶支架四*2","L型钢","L75*75*6",2,1800,null,75,6,6,0.54,"无重合面",null,405,null,null,"31NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台罐顶支架四*2","L型钢","L100*100*6",2,1605,null,100,6,6,{"v":0.642,"d":"0.64"},"无重合面",null,405,null,null,"31NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台一*1","[槽钢","[100*48*5.3",1,30700,null,48,5.3,5.3,{"v":4.09538,"d":"4.10"},"翼板重合",null,405,null,null,"31NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台一*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":23.4,"d":"23.40"},"31NM057-5图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台一*1","方（扁）钢","加强筋40*4",16,786,40,4,null,null,{"v":1.106688,"d":"1.11"},"无重合面",null,405,null,null,"31NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台四*1","[槽钢","[100*48*5.3",1,24300,null,48,5.3,5.3,{"v":3.24162,"d":"3.24"},"翼板重合",null,405,null,null,"31NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台四*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,17.94,"31NM057-5图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台四*1","方（扁）钢","加强筋40*4",12,786,40,4,null,null,{"v":0.830016,"d":"0.83"},"无重合面",null,405,null,null,"31NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台四*1","方（扁）钢","加强筋40*4",2,770,40,4,null,null,{"v":0.13552,"d":"0.14"},"无重合面",null,405,null,null,"31NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台四*1","方（扁）钢","加强筋40*4",1,1300,40,4,null,null,{"v":0.1144,"d":"0.11"},"无重合面",null,405,null,null,"31NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台三*1","[槽钢","[100*48*5.3",1,23900,null,48,5.3,5.3,{"v":3.18826,"d":"3.19"},"翼板重合",null,405,null,null,"31NM057-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台三*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":16.6,"d":"16.60"},"31NM057-6图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台三*1","方（扁）钢","加强筋40*4",11,786,40,4,null,null,{"v":0.760848,"d":"0.76"},"无重合面",null,405,null,null,"31NM057-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台五*1","[槽钢","[100*48*5.3",1,29600,null,48,5.3,5.3,{"v":3.94864,"d":"3.95"},"翼板重合",null,405,null,null,"31NM057-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台五*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":23.6,"d":"23.60"},"31NM057-6图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台五*1","方（扁）钢","加强筋40*4",20,786,40,4,null,null,{"v":1.38336,"d":"1.38"},"无重合面",null,405,null,null,"31NM057-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台二*2","[槽钢","[100*48*5.3",2,10400,null,48,5.3,5.3,{"v":2.77472,"d":"2.77"},"翼板重合",null,405,null,null,"31NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台二*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,10.92,"31NM057-7图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台二*2","方（扁）钢","加强筋40*4",6,786,40,4,null,null,{"v":0.415008,"d":"0.42"},"无重合面",null,405,null,null,"31NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台六*2","[槽钢","[100*48*5.3",2,10200,null,48,5.3,5.3,{"v":2.72136,"d":"2.72"},"翼板重合",null,405,null,null,"31NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台六*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":15,"d":"15.00"},"31NM057-7图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台六*2","方（扁）钢","加强筋40*4",10,786,40,4,null,null,{"v":0.69168,"d":"0.69"},"无重合面",null,405,null,null,"31NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台七*1","[槽钢","[100*48*5.3",1,36400,null,48,5.3,5.3,{"v":4.85576,"d":"4.86"},"翼板重合",null,405,null,null,"31NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台七*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":27.8,"d":"27.80"},"31NM057-7图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台七*1","方（扁）钢","加强筋40*4",18,786,40,4,null,null,{"v":1.245024,"d":"1.25"},"无重合面",null,405,null,null,"31NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台七*1","方（扁）钢","加强筋40*4",2,770,40,4,null,null,{"v":0.13552,"d":"0.14"},"无重合面",null,405,null,null,"31NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台七*1","方（扁）钢","加强筋40*4",1,1300,40,4,null,null,{"v":0.1144,"d":"0.11"},"无重合面",null,405,null,null,"31NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台九*2","[槽钢","[140*58*6",2,8950,null,58,6,6,{"v":2.8998,"d":"2.90"},"翼板重合",null,405,null,null,"31NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台九*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,15.68,"31NM057-8图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台九*2","L型钢","L50*50*5",1,1209,null,50,5,5,{"v":0.1209,"d":"0.12"},"无重合面",null,405,null,{"v":0.09672,"d":"0.10"},"31NM057-8","一般性腐蚀","环氧富锌漆",{"v":0.444444444444444,"d":"44%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台九*2","L型钢","L50*50*5",2,1386,null,50,5,5,{"v":0.2772,"d":"0.28"},"无重合面",null,405,null,null,"31NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十*1","[槽钢","[100*48*5.3",1,7250,null,48,5.3,5.3,{"v":0.96715,"d":"0.97"},"翼板重合",null,405,null,null,"31NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,5.82,"31NM057-8图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十*1","方（扁）钢","加强筋40*4",3,1186,40,4,null,null,{"v":0.313104,"d":"0.31"},"无重合面",null,405,null,null,"31NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十一*1","[槽钢","[100*48*5.3",1,6220,null,48,5.3,5.3,{"v":0.829748,"d":"0.83"},"翼板重合",null,405,null,null,"31NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十一*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,3.14,"31NM057-8图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十二*1","[槽钢","[100*48*5.3",1,13100,null,48,5.3,5.3,{"v":1.74754,"d":"1.75"},"翼板重合",null,405,null,null,"31NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十二*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,7.72,"31NM057-8图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十二*1","方（扁）钢","加强筋40*4",1,836,40,4,null,null,{"v":0.073568,"d":"0.07"},"无重合面",null,405,null,null,"31NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十二*1","方（扁）钢","加强筋40*4",2,1186,40,4,null,null,{"v":0.208736,"d":"0.21"},"无重合面",null,405,null,null,"31NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十三*1","[槽钢","[100*48*5.3",1,17600,null,48,5.3,5.3,{"v":2.34784,"d":"2.35"},"翼板重合",null,405,null,null,"31NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十三*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":13.8,"d":"13.80"},"31NM057-9图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十三*1","L型钢","L50*50*5",3,1386,null,50,5,5,{"v":0.4158,"d":"0.42"},"无重合面",null,405,null,null,"31NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十四*1","[槽钢","[100*48*5.3",1,10700,null,48,5.3,5.3,{"v":1.42738,"d":"1.43"},"翼板重合",null,405,null,null,"31NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十四*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":12.4,"d":"12.40"},"31NM057-9图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十四*1","方（扁）钢","加强筋40*4",1,4000,40,4,null,null,{"v":0.352,"d":"0.35"},"无重合面",null,405,null,null,"31NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十四*1","[槽钢","[100*48*5.3",1,7800,null,48,5.3,5.3,{"v":1.04052,"d":"1.04"},"翼板重合",null,405,null,null,"31NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十五*1","[槽钢","[100*48*5.3",1,10120,null,48,5.3,5.3,{"v":1.350008,"d":"1.35"},"翼板重合",null,405,null,null,"31NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十五*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,7.82,"31NM057-9图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十五*1","L型钢","L50*50*5",3,1186,null,50,5,5,{"v":0.3558,"d":"0.36"},"无重合面",null,405,null,null,"31NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十六*1","[槽钢","[100*48*5.3",1,17100,null,48,5.3,5.3,{"v":2.28114,"d":"2.28"},"翼板重合",null,405,null,null,"31NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十六*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,13.84,"31NM057-9图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十六*1","L型钢","L50*50*5",4,1286,null,50,5,5,{"v":0.5144,"d":"0.51"},"无重合面",null,405,null,null,"31NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台悬臂梁二*13","[槽钢","[126*53*5.5",13,1320,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":3.44916,"d":"3.45"},"无重合面",null,405,null,null,"31NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台罐顶平台支架三*2","[槽钢","[100*48*5.3",4,725,null,48,5.3,5.3,{"v":0.52606,"d":"0.53"},"无重合面",null,405,null,null,"31NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台罐顶平台支架三*2","L型钢","L100*100*6",2,840,null,100,6,6,{"v":0.336,"d":"0.34"},"无重合面",null,405,null,null,"31NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台罐顶平台支架四*2","[槽钢","[100*48*5.3",4,685,null,48,5.3,5.3,{"v":0.497036,"d":"0.50"},"无重合面",null,405,null,null,"31NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台罐顶平台支架四*2","L型钢","L100*100*6",2,840,null,100,6,6,{"v":0.336,"d":"0.34"},"无重合面",null,405,null,null,"31NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台八*2","[槽钢","[100*48*5.3",2,7120,null,48,5.3,5.3,{"v":1.899616,"d":"1.90"},"翼板重合",null,405,null,null,"31NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台八*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,10.52,"31NM057-10图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台八*2","方（扁）钢","加强筋40*4",6,1036,40,4,null,null,{"v":0.547008,"d":"0.55"},"无重合面",null,405,null,null,"31NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台三角架一*4","[槽钢","[126*53*5.5",4,1490,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.19796,"d":"1.20"},"无重合面",null,405,null,null,"31NM057-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台三角架一*4","[槽钢","[100*48*5.3",4,1648,null,48,5.3,5.3,{"v":1.1957888,"d":"1.20"},"无重合面",null,405,null,null,"31NM057-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台三角架二*2","[槽钢","[126*53*5.5",2,2160,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.86832,"d":"0.87"},"无重合面",null,405,null,null,"31NM057-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台三角架二*2","[槽钢","[100*48*5.3",2,3346,null,48,5.3,5.3,{"v":1.2139288000000001,"d":"1.21"},"无重合面",null,405,null,null,"31NM057-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台三角架三*6","[槽钢","[126*53*5.5",6,1490,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.79694,"d":"1.80"},"无重合面",null,405,null,null,"31NM057-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台三角架三*6","[槽钢","[100*48*5.3",6,1829,null,48,5.3,5.3,{"v":1.9906836,"d":"1.99"},"无重合面",null,405,null,null,"31NM057-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台三角架四*4","[槽钢","[126*53*5.5",4,1780,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.43112,"d":"1.43"},"无重合面",null,405,null,null,"31NM057-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台三角架四*4","[槽钢","[100*48*5.3",4,1829,null,48,5.3,5.3,{"v":1.3271224000000001,"d":"1.33"},"无重合面",null,405,null,null,"31NM057-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十七*1","[槽钢","[140*58*6",1,15100,null,58,6,6,{"v":2.4462,"d":"2.45"},"翼板重合",null,405,null,null,"31NM057-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十七*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,12.04,"31NM057-12图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十七*1","方（扁）钢","加强筋40*4",9,786,40,4,null,null,{"v":0.622512,"d":"0.62"},"无重合面",null,405,null,null,"31NM057-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十八*1","[槽钢","[100*48*5.3",1,19200,null,48,5.3,5.3,{"v":2.56128,"d":"2.56"},"翼板重合",null,405,null,null,"31NM057-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十八*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,14.08,"31NM057-12图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台平台十八*1","方（扁）钢","加强筋40*4",11,786,40,4,null,null,{"v":0.760848,"d":"0.76"},"无重合面",null,405,null,null,"31NM057-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台AD=2000直梯*2","方（扁）钢","钢板60*8",4,4728,60,8,null,null,{"v":2.572032,"d":"2.57"},"无重合面",null,405,null,null,"31NM057-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台AD=2000直梯*2","圆钢","圆钢Q18",14,500,18,{"$nulls":3},{"v":0.39564,"d":"0.40"},"无重合面",null,405,null,{"v":0.39564,"d":"0.40"},"31NM057-12","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台梯子入口*4","方（扁）钢","扁铁50*4",16,1400,50,4,null,null,{"v":2.4192,"d":"2.42"},"无重合面",null,405,null,null,"31NM057-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台梯子入口*4","方（扁）钢","扁铁50*4",16,1240,50,4,null,null,{"v":2.14272,"d":"2.14"},"无重合面",null,405,null,null,"31NM057-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台FH1=3200直梯*1","方（扁）钢","钢板60*8",2,4560,60,8,null,null,{"v":1.24032,"d":"1.24"},"无重合面",null,405,null,null,"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台FH1=3200直梯*1","圆钢","圆钢Q18",16,500,18,{"$nulls":3},{"v":0.45216,"d":"0.45"},"无重合面",null,405,null,{"v":0.45216,"d":"0.45"},"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台FH1=3200直梯*1","方（扁）钢","扁铁40*4",3,1870,40,4,null,null,{"v":0.49368,"d":"0.49"},"无重合面",null,405,null,null,"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台FH1=3200直梯*1","方（扁）钢","扁铁25*4",5,1130,25,4,null,null,{"v":0.3277,"d":"0.33"},"无重合面",null,405,null,null,"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台FH1=2800直梯*1","方（扁）钢","钢板60*8",2,3960,60,8,null,null,{"v":1.07712,"d":"1.08"},"无重合面",null,405,null,null,"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台FH1=2800直梯*1","圆钢","圆钢Q18",14,500,18,{"$nulls":3},{"v":0.39564,"d":"0.40"},"无重合面",null,405,null,{"v":0.39564,"d":"0.40"},"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台FH1=2800直梯*1","方（扁）钢","扁铁40*4",2,1870,40,4,null,null,{"v":0.32912,"d":"0.33"},"无重合面",null,405,null,null,"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台FH1=2800直梯*1","方（扁）钢","扁铁25*4",5,730,25,4,null,null,{"v":0.2117,"d":"0.21"},"无重合面",null,405,null,null,"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台FH1=4300直梯*2","方（扁）钢","钢板60*8",4,5460,60,8,null,null,{"v":2.97024,"d":"2.97"},"无重合面",null,405,null,null,"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台FH1=4300直梯*2","圆钢","圆钢Q18",38,500,18,{"$nulls":3},{"v":1.07388,"d":"1.07"},"无重合面",null,405,null,{"v":1.07388,"d":"1.07"},"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台FH1=4300直梯*2","方（扁）钢","扁铁40*4",8,1870,40,4,null,null,{"v":1.31648,"d":"1.32"},"无重合面",null,405,null,null,"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台FH1=4300直梯*2","方（扁）钢","扁铁25*4",10,2220,25,4,null,null,{"v":1.2876,"d":"1.29"},"无重合面",null,405,null,null,"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN14000  H8500*1","方（扁）钢","外侧板160*8",1,12580,160,8,null,null,{"v":4.22688,"d":"4.23"},"无重合面",null,405,null,null,"31NM057-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","方（扁）钢","内侧板160*8",1,11890,160,8,null,null,{"v":3.99504,"d":"4.00"},"无重合面",null,405,null,null,"31NM057-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","L型钢","L63*63*6",4,2500,null,63,6,6,1.26,"无重合面",null,405,null,null,"31NM057-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","L型钢","L63*63*6",2,226,null,63,6,6,{"v":0.056952,"d":"0.06"},"无重合面",null,405,null,null,"31NM057-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","方（扁）钢","踏板",38,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":20.064,"d":"20.06"},"31NM057-14图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离槽、剩余氨水槽联合操作台三角架五*5","[槽钢","[126*53*5.5",5,1378,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.38489,"d":"1.38"},"无重合面",null,405,null,null,"31NM057-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台三角架五*5","[槽钢","[100*48*5.3",5,1829,null,48,5.3,5.3,{"v":1.658903,"d":"1.66"},"无重合面",null,405,null,null,"31NM057-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离槽、剩余氨水槽联合操作台悬臂梁一*6","[槽钢","[126*53*5.5",6,1158,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.396548,"d":"1.40"},"无重合面",null,405,null,null,"31NM057-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离区域焦油中间槽操作台平台","[槽钢","[100*48*5.3",1,12000,null,48,5.3,5.3,{"v":1.6008,"d":"1.60"},"翼板重合",null,405,null,null,"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离区域焦油中间槽操作台平台","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":6.6,"d":"6.60"},"31NM058-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["一系焦油氨水分离区域焦油中间槽操作台平台","方（扁）钢","加强筋40*4",7,600,40,4,null,null,{"v":0.3696,"d":"0.37"},"无重合面",null,405,null,null,"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离区域焦油中间槽操作台平台支撑","[槽钢","[100*48*5.3",5,760,null,48,5.3,5.3,{"v":0.68932,"d":"0.69"},"无重合面",null,405,null,null,"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离区域焦油中间槽操作台KH1=3815直梯*1","L型钢","L63*63*6",2,5080,null,63,6,6,{"v":1.28016,"d":"1.28"},"无重合面",null,405,null,null,"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离区域焦油中间槽操作台KH1=3815直梯*1","方（扁）钢","扁铁40*4",4,1840,40,4,null,null,{"v":0.64768,"d":"0.65"},"无重合面",null,405,null,null,"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离区域焦油中间槽操作台KH1=3815直梯*1","方（扁）钢","扁铁25*4",5,3030,25,4,null,null,{"v":0.8787,"d":"0.88"},"无重合面",null,405,null,null,"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离区域焦油中间槽操作台KH1=3815直梯*1","圆钢","圆钢Q18",13,480,18,{"$nulls":3},{"v":0.3526848,"d":"0.35"},"无重合面",null,405,null,{"v":0.3526848,"d":"0.35"},"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["一系焦油氨水分离区域焦油中间槽操作台KH1=3815直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,405,null,{"v":0.15441264,"d":"0.15"},"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["一系焦油氨水分离区域焦油中间槽操作台栏杆10m","圆钢","圆钢 Q50*3",2,10000,50,{"$nulls":3},3.14,"无重合面",null,405,null,3.14,"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["一系焦油氨水分离区域焦油中间槽操作台栏杆10m","方（扁）钢","扁铁40*4",2,10000,40,4,null,null,1.76,"无重合面",null,405,null,null,"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["一系焦油氨水分离区域焦油中间槽操作台栏杆10m","方（扁）钢","踢腿板100*4",1,10000,100,4,null,null,2.08,"无重合面",null,405,null,null,"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台栏杆206m","圆钢","圆钢 Q50*3",2,206000,50,{"$nulls":3},{"v":64.684,"d":"64.68"},"无重合面",null,405,null,{"v":64.684,"d":"64.68"},"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台栏杆206m","方（扁）钢","扁铁40*4",2,206000,40,4,null,null,{"v":36.256,"d":"36.26"},"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台栏杆206m","方（扁）钢","踢腿板100*4",1,206000,100,4,null,null,{"v":42.848,"d":"42.85"},"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台45°斜梯T2B08a-10*2","[槽钢","[16b（160*63*6.5）",4,1400,null,63,6.5,6.5,{"v":1.3384,"d":"1.34"},"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台45°斜梯T2B08a-10*2","方（扁）钢","花纹板4.5",10,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,405,null,5.28,"31NM057-1-1图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台45斜梯护栏5.7m","圆钢","圆钢 Q50*3",2,5700,50,{"$nulls":3},{"v":1.7898,"d":"1.79"},"无重合面",null,405,null,{"v":1.7898,"d":"1.79"},"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台45斜梯护栏5.7m","方（扁）钢","扁铁40*4",2,5700,40,4,null,null,{"v":1.0032,"d":"1.00"},"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台45°斜梯T2B08a-14*1","[槽钢","[16b（160*63*6.5）",2,2000,null,63,6.5,6.5,{"v":0.956,"d":"0.96"},"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台45°斜梯T2B08a-14*1","方（扁）钢","花纹板4.5",14,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":7.392,"d":"7.39"},"31NM057-1-1图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台45斜梯护栏4m","圆钢","圆钢 Q50*3",2,4000,50,{"$nulls":3},{"v":1.256,"d":"1.26"},"无重合面",null,405,null,{"v":1.256,"d":"1.26"},"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台45斜梯护栏4m","方（扁）钢","扁铁40*4",2,4000,40,4,null,null,{"v":0.704,"d":"0.70"},"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台罐顶平台护栏246m","圆钢","圆钢 Q50*3",2,246000,50,{"$nulls":3},{"v":77.244,"d":"77.24"},"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台罐顶平台护栏246m","方（扁）钢","扁铁40*4",2,246000,40,4,null,null,{"v":43.296,"d":"43.30"},"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台罐顶平台护栏246m","方（扁）钢","踢腿板100*4",1,246000,100,4,null,null,{"v":51.168,"d":"51.17"},"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台盘梯护栏40m","圆钢","圆钢 Q50*3",2,40000,50,{"$nulls":3},12.56,"无重合面",null,405,null,12.56,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台盘梯护栏40m","方（扁）钢","扁铁40*4",2,40000,40,4,null,null,7.04,"无重合面",null,405,null,null,"31NM057-1-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","方（扁）钢","外侧板160*8",2,6050,160,8,null,null,{"v":4.0656,"d":"4.07"},"无重合面",null,405,null,null,"31NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","方（扁）钢","内侧板160*8",2,5670,160,8,null,null,{"v":3.81024,"d":"3.81"},"无重合面",null,405,null,null,"31NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","L型钢","L63*63*6",2,2500,null,63,6,6,0.63,"无重合面",null,405,null,null,"31NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,405,null,null,"31NM057-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","方（扁）钢","踏板",36,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":19.008,"d":"19.01"},"31NM057-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","方（扁）钢","外侧板160*8",2,6643,160,8,null,null,{"v":4.464096,"d":"4.46"},"无重合面",null,405,null,null,"31NM057-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","方（扁）钢","内侧板160*8",2,6220,160,8,null,null,{"v":4.17984,"d":"4.18"},"无重合面",null,405,null,null,"31NM057-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","L型钢","L63*63*6",2,2500,null,63,6,6,0.63,"无重合面",null,405,null,null,"31NM057-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,405,null,null,"31NM057-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","方（扁）钢","踏板",40,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,405,null,21.12,"31NM057-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台罐顶支架一*72","L型钢","L75*75*6",72,1740,null,75,6,6,{"v":18.792,"d":"18.79"},"无重合面",null,405,null,null,"31NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台罐顶支架二*4","L型钢","L100*100*6",4,840,null,100,6,6,{"v":0.672,"d":"0.67"},"无重合面",null,405,null,null,"31NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台罐顶支架二*4","[槽钢","[100*48*5.3",8,925,null,48,5.3,5.3,{"v":1.34236,"d":"1.34"},"无重合面",null,405,null,null,"31NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台罐顶支架三*2","L型钢","L100*100*6",2,840,null,100,6,6,{"v":0.336,"d":"0.34"},"无重合面",null,405,null,null,"31NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台罐顶支架三*2","[槽钢","[100*48*5.3",4,1125,null,48,5.3,5.3,{"v":0.8163,"d":"0.82"},"无重合面",null,405,null,null,"31NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台罐顶支架四*2","L型钢","L75*75*6",2,1800,null,75,6,6,0.54,"无重合面",null,405,null,null,"31NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台罐顶支架四*2","L型钢","L100*100*6",2,1605,null,100,6,6,{"v":0.642,"d":"0.64"},"无重合面",null,405,null,null,"31NM057-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台一*1","[槽钢","[100*48*5.3",1,30700,null,48,5.3,5.3,{"v":4.09538,"d":"4.10"},"翼板重合",null,405,null,null,"31NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台一*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":23.4,"d":"23.40"},"31NM057-5图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台一*1","方（扁）钢","加强筋40*4",16,786,40,4,null,null,{"v":1.106688,"d":"1.11"},"无重合面",null,405,null,null,"31NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台四*1","[槽钢","[100*48*5.3",1,24300,null,48,5.3,5.3,{"v":3.24162,"d":"3.24"},"翼板重合",null,405,null,null,"31NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台四*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,17.94,"31NM057-5图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台四*1","方（扁）钢","加强筋40*4",12,786,40,4,null,null,{"v":0.830016,"d":"0.83"},"无重合面",null,405,null,null,"31NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台四*1","方（扁）钢","加强筋40*4",2,770,40,4,null,null,{"v":0.13552,"d":"0.14"},"无重合面",null,405,null,null,"31NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台四*1","方（扁）钢","加强筋40*4",1,1300,40,4,null,null,{"v":0.1144,"d":"0.11"},"无重合面",null,405,null,null,"31NM057-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台三*1","[槽钢","[100*48*5.3",1,23900,null,48,5.3,5.3,{"v":3.18826,"d":"3.19"},"翼板重合",null,405,null,null,"31NM057-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台三*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":16.6,"d":"16.60"},"31NM057-6图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台三*1","方（扁）钢","加强筋40*4",11,786,40,4,null,null,{"v":0.760848,"d":"0.76"},"无重合面",null,405,null,null,"31NM057-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台五*1","[槽钢","[100*48*5.3",1,29600,null,48,5.3,5.3,{"v":3.94864,"d":"3.95"},"翼板重合",null,405,null,null,"31NM057-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台五*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":23.6,"d":"23.60"},"31NM057-6图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台五*1","方（扁）钢","加强筋40*4",20,786,40,4,null,null,{"v":1.38336,"d":"1.38"},"无重合面",null,405,null,null,"31NM057-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台二*2","[槽钢","[100*48*5.3",2,10400,null,48,5.3,5.3,{"v":2.77472,"d":"2.77"},"翼板重合",null,405,null,null,"31NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台二*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,10.92,"31NM057-7图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台二*2","方（扁）钢","加强筋40*4",6,786,40,4,null,null,{"v":0.415008,"d":"0.42"},"无重合面",null,405,null,null,"31NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台六*2","[槽钢","[100*48*5.3",2,10200,null,48,5.3,5.3,{"v":2.72136,"d":"2.72"},"翼板重合",null,405,null,null,"31NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台六*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":15,"d":"15.00"},"31NM057-7图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台六*2","方（扁）钢","加强筋40*4",10,786,40,4,null,null,{"v":0.69168,"d":"0.69"},"无重合面",null,405,null,null,"31NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台七*1","[槽钢","[100*48*5.3",1,36400,null,48,5.3,5.3,{"v":4.85576,"d":"4.86"},"翼板重合",null,405,null,null,"31NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台七*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":27.8,"d":"27.80"},"31NM057-7图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台七*1","方（扁）钢","加强筋40*4",18,786,40,4,null,null,{"v":1.245024,"d":"1.25"},"无重合面",null,405,null,null,"31NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台七*1","方（扁）钢","加强筋40*4",2,770,40,4,null,null,{"v":0.13552,"d":"0.14"},"无重合面",null,405,null,null,"31NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台七*1","方（扁）钢","加强筋40*4",1,1300,40,4,null,null,{"v":0.1144,"d":"0.11"},"无重合面",null,405,null,null,"31NM057-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台九*2","[槽钢","[140*58*6",2,8950,null,58,6,6,{"v":2.8998,"d":"2.90"},"翼板重合",null,405,null,null,"31NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台九*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,15.68,"31NM057-8图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台九*2","L型钢","L50*50*5",1,1209,null,50,5,5,{"v":0.1209,"d":"0.12"},"无重合面",null,405,null,{"v":0.09672,"d":"0.10"},"31NM057-8","一般性腐蚀","环氧富锌漆",{"v":0.444444444444444,"d":"44%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台九*2","L型钢","L50*50*5",2,1386,null,50,5,5,{"v":0.2772,"d":"0.28"},"无重合面",null,405,null,null,"31NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十*1","[槽钢","[100*48*5.3",1,7250,null,48,5.3,5.3,{"v":0.96715,"d":"0.97"},"翼板重合",null,405,null,null,"31NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,5.82,"31NM057-8图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十*1","方（扁）钢","加强筋40*4",3,1186,40,4,null,null,{"v":0.313104,"d":"0.31"},"无重合面",null,405,null,null,"31NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十一*1","[槽钢","[100*48*5.3",1,6220,null,48,5.3,5.3,{"v":0.829748,"d":"0.83"},"翼板重合",null,405,null,null,"31NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十一*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,3.14,"31NM057-8图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十二*1","[槽钢","[100*48*5.3",1,13100,null,48,5.3,5.3,{"v":1.74754,"d":"1.75"},"翼板重合",null,405,null,null,"31NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十二*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,7.72,"31NM057-8图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十二*1","方（扁）钢","加强筋40*4",1,836,40,4,null,null,{"v":0.073568,"d":"0.07"},"无重合面",null,405,null,null,"31NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十二*1","方（扁）钢","加强筋40*4",2,1186,40,4,null,null,{"v":0.208736,"d":"0.21"},"无重合面",null,405,null,null,"31NM057-8","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十三*1","[槽钢","[100*48*5.3",1,17600,null,48,5.3,5.3,{"v":2.34784,"d":"2.35"},"翼板重合",null,405,null,null,"31NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十三*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":13.8,"d":"13.80"},"31NM057-9图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十三*1","L型钢","L50*50*5",3,1386,null,50,5,5,{"v":0.4158,"d":"0.42"},"无重合面",null,405,null,null,"31NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十四*1","[槽钢","[100*48*5.3",1,10700,null,48,5.3,5.3,{"v":1.42738,"d":"1.43"},"翼板重合",null,405,null,null,"31NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十四*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":12.4,"d":"12.40"},"31NM057-9图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十四*1","方（扁）钢","加强筋40*4",1,4000,40,4,null,null,{"v":0.352,"d":"0.35"},"无重合面",null,405,null,null,"31NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十四*1","[槽钢","[100*48*5.3",1,7800,null,48,5.3,5.3,{"v":1.04052,"d":"1.04"},"翼板重合",null,405,null,null,"31NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十五*1","[槽钢","[100*48*5.3",1,10120,null,48,5.3,5.3,{"v":1.350008,"d":"1.35"},"翼板重合",null,405,null,null,"31NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十五*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,7.82,"31NM057-9图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十五*1","L型钢","L50*50*5",3,1186,null,50,5,5,{"v":0.3558,"d":"0.36"},"无重合面",null,405,null,null,"31NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十六*1","[槽钢","[100*48*5.3",1,17100,null,48,5.3,5.3,{"v":2.28114,"d":"2.28"},"翼板重合",null,405,null,null,"31NM057-9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十六*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,13.84,"31NM057-9图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十六*1","L型钢","L50*50*5",4,1286,null,50,5,5,{"v":0.5144,"d":"0.51"},"无重合面",null,405,null,null,"31NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台悬臂梁二*13","[槽钢","[126*53*5.5",13,1320,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":3.44916,"d":"3.45"},"无重合面",null,405,null,null,"31NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台罐顶平台支架三*2","[槽钢","[100*48*5.3",4,725,null,48,5.3,5.3,{"v":0.52606,"d":"0.53"},"无重合面",null,405,null,null,"31NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台罐顶平台支架三*2","L型钢","L100*100*6",2,840,null,100,6,6,{"v":0.336,"d":"0.34"},"无重合面",null,405,null,null,"31NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台罐顶平台支架四*2","[槽钢","[100*48*5.3",4,685,null,48,5.3,5.3,{"v":0.497036,"d":"0.50"},"无重合面",null,405,null,null,"31NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台罐顶平台支架四*2","L型钢","L100*100*6",2,840,null,100,6,6,{"v":0.336,"d":"0.34"},"无重合面",null,405,null,null,"31NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台八*2","[槽钢","[100*48*5.3",2,7120,null,48,5.3,5.3,{"v":1.899616,"d":"1.90"},"翼板重合",null,405,null,null,"31NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台八*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,10.52,"31NM057-10图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台八*2","方（扁）钢","加强筋40*4",6,1036,40,4,null,null,{"v":0.547008,"d":"0.55"},"无重合面",null,405,null,null,"31NM057-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台三角架一*4","[槽钢","[126*53*5.5",4,1490,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.19796,"d":"1.20"},"无重合面",null,405,null,null,"31NM057-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台三角架一*4","[槽钢","[100*48*5.3",4,1648,null,48,5.3,5.3,{"v":1.1957888,"d":"1.20"},"无重合面",null,405,null,null,"31NM057-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台三角架二*2","[槽钢","[126*53*5.5",2,2160,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.86832,"d":"0.87"},"无重合面",null,405,null,null,"31NM057-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台三角架二*2","[槽钢","[100*48*5.3",2,3346,null,48,5.3,5.3,{"v":1.2139288000000001,"d":"1.21"},"无重合面",null,405,null,null,"31NM057-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台三角架三*6","[槽钢","[126*53*5.5",6,1490,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.79694,"d":"1.80"},"无重合面",null,405,null,null,"31NM057-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台三角架三*6","[槽钢","[100*48*5.3",6,1829,null,48,5.3,5.3,{"v":1.9906836,"d":"1.99"},"无重合面",null,405,null,null,"31NM057-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台三角架四*4","[槽钢","[126*53*5.5",4,1780,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.43112,"d":"1.43"},"无重合面",null,405,null,null,"31NM057-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台三角架四*4","[槽钢","[100*48*5.3",4,1829,null,48,5.3,5.3,{"v":1.3271224000000001,"d":"1.33"},"无重合面",null,405,null,null,"31NM057-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十七*1","[槽钢","[140*58*6",1,15100,null,58,6,6,{"v":2.4462,"d":"2.45"},"翼板重合",null,405,null,null,"31NM057-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十七*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,12.04,"31NM057-12图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十七*1","方（扁）钢","加强筋40*4",9,786,40,4,null,null,{"v":0.622512,"d":"0.62"},"无重合面",null,405,null,null,"31NM057-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十八*1","[槽钢","[100*48*5.3",1,19200,null,48,5.3,5.3,{"v":2.56128,"d":"2.56"},"翼板重合",null,405,null,null,"31NM057-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十八*1","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,14.08,"31NM057-12图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台平台十八*1","方（扁）钢","加强筋40*4",11,786,40,4,null,null,{"v":0.760848,"d":"0.76"},"无重合面",null,405,null,null,"31NM057-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台AD=2000直梯*2","方（扁）钢","钢板60*8",4,4728,60,8,null,null,{"v":2.572032,"d":"2.57"},"无重合面",null,405,null,null,"31NM057-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台AD=2000直梯*2","圆钢","圆钢Q18",14,500,18,{"$nulls":3},{"v":0.39564,"d":"0.40"},"无重合面",null,405,null,{"v":0.39564,"d":"0.40"},"31NM057-12","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台梯子入口*4","方（扁）钢","扁铁50*4",16,1400,50,4,null,null,{"v":2.4192,"d":"2.42"},"无重合面",null,405,null,null,"31NM057-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台梯子入口*4","方（扁）钢","扁铁50*4",16,1240,50,4,null,null,{"v":2.14272,"d":"2.14"},"无重合面",null,405,null,null,"31NM057-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台FH1=3200直梯*1","方（扁）钢","钢板60*8",2,4560,60,8,null,null,{"v":1.24032,"d":"1.24"},"无重合面",null,405,null,null,"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台FH1=3200直梯*1","圆钢","圆钢Q18",16,500,18,{"$nulls":3},{"v":0.45216,"d":"0.45"},"无重合面",null,405,null,{"v":0.45216,"d":"0.45"},"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台FH1=3200直梯*1","方（扁）钢","扁铁40*4",3,1870,40,4,null,null,{"v":0.49368,"d":"0.49"},"无重合面",null,405,null,null,"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台FH1=3200直梯*1","方（扁）钢","扁铁25*4",5,1130,25,4,null,null,{"v":0.3277,"d":"0.33"},"无重合面",null,405,null,null,"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台FH1=2800直梯*1","方（扁）钢","钢板60*8",2,3960,60,8,null,null,{"v":1.07712,"d":"1.08"},"无重合面",null,405,null,null,"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台FH1=2800直梯*1","圆钢","圆钢Q18",14,500,18,{"$nulls":3},{"v":0.39564,"d":"0.40"},"无重合面",null,405,null,{"v":0.39564,"d":"0.40"},"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台FH1=2800直梯*1","方（扁）钢","扁铁40*4",2,1870,40,4,null,null,{"v":0.32912,"d":"0.33"},"无重合面",null,405,null,null,"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台FH1=2800直梯*1","方（扁）钢","扁铁25*4",5,730,25,4,null,null,{"v":0.2117,"d":"0.21"},"无重合面",null,405,null,null,"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台FH1=4300直梯*2","方（扁）钢","钢板60*8",4,5460,60,8,null,null,{"v":2.97024,"d":"2.97"},"无重合面",null,405,null,null,"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台FH1=4300直梯*2","圆钢","圆钢Q18",38,500,18,{"$nulls":3},{"v":1.07388,"d":"1.07"},"无重合面",null,405,null,{"v":1.07388,"d":"1.07"},"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台FH1=4300直梯*2","方（扁）钢","扁铁40*4",8,1870,40,4,null,null,{"v":1.31648,"d":"1.32"},"无重合面",null,405,null,null,"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台FH1=4300直梯*2","方（扁）钢","扁铁25*4",10,2220,25,4,null,null,{"v":1.2876,"d":"1.29"},"无重合面",null,405,null,null,"31NM057-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN14000  H8500*1","方（扁）钢","外侧板160*8",1,12580,160,8,null,null,{"v":4.22688,"d":"4.23"},"无重合面",null,405,null,null,"31NM057-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","方（扁）钢","内侧板160*8",1,11890,160,8,null,null,{"v":3.99504,"d":"4.00"},"无重合面",null,405,null,null,"31NM057-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","L型钢","L63*63*6",4,2500,null,63,6,6,1.26,"无重合面",null,405,null,null,"31NM057-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","L型钢","L63*63*6",2,226,null,63,6,6,{"v":0.056952,"d":"0.06"},"无重合面",null,405,null,null,"31NM057-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台盘梯DN12000  H4100*2","方（扁）钢","踏板",38,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":20.064,"d":"20.06"},"31NM057-14图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离槽、剩余氨水槽联合操作台三角架五*5","[槽钢","[126*53*5.5",5,1378,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.38489,"d":"1.38"},"无重合面",null,405,null,null,"31NM057-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台三角架五*5","[槽钢","[100*48*5.3",5,1829,null,48,5.3,5.3,{"v":1.658903,"d":"1.66"},"无重合面",null,405,null,null,"31NM057-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离槽、剩余氨水槽联合操作台悬臂梁一*6","[槽钢","[126*53*5.5",6,1158,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.396548,"d":"1.40"},"无重合面",null,405,null,null,"31NM057-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离区域焦油中间槽操作台平台","[槽钢","[100*48*5.3",1,12000,null,48,5.3,5.3,{"v":1.6008,"d":"1.60"},"翼板重合",null,405,null,null,"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离区域焦油中间槽操作台平台","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":6.6,"d":"6.60"},"31NM058-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系焦油氨水分离区域焦油中间槽操作台平台","方（扁）钢","加强筋40*4",7,600,40,4,null,null,{"v":0.3696,"d":"0.37"},"无重合面",null,405,null,null,"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离区域焦油中间槽操作台平台支撑","[槽钢","[100*48*5.3",5,760,null,48,5.3,5.3,{"v":0.68932,"d":"0.69"},"无重合面",null,405,null,null,"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离区域焦油中间槽操作台KH1=3815直梯*1","L型钢","L63*63*6",2,5080,null,63,6,6,{"v":1.28016,"d":"1.28"},"无重合面",null,405,null,null,"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离区域焦油中间槽操作台KH1=3815直梯*1","方（扁）钢","扁铁40*4",4,1840,40,4,null,null,{"v":0.64768,"d":"0.65"},"无重合面",null,405,null,null,"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离区域焦油中间槽操作台KH1=3815直梯*1","方（扁）钢","扁铁25*4",5,3030,25,4,null,null,{"v":0.8787,"d":"0.88"},"无重合面",null,405,null,null,"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离区域焦油中间槽操作台KH1=3815直梯*1","圆钢","圆钢Q18",13,480,18,{"$nulls":3},{"v":0.3526848,"d":"0.35"},"无重合面",null,405,null,{"v":0.3526848,"d":"0.35"},"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系焦油氨水分离区域焦油中间槽操作台KH1=3815直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,405,null,{"v":0.15441264,"d":"0.15"},"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系焦油氨水分离区域焦油中间槽操作台栏杆10m","圆钢","圆钢 Q50*3",2,10000,50,{"$nulls":3},3.14,"无重合面",null,405,null,3.14,"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系焦油氨水分离区域焦油中间槽操作台栏杆10m","方（扁）钢","扁铁40*4",2,10000,40,4,null,null,1.76,"无重合面",null,405,null,null,"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系焦油氨水分离区域焦油中间槽操作台栏杆10m","方（扁）钢","踢腿板100*4",1,10000,100,4,null,null,2.08,"无重合面",null,405,null,null,"31NM058-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离区域焦油槽操作台平台一","[槽钢","[100*48*5.3",2,800,null,48,5.3,5.3,{"v":0.21344,"d":"0.21"},"翼板重合",null,405,null,null,"31NM059-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离区域焦油槽操作台平台一","[槽钢","[100*48*5.3",2,5740,null,48,5.3,5.3,{"v":1.531432,"d":"1.53"},"翼板重合",null,405,null,null,"31NM059-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离区域焦油槽操作台平台一","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":9.2,"d":"9.20"},"31NM059-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["焦油氨水分离区域焦油槽操作台平台一","方（扁）钢","加强筋40*4",4,786,40,4,null,null,{"v":0.276672,"d":"0.28"},"无重合面",null,405,null,null,"31NM059-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离区域焦油槽操作台平台二","[槽钢","[100*48*5.3",1,800,null,48,5.3,5.3,{"v":0.10672,"d":"0.11"},"翼板重合",null,405,null,null,"31NM059-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离区域焦油槽操作台平台二","[槽钢","[100*48*5.3",2,1150,null,48,5.3,5.3,{"v":0.30682,"d":"0.31"},"翼板重合",null,405,null,null,"31NM059-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离区域焦油槽操作台平台二","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":2,"d":"2.00"},"31NM059-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["焦油氨水分离区域焦油槽操作台三角架一*4","[槽钢","[100*48*5.3",4,14800,null,48,5.3,5.3,{"v":10.73888,"d":"10.74"},"无重合面",null,405,null,null,"31NM059-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离区域焦油槽操作台三角架二*2","[槽钢","[100*48*5.3",2,2550,null,48,5.3,5.3,{"v":0.92514,"d":"0.93"},"无重合面",null,405,null,null,"31NM059-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离区域焦油槽操作台平台45°斜梯T2B06a-45","[槽钢","[16b（160*63*6.5）",2,6300,null,63,6.5,6.5,{"v":3.0114,"d":"3.01"},"无重合面",null,405,null,null,"31NM059-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离区域焦油槽操作台平台45°斜梯T2B06a-45","方（扁）钢","花纹板4.5",22,600,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,405,null,{"v":8.712,"d":"8.71"},"31NM059-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["焦油氨水分离区域焦油槽操作台45斜梯护栏13m","圆钢","圆钢 Q50*3",2,13000,50,{"$nulls":3},{"v":4.082,"d":"4.08"},"无重合面",null,405,null,{"v":4.082,"d":"4.08"},"31NM059-2","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["焦油氨水分离区域焦油槽操作台45斜梯护栏13m","方（扁）钢","扁铁40*4",2,13000,40,4,null,null,{"v":2.288,"d":"2.29"},"无重合面",null,405,null,null,"31NM059-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离区域焦油槽操作台平台护栏15m","圆钢","圆钢 Q50*3",2,15000,50,{"$nulls":3},4.71,"无重合面",null,405,null,null,"31NM059-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离区域焦油槽操作台平台护栏15m","方（扁）钢","扁铁40*4",2,15000,40,4,null,null,2.64,"无重合面",null,405,null,null,"31NM059-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离区域焦油槽操作台平台护栏15m","方（扁）钢","踢腿板100*4",1,15000,100,4,null,null,3.12,"无重合面",null,405,null,null,"31NM059-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台平台45°斜梯T2B08a-21.5","[槽钢","[16b（160*63*6.5）",4,3000,null,63,6.5,6.5,{"v":2.868,"d":"2.87"},"无重合面",null,406,null,null,"31NM060-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台平台45°斜梯T2B08a-21.5","方（扁）钢","花纹板4.5",20,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,407,null,10.56,"31NM060-1图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["焦油氨水分离区域陶瓷过滤器操作台45斜梯护栏13m","圆钢","圆钢 Q50*3",2,13000,50,{"$nulls":3},{"v":4.082,"d":"4.08"},"无重合面",null,408,null,{"v":4.082,"d":"4.08"},"31NM060-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["焦油氨水分离区域陶瓷过滤器操作台45斜梯护栏13m","方（扁）钢","扁铁40*4",2,13000,40,4,null,null,{"v":2.288,"d":"2.29"},"无重合面",null,409,null,null,"31NM060-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台平台护栏87m","圆钢","圆钢 Q50*3",2,87000,50,{"$nulls":3},{"v":27.318,"d":"27.32"},"无重合面",null,410,null,null,"31NM060-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台平台护栏87m","方（扁）钢","扁铁40*4",2,87000,40,4,null,null,{"v":15.312,"d":"15.31"},"无重合面",null,411,null,null,"31NM060-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台平台护栏87m","方（扁）钢","踢腿板100*4",1,87000,100,4,null,null,{"v":18.096,"d":"18.10"},"无重合面",null,412,null,null,"31NM060-1","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台KH1=4400直梯*2","L型钢","L63*63*6",4,5680,null,63,6,6,{"v":2.86272,"d":"2.86"},"无重合面",null,413,null,null,"31NM060-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台KH1=4400直梯*2","方（扁）钢","扁铁40*4",10,1840,40,4,null,null,{"v":1.6192,"d":"1.62"},"无重合面",null,414,null,null,"31NM060-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台KH1=4400直梯*2","方（扁）钢","扁铁25*4",10,3670,25,4,null,null,{"v":2.1286,"d":"2.13"},"无重合面",null,415,null,null,"31NM060-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台KH1=4400直梯*2","圆钢","圆钢Q18",30,480,18,{"$nulls":3},{"v":0.813888,"d":"0.81"},"无重合面",null,416,null,{"v":0.813888,"d":"0.81"},"31NM060-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["焦油氨水分离区域陶瓷过滤器操作台KH1=4400直梯*2","圆钢","圆钢Q18",4,1366,18,{"$nulls":3},{"v":0.30882528000000004,"d":"0.31"},"无重合面",null,417,null,{"v":0.30882528,"d":"0.31"},"31NM060-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["焦油氨水分离区域陶瓷过滤器操作台悬臂梁*25","[槽钢","[126*53*5.5",25,1380,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":6.9345,"d":"6.93"},"无重合面",null,418,null,null,"31NM060-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台平台支架*32","[槽钢","[100*48*5.3",32,1390,null,48,5.3,5.3,{"v":8.068672,"d":"8.07"},"无重合面",null,419,null,null,"31NM060-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台平台一","[槽钢","[100*48*5.3",1,8170,null,48,5.3,5.3,{"v":1.089878,"d":"1.09"},"翼板重合",null,420,null,null,"31NM060-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台平台一","[槽钢","[100*48*5.3",4,5480,null,48,5.3,5.3,{"v":2.924128,"d":"2.92"},"翼板重合",null,421,null,null,"31NM060-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台平台一","[槽钢","[100*48*5.3",3,7120,null,48,5.3,5.3,{"v":2.849424,"d":"2.85"},"翼板重合",null,422,null,null,"31NM060-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台平台一","[槽钢","[100*48*5.3",5,1200,null,48,5.3,5.3,{"v":0.8004,"d":"0.80"},"翼板重合",null,423,null,null,"31NM060-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台平台一","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,424,null,{"v":62,"d":"62.00"},"31NM060-3图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["焦油氨水分离区域陶瓷过滤器操作台平台一","方（扁）钢","加强筋60*6",29,1286,60,6,null,null,{"v":4.922808,"d":"4.92"},"无重合面",null,425,null,null,"31NM060-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台平台二","[槽钢","[100*48*5.3",6,1560,null,48,5.3,5.3,{"v":1.248624,"d":"1.25"},"翼板重合",null,426,null,null,"31NM060-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台平台二","[槽钢","[100*48*5.3",4,3600,null,48,5.3,5.3,{"v":1.92096,"d":"1.92"},"翼板重合",null,427,null,null,"31NM060-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台平台二","[槽钢","[100*48*5.3",4,8350,null,48,5.3,5.3,{"v":4.45556,"d":"4.46"},"翼板重合",null,428,null,null,"31NM060-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台平台二","[槽钢","[100*48*5.3",8,900,null,48,5.3,5.3,{"v":0.96048,"d":"0.96"},"翼板重合",null,429,null,null,"31NM060-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台平台二","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,430,null,{"v":46,"d":"46.00"},"31NM060-3图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["焦油氨水分离区域陶瓷过滤器操作台平台二","方（扁）钢","加强筋40*4",36,996,40,4,null,null,{"v":3.155328,"d":"3.16"},"无重合面",null,431,null,null,"31NM060-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["焦油氨水分离区域陶瓷过滤器操作台平台二","方（扁）钢","加强筋40*4",3,586,40,4,null,null,{"v":0.154704,"d":"0.15"},"无重合面",null,432,null,null,"31NM060-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["洗涤区域","其他",{"$nulls":7},"需手动计算","无重合面",null,433,{"$nulls":3},"重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"$error":"#VALUE!"}]
["一系洗涤区域操作台45斜梯护栏231m","圆钢","圆钢 Q50*3",2,231000,50,{"$nulls":3},{"v":72.534,"d":"72.53"},"无重合面",null,434,null,{"v":72.534,"d":"72.53"},"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["一系洗涤区域操作台45斜梯护栏231m","方（扁）钢","扁铁40*4",2,231000,40,4,null,null,{"v":40.656,"d":"40.66"},"无重合面",null,435,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台45°斜梯T2B08a-30*2","[槽钢","[16b（160*63*6.5）",4,4250,null,63,6.5,6.5,{"v":4.063,"d":"4.06"},"无重合面",null,436,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台45°斜梯T2B08a-30*2","方（扁）钢","花纹板4.5",30,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,437,null,15.84,"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台49°斜梯T2B07a-29*1","[槽钢","[16b（160*63*6.5）",2,4000,null,63,6.5,6.5,{"v":1.912,"d":"1.91"},"无重合面",null,438,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台49°斜梯T2B07a-29*1","方（扁）钢","花纹板4.5",13,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,439,null,{"v":6.006,"d":"6.01"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台41°斜梯T2B07a-22*1","[槽钢","[16b（160*63*6.5）",2,3200,null,63,6.5,6.5,{"v":1.5296,"d":"1.53"},"无重合面",null,440,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台41°斜梯T2B07a-22*1","方（扁）钢","花纹板4.5",12,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,441,null,{"v":5.544,"d":"5.54"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台40°斜梯T2B07a-20*1","[槽钢","[16b（160*63*6.5）",2,3100,null,63,6.5,6.5,{"v":1.4818,"d":"1.48"},"无重合面",null,442,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台40°斜梯T2B07a-20*1","方（扁）钢","花纹板4.5",11,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,443,null,{"v":5.082,"d":"5.08"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台51°斜梯T2B07a-30*3","[槽钢","[16b（160*63*6.5）",6,3800,null,63,6.5,6.5,{"v":5.4492,"d":"5.45"},"无重合面",null,444,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台51°斜梯T2B07a-30*3","方（扁）钢","花纹板4.5",36,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,445,null,{"v":16.632,"d":"16.63"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台49°斜梯T2B07a-30*5","[槽钢","[16b（160*63*6.5）",10,3900,null,63,6.5,6.5,{"v":9.321,"d":"9.32"},"无重合面",null,446,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台49°斜梯T2B07a-30*5","方（扁）钢","花纹板4.5",60,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,447,null,27.72,"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台46°斜梯T2B07a-27*4","[槽钢","[16b（160*63*6.5）",8,3800,null,63,6.5,6.5,{"v":7.2656,"d":"7.27"},"无重合面",null,448,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台46°斜梯T2B07a-27*4","方（扁）钢","花纹板4.5",48,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,449,null,{"v":22.176,"d":"22.18"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台50°斜梯T2B07a-30*4","[槽钢","[16b（160*63*6.5）",8,3900,null,63,6.5,6.5,{"v":7.4568,"d":"7.46"},"无重合面",null,450,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台50°斜梯T2B07a-30*4","方（扁）钢","花纹板4.5",48,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,451,null,{"v":22.176,"d":"22.18"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台47°斜梯T2B07a-28*1","[槽钢","[16b（160*63*6.5）",2,3900,null,63,6.5,6.5,{"v":1.8642,"d":"1.86"},"无重合面",null,452,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台47°斜梯T2B07a-28*1","方（扁）钢","花纹板4.5",12,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,453,null,{"v":5.544,"d":"5.54"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台33°斜梯T1B07a-17*1","[槽钢","[16b（160*63*6.5）",2,3200,null,63,6.5,6.5,{"v":1.5296,"d":"1.53"},"无重合面",null,454,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台33°斜梯T1B07a-17*1","方（扁）钢","花纹板4.5",11,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,455,null,{"v":5.082,"d":"5.08"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台27°斜梯T1B07a-13*1","[槽钢","[16b（160*63*6.5）",2,2800,null,63,6.5,6.5,{"v":1.3384,"d":"1.34"},"无重合面",null,456,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台27°斜梯T1B07a-13*1","方（扁）钢","花纹板4.5",10,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,457,null,4.62,"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台43°斜梯T2B07a-24*2","[槽钢","[16b（160*63*6.5）",4,3400,null,63,6.5,6.5,{"v":3.2504,"d":"3.25"},"无重合面",null,458,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台43°斜梯T2B07a-24*2","方（扁）钢","花纹板4.5",24,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,459,null,{"v":11.088,"d":"11.09"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台52°斜梯T2B07a-33*1","[槽钢","[16b（160*63*6.5）",2,4200,null,63,6.5,6.5,{"v":2.0076,"d":"2.01"},"无重合面",null,460,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台52°斜梯T2B07a-33*1","方（扁）钢","花纹板4.5",13,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,461,null,{"v":6.006,"d":"6.01"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台51°斜梯T2B07a-32.5*2","[槽钢","[16b（160*63*6.5）",4,4000,null,63,6.5,6.5,{"v":3.824,"d":"3.82"},"无重合面",null,462,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台51°斜梯T2B07a-32.5*2","方（扁）钢","花纹板4.5",26,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,463,null,{"v":12.012,"d":"12.01"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台盘梯栏杆15m","圆钢","圆钢 Q50*3",2,15000,50,{"$nulls":3},4.71,"无重合面",null,464,null,4.71,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["一系洗涤区域操作台盘梯栏杆15m","方（扁）钢","扁铁50*4",2,15000,50,4,null,null,3.24,"无重合面",null,465,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台护栏87m","圆钢","圆钢 Q50*3",2,910000,50,{"$nulls":3},285.74,"无重合面",null,466,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台护栏87m","方（扁）钢","扁铁40*4",2,910000,40,4,null,null,160.16,"无重合面",null,467,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台护栏87m","方（扁）钢","踢腿板100*4",1,910000,100,4,null,null,189.28,"无重合面",null,468,null,null,"FG110203-SS-FB02.23-1-1+","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台54°斜梯3600","[槽钢","[16b（160*63*6.5）",2,4200,null,63,6.5,6.5,{"v":2.0076,"d":"2.01"},"无重合面",null,469,null,null,"FG110203-SS-FB02.23-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台54°斜梯3600","方（扁）钢","花纹板4.5",15,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,470,null,5.46,"FG110203-SS-FB02.23-2图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台54°斜梯3600","圆钢","圆钢 Q33.5",16,600,33.5,{"$nulls":3},{"v":1.009824,"d":"1.01"},"无重合面",null,471,null,null,"FG110203-SS-FB02.23-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台54°斜梯3600","圆钢","圆钢 Q50*3",2,6600,50,{"$nulls":3},{"v":2.0724,"d":"2.07"},"无重合面",null,472,null,null,"FG110203-SS-FB02.23-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台54°斜梯3500","[槽钢","[16b（160*63*6.5）",2,4100,null,63,6.5,6.5,{"v":1.9598,"d":"1.96"},"无重合面",null,473,null,null,"FG110203-SS-FB02.23-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台54°斜梯3500","方（扁）钢","花纹板4.5",14,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,474,null,{"v":5.096,"d":"5.10"},"FG110203-SS-FB02.23-2图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台54°斜梯3500","圆钢","圆钢 Q33.5",16,600,33.5,{"$nulls":3},{"v":1.009824,"d":"1.01"},"无重合面",null,475,null,null,"FG110203-SS-FB02.23-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台54°斜梯3500","圆钢","圆钢 Q50*3",2,6500,50,{"$nulls":3},{"v":2.041,"d":"2.04"},"无重合面",null,476,null,null,"FG110203-SS-FB02.23-2","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台KH1=2400直梯*1","L型钢","L63*63*6",2,3680,null,63,6,6,{"v":0.92736,"d":"0.93"},"无重合面",null,477,null,null,"FG110203-SS-FB02.23-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台KH1=2400直梯*1","方（扁）钢","扁铁40*4",3,1840,40,4,null,null,{"v":0.48576,"d":"0.49"},"无重合面",null,478,null,null,"FG110203-SS-FB02.23-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台KH1=2400直梯*1","方（扁）钢","扁铁25*4",5,1670,25,4,null,null,{"v":0.4843,"d":"0.48"},"无重合面",null,479,null,null,"FG110203-SS-FB02.23-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台KH1=2400直梯*1","圆钢","圆钢Q18",8,480,18,{"$nulls":3},{"v":0.21703680000000003,"d":"0.22"},"无重合面",null,480,null,{"v":0.2170368,"d":"0.22"},"FG110203-SS-FB02.23-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["一系洗涤区域操作台KH1=2400直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,481,null,{"v":0.15441264,"d":"0.15"},"FG110203-SS-FB02.23-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["一系洗涤区域操作台KH1=1800直梯*1","L型钢","L63*63*6",2,3080,null,63,6,6,{"v":0.77616,"d":"0.78"},"无重合面",null,482,null,null,"FG110203-SS-FB02.23-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台KH1=1800直梯*1","方（扁）钢","扁铁40*4",3,1840,40,4,null,null,{"v":0.48576,"d":"0.49"},"无重合面",null,483,null,null,"FG110203-SS-FB02.23-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台KH1=1800直梯*1","方（扁）钢","扁铁25*4",5,1070,25,4,null,null,{"v":0.3103,"d":"0.31"},"无重合面",null,484,null,null,"FG110203-SS-FB02.23-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台KH1=1800直梯*1","圆钢","圆钢Q18",7,480,18,{"$nulls":3},{"v":0.1899072,"d":"0.19"},"无重合面",null,485,null,{"v":0.1899072,"d":"0.19"},"FG110203-SS-FB02.23-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["一系洗涤区域操作台KH1=1800直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,486,null,{"v":0.15441264,"d":"0.15"},"FG110203-SS-FB02.23-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["一系洗涤区域操作台KH1=2000直梯*1","L型钢","L63*63*6",2,3280,null,63,6,6,{"v":0.82656,"d":"0.83"},"无重合面",null,487,null,null,"FG110203-SS-FB02.23-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台KH1=2000直梯*1","方（扁）钢","扁铁40*4",3,1840,40,4,null,null,{"v":0.48576,"d":"0.49"},"无重合面",null,488,null,null,"FG110203-SS-FB02.23-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台KH1=2000直梯*1","方（扁）钢","扁铁25*4",5,1270,25,4,null,null,{"v":0.3683,"d":"0.37"},"无重合面",null,489,null,null,"FG110203-SS-FB02.23-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台KH1=2000直梯*1","圆钢","圆钢Q18",7,480,18,{"$nulls":3},{"v":0.1899072,"d":"0.19"},"无重合面",null,490,null,{"v":0.1899072,"d":"0.19"},"FG110203-SS-FB02.23-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["一系洗涤区域操作台KH1=2000直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,491,null,{"v":0.15441264,"d":"0.15"},"FG110203-SS-FB02.23-3","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["一系洗涤区域操作台盘梯800*4","方（扁）钢","外侧板160*8",4,1320,160,8,null,null,{"v":1.77408,"d":"1.77"},"无重合面",null,492,null,null,"FG110203-SS-FB02.23-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台盘梯800*4","方（扁）钢","内侧板160*8",4,1130,160,8,null,null,{"v":1.51872,"d":"1.52"},"无重合面",null,493,null,null,"FG110203-SS-FB02.23-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台盘梯800*4","L型钢","L63*63*6",16,226,null,63,6,6,{"v":0.455616,"d":"0.46"},"无重合面",null,494,null,null,"FG110203-SS-FB02.23-4","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台盘梯800*4","方（扁）钢","踏板",16,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,495,null,{"v":8.448,"d":"8.45"},"FG110203-SS-FB02.23-4图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台盘梯900*2","方（扁）钢","外侧板160*8",2,1480,160,8,null,null,{"v":0.99456,"d":"0.99"},"无重合面",null,496,null,null,"FG110203-SS-FB02.23-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台盘梯900*2","方（扁）钢","内侧板160*8",2,1270,160,8,null,null,{"v":0.85344,"d":"0.85"},"无重合面",null,497,null,null,"FG110203-SS-FB02.23-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台盘梯900*2","L型钢","L63*63*6",8,226,null,63,6,6,{"v":0.227808,"d":"0.23"},"无重合面",null,498,null,null,"FG110203-SS-FB02.23-5","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台盘梯900*2","方（扁）钢","踏板",10,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,499,null,5.28,"FG110203-SS-FB02.23-5图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台盘梯1400","方（扁）钢","外侧板160*8",1,2230,160,8,null,null,{"v":0.74928,"d":"0.75"},"无重合面",null,500,null,null,"FG110203-SS-FB02.23-6","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台盘梯1400","方（扁）钢","内侧板160*8",1,1980,160,8,null,null,{"v":0.66528,"d":"0.67"},"无重合面",null,501,null,null,"FG110203-SS-FB02.23-6","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台盘梯1400","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,502,null,null,"FG110203-SS-FB02.23-6","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台盘梯1400","方（扁）钢","踏板",7,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,503,null,{"v":3.696,"d":"3.70"},"FG110203-SS-FB02.23-6图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台盘梯1500","方（扁）钢","外侧板160*8",1,2400,160,8,null,null,{"v":0.8064,"d":"0.81"},"无重合面",null,504,null,null,"FG110203-SS-FB02.23-7","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台盘梯1500","方（扁）钢","内侧板160*8",1,2100,160,8,null,null,{"v":0.7056,"d":"0.71"},"无重合面",null,505,null,null,"FG110203-SS-FB02.23-7","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台盘梯1500","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,506,null,null,"FG110203-SS-FB02.23-7","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台盘梯1500","方（扁）钢","踏板",7,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,507,null,{"v":3.696,"d":"3.70"},"FG110203-SS-FB02.23-7图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台盘梯1000*2","方（扁）钢","外侧板160*8",2,1600,160,8,null,null,{"v":1.0752,"d":"1.08"},"无重合面",null,508,null,null,"FG110203-SS-FB02.23-8、9","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台盘梯1000*2","方（扁）钢","内侧板160*8",2,1400,160,8,null,null,{"v":0.9408,"d":"0.94"},"无重合面",null,509,null,null,"FG110203-SS-FB02.23-8、9","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台盘梯1000*2","L型钢","L63*63*6",8,226,null,63,6,6,{"v":0.227808,"d":"0.23"},"无重合面",null,510,null,null,"FG110203-SS-FB02.23-8、9","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台盘梯1000*2","方（扁）钢","踏板",10,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,511,null,5.28,"FG110203-SS-FB02.23-8、9图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台AD=800直梯*2","方（扁）钢","钢板60*8",4,3370,60,8,null,null,{"v":1.83328,"d":"1.83"},"无重合面",null,512,null,null,"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台AD=800直梯*2","圆钢","圆钢Q18",6,500,18,{"$nulls":3},{"v":0.16956,"d":"0.17"},"无重合面",null,513,null,{"v":0.16956,"d":"0.17"},"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["一系洗涤区域操作台AD=950直梯*2","方（扁）钢","钢板60*8",4,3500,60,8,null,null,{"v":1.904,"d":"1.90"},"无重合面",null,514,null,null,"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台AD=950直梯*2","圆钢","圆钢Q18",6,500,18,{"$nulls":3},{"v":0.16956,"d":"0.17"},"无重合面",null,515,null,{"v":0.16956,"d":"0.17"},"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["一系洗涤区域操作台AD=700直梯*2","方（扁）钢","钢板60*8",4,3270,60,8,null,null,{"v":1.77888,"d":"1.78"},"无重合面",null,516,null,null,"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台AD=700直梯*2","圆钢","圆钢Q18",6,500,18,{"$nulls":3},{"v":0.16956,"d":"0.17"},"无重合面",null,517,null,{"v":0.16956,"d":"0.17"},"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["一系洗涤区域操作台AD=750直梯*1","方（扁）钢","钢板60*8",4,3300,60,8,null,null,{"v":1.7952,"d":"1.80"},"无重合面",null,518,null,null,"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台AD=750直梯*1","圆钢","圆钢Q18",6,500,18,{"$nulls":3},{"v":0.16956,"d":"0.17"},"无重合面",null,519,null,{"v":0.16956,"d":"0.17"},"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["一系洗涤区域操作台AD=1100直梯*1","方（扁）钢","钢板60*8",2,3670,60,8,null,null,{"v":0.99824,"d":"1.00"},"无重合面",null,520,null,null,"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台AD=1100直梯*1","圆钢","圆钢Q18",4,500,18,{"$nulls":3},{"v":0.11304,"d":"0.11"},"无重合面",null,521,null,{"v":0.11304,"d":"0.11"},"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["一系洗涤区域操作台AD=600直梯*1","方（扁）钢","钢板60*8",2,3170,60,8,null,null,{"v":0.86224,"d":"0.86"},"无重合面",null,522,null,null,"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台AD=600直梯*1","圆钢","圆钢Q18",3,500,18,{"$nulls":3},{"v":0.08478,"d":"0.08"},"无重合面",null,523,null,{"v":0.08478,"d":"0.08"},"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["一系洗涤区域操作台FH1=2200直梯*2","方（扁）钢","钢板60*8",4,3560,60,8,null,null,{"v":1.93664,"d":"1.94"},"无重合面",null,524,null,null,"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台FH1=2200直梯*2","圆钢","圆钢Q18",24,500,18,{"$nulls":3},{"v":0.67824,"d":"0.68"},"无重合面",null,525,null,{"v":0.67824,"d":"0.68"},"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["一系洗涤区域操作台FH1=2200直梯*2","方（扁）钢","扁铁40*4",4,1870,40,4,null,null,{"v":0.65824,"d":"0.66"},"无重合面",null,526,null,null,"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台FH1=2200直梯*2","方（扁）钢","扁铁25*4",10,530,25,4,null,null,{"v":0.3074,"d":"0.31"},"无重合面",null,527,null,null,"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台梯子入口*3","方（扁）钢","扁铁50*4",12,1400,50,4,null,null,{"v":1.8144,"d":"1.81"},"无重合面",null,528,null,null,"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台梯子入口*3","方（扁）钢","扁铁50*4",12,1240,50,4,null,null,{"v":1.60704,"d":"1.61"},"无重合面",null,529,null,null,"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台FH1=2500直梯*1","方（扁）钢","钢板60*8",2,3860,60,8,null,null,{"v":1.04992,"d":"1.05"},"无重合面",null,530,null,null,"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台FH1=2500直梯*1","圆钢","圆钢Q18",13,500,18,{"$nulls":3},{"v":0.36738,"d":"0.37"},"无重合面",null,531,null,{"v":0.36738,"d":"0.37"},"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0.5,"d":"50%"}]
["一系洗涤区域操作台FH1=2500直梯*1","方（扁）钢","扁铁40*4",2,1870,40,4,null,null,{"v":0.32912,"d":"0.33"},"无重合面",null,532,null,null,"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台FH1=2500直梯*1","方（扁）钢","扁铁25*4",5,530,25,4,null,null,{"v":0.1537,"d":"0.15"},"无重合面",null,533,null,null,"FG110203-SS-FB02.23-10","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台一","[槽钢","[100*48*5.3",1,34500,null,48,5.3,5.3,{"v":4.6023,"d":"4.60"},"翼板重合",null,534,null,null,"FG110203-SS-FB02.23-11","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台一","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,535,null,{"v":29.2,"d":"29.20"},"FG110203-SS-FB02.23-11图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台一","方（扁）钢","加强筋40*4",18,1000,40,4,null,null,{"v":1.584,"d":"1.58"},"无重合面",null,536,null,null,"FG110203-SS-FB02.23-11","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二","[槽钢","[100*48*5.3",1,23900,null,48,5.3,5.3,{"v":3.18826,"d":"3.19"},"翼板重合",null,537,null,null,"FG110203-SS-FB02.23-11","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,538,null,{"v":18.6,"d":"18.60"},"FG110203-SS-FB02.23-11图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台二","方（扁）钢","加强筋40*4",4,1000,40,4,null,null,{"v":0.352,"d":"0.35"},"无重合面",null,539,null,null,"FG110203-SS-FB02.23-11","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二","方（扁）钢","加强筋40*4",8,900,40,4,null,null,{"v":0.6336,"d":"0.63"},"无重合面",null,540,null,null,"FG110203-SS-FB02.23-11","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三","[槽钢","[100*48*5.3",1,26400,null,48,5.3,5.3,{"v":3.52176,"d":"3.52"},"翼板重合",null,541,null,null,"FG110203-SS-FB02.23-12","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,542,null,{"v":17.4,"d":"17.40"},"FG110203-SS-FB02.23-12图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台三","方（扁）钢","加强筋40*4",10,1000,40,4,null,null,0.88,"无重合面",null,543,null,null,"FG110203-SS-FB02.23-12","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台四*6","[槽钢","[100*48*5.3",6,14200,null,48,5.3,5.3,{"v":11.36568,"d":"11.37"},"翼板重合",null,544,null,null,"FG110203-SS-FB02.23-12","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台四*6","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,545,null,{"v":64.8,"d":"64.80"},"FG110203-SS-FB02.23-12图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台四*6","方（扁）钢","加强筋40*4",36,1000,40,4,null,null,{"v":3.168,"d":"3.17"},"无重合面",null,546,null,null,"FG110203-SS-FB02.23-12","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台六","[槽钢","[100*48*5.3",1,76600,null,48,5.3,5.3,{"v":10.21844,"d":"10.22"},"翼板重合",null,547,null,null,"FG110203-SS-FB02.23-13","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台六","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,548,null,{"v":64.8,"d":"64.80"},"FG110203-SS-FB02.23-13图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台六","方（扁）钢","加强筋40*4",37,1000,40,4,null,null,{"v":3.256,"d":"3.26"},"无重合面",null,549,null,null,"FG110203-SS-FB02.23-13","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台六","方（扁）钢","加强筋40*4",4,700,40,4,null,null,{"v":0.2464,"d":"0.25"},"无重合面",null,550,null,null,"FG110203-SS-FB02.23-13","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台八","[槽钢","[16b（160*63*6.5）",2,1000,null,63,6.5,6.5,{"v":0.352,"d":"0.35"},"翼板重合",null,551,null,null,"FG110203-SS-FB02.23-14","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台八","[槽钢","[16b（160*63*6.5）",2,33900,null,63,6.5,6.5,{"v":11.9328,"d":"11.93"},"翼板重合",null,552,null,null,"FG110203-SS-FB02.23-14","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台八","[槽钢","[100*48*5.3",1,48600,null,48,5.3,5.3,{"v":6.48324,"d":"6.48"},"翼板重合",null,553,null,null,"FG110203-SS-FB02.23-14","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台八","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,554,null,{"v":102.8,"d":"102.80"},"FG110203-SS-FB02.23-14图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台八","方（扁）钢","加强筋40*4",41,1000,40,4,null,null,{"v":3.608,"d":"3.61"},"无重合面",null,555,null,null,"FG110203-SS-FB02.23-14","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台八","方（扁）钢","加强筋40*4",22,900,40,4,null,null,{"v":1.7424,"d":"1.74"},"无重合面",null,556,null,null,"FG110203-SS-FB02.23-14","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台五*2","[槽钢","[100*48*5.3",2,7100,null,48,5.3,5.3,{"v":1.89428,"d":"1.89"},"翼板重合",null,557,null,null,"FG110203-SS-FB02.23-14","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台五*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,558,null,{"v":10,"d":"10.00"},"FG110203-SS-FB02.23-14图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台五*2","方（扁）钢","加强筋40*4",2,1000,40,4,null,null,{"v":0.176,"d":"0.18"},"无重合面",null,559,null,null,"FG110203-SS-FB02.23-15","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台七","[槽钢","[100*48*5.3",2,7100,null,48,5.3,5.3,{"v":1.89428,"d":"1.89"},"翼板重合",null,560,null,null,"FG110203-SS-FB02.23-15","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台七","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,561,null,{"v":10,"d":"10.00"},"FG110203-SS-FB02.23-15图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台七","方（扁）钢","加强筋40*4",2,1000,40,4,null,null,{"v":0.176,"d":"0.18"},"无重合面",null,562,null,null,"FG110203-SS-FB02.23-15","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台九","[槽钢","[100*48*5.3",1,26600,null,48,5.3,5.3,{"v":3.54844,"d":"3.55"},"翼板重合",null,563,null,null,"FG110203-SS-FB02.23-15","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台九","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,564,null,{"v":20,"d":"20.00"},"FG110203-SS-FB02.23-15图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台九","方（扁）钢","加强筋40*4",13,800,40,4,null,null,{"v":0.9152,"d":"0.92"},"无重合面",null,565,null,null,"FG110203-SS-FB02.23-15","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十","[槽钢","[100*48*5.3",1,7200,null,48,5.3,5.3,{"v":0.96048,"d":"0.96"},"翼板重合",null,566,null,null,"FG110203-SS-FB02.23-15","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,567,null,{"v":4,"d":"4.00"},"FG110203-SS-FB02.23-15图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台十","方（扁）钢","加强筋40*4",1,800,40,4,null,null,{"v":0.0704,"d":"0.07"},"无重合面",null,568,null,null,"FG110203-SS-FB02.23-15","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十二*2","[槽钢","[100*48*5.3",2,19500,null,48,5.3,5.3,{"v":5.2026,"d":"5.20"},"翼板重合",null,569,null,null,"FG110203-SS-FB02.23-16","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十二*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,570,null,{"v":28.4,"d":"28.40"},"FG110203-SS-FB02.23-16图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台十二*2","方（扁）钢","加强筋40*4",12,1000,40,4,null,null,{"v":1.056,"d":"1.06"},"无重合面",null,571,null,null,"FG110203-SS-FB02.23-16","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十二*2","方（扁）钢","加强筋40*4",4,900,40,4,null,null,{"v":0.3168,"d":"0.32"},"无重合面",null,572,null,null,"FG110203-SS-FB02.23-16","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十四","[槽钢","[100*48*5.3",1,25500,null,48,5.3,5.3,{"v":3.4017,"d":"3.40"},"翼板重合",null,573,null,null,"FG110203-SS-FB02.23-16","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十四","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,574,null,{"v":23,"d":"23.00"},"FG110203-SS-FB02.23-16图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台十四","方（扁）钢","加强筋40*4",12,1000,40,4,null,null,{"v":1.056,"d":"1.06"},"无重合面",null,575,null,null,"FG110203-SS-FB02.23-16","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十四","方（扁）钢","加强筋60*6",1,1400,60,6,null,null,{"v":0.1848,"d":"0.18"},"无重合面",null,576,null,null,"FG110203-SS-FB02.23-16","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十一","[槽钢","[16b（160*63*6.5）",2,800,null,63,6.5,6.5,{"v":0.2816,"d":"0.28"},"翼板重合",null,577,null,null,"FG110203-SS-FB02.23-17","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十一","[槽钢","[16b（160*63*6.5）",2,5900,null,63,6.5,6.5,{"v":2.0768,"d":"2.08"},"翼板重合",null,578,null,null,"FG110203-SS-FB02.23-17","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十一","[槽钢","[100*48*5.3",1,16100,null,48,5.3,5.3,{"v":2.14774,"d":"2.15"},"翼板重合",null,579,null,null,"FG110203-SS-FB02.23-17","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十一","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,580,null,{"v":19,"d":"19.00"},"FG110203-SS-FB02.23-17图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台十一","方（扁）钢","加强筋40*4",10,800,40,4,null,null,{"v":0.704,"d":"0.70"},"无重合面",null,581,null,null,"FG110203-SS-FB02.23-17","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十三","[槽钢","[100*48*5.3",1,10700,null,48,5.3,5.3,{"v":1.42738,"d":"1.43"},"翼板重合",null,582,null,null,"FG110203-SS-FB02.23-17","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十三","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,583,null,{"v":10.8,"d":"10.80"},"FG110203-SS-FB02.23-17图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台十三","方（扁）钢","加强筋60*6",5,1400,60,6,null,null,{"v":0.924,"d":"0.92"},"无重合面",null,584,null,null,"FG110203-SS-FB02.23-17","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十二","[槽钢","[100*48*5.3",1,5000,null,48,5.3,5.3,{"v":0.667,"d":"0.67"},"翼板重合",null,585,null,null,"FG110203-SS-FB02.23-17","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十二","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,586,null,{"v":3,"d":"3.00"},"FG110203-SS-FB02.23-17图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台二十二","方（扁）钢","加强筋40*4",1,1000,40,4,null,null,{"v":0.088,"d":"0.09"},"无重合面",null,587,null,null,"FG110203-SS-FB02.23-17","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十五","[槽钢","[100*48*5.3",1,18000,null,48,5.3,5.3,{"v":2.4012,"d":"2.40"},"翼板重合",null,588,null,null,"FG110203-SS-FB02.23-18","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十五","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,589,null,{"v":17.4,"d":"17.40"},"FG110203-SS-FB02.23-18图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台十五","方（扁）钢","加强筋40*4",6,1000,40,4,null,null,{"v":0.528,"d":"0.53"},"无重合面",null,590,null,null,"FG110203-SS-FB02.23-18","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十五","方（扁）钢","加强筋60*6",2,1200,60,6,null,null,{"v":0.3168,"d":"0.32"},"无重合面",null,591,null,null,"FG110203-SS-FB02.23-18","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十六","[槽钢","[100*48*5.3",1,25600,null,48,5.3,5.3,{"v":3.41504,"d":"3.42"},"翼板重合",null,592,null,null,"FG110203-SS-FB02.23-18","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十六","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,593,null,{"v":24.2,"d":"24.20"},"FG110203-SS-FB02.23-18图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台十六","方（扁）钢","加强筋40*4",10,1000,40,4,null,null,0.88,"无重合面",null,594,null,null,"FG110203-SS-FB02.23-18","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十六","方（扁）钢","加强筋60*6",3,1400,60,6,null,null,{"v":0.5544,"d":"0.55"},"无重合面",null,595,null,null,"FG110203-SS-FB02.23-18","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十七","[槽钢","[100*48*5.3",1,20000,null,48,5.3,5.3,{"v":2.668,"d":"2.67"},"翼板重合",null,596,null,null,"FG110203-SS-FB02.23-19","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十七","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,597,null,{"v":14.6,"d":"14.60"},"FG110203-SS-FB02.23-19图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台十七","方（扁）钢","加强筋40*4",8,1000,40,4,null,null,{"v":0.704,"d":"0.70"},"无重合面",null,598,null,null,"FG110203-SS-FB02.23-19","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十八","[槽钢","[100*48*5.3",1,27100,null,48,5.3,5.3,{"v":3.61514,"d":"3.62"},"翼板重合",null,599,null,null,"FG110203-SS-FB02.23-19","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十八","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,600,null,{"v":23.2,"d":"23.20"},"FG110203-SS-FB02.23-19图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台十八","方（扁）钢","加强筋40*4",1,1000,40,4,null,null,{"v":0.088,"d":"0.09"},"无重合面",null,601,null,null,"FG110203-SS-FB02.23-19","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十九*3","[槽钢","[100*48*5.3",3,16200,null,48,5.3,5.3,{"v":6.48324,"d":"6.48"},"翼板重合",null,602,null,null,"FG110203-SS-FB02.23-20","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台十九*3","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,603,null,{"v":37.2,"d":"37.20"},"FG110203-SS-FB02.23-20图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台十九*3","方（扁）钢","加强筋40*4",21,1000,40,4,null,null,{"v":1.848,"d":"1.85"},"无重合面",null,604,null,null,"FG110203-SS-FB02.23-20","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十","[槽钢","[100*48*5.3",1,16600,null,48,5.3,5.3,{"v":2.21444,"d":"2.21"},"翼板重合",null,605,null,null,"FG110203-SS-FB02.23-20","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,606,null,{"v":12.6,"d":"12.60"},"FG110203-SS-FB02.23-20图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台二十","方（扁）钢","加强筋40*4",7,1000,40,4,null,null,{"v":0.616,"d":"0.62"},"无重合面",null,607,null,null,"FG110203-SS-FB02.23-20","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十一*2","[槽钢","[100*48*5.3",2,19600,null,48,5.3,5.3,{"v":5.22928,"d":"5.23"},"翼板重合",null,608,null,null,"FG110203-SS-FB02.23-21","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十一*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,609,null,{"v":28.8,"d":"28.80"},"FG110203-SS-FB02.23-21图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台二十一*2","方（扁）钢","加强筋40*4",16,1000,40,4,null,null,{"v":1.408,"d":"1.41"},"无重合面",null,610,null,null,"FG110203-SS-FB02.23-21","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十三","[槽钢","[100*48*5.3",1,16100,null,48,5.3,5.3,{"v":2.14774,"d":"2.15"},"翼板重合",null,611,null,null,"FG110203-SS-FB02.23-21","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十三","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,612,null,{"v":12.2,"d":"12.20"},"FG110203-SS-FB02.23-21图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台二十三","方（扁）钢","加强筋40*4",6,1000,40,4,null,null,{"v":0.528,"d":"0.53"},"无重合面",null,613,null,null,"FG110203-SS-FB02.23-21","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十四","[槽钢","[100*48*5.3",1,73200,null,48,5.3,5.3,{"v":9.76488,"d":"9.76"},"翼板重合",null,614,null,null,"FG110203-SS-FB02.23-22","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十四","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,615,null,{"v":74.6,"d":"74.60"},"FG110203-SS-FB02.23-22图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台二十四","方（扁）钢","加强筋40*4",43,1000,40,4,null,null,{"v":3.784,"d":"3.78"},"无重合面",null,616,null,null,"FG110203-SS-FB02.23-22","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十四","方（扁）钢","加强筋60*6",1,1200,60,6,null,null,{"v":0.1584,"d":"0.16"},"无重合面",null,617,null,null,"FG110203-SS-FB02.23-22","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十六","[槽钢","[100*48*5.3",1,18700,null,48,5.3,5.3,{"v":2.49458,"d":"2.49"},"翼板重合",null,618,null,null,"FG110203-SS-FB02.23-23","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十六","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,619,null,{"v":13.8,"d":"13.80"},"FG110203-SS-FB02.23-23图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台二十六","方（扁）钢","加强筋40*4",7,1000,40,4,null,null,{"v":0.616,"d":"0.62"},"无重合面",null,620,null,null,"FG110203-SS-FB02.23-23","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十九","[槽钢","[100*48*5.3",1,32000,null,48,5.3,5.3,{"v":4.2688,"d":"4.27"},"翼板重合",null,621,null,null,"FG110203-SS-FB02.23-23","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十九","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,622,null,{"v":27.2,"d":"27.20"},"FG110203-SS-FB02.23-23图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台二十九","方（扁）钢","加强筋40*4",15,1000,40,4,null,null,1.32,"无重合面",null,623,null,null,"FG110203-SS-FB02.23-23","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十五*2","[槽钢","[100*48*5.3",2,12500,null,48,5.3,5.3,{"v":3.335,"d":"3.34"},"翼板重合",null,624,null,null,"FG110203-SS-FB02.23-24","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十五*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,625,null,{"v":19.2,"d":"19.20"},"FG110203-SS-FB02.23-24图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台二十五*2","方（扁）钢","加强筋40*4",10,1000,40,4,null,null,0.88,"无重合面",null,626,null,null,"FG110203-SS-FB02.23-24","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十五*2","方（扁）钢","加强筋60*6",1,1200,60,6,null,null,{"v":0.1584,"d":"0.16"},"无重合面",null,627,null,null,"FG110203-SS-FB02.23-24","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十七","[槽钢","[100*48*5.3",1,7800,null,48,5.3,5.3,{"v":1.04052,"d":"1.04"},"翼板重合",null,628,null,null,"FG110203-SS-FB02.23-24","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十七","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,629,null,{"v":5.6,"d":"5.60"},"FG110203-SS-FB02.23-24图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台二十七","方（扁）钢","加强筋40*4",3,1000,40,4,null,null,{"v":0.264,"d":"0.26"},"无重合面",null,630,null,null,"FG110203-SS-FB02.23-24","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十八","[槽钢","[100*48*5.3",1,6500,null,48,5.3,5.3,{"v":0.8671,"d":"0.87"},"翼板重合",null,631,null,null,"FG110203-SS-FB02.23-24","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台二十八","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,632,null,{"v":4.4,"d":"4.40"},"FG110203-SS-FB02.23-24图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台二十八","方（扁）钢","加强筋40*4",2,1000,40,4,null,null,{"v":0.176,"d":"0.18"},"无重合面",null,633,null,null,"FG110203-SS-FB02.23-24","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十*2","[槽钢","[100*48*5.3",2,6450,null,48,5.3,5.3,{"v":1.72086,"d":"1.72"},"翼板重合",null,634,null,null,"FG110203-SS-FB02.23-24","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,635,null,{"v":8.8,"d":"8.80"},"FG110203-SS-FB02.23-24图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台三十*2","方（扁）钢","加强筋40*4",4,1000,40,4,null,null,{"v":0.352,"d":"0.35"},"无重合面",null,636,null,null,"FG110203-SS-FB02.23-24","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十一*2","[槽钢","[100*48*5.3",2,31300,null,48,5.3,5.3,{"v":8.35084,"d":"8.35"},"翼板重合",null,637,null,null,"FG110203-SS-FB02.23-25","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十一*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,638,null,{"v":60,"d":"60.00"},"FG110203-SS-FB02.23-25图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台三十一*2","方（扁）钢","加强筋40*4",26,1000,40,4,null,null,{"v":2.288,"d":"2.29"},"无重合面",null,639,null,null,"FG110203-SS-FB02.23-25","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十一*2","方（扁）钢","加强筋60*6",6,1200,60,6,null,null,{"v":0.9504,"d":"0.95"},"无重合面",null,640,null,null,"FG110203-SS-FB02.23-25","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十八","[槽钢","[100*48*5.3",1,25400,null,48,5.3,5.3,{"v":3.38836,"d":"3.39"},"翼板重合",null,641,null,null,"FG110203-SS-FB02.23-25","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十八","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,642,null,{"v":23,"d":"23.00"},"FG110203-SS-FB02.23-25图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台三十八","方（扁）钢","加强筋40*4",16,1000,40,4,null,null,{"v":1.408,"d":"1.41"},"无重合面",null,643,null,null,"FG110203-SS-FB02.23-25","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十二","[槽钢","[100*48*5.3",1,29300,null,48,5.3,5.3,{"v":3.90862,"d":"3.91"},"翼板重合",null,644,null,null,"FG110203-SS-FB02.23-26","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十二","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,645,null,{"v":22,"d":"22.00"},"FG110203-SS-FB02.23-26图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台三十二","方（扁）钢","加强筋40*4",12,1000,40,4,null,null,{"v":1.056,"d":"1.06"},"无重合面",null,646,null,null,"FG110203-SS-FB02.23-26","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十三","[槽钢","[100*48*5.3",1,46700,null,48,5.3,5.3,{"v":6.22978,"d":"6.23"},"翼板重合",null,647,null,null,"FG110203-SS-FB02.23-26","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十三","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,648,null,{"v":41.8,"d":"41.80"},"FG110203-SS-FB02.23-26图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台三十三","方（扁）钢","加强筋40*4",24,1000,40,4,null,null,{"v":2.112,"d":"2.11"},"无重合面",null,649,null,null,"FG110203-SS-FB02.23-26","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十四","[槽钢","[100*48*5.3",1,17200,null,48,5.3,5.3,{"v":2.29448,"d":"2.29"},"翼板重合",null,650,null,null,"FG110203-SS-FB02.23-27","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十四","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,651,null,{"v":15.2,"d":"15.20"},"FG110203-SS-FB02.23-27图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台三十四","方（扁）钢","加强筋40*4",8,1000,40,4,null,null,{"v":0.704,"d":"0.70"},"无重合面",null,652,null,null,"FG110203-SS-FB02.23-27","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十五","[槽钢","[100*48*5.3",1,26200,null,48,5.3,5.3,{"v":3.49508,"d":"3.50"},"翼板重合",null,653,null,null,"FG110203-SS-FB02.23-27","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十五","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,654,null,{"v":22,"d":"22.00"},"FG110203-SS-FB02.23-27图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台三十五","方（扁）钢","加强筋40*4",14,1000,40,4,null,null,{"v":1.232,"d":"1.23"},"无重合面",null,655,null,null,"FG110203-SS-FB02.23-27","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十六","[槽钢","[100*48*5.3",1,20000,null,48,5.3,5.3,{"v":2.668,"d":"2.67"},"翼板重合",null,656,null,null,"FG110203-SS-FB02.23-28","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十六","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,657,null,{"v":18.2,"d":"18.20"},"FG110203-SS-FB02.23-28图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台三十六","方（扁）钢","加强筋40*4",7,1000,40,4,null,null,{"v":0.616,"d":"0.62"},"无重合面",null,658,null,null,"FG110203-SS-FB02.23-28","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十六","方（扁）钢","加强筋60*6",1,1800,60,6,null,null,{"v":0.2376,"d":"0.24"},"无重合面",null,659,null,null,"FG110203-SS-FB02.23-25","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十七","[槽钢","[100*48*5.3",1,51200,null,48,5.3,5.3,{"v":6.83008,"d":"6.83"},"翼板重合",null,660,null,null,"FG110203-SS-FB02.23-28","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十七","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,661,null,{"v":43,"d":"43.00"},"FG110203-SS-FB02.23-28图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台三十七","方（扁）钢","加强筋40*4",27,1000,40,4,null,null,{"v":2.376,"d":"2.38"},"无重合面",null,662,null,null,"FG110203-SS-FB02.23-28","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十九","[槽钢","[100*48*5.3",1,14000,null,48,5.3,5.3,{"v":1.8676,"d":"1.87"},"翼板重合",null,663,null,null,"FG110203-SS-FB02.23-29","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台三十九","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,664,null,{"v":11.2,"d":"11.20"},"FG110203-SS-FB02.23-29图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台三十九","方（扁）钢","加强筋40*4",6,1000,40,4,null,null,{"v":0.528,"d":"0.53"},"无重合面",null,665,null,null,"FG110203-SS-FB02.23-29","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台四十一*2","[槽钢","[100*48*5.3",2,26400,null,48,5.3,5.3,{"v":7.04352,"d":"7.04"},"翼板重合",null,666,null,null,"FG110203-SS-FB02.23-29","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台四十一*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,667,null,{"v":53.2,"d":"53.20"},"FG110203-SS-FB02.23-29图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台四十一*2","方（扁）钢","加强筋40*4",36,1000,40,4,null,null,{"v":3.168,"d":"3.17"},"无重合面",null,668,null,null,"FG110203-SS-FB02.23-29","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台四十","[槽钢","[100*48*5.3",1,28000,null,48,5.3,5.3,{"v":3.7352,"d":"3.74"},"翼板重合",null,669,null,null,"FG110203-SS-FB02.23-30","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台四十","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,670,null,{"v":27.8,"d":"27.80"},"FG110203-SS-FB02.23-30图纸标明面积、无具体尺寸","重度腐蚀","石墨烯改性钛基纳米重防腐涂料","钢构面积为0"]
["一系洗涤区域操作台平台四十","方（扁）钢","加强筋40*4",20,1000,40,4,null,null,1.76,"无重合面",null,671,null,null,"FG110203-SS-FB02.23-30","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台悬臂梁一*166","[槽钢","[126*53*5.5",166,1080,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":36.03528,"d":"36.04"},"无重合面",null,672,null,null,"FG110203-SS-FB02.23-31","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台悬臂梁二*15","[槽钢","[126*53*5.5",15,990,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":2.98485,"d":"2.98"},"无重合面",null,673,null,null,"FG110203-SS-FB02.23-31","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台悬臂梁三*8","[槽钢","[126*53*5.5",8,1290,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":2.07432,"d":"2.07"},"无重合面",null,674,null,null,"FG110203-SS-FB02.23-31","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱一*4","[槽钢","[100*48*5.3",4,10300,null,48,5.3,5.3,{"v":7.47368,"d":"7.47"},"无重合面",null,675,null,null,"FG110203-SS-FB02.23-31","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱一*4","L型钢","L50*50*5",4,800,null,50,5,5,0.32,"无重合面",null,676,null,null,"FG110203-SS-FB02.23-31","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱一*4","L型钢","L50*50*5",8,1130,null,50,5,5,{"v":0.904,"d":"0.90"},"无重合面",null,677,null,null,"FG110203-SS-FB02.23-31","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱二*8","[槽钢","[100*48*5.3",8,12600,null,48,5.3,5.3,{"v":18.28512,"d":"18.29"},"无重合面",null,678,null,null,"FG110203-SS-FB02.23-29","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱二*8","L型钢","L50*50*5",16,700,null,50,5,5,1.12,"无重合面",null,679,null,null,"FG110203-SS-FB02.23-31","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱二*8","L型钢","L50*50*5",32,800,null,50,5,5,2.56,"无重合面",null,680,null,null,"FG110203-SS-FB02.23-31","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱二*8","L型钢","L50*50*5",32,1000,null,50,5,5,{"v":3.2,"d":"3.20"},"无重合面",null,681,null,null,"FG110203-SS-FB02.23-31","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱二*8","L型钢","L50*50*5",32,1130,null,50,5,5,{"v":3.616,"d":"3.62"},"无重合面",null,682,null,null,"FG110203-SS-FB02.23-31","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱三*4","[槽钢","[100*48*5.3",4,12400,null,48,5.3,5.3,{"v":8.99744,"d":"9.00"},"无重合面",null,683,null,null,"FG110203-SS-FB02.23-32","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱三*4","L型钢","L50*50*5",8,500,null,50,5,5,{"v":0.4,"d":"0.40"},"无重合面",null,684,null,null,"FG110203-SS-FB02.23-32","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱三*4","L型钢","L50*50*5",16,800,null,50,5,5,1.28,"无重合面",null,685,null,null,"FG110203-SS-FB02.23-32","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱三*4","L型钢","L50*50*5",16,1000,null,50,5,5,{"v":1.6,"d":"1.60"},"无重合面",null,686,null,null,"FG110203-SS-FB02.23-32","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱三*4","L型钢","L50*50*5",16,1130,null,50,5,5,{"v":1.808,"d":"1.81"},"无重合面",null,687,null,null,"FG110203-SS-FB02.23-32","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱四*4","[槽钢","[100*48*5.3",4,4100,null,48,5.3,5.3,{"v":2.97496,"d":"2.97"},"无重合面",null,688,null,null,"FG110203-SS-FB02.23-32","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱四*4","L型钢","L50*50*5",16,800,null,50,5,5,1.28,"无重合面",null,689,null,null,"FG110203-SS-FB02.23-32","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱五","[槽钢","[100*48*5.3",1,4100,null,48,5.3,5.3,{"v":0.74374,"d":"0.74"},"无重合面",null,690,null,null,"FG110203-SS-FB02.23-32","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱五","L型钢","L50*50*5",2,850,null,50,5,5,0.17,"无重合面",null,691,null,null,"FG110203-SS-FB02.23-32","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱六","[槽钢","[100*48*5.3",1,6200,null,48,5.3,5.3,{"v":1.12468,"d":"1.12"},"无重合面",null,692,null,null,"FG110203-SS-FB02.23-33","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱六","L型钢","L50*50*5",1,2640,null,50,5,5,{"v":0.264,"d":"0.26"},"无重合面",null,693,null,null,"FG110203-SS-FB02.23-33","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱七","[槽钢","[100*48*5.3",1,12400,null,48,5.3,5.3,{"v":2.24936,"d":"2.25"},"无重合面",null,694,null,null,"FG110203-SS-FB02.23-33","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱七","L型钢","L50*50*5",1,14100,null,50,5,5,1.41,"无重合面",null,695,null,null,"FG110203-SS-FB02.23-33","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱八*2","[槽钢","[100*48*5.3",2,10000,null,48,5.3,5.3,{"v":3.628,"d":"3.63"},"无重合面",null,696,null,null,"FG110203-SS-FB02.23-33","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱八*2","L型钢","L50*50*5",2,3100,null,50,5,5,0.62,"无重合面",null,697,null,null,"FG110203-SS-FB02.23-33","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台三角架一*10","[槽钢","[126*53*5.5",10,1480,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":2.9748,"d":"2.97"},"无重合面",null,698,null,null,"FG110203-SS-FB02.23-34","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台三角架一*10","[槽钢","[100*48*5.3",10,1660,null,48,5.3,5.3,{"v":3.01124,"d":"3.01"},"无重合面",null,699,null,null,"FG110203-SS-FB02.23-34","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台三角架二*7","[槽钢","[126*53*5.5",7,1880,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":2.64516,"d":"2.65"},"无重合面",null,700,null,null,"FG110203-SS-FB02.23-34","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台三角架二*7","[槽钢","[100*48*5.3",7,2220,null,48,5.3,5.3,{"v":2.818956,"d":"2.82"},"无重合面",null,701,null,null,"FG110203-SS-FB02.23-34","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台支架一二三*11*24*24","[槽钢","[100*48*5.3",1,84600,null,48,5.3,5.3,{"v":15.34644,"d":"15.35"},"无重合面",null,702,null,null,"FG110203-SS-FB02.23-35","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁一*8","[槽钢","[220*79*9",8,6290,null,79,9,9,{"v":14.99536,"d":"15.00"},"无重合面",null,703,null,null,"FG110203-SS-FB02.23-36","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁一*8","L型钢","L180*110*10",16,150,null,100,10,10,0.48,"无重合面",null,704,null,null,"FG110203-SS-FB02.23-36","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁二*8","[槽钢","[220*79*9",8,4830,null,79,9,9,{"v":11.51472,"d":"11.51"},"无重合面",null,705,null,null,"FG110203-SS-FB02.23-36","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁二*8","L型钢","L180*110*10",16,150,null,100,10,10,0.48,"无重合面",null,706,null,null,"FG110203-SS-FB02.23-36","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁三*16","[槽钢","[220*79*9",16,6620,null,79,9,9,{"v":31.56416,"d":"31.56"},"无重合面",null,707,null,null,"FG110203-SS-FB02.23-37","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁三*16","L型钢","L180*110*10",32,150,null,100,10,10,0.96,"无重合面",null,708,null,null,"FG110203-SS-FB02.23-37","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁四*16","[槽钢","[220*79*9",16,4630,null,79,9,9,{"v":22.07584,"d":"22.08"},"无重合面",null,709,null,null,"FG110203-SS-FB02.23-37","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁四*16","L型钢","L180*110*10",32,150,null,100,10,10,0.96,"无重合面",null,710,null,null,"FG110203-SS-FB02.23-37","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁五*6","[槽钢","[220*79*9",6,6550,null,79,9,9,{"v":11.7114,"d":"11.71"},"无重合面",null,711,null,null,"FG110203-SS-FB02.23-38","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁五*6","L型钢","L180*110*10",12,150,null,100,10,10,0.36,"无重合面",null,712,null,null,"FG110203-SS-FB02.23-38","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁六*6","[槽钢","[220*79*9",6,4940,null,79,9,9,{"v":8.83272,"d":"8.83"},"无重合面",null,713,null,null,"FG110203-SS-FB02.23-38","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁六*6","L型钢","L180*110*10",12,150,null,100,10,10,0.36,"无重合面",null,714,null,null,"FG110203-SS-FB02.23-38","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁七","[槽钢","[220*79*9",1,6400,null,79,9,9,{"v":1.9072,"d":"1.91"},"无重合面",null,715,null,null,"FG110203-SS-FB02.23-39","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁七","L型钢","L180*110*10",2,150,null,100,10,10,0.06,"无重合面",null,716,null,null,"FG110203-SS-FB02.23-39","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁八","[槽钢","[220*79*9",1,4500,null,79,9,9,{"v":1.341,"d":"1.34"},"无重合面",null,717,null,null,"FG110203-SS-FB02.23-39","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁八","L型钢","L180*110*10",2,150,null,100,10,10,0.06,"无重合面",null,718,null,null,"FG110203-SS-FB02.23-39","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁九*2","[槽钢","[220*79*9",2,3800,null,79,9,9,{"v":2.2648,"d":"2.26"},"无重合面",null,719,null,null,"FG110203-SS-FB02.23-40","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁九*2","L型钢","L180*110*10",4,150,null,100,10,10,0.12,"无重合面",null,720,null,null,"FG110203-SS-FB02.23-40","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁十","[槽钢","[220*79*9",1,4940,null,79,9,9,{"v":1.47212,"d":"1.47"},"无重合面",null,721,null,null,"FG110203-SS-FB02.23-40","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁十","L型钢","L180*110*10",2,150,null,100,10,10,0.06,"无重合面",null,722,null,null,"FG110203-SS-FB02.23-40","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁十一","[槽钢","[220*79*9",1,6550,null,79,9,9,{"v":1.9519,"d":"1.95"},"无重合面",null,723,null,null,"FG110203-SS-FB02.23-41","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁十一","L型钢","L180*110*10",2,150,null,100,10,10,0.06,"无重合面",null,724,null,null,"FG110203-SS-FB02.23-41","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁十二","[槽钢","[220*79*9",1,4640,null,79,9,9,{"v":1.38272,"d":"1.38"},"无重合面",null,725,null,null,"FG110203-SS-FB02.23-41","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁十二","L型钢","L180*110*10",2,150,null,100,10,10,0.06,"无重合面",null,726,null,null,"FG110203-SS-FB02.23-41","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁十三","[槽钢","[220*79*9",1,6620,null,79,9,9,{"v":1.97276,"d":"1.97"},"无重合面",null,727,null,null,"FG110203-SS-FB02.23-42","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台槽钢梁十三","L型钢","L180*110*10",2,150,null,100,10,10,0.06,"无重合面",null,728,null,null,"FG110203-SS-FB02.23-42","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱九*2","[槽钢","[100*48*5.3",2,12100,null,48,5.3,5.3,{"v":4.38988,"d":"4.39"},"无重合面",null,729,null,null,"FG110203-SS-FB02.23-42","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["一系洗涤区域操作台平台支柱九*2","L型钢","L50*50*5",2,12500,null,50,5,5,{"v":2.5,"d":"2.50"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-42","重度腐蚀","石墨烯改性钛基纳米重防腐涂料",{"v":0,"d":"0%"}]
["二系洗涤区域操作台45斜梯护栏231m","圆钢","圆钢 Q50*3",2,231000,50,{"$nulls":3},{"v":72.534,"d":"72.53"},"无重合面",null,730,null,{"v":72.534,"d":"72.53"},"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系洗涤区域操作台45斜梯护栏231m","方（扁）钢","扁铁40*4",2,231000,40,4,null,null,{"v":40.656,"d":"40.66"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台45°斜梯T2B08a-30*2","[槽钢","[16b（160*63*6.5）",4,4250,null,63,6.5,6.5,{"v":4.063,"d":"4.06"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台45°斜梯T2B08a-30*2","方（扁）钢","花纹板4.5",30,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,15.84,"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台49°斜梯T2B07a-29*1","[槽钢","[16b（160*63*6.5）",2,4000,null,63,6.5,6.5,{"v":1.912,"d":"1.91"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台49°斜梯T2B07a-29*1","方（扁）钢","花纹板4.5",13,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":6.006,"d":"6.01"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台41°斜梯T2B07a-22*1","[槽钢","[16b（160*63*6.5）",2,3200,null,63,6.5,6.5,{"v":1.5296,"d":"1.53"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台41°斜梯T2B07a-22*1","方（扁）钢","花纹板4.5",12,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":5.544,"d":"5.54"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台40°斜梯T2B07a-20*1","[槽钢","[16b（160*63*6.5）",2,3100,null,63,6.5,6.5,{"v":1.4818,"d":"1.48"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台40°斜梯T2B07a-20*1","方（扁）钢","花纹板4.5",11,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":5.082,"d":"5.08"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台51°斜梯T2B07a-30*3","[槽钢","[16b（160*63*6.5）",6,3800,null,63,6.5,6.5,{"v":5.4492,"d":"5.45"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台51°斜梯T2B07a-30*3","方（扁）钢","花纹板4.5",36,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":16.632,"d":"16.63"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台49°斜梯T2B07a-30*5","[槽钢","[16b（160*63*6.5）",10,3900,null,63,6.5,6.5,{"v":9.321,"d":"9.32"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台49°斜梯T2B07a-30*5","方（扁）钢","花纹板4.5",60,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,27.72,"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台46°斜梯T2B07a-27*4","[槽钢","[16b（160*63*6.5）",8,3800,null,63,6.5,6.5,{"v":7.2656,"d":"7.27"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台46°斜梯T2B07a-27*4","方（扁）钢","花纹板4.5",48,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":22.176,"d":"22.18"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台50°斜梯T2B07a-30*4","[槽钢","[16b（160*63*6.5）",8,3900,null,63,6.5,6.5,{"v":7.4568,"d":"7.46"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台50°斜梯T2B07a-30*4","方（扁）钢","花纹板4.5",48,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":22.176,"d":"22.18"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台47°斜梯T2B07a-28*1","[槽钢","[16b（160*63*6.5）",2,3900,null,63,6.5,6.5,{"v":1.8642,"d":"1.86"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台47°斜梯T2B07a-28*1","方（扁）钢","花纹板4.5",12,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":5.544,"d":"5.54"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台33°斜梯T1B07a-17*1","[槽钢","[16b（160*63*6.5）",2,3200,null,63,6.5,6.5,{"v":1.5296,"d":"1.53"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台33°斜梯T1B07a-17*1","方（扁）钢","花纹板4.5",11,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":5.082,"d":"5.08"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台27°斜梯T1B07a-13*1","[槽钢","[16b（160*63*6.5）",2,2800,null,63,6.5,6.5,{"v":1.3384,"d":"1.34"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台27°斜梯T1B07a-13*1","方（扁）钢","花纹板4.5",10,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,4.62,"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台43°斜梯T2B07a-24*2","[槽钢","[16b（160*63*6.5）",4,3400,null,63,6.5,6.5,{"v":3.2504,"d":"3.25"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台43°斜梯T2B07a-24*2","方（扁）钢","花纹板4.5",24,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":11.088,"d":"11.09"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台52°斜梯T2B07a-33*1","[槽钢","[16b（160*63*6.5）",2,4200,null,63,6.5,6.5,{"v":2.0076,"d":"2.01"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台52°斜梯T2B07a-33*1","方（扁）钢","花纹板4.5",13,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":6.006,"d":"6.01"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台51°斜梯T2B07a-32.5*2","[槽钢","[16b（160*63*6.5）",4,4000,null,63,6.5,6.5,{"v":3.824,"d":"3.82"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台51°斜梯T2B07a-32.5*2","方（扁）钢","花纹板4.5",26,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":12.012,"d":"12.01"},"FG110203-SS-FB02.23-1-1+图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台盘梯栏杆15m","圆钢","圆钢 Q50*3",2,15000,50,{"$nulls":3},4.71,"无重合面",null,730,null,4.71,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系洗涤区域操作台盘梯栏杆15m","方（扁）钢","扁铁50*4",2,15000,50,4,null,null,3.24,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台护栏87m","圆钢","圆钢 Q50*3",2,910000,50,{"$nulls":3},285.74,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台护栏87m","方（扁）钢","扁铁40*4",2,910000,40,4,null,null,160.16,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台护栏87m","方（扁）钢","踢腿板100*4",1,910000,100,4,null,null,189.28,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-1-1+","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台54°斜梯3600","[槽钢","[16b（160*63*6.5）",2,4200,null,63,6.5,6.5,{"v":2.0076,"d":"2.01"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台54°斜梯3600","方（扁）钢","花纹板4.5",15,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,5.46,"FG110203-SS-FB02.23-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台54°斜梯3600","圆钢","圆钢 Q33.5",16,600,33.5,{"$nulls":3},{"v":1.009824,"d":"1.01"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台54°斜梯3600","圆钢","圆钢 Q50*3",2,6600,50,{"$nulls":3},{"v":2.0724,"d":"2.07"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台54°斜梯3500","[槽钢","[16b（160*63*6.5）",2,4100,null,63,6.5,6.5,{"v":1.9598,"d":"1.96"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台54°斜梯3500","方（扁）钢","花纹板4.5",14,700,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":5.096,"d":"5.10"},"FG110203-SS-FB02.23-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台54°斜梯3500","圆钢","圆钢 Q33.5",16,600,33.5,{"$nulls":3},{"v":1.009824,"d":"1.01"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台54°斜梯3500","圆钢","圆钢 Q50*3",2,6500,50,{"$nulls":3},{"v":2.041,"d":"2.04"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台KH1=2400直梯*1","L型钢","L63*63*6",2,3680,null,63,6,6,{"v":0.92736,"d":"0.93"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台KH1=2400直梯*1","方（扁）钢","扁铁40*4",3,1840,40,4,null,null,{"v":0.48576,"d":"0.49"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台KH1=2400直梯*1","方（扁）钢","扁铁25*4",5,1670,25,4,null,null,{"v":0.4843,"d":"0.48"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台KH1=2400直梯*1","圆钢","圆钢Q18",8,480,18,{"$nulls":3},{"v":0.21703680000000003,"d":"0.22"},"无重合面",null,730,null,{"v":0.2170368,"d":"0.22"},"FG110203-SS-FB02.23-3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系洗涤区域操作台KH1=2400直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,730,null,{"v":0.15441264,"d":"0.15"},"FG110203-SS-FB02.23-3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系洗涤区域操作台KH1=1800直梯*1","L型钢","L63*63*6",2,3080,null,63,6,6,{"v":0.77616,"d":"0.78"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台KH1=1800直梯*1","方（扁）钢","扁铁40*4",3,1840,40,4,null,null,{"v":0.48576,"d":"0.49"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台KH1=1800直梯*1","方（扁）钢","扁铁25*4",5,1070,25,4,null,null,{"v":0.3103,"d":"0.31"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台KH1=1800直梯*1","圆钢","圆钢Q18",7,480,18,{"$nulls":3},{"v":0.1899072,"d":"0.19"},"无重合面",null,730,null,{"v":0.1899072,"d":"0.19"},"FG110203-SS-FB02.23-3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系洗涤区域操作台KH1=1800直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,730,null,{"v":0.15441264,"d":"0.15"},"FG110203-SS-FB02.23-3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系洗涤区域操作台KH1=2000直梯*1","L型钢","L63*63*6",2,3280,null,63,6,6,{"v":0.82656,"d":"0.83"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台KH1=2000直梯*1","方（扁）钢","扁铁40*4",3,1840,40,4,null,null,{"v":0.48576,"d":"0.49"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台KH1=2000直梯*1","方（扁）钢","扁铁25*4",5,1270,25,4,null,null,{"v":0.3683,"d":"0.37"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台KH1=2000直梯*1","圆钢","圆钢Q18",7,480,18,{"$nulls":3},{"v":0.1899072,"d":"0.19"},"无重合面",null,730,null,{"v":0.1899072,"d":"0.19"},"FG110203-SS-FB02.23-3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系洗涤区域操作台KH1=2000直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,730,null,{"v":0.15441264,"d":"0.15"},"FG110203-SS-FB02.23-3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系洗涤区域操作台盘梯800*4","方（扁）钢","外侧板160*8",4,1320,160,8,null,null,{"v":1.77408,"d":"1.77"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台盘梯800*4","方（扁）钢","内侧板160*8",4,1130,160,8,null,null,{"v":1.51872,"d":"1.52"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台盘梯800*4","L型钢","L63*63*6",16,226,null,63,6,6,{"v":0.455616,"d":"0.46"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台盘梯800*4","方（扁）钢","踏板",16,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":8.448,"d":"8.45"},"FG110203-SS-FB02.23-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台盘梯900*2","方（扁）钢","外侧板160*8",2,1480,160,8,null,null,{"v":0.99456,"d":"0.99"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台盘梯900*2","方（扁）钢","内侧板160*8",2,1270,160,8,null,null,{"v":0.85344,"d":"0.85"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台盘梯900*2","L型钢","L63*63*6",8,226,null,63,6,6,{"v":0.227808,"d":"0.23"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台盘梯900*2","方（扁）钢","踏板",10,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,5.28,"FG110203-SS-FB02.23-5图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台盘梯1400","方（扁）钢","外侧板160*8",1,2230,160,8,null,null,{"v":0.74928,"d":"0.75"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台盘梯1400","方（扁）钢","内侧板160*8",1,1980,160,8,null,null,{"v":0.66528,"d":"0.67"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台盘梯1400","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-6","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台盘梯1400","方（扁）钢","踏板",7,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":3.696,"d":"3.70"},"FG110203-SS-FB02.23-6图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台盘梯1500","方（扁）钢","外侧板160*8",1,2400,160,8,null,null,{"v":0.8064,"d":"0.81"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台盘梯1500","方（扁）钢","内侧板160*8",1,2100,160,8,null,null,{"v":0.7056,"d":"0.71"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台盘梯1500","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-7","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台盘梯1500","方（扁）钢","踏板",7,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":3.696,"d":"3.70"},"FG110203-SS-FB02.23-7图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台盘梯1000*2","方（扁）钢","外侧板160*8",2,1600,160,8,null,null,{"v":1.0752,"d":"1.08"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-8、9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台盘梯1000*2","方（扁）钢","内侧板160*8",2,1400,160,8,null,null,{"v":0.9408,"d":"0.94"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-8、9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台盘梯1000*2","L型钢","L63*63*6",8,226,null,63,6,6,{"v":0.227808,"d":"0.23"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-8、9","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台盘梯1000*2","方（扁）钢","踏板",10,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,5.28,"FG110203-SS-FB02.23-8、9图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台AD=800直梯*2","方（扁）钢","钢板60*8",4,3370,60,8,null,null,{"v":1.83328,"d":"1.83"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台AD=800直梯*2","圆钢","圆钢Q18",6,500,18,{"$nulls":3},{"v":0.16956,"d":"0.17"},"无重合面",null,730,null,{"v":0.16956,"d":"0.17"},"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系洗涤区域操作台AD=950直梯*2","方（扁）钢","钢板60*8",4,3500,60,8,null,null,{"v":1.904,"d":"1.90"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台AD=950直梯*2","圆钢","圆钢Q18",6,500,18,{"$nulls":3},{"v":0.16956,"d":"0.17"},"无重合面",null,730,null,{"v":0.16956,"d":"0.17"},"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系洗涤区域操作台AD=700直梯*2","方（扁）钢","钢板60*8",4,3270,60,8,null,null,{"v":1.77888,"d":"1.78"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台AD=700直梯*2","圆钢","圆钢Q18",6,500,18,{"$nulls":3},{"v":0.16956,"d":"0.17"},"无重合面",null,730,null,{"v":0.16956,"d":"0.17"},"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系洗涤区域操作台AD=750直梯*1","方（扁）钢","钢板60*8",4,3300,60,8,null,null,{"v":1.7952,"d":"1.80"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台AD=750直梯*1","圆钢","圆钢Q18",6,500,18,{"$nulls":3},{"v":0.16956,"d":"0.17"},"无重合面",null,730,null,{"v":0.16956,"d":"0.17"},"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系洗涤区域操作台AD=1100直梯*1","方（扁）钢","钢板60*8",2,3670,60,8,null,null,{"v":0.99824,"d":"1.00"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台AD=1100直梯*1","圆钢","圆钢Q18",4,500,18,{"$nulls":3},{"v":0.11304,"d":"0.11"},"无重合面",null,730,null,{"v":0.11304,"d":"0.11"},"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系洗涤区域操作台AD=600直梯*1","方（扁）钢","钢板60*8",2,3170,60,8,null,null,{"v":0.86224,"d":"0.86"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台AD=600直梯*1","圆钢","圆钢Q18",3,500,18,{"$nulls":3},{"v":0.08478,"d":"0.08"},"无重合面",null,730,null,{"v":0.08478,"d":"0.08"},"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系洗涤区域操作台FH1=2200直梯*2","方（扁）钢","钢板60*8",4,3560,60,8,null,null,{"v":1.93664,"d":"1.94"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台FH1=2200直梯*2","圆钢","圆钢Q18",24,500,18,{"$nulls":3},{"v":0.67824,"d":"0.68"},"无重合面",null,730,null,{"v":0.67824,"d":"0.68"},"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系洗涤区域操作台FH1=2200直梯*2","方（扁）钢","扁铁40*4",4,1870,40,4,null,null,{"v":0.65824,"d":"0.66"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台FH1=2200直梯*2","方（扁）钢","扁铁25*4",10,530,25,4,null,null,{"v":0.3074,"d":"0.31"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台梯子入口*3","方（扁）钢","扁铁50*4",12,1400,50,4,null,null,{"v":1.8144,"d":"1.81"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台梯子入口*3","方（扁）钢","扁铁50*4",12,1240,50,4,null,null,{"v":1.60704,"d":"1.61"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台FH1=2500直梯*1","方（扁）钢","钢板60*8",2,3860,60,8,null,null,{"v":1.04992,"d":"1.05"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台FH1=2500直梯*1","圆钢","圆钢Q18",13,500,18,{"$nulls":3},{"v":0.36738,"d":"0.37"},"无重合面",null,730,null,{"v":0.36738,"d":"0.37"},"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["二系洗涤区域操作台FH1=2500直梯*1","方（扁）钢","扁铁40*4",2,1870,40,4,null,null,{"v":0.32912,"d":"0.33"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台FH1=2500直梯*1","方（扁）钢","扁铁25*4",5,530,25,4,null,null,{"v":0.1537,"d":"0.15"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-10","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台一","[槽钢","[100*48*5.3",1,34500,null,48,5.3,5.3,{"v":4.6023,"d":"4.60"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台一","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":29.2,"d":"29.20"},"FG110203-SS-FB02.23-11图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台一","方（扁）钢","加强筋40*4",18,1000,40,4,null,null,{"v":1.584,"d":"1.58"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二","[槽钢","[100*48*5.3",1,23900,null,48,5.3,5.3,{"v":3.18826,"d":"3.19"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":18.6,"d":"18.60"},"FG110203-SS-FB02.23-11图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台二","方（扁）钢","加强筋40*4",4,1000,40,4,null,null,{"v":0.352,"d":"0.35"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二","方（扁）钢","加强筋40*4",8,900,40,4,null,null,{"v":0.6336,"d":"0.63"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-11","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三","[槽钢","[100*48*5.3",1,26400,null,48,5.3,5.3,{"v":3.52176,"d":"3.52"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":17.4,"d":"17.40"},"FG110203-SS-FB02.23-12图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台三","方（扁）钢","加强筋40*4",10,1000,40,4,null,null,0.88,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台四*6","[槽钢","[100*48*5.3",6,14200,null,48,5.3,5.3,{"v":11.36568,"d":"11.37"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台四*6","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":64.8,"d":"64.80"},"FG110203-SS-FB02.23-12图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台四*6","方（扁）钢","加强筋40*4",36,1000,40,4,null,null,{"v":3.168,"d":"3.17"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-12","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台六","[槽钢","[100*48*5.3",1,76600,null,48,5.3,5.3,{"v":10.21844,"d":"10.22"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台六","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":64.8,"d":"64.80"},"FG110203-SS-FB02.23-13图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台六","方（扁）钢","加强筋40*4",37,1000,40,4,null,null,{"v":3.256,"d":"3.26"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台六","方（扁）钢","加强筋40*4",4,700,40,4,null,null,{"v":0.2464,"d":"0.25"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-13","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台八","[槽钢","[16b（160*63*6.5）",2,1000,null,63,6.5,6.5,{"v":0.352,"d":"0.35"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台八","[槽钢","[16b（160*63*6.5）",2,33900,null,63,6.5,6.5,{"v":11.9328,"d":"11.93"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台八","[槽钢","[100*48*5.3",1,48600,null,48,5.3,5.3,{"v":6.48324,"d":"6.48"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台八","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":102.8,"d":"102.80"},"FG110203-SS-FB02.23-14图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台八","方（扁）钢","加强筋40*4",41,1000,40,4,null,null,{"v":3.608,"d":"3.61"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台八","方（扁）钢","加强筋40*4",22,900,40,4,null,null,{"v":1.7424,"d":"1.74"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台五*2","[槽钢","[100*48*5.3",2,7100,null,48,5.3,5.3,{"v":1.89428,"d":"1.89"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-14","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台五*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":10,"d":"10.00"},"FG110203-SS-FB02.23-14图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台五*2","方（扁）钢","加强筋40*4",2,1000,40,4,null,null,{"v":0.176,"d":"0.18"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台七","[槽钢","[100*48*5.3",2,7100,null,48,5.3,5.3,{"v":1.89428,"d":"1.89"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台七","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":10,"d":"10.00"},"FG110203-SS-FB02.23-15图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台七","方（扁）钢","加强筋40*4",2,1000,40,4,null,null,{"v":0.176,"d":"0.18"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台九","[槽钢","[100*48*5.3",1,26600,null,48,5.3,5.3,{"v":3.54844,"d":"3.55"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台九","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":20,"d":"20.00"},"FG110203-SS-FB02.23-15图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台九","方（扁）钢","加强筋40*4",13,800,40,4,null,null,{"v":0.9152,"d":"0.92"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十","[槽钢","[100*48*5.3",1,7200,null,48,5.3,5.3,{"v":0.96048,"d":"0.96"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":4,"d":"4.00"},"FG110203-SS-FB02.23-15图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台十","方（扁）钢","加强筋40*4",1,800,40,4,null,null,{"v":0.0704,"d":"0.07"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-15","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十二*2","[槽钢","[100*48*5.3",2,19500,null,48,5.3,5.3,{"v":5.2026,"d":"5.20"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十二*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":28.4,"d":"28.40"},"FG110203-SS-FB02.23-16图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台十二*2","方（扁）钢","加强筋40*4",12,1000,40,4,null,null,{"v":1.056,"d":"1.06"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十二*2","方（扁）钢","加强筋40*4",4,900,40,4,null,null,{"v":0.3168,"d":"0.32"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十四","[槽钢","[100*48*5.3",1,25500,null,48,5.3,5.3,{"v":3.4017,"d":"3.40"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十四","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":23,"d":"23.00"},"FG110203-SS-FB02.23-16图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台十四","方（扁）钢","加强筋40*4",12,1000,40,4,null,null,{"v":1.056,"d":"1.06"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十四","方（扁）钢","加强筋60*6",1,1400,60,6,null,null,{"v":0.1848,"d":"0.18"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-16","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十一","[槽钢","[16b（160*63*6.5）",2,800,null,63,6.5,6.5,{"v":0.2816,"d":"0.28"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-17","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十一","[槽钢","[16b（160*63*6.5）",2,5900,null,63,6.5,6.5,{"v":2.0768,"d":"2.08"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-17","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十一","[槽钢","[100*48*5.3",1,16100,null,48,5.3,5.3,{"v":2.14774,"d":"2.15"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-17","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十一","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":19,"d":"19.00"},"FG110203-SS-FB02.23-17图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台十一","方（扁）钢","加强筋40*4",10,800,40,4,null,null,{"v":0.704,"d":"0.70"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-17","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十三","[槽钢","[100*48*5.3",1,10700,null,48,5.3,5.3,{"v":1.42738,"d":"1.43"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-17","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十三","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":10.8,"d":"10.80"},"FG110203-SS-FB02.23-17图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台十三","方（扁）钢","加强筋60*6",5,1400,60,6,null,null,{"v":0.924,"d":"0.92"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-17","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十二","[槽钢","[100*48*5.3",1,5000,null,48,5.3,5.3,{"v":0.667,"d":"0.67"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-17","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十二","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":3,"d":"3.00"},"FG110203-SS-FB02.23-17图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台二十二","方（扁）钢","加强筋40*4",1,1000,40,4,null,null,{"v":0.088,"d":"0.09"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-17","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十五","[槽钢","[100*48*5.3",1,18000,null,48,5.3,5.3,{"v":2.4012,"d":"2.40"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十五","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":17.4,"d":"17.40"},"FG110203-SS-FB02.23-18图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台十五","方（扁）钢","加强筋40*4",6,1000,40,4,null,null,{"v":0.528,"d":"0.53"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十五","方（扁）钢","加强筋60*6",2,1200,60,6,null,null,{"v":0.3168,"d":"0.32"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十六","[槽钢","[100*48*5.3",1,25600,null,48,5.3,5.3,{"v":3.41504,"d":"3.42"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十六","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":24.2,"d":"24.20"},"FG110203-SS-FB02.23-18图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台十六","方（扁）钢","加强筋40*4",10,1000,40,4,null,null,0.88,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十六","方（扁）钢","加强筋60*6",3,1400,60,6,null,null,{"v":0.5544,"d":"0.55"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-18","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十七","[槽钢","[100*48*5.3",1,20000,null,48,5.3,5.3,{"v":2.668,"d":"2.67"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十七","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":14.6,"d":"14.60"},"FG110203-SS-FB02.23-19图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台十七","方（扁）钢","加强筋40*4",8,1000,40,4,null,null,{"v":0.704,"d":"0.70"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十八","[槽钢","[100*48*5.3",1,27100,null,48,5.3,5.3,{"v":3.61514,"d":"3.62"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十八","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":23.2,"d":"23.20"},"FG110203-SS-FB02.23-19图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台十八","方（扁）钢","加强筋40*4",1,1000,40,4,null,null,{"v":0.088,"d":"0.09"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-19","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十九*3","[槽钢","[100*48*5.3",3,16200,null,48,5.3,5.3,{"v":6.48324,"d":"6.48"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台十九*3","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":37.2,"d":"37.20"},"FG110203-SS-FB02.23-20图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台十九*3","方（扁）钢","加强筋40*4",21,1000,40,4,null,null,{"v":1.848,"d":"1.85"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十","[槽钢","[100*48*5.3",1,16600,null,48,5.3,5.3,{"v":2.21444,"d":"2.21"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":12.6,"d":"12.60"},"FG110203-SS-FB02.23-20图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台二十","方（扁）钢","加强筋40*4",7,1000,40,4,null,null,{"v":0.616,"d":"0.62"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-20","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十一*2","[槽钢","[100*48*5.3",2,19600,null,48,5.3,5.3,{"v":5.22928,"d":"5.23"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十一*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":28.8,"d":"28.80"},"FG110203-SS-FB02.23-21图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台二十一*2","方（扁）钢","加强筋40*4",16,1000,40,4,null,null,{"v":1.408,"d":"1.41"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十三","[槽钢","[100*48*5.3",1,16100,null,48,5.3,5.3,{"v":2.14774,"d":"2.15"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十三","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":12.2,"d":"12.20"},"FG110203-SS-FB02.23-21图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台二十三","方（扁）钢","加强筋40*4",6,1000,40,4,null,null,{"v":0.528,"d":"0.53"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-21","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十四","[槽钢","[100*48*5.3",1,73200,null,48,5.3,5.3,{"v":9.76488,"d":"9.76"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十四","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":74.6,"d":"74.60"},"FG110203-SS-FB02.23-22图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台二十四","方（扁）钢","加强筋40*4",43,1000,40,4,null,null,{"v":3.784,"d":"3.78"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十四","方（扁）钢","加强筋60*6",1,1200,60,6,null,null,{"v":0.1584,"d":"0.16"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-22","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十六","[槽钢","[100*48*5.3",1,18700,null,48,5.3,5.3,{"v":2.49458,"d":"2.49"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十六","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":13.8,"d":"13.80"},"FG110203-SS-FB02.23-23图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台二十六","方（扁）钢","加强筋40*4",7,1000,40,4,null,null,{"v":0.616,"d":"0.62"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十九","[槽钢","[100*48*5.3",1,32000,null,48,5.3,5.3,{"v":4.2688,"d":"4.27"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十九","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":27.2,"d":"27.20"},"FG110203-SS-FB02.23-23图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台二十九","方（扁）钢","加强筋40*4",15,1000,40,4,null,null,1.32,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-23","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十五*2","[槽钢","[100*48*5.3",2,12500,null,48,5.3,5.3,{"v":3.335,"d":"3.34"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十五*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":19.2,"d":"19.20"},"FG110203-SS-FB02.23-24图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台二十五*2","方（扁）钢","加强筋40*4",10,1000,40,4,null,null,0.88,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十五*2","方（扁）钢","加强筋60*6",1,1200,60,6,null,null,{"v":0.1584,"d":"0.16"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十七","[槽钢","[100*48*5.3",1,7800,null,48,5.3,5.3,{"v":1.04052,"d":"1.04"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十七","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":5.6,"d":"5.60"},"FG110203-SS-FB02.23-24图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台二十七","方（扁）钢","加强筋40*4",3,1000,40,4,null,null,{"v":0.264,"d":"0.26"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十八","[槽钢","[100*48*5.3",1,6500,null,48,5.3,5.3,{"v":0.8671,"d":"0.87"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台二十八","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":4.4,"d":"4.40"},"FG110203-SS-FB02.23-24图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台二十八","方（扁）钢","加强筋40*4",2,1000,40,4,null,null,{"v":0.176,"d":"0.18"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十*2","[槽钢","[100*48*5.3",2,6450,null,48,5.3,5.3,{"v":1.72086,"d":"1.72"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":8.8,"d":"8.80"},"FG110203-SS-FB02.23-24图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台三十*2","方（扁）钢","加强筋40*4",4,1000,40,4,null,null,{"v":0.352,"d":"0.35"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-24","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十一*2","[槽钢","[100*48*5.3",2,31300,null,48,5.3,5.3,{"v":8.35084,"d":"8.35"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十一*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":60,"d":"60.00"},"FG110203-SS-FB02.23-25图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台三十一*2","方（扁）钢","加强筋40*4",26,1000,40,4,null,null,{"v":2.288,"d":"2.29"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十一*2","方（扁）钢","加强筋60*6",6,1200,60,6,null,null,{"v":0.9504,"d":"0.95"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十八","[槽钢","[100*48*5.3",1,25400,null,48,5.3,5.3,{"v":3.38836,"d":"3.39"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十八","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":23,"d":"23.00"},"FG110203-SS-FB02.23-25图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台三十八","方（扁）钢","加强筋40*4",16,1000,40,4,null,null,{"v":1.408,"d":"1.41"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十二","[槽钢","[100*48*5.3",1,29300,null,48,5.3,5.3,{"v":3.90862,"d":"3.91"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十二","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":22,"d":"22.00"},"FG110203-SS-FB02.23-26图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台三十二","方（扁）钢","加强筋40*4",12,1000,40,4,null,null,{"v":1.056,"d":"1.06"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十三","[槽钢","[100*48*5.3",1,46700,null,48,5.3,5.3,{"v":6.22978,"d":"6.23"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十三","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":41.8,"d":"41.80"},"FG110203-SS-FB02.23-26图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台三十三","方（扁）钢","加强筋40*4",24,1000,40,4,null,null,{"v":2.112,"d":"2.11"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-26","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十四","[槽钢","[100*48*5.3",1,17200,null,48,5.3,5.3,{"v":2.29448,"d":"2.29"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十四","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":15.2,"d":"15.20"},"FG110203-SS-FB02.23-27图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台三十四","方（扁）钢","加强筋40*4",8,1000,40,4,null,null,{"v":0.704,"d":"0.70"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十五","[槽钢","[100*48*5.3",1,26200,null,48,5.3,5.3,{"v":3.49508,"d":"3.50"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十五","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":22,"d":"22.00"},"FG110203-SS-FB02.23-27图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台三十五","方（扁）钢","加强筋40*4",14,1000,40,4,null,null,{"v":1.232,"d":"1.23"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-27","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十六","[槽钢","[100*48*5.3",1,20000,null,48,5.3,5.3,{"v":2.668,"d":"2.67"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十六","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":18.2,"d":"18.20"},"FG110203-SS-FB02.23-28图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台三十六","方（扁）钢","加强筋40*4",7,1000,40,4,null,null,{"v":0.616,"d":"0.62"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十六","方（扁）钢","加强筋60*6",1,1800,60,6,null,null,{"v":0.2376,"d":"0.24"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-25","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十七","[槽钢","[100*48*5.3",1,51200,null,48,5.3,5.3,{"v":6.83008,"d":"6.83"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十七","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":43,"d":"43.00"},"FG110203-SS-FB02.23-28图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台三十七","方（扁）钢","加强筋40*4",27,1000,40,4,null,null,{"v":2.376,"d":"2.38"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-28","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十九","[槽钢","[100*48*5.3",1,14000,null,48,5.3,5.3,{"v":1.8676,"d":"1.87"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台三十九","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":11.2,"d":"11.20"},"FG110203-SS-FB02.23-29图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台三十九","方（扁）钢","加强筋40*4",6,1000,40,4,null,null,{"v":0.528,"d":"0.53"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台四十一*2","[槽钢","[100*48*5.3",2,26400,null,48,5.3,5.3,{"v":7.04352,"d":"7.04"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台四十一*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":53.2,"d":"53.20"},"FG110203-SS-FB02.23-29图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台四十一*2","方（扁）钢","加强筋40*4",36,1000,40,4,null,null,{"v":3.168,"d":"3.17"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台四十","[槽钢","[100*48*5.3",1,28000,null,48,5.3,5.3,{"v":3.7352,"d":"3.74"},"翼板重合",null,730,null,null,"FG110203-SS-FB02.23-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台四十","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":27.8,"d":"27.80"},"FG110203-SS-FB02.23-30图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["二系洗涤区域操作台平台四十","方（扁）钢","加强筋40*4",20,1000,40,4,null,null,1.76,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-30","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台悬臂梁一*166","[槽钢","[126*53*5.5",166,1080,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":36.03528,"d":"36.04"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台悬臂梁二*15","[槽钢","[126*53*5.5",15,990,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":2.98485,"d":"2.98"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台悬臂梁三*8","[槽钢","[126*53*5.5",8,1290,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":2.07432,"d":"2.07"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱一*4","[槽钢","[100*48*5.3",4,10300,null,48,5.3,5.3,{"v":7.47368,"d":"7.47"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱一*4","L型钢","L50*50*5",4,800,null,50,5,5,0.32,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱一*4","L型钢","L50*50*5",8,1130,null,50,5,5,{"v":0.904,"d":"0.90"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱二*8","[槽钢","[100*48*5.3",8,12600,null,48,5.3,5.3,{"v":18.28512,"d":"18.29"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-29","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱二*8","L型钢","L50*50*5",16,700,null,50,5,5,1.12,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱二*8","L型钢","L50*50*5",32,800,null,50,5,5,2.56,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱二*8","L型钢","L50*50*5",32,1000,null,50,5,5,{"v":3.2,"d":"3.20"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱二*8","L型钢","L50*50*5",32,1130,null,50,5,5,{"v":3.616,"d":"3.62"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-31","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱三*4","[槽钢","[100*48*5.3",4,12400,null,48,5.3,5.3,{"v":8.99744,"d":"9.00"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱三*4","L型钢","L50*50*5",8,500,null,50,5,5,{"v":0.4,"d":"0.40"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱三*4","L型钢","L50*50*5",16,800,null,50,5,5,1.28,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱三*4","L型钢","L50*50*5",16,1000,null,50,5,5,{"v":1.6,"d":"1.60"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱三*4","L型钢","L50*50*5",16,1130,null,50,5,5,{"v":1.808,"d":"1.81"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱四*4","[槽钢","[100*48*5.3",4,4100,null,48,5.3,5.3,{"v":2.97496,"d":"2.97"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱四*4","L型钢","L50*50*5",16,800,null,50,5,5,1.28,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱五","[槽钢","[100*48*5.3",1,4100,null,48,5.3,5.3,{"v":0.74374,"d":"0.74"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱五","L型钢","L50*50*5",2,850,null,50,5,5,0.17,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-32","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱六","[槽钢","[100*48*5.3",1,6200,null,48,5.3,5.3,{"v":1.12468,"d":"1.12"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-33","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱六","L型钢","L50*50*5",1,2640,null,50,5,5,{"v":0.264,"d":"0.26"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-33","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱七","[槽钢","[100*48*5.3",1,12400,null,48,5.3,5.3,{"v":2.24936,"d":"2.25"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-33","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱七","L型钢","L50*50*5",1,14100,null,50,5,5,1.41,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-33","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱八*2","[槽钢","[100*48*5.3",2,10000,null,48,5.3,5.3,{"v":3.628,"d":"3.63"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-33","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱八*2","L型钢","L50*50*5",2,3100,null,50,5,5,0.62,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-33","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台三角架一*10","[槽钢","[126*53*5.5",10,1480,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":2.9748,"d":"2.97"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-34","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台三角架一*10","[槽钢","[100*48*5.3",10,1660,null,48,5.3,5.3,{"v":3.01124,"d":"3.01"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-34","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台三角架二*7","[槽钢","[126*53*5.5",7,1880,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":2.64516,"d":"2.65"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-34","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台三角架二*7","[槽钢","[100*48*5.3",7,2220,null,48,5.3,5.3,{"v":2.818956,"d":"2.82"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-34","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台支架一二三*11*24*24","[槽钢","[100*48*5.3",1,84600,null,48,5.3,5.3,{"v":15.34644,"d":"15.35"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-35","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁一*8","[槽钢","[220*79*9",8,6290,null,79,9,9,{"v":14.99536,"d":"15.00"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-36","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁一*8","L型钢","L180*110*10",16,150,null,100,10,10,0.48,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-36","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁二*8","[槽钢","[220*79*9",8,4830,null,79,9,9,{"v":11.51472,"d":"11.51"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-36","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁二*8","L型钢","L180*110*10",16,150,null,100,10,10,0.48,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-36","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁三*16","[槽钢","[220*79*9",16,6620,null,79,9,9,{"v":31.56416,"d":"31.56"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-37","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁三*16","L型钢","L180*110*10",32,150,null,100,10,10,0.96,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-37","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁四*16","[槽钢","[220*79*9",16,4630,null,79,9,9,{"v":22.07584,"d":"22.08"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-37","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁四*16","L型钢","L180*110*10",32,150,null,100,10,10,0.96,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-37","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁五*6","[槽钢","[220*79*9",6,6550,null,79,9,9,{"v":11.7114,"d":"11.71"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁五*6","L型钢","L180*110*10",12,150,null,100,10,10,0.36,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁六*6","[槽钢","[220*79*9",6,4940,null,79,9,9,{"v":8.83272,"d":"8.83"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁六*6","L型钢","L180*110*10",12,150,null,100,10,10,0.36,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-38","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁七","[槽钢","[220*79*9",1,6400,null,79,9,9,{"v":1.9072,"d":"1.91"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-39","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁七","L型钢","L180*110*10",2,150,null,100,10,10,0.06,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-39","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁八","[槽钢","[220*79*9",1,4500,null,79,9,9,{"v":1.341,"d":"1.34"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-39","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁八","L型钢","L180*110*10",2,150,null,100,10,10,0.06,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-39","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁九*2","[槽钢","[220*79*9",2,3800,null,79,9,9,{"v":2.2648,"d":"2.26"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁九*2","L型钢","L180*110*10",4,150,null,100,10,10,0.12,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁十","[槽钢","[220*79*9",1,4940,null,79,9,9,{"v":1.47212,"d":"1.47"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁十","L型钢","L180*110*10",2,150,null,100,10,10,0.06,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-40","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁十一","[槽钢","[220*79*9",1,6550,null,79,9,9,{"v":1.9519,"d":"1.95"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁十一","L型钢","L180*110*10",2,150,null,100,10,10,0.06,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁十二","[槽钢","[220*79*9",1,4640,null,79,9,9,{"v":1.38272,"d":"1.38"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁十二","L型钢","L180*110*10",2,150,null,100,10,10,0.06,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-41","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁十三","[槽钢","[220*79*9",1,6620,null,79,9,9,{"v":1.97276,"d":"1.97"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-42","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台槽钢梁十三","L型钢","L180*110*10",2,150,null,100,10,10,0.06,"无重合面",null,730,null,null,"FG110203-SS-FB02.23-42","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱九*2","[槽钢","[100*48*5.3",2,12100,null,48,5.3,5.3,{"v":4.38988,"d":"4.39"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-42","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["二系洗涤区域操作台平台支柱九*2","L型钢","L50*50*5",2,12500,null,50,5,5,{"v":2.5,"d":"2.50"},"无重合面",null,730,null,null,"FG110203-SS-FB02.23-42","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域","其他",{"$nulls":7},"需手动计算","无重合面",null,730,{"$nulls":3},"一般性腐蚀","环氧富锌漆",{"$error":"#VALUE!"}]
["油库区域粗苯贮槽操作台平台栏杆101m","圆钢","圆钢 Q50*3",2,101000,50,{"$nulls":3},{"v":31.714,"d":"31.71"},"无重合面",null,730,null,null,"32NM034-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域粗苯贮槽操作台平台栏杆101m","方（扁）钢","扁铁50*4",2,101000,50,4,null,null,{"v":21.816,"d":"21.82"},"无重合面",null,730,null,null,"32NM034-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域粗苯贮槽操作台盘梯护栏40m","圆钢","圆钢 Q50*3",2,44000,50,{"$nulls":3},{"v":13.816,"d":"13.82"},"无重合面",null,730,null,{"v":13.816,"d":"13.82"},"32NM034-1","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["油库区域粗苯贮槽操作台盘梯护栏40m","方（扁）钢","扁铁40*4",2,44000,40,4,null,null,{"v":7.744,"d":"7.74"},"无重合面",null,730,null,null,"32NM034-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域粗苯贮槽操作台盘梯DN11500  H13300*2","方（扁）钢","外侧板160*8",2,19700,160,8,null,null,{"v":13.2384,"d":"13.24"},"无重合面",null,730,null,null,"32NM034-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域粗苯贮槽操作台盘梯DN11500  H13300*2","方（扁）钢","内侧板160*8",2,18400,160,8,null,null,{"v":12.3648,"d":"12.36"},"无重合面",null,730,null,null,"32NM034-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域粗苯贮槽操作台盘梯DN11500  H13300*2","L型钢","L63*63*6",12,2500,null,63,6,6,3.78,"无重合面",null,730,null,null,"32NM034-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域粗苯贮槽操作台盘梯DN11500  H13300*2","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,730,null,null,"32NM034-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域粗苯贮槽操作台盘梯DN11500  H13300*2","方（扁）钢","踏板",118,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":62.304,"d":"62.30"},"32NM034-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域粗苯贮槽操作台平台","[槽钢","[250*80*9",2,15000,null,80,9,9,9.06,"无重合面",null,730,null,null,"32NM034-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域粗苯贮槽操作台平台","[槽钢","[250*80*9",2,976,null,80,9,9,{"v":0.589504,"d":"0.59"},"无重合面",null,730,null,null,"32NM034-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域粗苯贮槽操作台平台","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":30,"d":"30.00"},"32NM034-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域粗苯贮槽操作台平台","方（扁）钢","加强筋40*4",14,982,40,4,null,null,{"v":1.209824,"d":"1.21"},"无重合面",null,730,null,null,"32NM034-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域粗苯贮槽操作台平台支架*2","[槽钢","[126*53*5.5",4,1367,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.099068,"d":"1.10"},"无重合面",null,730,null,null,"32NM034-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域粗苯贮槽操作台平台支架*2","L型钢","L100*100*6",2,1040,null,100,6,6,{"v":0.416,"d":"0.42"},"无重合面",null,730,null,null,"32NM034-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域粗苯贮槽操作台罐顶支架一*2","L型钢","L75*75*6",2,1500,null,75,6,6,0.45,"无重合面",null,730,null,null,"32NM034-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域粗苯贮槽操作台罐顶支架二*2","L型钢","L75*75*6",2,2500,null,75,6,6,0.75,"无重合面",null,730,null,null,"32NM034-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["焦油贮槽操作台","其他",{"$nulls":7},"需手动计算","无重合面",null,730,null,null,"32NM034-4","一般性腐蚀","环氧富锌漆",{"$error":"#VALUE!"}]
["油库区域焦油贮槽操作台平台栏杆101m","圆钢","圆钢 Q50*3",2,380000,50,{"$nulls":3},119.32,"无重合面",null,730,null,null,"32NM035-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油贮槽操作台平台栏杆101m","方（扁）钢","扁铁50*4",2,380000,50,4,null,null,82.08,"无重合面",null,730,null,null,"32NM035-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油贮槽操作台盘梯护栏40m","圆钢","圆钢 Q50*3",2,77000,50,{"$nulls":3},{"v":24.178,"d":"24.18"},"无重合面",null,730,null,{"v":24.178,"d":"24.18"},"32NM035-1","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["油库区域焦油贮槽操作台盘梯护栏40m","方（扁）钢","扁铁40*4",2,77000,40,4,null,null,{"v":13.552,"d":"13.55"},"无重合面",null,730,null,null,"32NM035-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油贮槽操作台盘梯DN13500  H11600*4","方（扁）钢","外侧板160*8",4,17220,160,8,null,null,{"v":23.14368,"d":"23.14"},"无重合面",null,730,null,null,"32NM035-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油贮槽操作台盘梯DN13500  H11600*4","方（扁）钢","内侧板160*8",4,16240,160,8,null,null,{"v":21.82656,"d":"21.83"},"无重合面",null,730,null,null,"32NM035-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油贮槽操作台盘梯DN13500  H11600*4","L型钢","L63*63*6",24,2500,null,63,6,6,7.56,"无重合面",null,730,null,null,"32NM035-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油贮槽操作台盘梯DN13500  H11600*4","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,730,null,null,"32NM035-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油贮槽操作台盘梯DN13500  H11600*4","方（扁）钢","踏板",208,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":109.824,"d":"109.82"},"32NM035-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域焦油贮槽操作台平台一*4","[槽钢","[100*48*5.3",4,27600,null,48,5.3,5.3,{"v":20.02656,"d":"20.03"},"无重合面",null,730,null,null,"32NM035-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油贮槽操作台平台一*4","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":83.2,"d":"83.20"},"32NM035-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域焦油贮槽操作台平台一*4","方（扁）钢","加强筋40*4",44,786,40,4,null,null,{"v":3.043392,"d":"3.04"},"无重合面",null,730,null,null,"32NM035-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油贮槽操作台平台二*2","[槽钢","[200*75*9",4,8900,null,75,9,9,{"v":10.0392,"d":"10.04"},"无重合面",null,730,null,null,"32NM035-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油贮槽操作台平台二*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":28.4,"d":"28.40"},"32NM035-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域焦油贮槽操作台平台二*2","方（扁）钢","加强筋40*4",16,776,40,4,null,null,{"v":1.092608,"d":"1.09"},"无重合面",null,730,null,null,"32NM035-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油贮槽操作台平台支架一*4","[槽钢","[126*53*5.5",8,1220,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.96176,"d":"1.96"},"无重合面",null,730,null,null,"32NM035-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油贮槽操作台平台支架一*4","L型钢","L100*100*6",4,840,null,100,6,6,{"v":0.672,"d":"0.67"},"无重合面",null,730,null,null,"32NM035-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油贮槽操作台梯蹬","圆钢","圆钢 Q89*6",4,6100,89,{"$nulls":3},{"v":6.818824000000001,"d":"6.82"},"无重合面",null,730,null,{"v":6.818824,"d":"6.82"},"32NM035-4","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["油库区域焦油贮槽操作台梯蹬","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,8.56,"32NM035-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域焦油贮槽操作台罐顶支架","L型钢","L75*75*6",40,1500,null,75,6,6,{"v":9,"d":"9.00"},"无重合面",null,730,null,null,"32NM035-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油贮槽操作台平台三*2","[槽钢","[200*75*9",4,9000,null,75,9,9,{"v":10.152,"d":"10.15"},"无重合面",null,730,null,null,"32NM035-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油贮槽操作台平台三*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":27.6,"d":"27.60"},"32NM035-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域焦油贮槽操作台平台三*2","方（扁）钢","加强筋40*4",16,776,40,4,null,null,{"v":1.092608,"d":"1.09"},"无重合面",null,730,null,null,"32NM035-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油贮槽操作台平台支架二*4","[槽钢","[126*53*5.5",8,1220,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.96176,"d":"1.96"},"无重合面",null,730,null,null,"32NM035-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油贮槽操作台平台支架二*4","L型钢","L100*100*6",4,840,null,100,6,6,{"v":0.672,"d":"0.67"},"无重合面",null,730,null,null,"32NM035-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域洗油贮槽操作台平台栏杆42m*2","圆钢","圆钢 Q50*3",2,84000,50,{"$nulls":3},{"v":26.376,"d":"26.38"},"无重合面",null,730,null,null,"32NM036-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域洗油贮槽操作台平台栏杆42m*2","方（扁）钢","扁铁50*4",2,84000,50,4,null,null,{"v":18.144,"d":"18.14"},"无重合面",null,730,null,null,"32NM036-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域洗油贮槽操作台盘梯护栏13m*2","圆钢","圆钢 Q50*3",2,26000,50,{"$nulls":3},{"v":8.164,"d":"8.16"},"无重合面",null,730,null,{"v":8.164,"d":"8.16"},"32NM036-1","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["油库区域洗油贮槽操作台盘梯护栏13m*2","方（扁）钢","扁铁40*4",2,26000,40,4,null,null,{"v":4.576,"d":"4.58"},"无重合面",null,730,null,null,"32NM036-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域洗油贮槽操作台盘梯DN7700  H7500*2","方（扁）钢","外侧板160*8",2,11400,160,8,null,null,{"v":7.6608,"d":"7.66"},"无重合面",null,730,null,null,"32NM036-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域洗油贮槽操作台盘梯DN7700  H7500*2","方（扁）钢","内侧板160*8",2,10300,160,8,null,null,{"v":6.9216,"d":"6.92"},"无重合面",null,730,null,null,"32NM036-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域洗油贮槽操作台盘梯DN7700  H7500*2","L型钢","L63*63*6",6,2500,null,63,6,6,1.89,"无重合面",null,730,null,null,"32NM036-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域洗油贮槽操作台盘梯DN7700  H7500*2","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,730,null,null,"32NM036-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域洗油贮槽操作台盘梯DN7700  H7500*2","方（扁）钢","踏板",66,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":34.848,"d":"34.85"},"32NM036-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域洗油贮槽操作台平台一*2","[槽钢","[100*48*5.3",2,4500,null,48,5.3,5.3,{"v":1.6326,"d":"1.63"},"无重合面",null,730,null,null,"32NM036-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域洗油贮槽操作台平台一*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":5.6,"d":"5.60"},"32NM036-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域洗油贮槽操作台平台一*2","方（扁）钢","加强筋40*4",2,786,40,4,null,null,{"v":0.138336,"d":"0.14"},"无重合面",null,730,null,null,"32NM036-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域洗油贮槽操作台罐顶支架一*2","L型钢","L75*75*6",2,1700,null,75,6,6,0.51,"无重合面",null,730,null,null,"32NM036-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域洗油贮槽操作台罐顶支架二*2","L型钢","L75*75*6",10,1300,null,75,6,6,1.95,"无重合面",null,730,null,null,"32NM036-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域洗油贮槽操作台平台支架*2","[槽钢","[126*53*5.5",4,817,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.656868,"d":"0.66"},"无重合面",null,730,null,null,"32NM036-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域洗油贮槽操作台平台支架*2","L型钢","L100*100*6",2,840,null,100,6,6,{"v":0.336,"d":"0.34"},"无重合面",null,730,null,null,"32NM036-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域洗油贮槽操作台平台二*2","[槽钢","[100*48*5.3",4,10800,null,48,5.3,5.3,{"v":7.83648,"d":"7.84"},"无重合面",null,730,null,null,"32NM036-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域洗油贮槽操作台平台二*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":14.8,"d":"14.80"},"32NM036-4图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域洗油贮槽操作台平台二*2","方（扁）钢","加强筋40*4",8,786,40,4,null,null,{"v":0.553344,"d":"0.55"},"无重合面",null,730,null,null,"32NM036-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域洗油贮槽操作台梯蹬*2","圆钢","圆钢 Q89*6",2,1600,89,{"$nulls":3},{"v":0.8942720000000001,"d":"0.89"},"无重合面",null,730,null,{"v":0.894272,"d":"0.89"},"32NM036-5","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["油库区域洗油贮槽操作台梯蹬*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":1.6,"d":"1.60"},"32NM036-5图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域洗油贮槽操作台平台三*2","[槽钢","[100*48*5.3",8,800,null,48,5.3,5.3,{"v":1.16096,"d":"1.16"},"无重合面",null,730,null,null,"32NM036-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域洗油贮槽操作台平台三*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":2.4,"d":"2.40"},"32NM036-5图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域洗油贮槽操作台罐顶支架三*2","L型钢","L75*75*6",2,1600,null,75,6,6,0.48,"无重合面",null,730,null,null,"32NM036-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域洗油贮槽操作台罐顶支架四*2","L型钢","L75*75*6",2,1500,null,75,6,6,0.45,"无重合面",null,730,null,null,"32NM036-5","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠贮槽操作台平台栏杆42m*2","圆钢","圆钢 Q50*3",2,96000,50,{"$nulls":3},{"v":30.144,"d":"30.14"},"无重合面",null,730,null,null,"32NM037-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠贮槽操作台平台栏杆42m*2","方（扁）钢","扁铁50*4",2,96000,50,4,null,null,{"v":20.736,"d":"20.74"},"无重合面",null,730,null,null,"32NM037-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠贮槽操作台盘梯护栏13m*2","圆钢","圆钢 Q50*3",2,30000,50,{"$nulls":3},9.42,"无重合面",null,730,null,9.42,"32NM037-1","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["油库区域氢氧化钠贮槽操作台盘梯护栏13m*2","方（扁）钢","扁铁40*4",2,30000,40,4,null,null,5.28,"无重合面",null,730,null,null,"32NM037-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠贮槽操作台盘梯DN11000  H8600*2","方（扁）钢","外侧板160*8",2,12700,160,8,null,null,{"v":8.5344,"d":"8.53"},"无重合面",null,730,null,null,"32NM037-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠贮槽操作台盘梯DN11000  H8600*2","方（扁）钢","内侧板160*8",2,11900,160,8,null,null,{"v":7.9968,"d":"8.00"},"无重合面",null,730,null,null,"32NM037-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠贮槽操作台盘梯DN11000  H8600*2","L型钢","L63*63*6",8,2500,null,63,6,6,2.52,"无重合面",null,730,null,null,"32NM037-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠贮槽操作台盘梯DN11000  H8600*2","L型钢","L63*63*6",4,226,null,63,6,6,{"v":0.113904,"d":"0.11"},"无重合面",null,730,null,null,"32NM037-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠贮槽操作台盘梯DN11000  H8600*2","方（扁）钢","踏板",76,800,{"$nulls":4},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":40.128,"d":"40.13"},"32NM037-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域氢氧化钠贮槽操作台平台一*2","[槽钢","[100*48*5.3",2,3600,null,48,5.3,5.3,{"v":1.30608,"d":"1.31"},"无重合面",null,730,null,null,"32NM037-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠贮槽操作台平台一*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":8.8,"d":"8.80"},"32NM037-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域氢氧化钠贮槽操作台平台一*2","方（扁）钢","加强筋40*4",4,786,40,4,null,null,{"v":0.276672,"d":"0.28"},"无重合面",null,730,null,null,"32NM037-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠贮槽操作台平台支架*2","[槽钢","[126*53*5.5",4,1150,null,{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":0.9246,"d":"0.92"},"无重合面",null,730,null,null,"32NM037-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠贮槽操作台平台支架*2","L型钢","L100*100*6",2,840,null,100,6,6,{"v":0.336,"d":"0.34"},"无重合面",null,730,null,null,"32NM037-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠贮槽操作台梯蹬*2","圆钢","圆钢 Q89*6",2,3500,89,{"$nulls":3},{"v":1.9562200000000003,"d":"1.96"},"无重合面",null,730,null,{"v":1.95622,"d":"1.96"},"32NM037-3","一般性腐蚀","环氧富锌漆",{"v":0.5,"d":"50%"}]
["油库区域氢氧化钠贮槽操作台梯蹬*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":5.2,"d":"5.20"},"32NM037-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域氢氧化钠贮槽操作台平台二*2","[槽钢","[100*48*5.3",8,800,null,48,5.3,5.3,{"v":1.16096,"d":"1.16"},"无重合面",null,730,null,null,"32NM037-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠贮槽操作台平台二*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":2.4,"d":"2.40"},"32NM037-3图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域氢氧化钠贮槽操作台罐顶支架三*2","L型钢","L75*75*6",2,1200,null,75,6,6,0.36,"无重合面",null,730,null,null,"32NM037-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠贮槽操作台罐顶支架一*2","L型钢","L75*75*6",2,1300,null,75,6,6,0.39,"无重合面",null,730,null,null,"32NM037-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠贮槽操作台罐顶支架二*2","L型钢","L75*75*6",10,1300,null,75,6,6,1.95,"无重合面",null,730,null,null,"32NM037-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域苯放空槽苯分离水槽联合平台栏杆13.6m","圆钢","圆钢 Q50*3",2,13600,50,{"$nulls":3},{"v":4.2704,"d":"4.27"},"无重合面",null,730,null,null,"32NM038-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域苯放空槽苯分离水槽联合平台栏杆13.6m","方（扁）钢","扁铁50*4",2,13600,50,4,null,null,{"v":2.9376,"d":"2.94"},"无重合面",null,730,null,null,"32NM038-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域苯放空槽苯分离水槽联合平台立柱13.6m","[槽钢","[100*48*5.3",1,2100,null,48,5.3,5.3,{"v":0.38094,"d":"0.38"},"无重合面",null,730,null,null,"32NM038-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域苯放空槽苯分离水槽联合平台一","[槽钢","[100*48*5.3",1,17200,null,48,5.3,5.3,{"v":3.12008,"d":"3.12"},"无重合面",null,730,null,null,"32NM038-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域苯放空槽苯分离水槽联合平台一","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":14.4,"d":"14.40"},"32NM038-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域苯放空槽苯分离水槽联合平台一","方（扁）钢","加强筋40*4",8,900,40,4,null,null,{"v":0.6336,"d":"0.63"},"无重合面",null,730,null,null,"32NM038-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域苯放空槽苯分离水槽联合平台二","[槽钢","[100*48*5.3",1,3700,null,48,5.3,5.3,{"v":0.67118,"d":"0.67"},"无重合面",null,730,null,null,"32NM038-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域苯放空槽苯分离水槽联合平台二","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":2.6,"d":"2.60"},"32NM038-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域苯放空槽苯分离水槽联合平台二","方（扁）钢","加强筋40*4",1,800,40,4,null,null,{"v":0.0704,"d":"0.07"},"无重合面",null,730,null,null,"32NM038-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油放空槽联合平台栏杆27.1m","圆钢","圆钢 Q50*3",2,27100,50,{"$nulls":3},{"v":8.5094,"d":"8.51"},"无重合面",null,730,null,null,"32NM039-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油放空槽联合平台栏杆27.1m","方（扁）钢","扁铁50*4",2,27100,50,4,null,null,{"v":5.8536,"d":"5.85"},"无重合面",null,730,null,null,"32NM039-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油放空槽联合平台栏杆27.1m","[槽钢","[100*48*5.3",1,4170,null,48,5.3,5.3,{"v":0.756438,"d":"0.76"},"无重合面",null,730,null,null,"32NM039-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油放空槽联合平台一*2","[槽钢","[100*48*5.3",2,17200,null,48,5.3,5.3,{"v":6.24016,"d":"6.24"},"无重合面",null,730,null,null,"32NM039-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油放空槽联合平台一*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":28.8,"d":"28.80"},"32NM039-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域焦油放空槽联合平台一*2","方（扁）钢","加强筋40*4",16,900,40,4,null,null,{"v":1.2672,"d":"1.27"},"无重合面",null,730,null,null,"32NM039-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油放空槽联合平台二*2","[槽钢","[100*48*5.3",2,3700,null,48,5.3,5.3,{"v":1.34236,"d":"1.34"},"无重合面",null,730,null,null,"32NM039-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域焦油放空槽联合平台二*2","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":5.2,"d":"5.20"},"32NM039-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域焦油放空槽联合平台二*2","方（扁）钢","加强筋40*4",2,800,40,4,null,null,{"v":0.1408,"d":"0.14"},"无重合面",null,730,null,null,"32NM039-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠放空槽 洗油放空槽联合平台栏杆13.6m","圆钢","圆钢 Q50*3",2,13600,50,{"$nulls":3},{"v":4.2704,"d":"4.27"},"无重合面",null,730,null,null,"32NM040-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠放空槽 洗油放空槽联合平台栏杆13.6m","方（扁）钢","扁铁50*4",2,13600,50,4,null,null,{"v":2.9376,"d":"2.94"},"无重合面",null,730,null,null,"32NM040-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠放空槽 洗油放空槽联合平台立柱13.6m","[槽钢","[100*48*5.3",1,2100,null,48,5.3,5.3,{"v":0.38094,"d":"0.38"},"无重合面",null,730,null,null,"32NM040-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠放空槽 洗油放空槽联合平台一","[槽钢","[100*48*5.3",1,17200,null,48,5.3,5.3,{"v":3.12008,"d":"3.12"},"无重合面",null,730,null,null,"32NM040-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠放空槽 洗油放空槽联合平台一","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":14.4,"d":"14.40"},"32NM040-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域氢氧化钠放空槽 洗油放空槽联合平台一","方（扁）钢","加强筋40*4",8,900,40,4,null,null,{"v":0.6336,"d":"0.63"},"无重合面",null,730,null,null,"32NM040-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠放空槽 洗油放空槽联合平台二","[槽钢","[100*48*5.3",1,3700,null,48,5.3,5.3,{"v":0.67118,"d":"0.67"},"无重合面",null,730,null,null,"32NM040-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域氢氧化钠放空槽 洗油放空槽联合平台二","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":2.6,"d":"2.60"},"32NM040-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域氢氧化钠放空槽 洗油放空槽联合平台二","方（扁）钢","加强筋40*4",1,800,40,4,null,null,{"v":0.0704,"d":"0.07"},"无重合面",null,730,null,null,"32NM040-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台栏杆18m","圆钢","圆钢 Q50*3",2,18000,50,{"$nulls":3},{"v":5.652,"d":"5.65"},"无重合面",null,730,null,null,"32NM042-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台栏杆18m","方（扁）钢","扁铁50*4",2,18000,50,4,null,null,{"v":3.888,"d":"3.89"},"无重合面",null,730,null,null,"32NM042-1","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台一","[槽钢","[100*48*5.3",1,18500,null,48,5.3,5.3,{"v":3.3559,"d":"3.36"},"无重合面",null,730,null,null,"32NM042-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台一","方（扁）钢","花纹板4.5",null,"",{"$nulls":4},"",null,null,730,null,{"v":13.4,"d":"13.40"},"32NM042-2","一般性腐蚀","环氧富锌漆",""]
["油库区域清洗油槽平台一","方（扁）钢","加强筋40*4",6,750,40,4,null,null,{"v":0.396,"d":"0.40"},"无重合面",null,730,null,null,"32NM042-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台二","[槽钢","[100*48*5.3",1,5700,null,48,5.3,5.3,{"v":1.03398,"d":"1.03"},"无重合面",null,730,null,null,"32NM040-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台二","方（扁）钢","花纹板4.5",{"$nulls":6},{"v":0,"d":"0.00"},"无重合面",null,730,null,{"v":3.2,"d":"3.20"},"32NM040-2图纸标明面积、无具体尺寸","一般性腐蚀","环氧富锌漆","钢构面积为0"]
["油库区域清洗油槽平台二","方（扁）钢","加强筋40*4",2,800,"40",4,null,null,{"v":0.1408,"d":"0.14"},"无重合面",null,730,null,null,"32NM040-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台悬臂梁*3","[槽钢","[126*53*5.5",3,974,{"v":126,"d":"126.00"},{"v":53,"d":"53.00"},{"v":5.5,"d":"5.50"},{"v":5.5,"d":"5.50"},{"v":1.323666,"d":"1.32"},"无重合面",null,730,null,null,"32NM042-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台三角架*4","[槽钢","[100*48*5.3",4,1700,100,48,5.3,5.3,{"v":2.59352,"d":"2.59"},"无重合面",null,730,null,null,"32NM042-2","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台梯子入口","方（扁）钢","扁铁50*4",4,1400,"50",4,null,null,{"v":0.6048,"d":"0.60"},"无重合面",null,730,null,null,"32NM042-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台梯子入口","方（扁）钢","扁铁50*4",4,1240,"50",4,null,null,{"v":0.53568,"d":"0.54"},"无重合面",null,730,null,null,"32NM042-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台KH1=4450直梯*1","L型钢","L63*63*6",2,5780,63,63,6,6,{"v":2.91312,"d":"2.91"},"无重合面",null,730,null,null,"32NM042-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台KH1=4450直梯*1","方（扁）钢","扁铁40*4",5,1840,"40",4,null,null,{"v":0.8096,"d":"0.81"},"无重合面",null,730,null,null,"32NM042-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台KH1=4450直梯*1","方（扁）钢","扁铁25*4",5,3750,"25",4,null,null,{"v":1.0875,"d":"1.09"},"无重合面",null,730,null,null,"32NM042-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台KH1=4450直梯*1","圆钢","圆钢Q18",15,480,18,{"$nulls":3},{"v":0.406944,"d":"0.41"},"无重合面",null,730,null,null,"32NM042-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台KH1=4450直梯*1","圆钢","圆钢Q18",2,1366,18,{"$nulls":3},{"v":0.15441264000000002,"d":"0.15"},"无重合面",null,730,null,null,"32NM042-3","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台FH1=3350直梯*1","方（扁）钢","钢板60*8",2,4560,"60",8,null,null,{"v":1.24032,"d":"1.24"},"无重合面",null,730,null,null,"32NM042-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台FH1=3350直梯*1","圆钢","圆钢Q18",16,500,18,{"$nulls":3},{"v":0.45216,"d":"0.45"},"无重合面",null,730,null,null,"32NM042-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台FH1=3350直梯*1","方（扁）钢","扁铁40*4",3,1870,"40",4,null,null,{"v":0.49368,"d":"0.49"},"无重合面",null,730,null,null,"32NM042-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
["油库区域清洗油槽平台FH1=3350直梯*1","方（扁）钢","扁铁25*4",5,1230,"25",4,null,null,{"v":0.3567,"d":"0.36"},"无重合面",null,730,null,null,"32NM042-4","一般性腐蚀","环氧富锌漆",{"v":0,"d":"0%"}]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
[{"$nulls":9},"",null,null,"",{"$nulls":4},"环氧富锌漆"]
["汇总",{"$nulls":8},{"v":8458.56145955999,"d":"8458.56"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},{"v":3518.6104824,"d":"3518.61"}]
["工程量汇总",{"$nulls":8},{"v":8458.56145955999,"d":"钢结构： 8458.56㎡"},{"$nulls":3},{"v":3518.6104824,"d":"平台： 3518.61㎡"}]

{"sheet":"5.干熄焦-管道","index":4,"n_rows":21,"n_cols":10,"rows_kept":21,"flags":["formulas_cached_only"]}
["2024年广西钢铁集团焦化厂除锈防腐检修工程——干熄焦发电车间工程量（管道）"]
["车间","区域","施工环境描述","材料名称","管道直径mm","材料长度m\n","面积","腐蚀程度","推荐采用防腐涂料","备注"]
["干熄焦","装入装置至环境除尘总管接口处(三座炉)","作业高度约40m，作业环境存在煤气中毒、高空坠落、高温烫伤等危险源。","环境除尘管道",1520,147.9,{"v":705.8971200000001,"d":"705.90"},"一般性腐蚀","环氧富锌漆"]
["干熄焦","1#2#3#干熄炉至环境除尘管总至环境除尘站","作业高度约30m，作业环境存在煤气中毒、高空坠落、高温烫伤等危险源。","环境除尘管道",2420,120,{"v":911.856,"d":"911.86"},"高温+一般性腐蚀","有机硅耐高温漆200μm","高温管道（最高120°）"]
["干熄焦","副省煤器至干熄炉空废导层的废气导入管道(三座炉)","作业高度约24m，作业环境存在煤气中毒、高空坠落、高温烫伤等危险源。","废气导入管道",950,162,{"v":483.24600000000004,"d":"483.25"},"高温重度腐蚀","石墨烯改性钛基纳米重防腐涂料底漆BZ-7408","高温管道（最高180°）"]
["干熄焦","副省煤器至干熄炉装入装置层的预存室压力调节阀管道(三座炉)","作业高度约40m，作业环境存在煤气中毒、高空坠落、高温烫伤等危险源。","预存室压力调节阀管道",950,141,{"v":420.603,"d":"420.60"},"高温重度腐蚀","石墨烯改性钛基纳米重防腐涂料底漆BZ-7408","高温管道（最高180°）"]
["干熄焦","干熄炉6楼空气导入管道(三座炉)","作业高度约30m，作业环境存在煤气中毒、高空坠落、高温烫伤等危险源。","空气导入管道",1000,81.9,{"v":257.16600000000005,"d":"257.17"},"一般性腐蚀","环氧富锌漆"]
["干熄焦","干熄炉6层至干熄炉一楼尾焦管(三座炉)","作业高度约30m，作业环境存在煤气中毒、高空坠落、高温烫伤等危险源。","尾焦管",440,114,{"v":157.50240000000002,"d":"157.50"},"一般性腐蚀","环氧富锌漆"]
["干熄焦","循环风机入口管道7mx2根(三座炉)","作业高度约10m，作业环境存在煤气中毒、高空坠落、高温烫伤等危险源。","循环气体管道",2200,42,{"v":290.1360000000001,"d":"290.14"},"高温+一般性腐蚀","有机硅耐高温漆200μm","高温管道（最高200°）"]
["干熄焦","一次除尘下灰管5m、新增直排放灰管7.5m。(三座炉)","作业高度约6m，作业环境存在煤气中毒、高空坠落、高温烫伤等危险源。","排灰管道",250,37.5,{"v":29.4375,"d":"29.44"},"一般性腐蚀","环氧富锌漆"]
["干熄焦","1#2#3#干熄炉皮带通廊除尘管总管至环境除尘站","作业高度约20m，作业环境存在煤气中毒、高空坠落、高温烫伤等危险源。","排灰管道",800,110,{"v":276.32000000000005,"d":"276.32"},"高温+一般性腐蚀","有机硅耐高温漆200μm","高温管道（最高120°）"]
["干熄焦","皮带通廊除尘管至总管接入口(三座炉)","作业高度约20m，作业环境存在煤气中毒、高空坠落、高温烫伤等危险源。","排灰管道",800,66,{"v":165.79200000000003,"d":"165.79"},"一般性腐蚀","环氧富锌漆"]
["干熄焦","焦侧路管廊架至干熄炉3楼烘炉人孔煤气管道（三座干熄炉）","作业高度约16m，作业环境存在煤气中毒、高空坠落、高温烫伤等危险源。","煤气管道",273,174,{"v":149.15628,"d":"149.16"},"一般性腐蚀","环氧富锌漆"]
["干熄焦","转运站至环境除尘及焦炉除尘管","作业高度约16m，作业环境存在煤气中毒、高空坠落、高温烫伤等危险源。","排灰管道",720,122.5,{"v":276.94800000000004,"d":"276.95"},"一般性腐蚀","环氧富锌漆"]
["干熄焦","缓冲仓顶出口至筛焦除尘管","作业高度约16m，作业环境存在煤气中毒、高空坠落等危险源。","排灰管道",800,76.32,{"v":191.71584000000001,"d":"191.72"},"重度腐蚀","石墨烯改性钛基纳米重防腐涂料BZ-7405、BZ-7413"]
["干熄焦","筛焦楼除尘至筛焦除尘站（主体管）","作业高度约8.8m，作业环境存在煤气中毒、高空坠落等危险源。","排灰管道",1320,51.7,{"v":214.28616000000002,"d":"214.29"},"重度腐蚀","石墨烯改性钛基纳米重防腐涂料BZ-7405、BZ-7413"]
["干熄焦","筛焦楼除尘至筛焦除尘站（变径）","作业高度约16m，作业环境存在煤气中毒、高空坠落等危险源。","排灰管道",1120,14.42,{"v":50.712256000000004,"d":"50.71"},"重度腐蚀","石墨烯改性钛基纳米重防腐涂料BZ-7405、BZ-7413"]
["干熄焦","筛焦楼除尘至筛焦除尘站（变径）","作业高度约20m，作业环境存在煤气中毒、高空坠落、高温烫伤等危险源。","排灰管道",2020,20,{"v":126.85600000000001,"d":"126.86"},"重度腐蚀","石墨烯改性钛基纳米重防腐涂料BZ-7405、BZ-7413"]
["干熄焦","筛焦楼除尘至筛焦除尘站（变径）","作业高度约20m，作业环境存在煤气中毒、高空坠落、高温烫伤等危险源。","排灰管道",1620,14.86,{"v":75.589848,"d":"75.59"},"重度腐蚀","石墨烯改性钛基纳米重防腐涂料BZ-7405、BZ-7413"]
["干熄焦","缓冲仓底部1-8#仓除尘管","作业高度3m，作业环境存在粉尘、机械伤害等危险源","排灰管道",500,185.075,{"v":290.56775,"d":"290.57"},"一般性腐蚀","环氧富锌漆"]
["汇总",{"$nulls":5},{"v":1563.009104,"d":"1563.01㎡"},null,7]

{"sheet":"6.干熄焦-钢构","index":5,"n_rows":424,"n_cols":18,"rows_kept":424,"merged":[[148,0,148,8],[148,9,148,11],[148,13,148,14],[149,0,149,8],[149,9,149,11],[149,13,149,14]],"flags":["formulas_cached_only"]}
["2024年广西钢铁集团焦化厂除锈防腐检修工程——干熄焦钢构"]
["干熄焦防腐区域1","钢构展开面积计算（忽略截断面）     无翼板、腹板概念的钢材例如方钢，长边按腹板计，短边按翼板计。圆钢直径计入“F”列单元格。",{"$nulls":11},"平台防腐"]
["区域/部位","材料型号","规格","数量","单根长","腹板H","翼板B","翼板厚t2","腹板厚t1","面积：㎡","重合情况","手动计算","序号","单面","双面","备注","腐蚀程度","推荐采用防腐涂料"]
["8.606m","H/工字钢","HN600X200X11/17",2,11200,600,200,11,17,"",null,null,1,{"v":0,"d":"0.00"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["8.606m","[槽钢","[12.6（126*53*5.5）",17,2650,126,53,5.5,5.5,"",null,null,2,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["8.606m","H/工字钢","HN400X200X8/13",8,2650,400,200,8,13,"",null,null,3,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["8.606m","H/工字钢","HN300X150X6.5/9",2,2650,300,150,6.5,9,"",null,null,4,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["8.606m","2L型钢","2L100X100X6",10,3744.32904536981,0,100,6,0,"",null,null,5,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["8.606m","H/工字钢","BH700X400X16/30",2,10600,700,400,16,30,"",null,null,6,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["8.606m","H/工字钢","HM588X300X12/20",1,14800,588,300,12,20,"",null,null,7,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["8.606m","H/工字钢","HW200X200X8/12",2,10600,200,200,8,12,{"v":20.6912,"d":"20.69"},"翼板重合",null,8,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["16.234m","H/工字钢","HN500X200X10/16",1,58800,500,200,10,16,{"v":92.1984,"d":"92.20"},"翼板重合",null,9,{"v":259.324584,"d":"259.32"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["16.234m","H/工字钢","HN600X200X11/17",1,49000,600,200,11,17,{"v":86.534,"d":"86.53"},"翼板重合",null,10,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["16.234m","H/工字钢","HN400X200X8/13",1,33900,400,200,8,13,{"v":53.3586,"d":"53.36"},"无重合面",null,11,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["16.234m","H/工字钢","HN700X300X13/24",1,5500,700,300,13,24,{"v":12.386,"d":"12.39"},"翼板重合",null,12,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["16.234m","H/工字钢","BH900X300X16/28",1,22750,900,300,16,28,{"v":60.151,"d":"60.15"},"翼板重合",null,13,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["16.234m","H/工字钢","BH1100X400X16/36",1,17000,1100,400,16,36,{"v":56.576,"d":"56.58"},"翼板重合",null,14,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["16.234m","H/工字钢","HN350X175X7/11",1,34920,350,175,7,11,{"v":42.00876,"d":"42.01"},"翼板重合",null,15,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["16.234m","H/工字钢","HN294X200X8/12",1,6000,294,200,8,12,{"v":6.984,"d":"6.98"},"翼板重合",null,16,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["16.234m","H/工字钢","HN250X125X6/9",1,8650,250,125,6,9,{"v":7.41305,"d":"7.41"},"翼板重合",null,17,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["16.234m","H/工字钢","HN588X300X12/20",1,8740,588,300,12,20,{"v":17.79464,"d":"17.79"},"翼板重合",null,18,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["16.234m","H/工字钢","HN200X100X5.5/8",1,81720,200,100,5.5,8,{"v":55.89648,"d":"55.90"},"翼板重合",null,19,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["16.234m","[槽钢","[16b（160*63*6.5）",3,1200,160,63,6.5,6.5,{"v":1.7856,"d":"1.79"},"翼板重合",null,20,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["16.234m","[槽钢","[12.6（126*53*5.5）",1,46500,126,53,5.5,5.5,{"v":18.6,"d":"18.60"},"翼板重合",null,21,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["16.234m","[槽钢","[10（100*48*5.3）",1,103900,100,48,5.3,5.3,{"v":34.64026,"d":"34.64"},"翼板重合",null,22,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["16.234m","2L型钢","2L75X75X6/ V7,(-100)",1,18114,0,75,6,0,{"v":2.7171,"d":"2.72"},"无重合面",null,23,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["16.234m","2L型钢","2L75X75X6/ V7,(-120)",1,18114,0,75,6,0,{"v":2.7171,"d":"2.72"},"无重合面",null,24,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["16.234m","2L型钢","2L75X75X6/ V7,(-150)",1,14909,0,75,6,0,{"v":2.23635,"d":"2.24"},"无重合面",null,25,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["16.234m","2L型钢","2L75X75X6/ V7,(-180)",1,24063,0,75,6,0,{"v":3.60945,"d":"3.61"},"无重合面",null,26,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["20.184m","H/工字钢","HN500X200X10/16",1,77800,500,200,10,16,{"v":137.5504,"d":"137.55"},"无重合面",null,27,{"v":226.932659,"d":"226.93"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["20.184m","H/工字钢","HN600X200X11/17",1,19700,600,200,11,17,{"v":34.7902,"d":"34.79"},"翼板重合",null,28,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["20.184m","H/工字钢","HN700X300X13/24",1,34200,700,300,13,24,{"v":77.0184,"d":"77.02"},"翼板重合",null,29,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["20.184m","H/工字钢","HN400X200X8/13",1,51300,400,200,8,13,{"v":80.7462,"d":"80.75"},"无重合面",null,30,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["20.184m","H/工字钢","HN350X175X7/11",1,63977,350,175,7,11,{"v":76.964331,"d":"76.96"},"翼板重合",null,31,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["20.184m","H/工字钢","HN300X150X6.5/9",1,1200,300,150,6.5,9,{"v":1.2384,"d":"1.24"},"翼板重合",null,32,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["20.184m","H/工字钢","HN200X100X5.5/8",1,103610,200,100,5.5,8,{"v":70.86924,"d":"70.87"},"翼板重合",null,33,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["20.184m","[槽钢","[16b（160*63*6.5）",1,6000,160,63,6.5,6.5,{"v":2.976,"d":"2.98"},"翼板重合",null,34,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["20.184m","[槽钢","[12.6（126*53*5.5）",20,2000,126,53,5.5,5.5,{"v":16,"d":"16.00"},"翼板重合",null,35,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["20.184m","2L型钢","2L75X75X6/ V7,(-100)",1,34642,0,75,6,0,{"v":5.1963,"d":"5.20"},"无重合面",null,36,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["20.184m","2L型钢","2L75X75X6/ V7,(-150)",1,27950,0,75,6,0,{"v":4.1925,"d":"4.19"},"无重合面",null,37,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["20.184m","2L型钢","2L75X75X6/ V7,(-180)",1,17363,0,75,6,0,{"v":2.60445,"d":"2.60"},"无重合面",null,38,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["34.029m","H/工字钢","HN600X200X11/17",1,22360,600,200,11,17,{"v":39.48776,"d":"39.49"},"翼板重合",null,39,{"v":157.84777876,"d":"157.85"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["34.029m","H/工字钢","HN500X200X10/16",1,92960,500,200,10,16,{"v":164.35328,"d":"164.35"},"无重合面",null,40,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["34.029m","H/工字钢","HW200X200X8/12",1,5700,200,200,8,12,{"v":5.5632,"d":"5.56"},"翼板重合",null,41,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["34.029m","H/工字钢","HN400X200X8/13",4,12200,400,200,8,13,{"v":76.8112,"d":"76.81"},"无重合面",null,42,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["34.029m","H/工字钢","HN350X175X7/11",1,28700,350,175,7,11,{"v":39.5486,"d":"39.55"},"无重合面",null,43,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["34.029m","H/工字钢","HN300X150X6.5/9",1,24890,300,150,6.5,9,{"v":25.68648,"d":"25.69"},"翼板重合",null,44,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["34.029m","H/工字钢","HN200X100X5.5/8",1,48320,200,100,5.5,8,{"v":33.05088,"d":"33.05"},"翼板重合",null,45,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["34.029m","[槽钢","[16b（160*63*6.5）",1,38800,160,63,6.5,6.5,{"v":19.2448,"d":"19.24"},"翼板重合",null,46,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["34.029m","[槽钢","[12.6（126*53*5.5）",1,24000,126,53,5.5,5.5,{"v":10.872,"d":"10.87"},"无重合面",null,47,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["34.029m","2L型钢","2L100X100X6",1,41904,0,100,6,0,{"v":8.3808,"d":"8.38"},"无重合面",null,48,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["34.029m","2L型钢","2L75X75X6/ V7,(-150)",1,31614,0,75,6,0,{"v":2.37105,"d":"2.37"},"翼板重合",null,49,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["34.029m","2L型钢","2L75X75X6/ V7,(-180)",1,16595,0,75,6,0,{"v":1.244625,"d":"1.24"},"翼板重合",null,50,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","H/工字钢","BH1000X400X16/36",2,16000,1000,400,16,36,{"v":100.096,"d":"100.10"},"翼板重合",null,51,{"v":433.864941,"d":"433.86"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","H/工字钢","BH1400X450X20/45",2,17000,1400,450,20,45,138.04,"翼板重合",null,52,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","H/工字钢","HW200X200X8/12",1,20569,200,200,8,12,{"v":20.075344,"d":"20.08"},"翼板重合",null,53,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","H/工字钢","HW150X150X7/11",2,1300,150,150,7,11,{"v":1.8928,"d":"1.89"},"翼板重合",null,54,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","H/工字钢","HN700X300X13/24",1,38780,700,300,13,24,{"v":87.33256,"d":"87.33"},"翼板重合",null,55,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","H/工字钢","HM488X300X11/18",1,30400,488,300,11,18,{"v":55.936,"d":"55.94"},"翼板重合",null,56,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","H/工字钢","HM340X250X9/14",1,8000,340,250,9,14,{"v":11.216,"d":"11.22"},"翼板重合",null,57,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","H/工字钢","HM294X200X8/12",1,26950,294,200,8,12,{"v":31.3698,"d":"31.37"},"翼板重合",null,58,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","H/工字钢","HN600X200X11/17",1,52200,600,200,11,17,{"v":92.1852,"d":"92.19"},"翼板重合",null,59,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","H/工字钢","HN500X200X10/16",1,32600,500,200,10,16,{"v":57.6368,"d":"57.64"},"无重合面",null,60,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","H/工字钢","HN400X200X8/13",2,12200,400,200,8,13,{"v":38.4056,"d":"38.41"},"无重合面",null,61,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","H/工字钢","HN350X175X7/11",1,30000,350,175,7,11,36.09,"翼板重合",null,62,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","H/工字钢","HN300X150X6.5/9",1,24452,300,150,6.5,9,{"v":25.234464,"d":"25.23"},"翼板重合",null,63,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","H/工字钢","HN200X100X5.5/8",1,56300,200,100,5.5,8,{"v":38.5092,"d":"38.51"},"翼板重合",null,64,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","[槽钢","[16b（160*63*6.5）",1,3600,160,63,6.5,6.5,{"v":1.7856,"d":"1.79"},"翼板重合",null,65,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","[槽钢","[12.6（126*53*5.5）",1,206200,126,53,5.5,5.5,82.48,"翼板重合",null,66,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","2L型钢","2L75X75X6/ V7,(-100)",1,34128,0,75,6,0,{"v":5.1192,"d":"5.12"},"无重合面",null,67,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","2L型钢","2L75X75X6/ V7,(-150)",1,22126,0,75,6,0,{"v":3.3189,"d":"3.32"},"无重合面",null,68,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["40.389m","2L型钢","2L75X75X6/ V7,(-180)",1,23970,0,75,6,0,{"v":3.5955,"d":"3.60"},"无重合面",null,69,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["46.077m","H/工字钢","HW400X400X13/21",2,17000,400,400,13,21,{"v":80.172,"d":"80.17"},"无重合面",null,70,{"v":0,"d":"0.00"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["46.077m","H/工字钢","HW350X350X12/19",6,2250,350,350,12,19,{"v":27.837,"d":"27.84"},"无重合面",null,71,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["46.077m","H/工字钢","HN500X200X10/16",1,145000,500,200,10,16,256.36,"无重合面",null,72,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["46.077m","H/工字钢","HN350X175X7/11",1,11600,350,175,7,11,{"v":15.9848,"d":"15.98"},"无重合面",null,73,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["46.077m","2L型钢","2L75X75X6/ V7,(-150)",1,80434,0,75,6,0,{"v":12.0651,"d":"12.07"},"无重合面",null,74,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["46.077m","方（扁）钢","空号/V11,(-150)",1,42499,0,75,6,0,{"v":6.37485,"d":"6.37"},"无重合面",null,75,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["55.648m","H/工字钢","BH2500X500/350X20X40/25",2,20000,350,20,40,25,{"v":29.2,"d":"29.20"},"无重合面",null,76,{"v":0,"d":"0.00"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["55.648m","H/工字钢","BH2500X450/350X20X30/20",2,15200,350,20,40,25,{"v":22.192,"d":"22.19"},"无重合面",null,77,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["55.648m","H/工字钢","HW200X200X8/12",1,70400,200,200,8,12,{"v":82.7904,"d":"82.79"},"无重合面",null,78,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["55.648m","2L型钢","2L63X63X8",18,2250,0,63,8,0,{"v":5.103,"d":"5.10"},"无重合面",null,79,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["55.648m","2L型钢","L100X100X7",1,121612,0,100,7,0,{"v":24.3224,"d":"24.32"},"无重合面",null,80,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["57.898m","其他","BH2500X500/350X20X40/25",2,20000,2240,500,40,25,"需手动计算",null,{"v":205.2,"d":"205.20"},81,{"v":0,"d":"0.00"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["57.898m","其他","BH2500X450/350X20X30/20",2,15200,2240,450,40,25,"需手动计算",null,{"v":155.952,"d":"155.95"},82,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["57.898m","H/工字钢","HW200X200X8/12",1,77300,200,200,8,12,{"v":75.4448,"d":"75.44"},"翼板重合",null,83,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["57.898m","其他","用HN500X200X10X16切割蜂窝梁",2,16000,500,200,10,16,"需手动计算",null,{"v":41,"d":"41.00"},84,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["57.898m","H/工字钢","HN500X200X10/16",2,16000,500,200,10,16,{"v":50.176,"d":"50.18"},"翼板重合",null,85,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["57.898m","H/工字钢","HN200X100X5.5/8",8,2250,200,100,5.5,8,{"v":12.312,"d":"12.31"},"翼板重合",null,86,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["57.898m","其他","2[10",32,2250,100,48,5.3,5.3,"需手动计算","翼板重合",{"v":21.312,"d":"21.31"},87,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["57.898m","其他","2[20b",2,1250,200,73,7,7,"需手动计算","翼板重合",1.73,88,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["57.898m","[槽钢","[10（100*48*5.3）",11,1200,100,48,5.3,5.3,{"v":4.40088,"d":"4.40"},"翼板重合",null,89,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["57.898m","2L型钢","2L125X125X10",6,2250,0,125,10,0,{"v":1.6875,"d":"1.69"},"翼板重合",null,90,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["57.898m","2L型钢","2L100X100X8",42,2718,0,100,8,0,{"v":11.4156,"d":"11.42"},"翼板重合",null,91,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["57.898m","L型钢","L75X75X10",28,1645,0,75,10,0,{"v":3.4545,"d":"3.45"},"翼板重合",null,92,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["57.979m",null,"平面钢结构在57.898m图纸",{"$nulls":6},"",null,null,93,{"v":214.4,"d":"214.40"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["60.834m","H/工字钢","HN350X175X7/11",1,75810,350,175,7,11,{"v":91.19943,"d":"91.20"},"翼板重合",null,94,{"v":52.486,"d":"52.49"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["60.834m","H/工字钢","HW150X150X7/11",14,1630,150,150,7,11,{"v":16.61296,"d":"16.61"},"翼板重合",null,95,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["A/C/E线立面图","H/工字钢","HW350X350X12/19",2,12200,350,350,12,19,{"v":50.3128,"d":"50.31"},"无重合面",null,96,{"v":0,"d":"0.00"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["A/C/E线立面图","H/工字钢","HW300X300X10/15",2,17000,300,300,10,15,60.18,"无重合面",null,97,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["A/C/E线立面图","H/工字钢","HW200X200X8/12",1,12600,200,200,8,12,{"v":14.8176,"d":"14.82"},"无重合面",null,98,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["A/C/E线立面图","H/工字钢","HW400X400X13/21",2,14264,400,400,13,21,{"v":67.269024,"d":"67.27"},"无重合面",null,99,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["A/C/E线立面图","H/工字钢","HW300X300X10/15",1,115330,300,300,10,15,{"v":204.1341,"d":"204.13"},"无重合面",null,100,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["A/C/E线立面图","H/工字钢","HW250X250X9/14",1,38896,250,250,9,14,{"v":57.254912,"d":"57.25"},"无重合面",null,101,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["A/C/E线立面图","H/工字钢","HW200X200X8/12",1,104816,200,200,8,12,{"v":123.263616,"d":"123.26"},"无重合面",null,102,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["A/C/E线立面图","H/工字钢","HW300X300X10/15",1,36651,300,300,10,15,{"v":64.87227,"d":"64.87"},"无重合面",null,103,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["A/C/E线立面图","H/工字钢","HW350X350X12/19",1,13845,350,350,12,19,{"v":28.54839,"d":"28.55"},"无重合面",null,104,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["A/C/E线立面图","H/工字钢","BH600X600X20/40(Q345-B)",2,33710,600,600,20,40,{"v":237.3184,"d":"237.32"},"无重合面",null,105,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["A/C/E线立面图","H/工字钢","BH600X600X18/36(Q345-B)",1,42133,600,600,18,36,{"v":148.645224,"d":"148.65"},"无重合面",null,106,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["A/C/E线立面图","H/工字钢","BH600X600X18/32(Q345-B)",3,12356.3333333333,600,600,18,32,{"v":131.07598399999964,"d":"131.08"},"无重合面",null,107,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["A/C/E线立面图","H/工字钢","HW200X200X8/12",1,2100,200,200,8,12,{"v":2.4696,"d":"2.47"},"无重合面",null,108,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["B/D/F线立面图","H/工字钢","HW350X350X12/19",2,12200,350,350,12,19,{"v":50.3128,"d":"50.31"},"无重合面",null,109,{"v":0,"d":"0.00"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["B/D/F线立面图","H/工字钢","HW300X300X10/15",2,17000,300,300,10,15,60.18,"无重合面",null,110,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["B/D/F线立面图","H/工字钢","HW200X200X8/12",1,12600,200,200,8,12,{"v":14.8176,"d":"14.82"},"无重合面",null,111,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["B/D/F线立面图","H/工字钢","HW400X400X13/21",2,14264,400,400,13,21,{"v":67.269024,"d":"67.27"},"无重合面",null,112,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["B/D/F线立面图","H/工字钢","HW300X300X10/15",1,115330,300,300,10,15,{"v":204.1341,"d":"204.13"},"无重合面",null,113,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["B/D/F线立面图","H/工字钢","HW250X250X9/14",1,38896,250,250,9,14,{"v":57.254912,"d":"57.25"},"无重合面",null,114,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["B/D/F线立面图","H/工字钢","HW200X200X8/12",1,104816,200,200,8,12,{"v":123.263616,"d":"123.26"},"无重合面",null,115,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["B/D/F线立面图","H/工字钢","HW300X300X10/15",1,36651,300,300,10,15,{"v":64.87227,"d":"64.87"},"无重合面",null,116,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["B/D/F线立面图","H/工字钢","HW350X350X12/19",1,13845,350,350,12,19,{"v":28.54839,"d":"28.55"},"无重合面",null,117,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["B/D/F线立面图","H/工字钢","BH600X600X20/40(Q345-B)",2,33710,600,600,20,40,{"v":237.3184,"d":"237.32"},"无重合面",null,118,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["B/D/F线立面图","H/工字钢","BH600X600X18/36(Q345-B)",1,42133,600,600,18,36,{"v":148.645224,"d":"148.65"},"无重合面",null,119,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["B/D/F线立面图","H/工字钢","BH600X600X18/32(Q345-B)",3,12355,600,600,18,32,{"v":131.06184,"d":"131.06"},"无重合面",null,120,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["B/D/F线立面图","H/工字钢","HW200X200X8/12",1,2100,200,200,8,12,{"v":2.4696,"d":"2.47"},"无重合面",null,121,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["1线、2线立面图","H/工字钢","HW300X300X10/15",1,16000,300,300,10,15,28.32,"无重合面",null,122,{"v":0,"d":"0.00"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["1线、2线立面图","H/工字钢","HW400X400X13/21",1,101646,400,400,13,21,{"v":239.681268,"d":"239.68"},"无重合面",null,123,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["1线、2线立面图","H/工字钢","HW350X350X12/19",4,6122,350,350,12,19,{"v":50.494256,"d":"50.49"},"无重合面",null,124,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["1线、2线立面图","H/工字钢","HW300X300X10/15",1,91307,300,300,10,15,{"v":161.61339,"d":"161.61"},"无重合面",null,125,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["1线、2线立面图","H/工字钢","HW250X250X9/14",1,108550,250,250,9,14,{"v":159.7856,"d":"159.79"},"无重合面",null,126,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["1线、2线立面图","H/工字钢","HW200X200X8/12",1,22034,200,200,8,12,{"v":25.911984,"d":"25.91"},"无重合面",null,127,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["1线、2线立面图","H/工字钢","HW150X150X7/10",16,3175,150,150,7,10,{"v":44.704,"d":"44.70"},"无重合面",null,128,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["1线、2线立面图","H/工字钢","HW350X350X12/19",1,53144,350,350,12,19,{"v":109.582928,"d":"109.58"},"无重合面",null,129,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["3线立面图","H/工字钢","HW300X300X10/15",1,16000,300,300,10,15,28.32,"无重合面",null,130,{"v":0,"d":"0.00"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["3线立面图","H/工字钢","HW400X400X13/21",1,70097,400,400,13,21,{"v":165.288726,"d":"165.29"},"无重合面",null,131,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["3线立面图","H/工字钢","HW350X350X12/19",2,6122,350,350,12,19,{"v":25.247128,"d":"25.25"},"无重合面",null,132,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["3线立面图","H/工字钢","HW300X300X10/15",1,58316,300,300,10,15,{"v":103.21932,"d":"103.22"},"无重合面",null,133,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["3线立面图","H/工字钢","HW250X250X9/14",4,5621,250,250,9,14,{"v":33.096448,"d":"33.10"},"无重合面",null,134,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["3线立面图","H/工字钢","HW200X200X8/12",2,3638,200,200,8,12,{"v":8.556576,"d":"8.56"},"无重合面",null,135,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["3线立面图","H/工字钢","HW150X150X7/10",8,3174,150,150,7,10,{"v":22.34496,"d":"22.34"},"无重合面",null,136,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["3线立面图","H/工字钢","HW350X350X12/19",1,26572,350,350,12,19,{"v":54.791464,"d":"54.79"},"无重合面",null,137,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["机械室北外墙",{"$nulls":8},"",null,null,138,{"v":47.7,"d":"47.70"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["机械室南外墙",{"$nulls":8},"",null,null,139,{"v":47.7,"d":"47.70"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["机械室西外墙",{"$nulls":8},"",null,null,140,74.72,"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["机械室东外墙",{"$nulls":8},"",null,null,141,{"v":68,"d":"68.00"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["机械室顶面",{"$nulls":8},"",null,null,142,{"v":169,"d":"169.00"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["机械室地板背面",{"$nulls":8},"",null,null,143,{"v":169,"d":"169.00"},"/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["其他零散部位",{"$nulls":8},"",null,null,144,"/",121.2,null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["汇总",{"$nulls":8},{"v":6815.751018,"d":"6815.75"},null,{"v":425.194,"d":"425.19"},null,{"v":1920.97596276,"d":"1920.98"},{"v":121.2,"d":"121.20"}]
["单个干熄炉（提升井）工程量汇总",{"$nulls":8},{"v":7240.945018,"d":"钢结构： 7240.95㎡"},{"$nulls":3},{"v":2042.17596276,"d":"平台： 2042.18㎡"}]
["2个干熄炉（提升井）工程量汇总",{"$nulls":8},{"v":14481.890036,"d":"钢结构： 14481.89㎡"},{"$nulls":3},{"v":4084.35192552,"d":"平台： 4084.35㎡"}]
[]
["干熄焦防腐区域2","钢构展开面积计算（忽略截断面）     无翼板、腹板概念的钢材例如方钢，长边按腹板计，短边按翼板计。圆钢直径计入“F”列单元格。",{"$nulls":11},"平台防腐"]
["区域/部位","材料型号","规格","数量：根","单根长","腹板H","翼板B","翼板厚t2","腹板厚t1","面积：㎡","重合情况","手动计算","序号","单面","双面","备注","腐蚀程度","推荐采用防腐涂料"]
["环境除尘管支撑结构工字钢","H/工字钢","HW200X150X10X10",4,16000,200,150,10,10,62.72,"无重合面",null,1,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["环境除尘管支撑结构工字钢","[槽钢","HW400X200X10X10",2,16000,400,200,10,10,50.56,"无重合面",null,2,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["环境除尘管支撑结构工字钢","H/工字钢","HW200X200X10X10",4,20000,200,200,10,10,{"v":94.4,"d":"94.40"},"无重合面",null,3,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["环境除尘管支撑结构工字钢","H/工字钢","HW200X100X10X10",4,8000,200,100,10,10,24.96,"无重合面",null,4,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["环境除尘管支撑L型钢","L型钢","L70X70X6",1,34000,70,70,6,null,9.52,"无重合面",null,5,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["环境除尘管支撑L型钢","L型钢","L50X50X6",1,168000,70,50,6,null,40.32,"无重合面",null,6,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["皮带通廊小除尘管支架","H/工字钢","HW400X200X10X10",4,16000,400,200,10,10,101.12,"无重合面",null,6,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["皮带通廊小除尘管支架","L型钢","L60X60X6",62,850,60,60,6,null,{"v":12.648,"d":"12.65"},"无重合面",null,6,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["总灰仓6.6m","H/工字钢","HN450X300X11X18",6,7600,440,300,11,18,{"v":79.5264,"d":"79.53"},"翼板重合",null,6,"/",111.506,null,"一般性腐蚀","环氧富锌漆"]
["总灰仓6.6m","H/工字钢","HN400X200X8X13",2,7600,400,200,8,13,{"v":20.8848,"d":"20.88"},"翼板重合",null,6,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["总灰仓6.6m","H/工字钢","HW250X250X9X14",4,2500,250,250,9,14,12.22,"翼板重合",null,6,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["总灰仓6.6m","H/工字钢","HN250X125X7X11",2,2575,250,125,7,11,{"v":4.39295,"d":"4.39"},"翼板重合",null,6,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["总灰仓8.05m",null,"/","/","/","/","/","/","/","",null,null,6,"/",10.88,null,"一般性腐蚀","环氧富锌漆"]
["总灰仓14.0m","H/工字钢","HN700X300X13X24",1,45468,700,300,13,24,{"v":116.034336,"d":"116.03"},"无重合面",null,6,"/",36.36,null,"一般性腐蚀","环氧富锌漆"]
["总灰仓18.5m","H/工字钢","HN450X200X9X14",4,7600,450,200,9,14,{"v":44.7488,"d":"44.75"},"翼板重合",null,6,"/",36.36,null,"一般性腐蚀","环氧富锌漆"]
["总灰仓18.5m","H/工字钢","HN250X125X6X9",4,3767,250,125,6,9,{"v":12.913276,"d":"12.91"},"翼板重合",null,6,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["总灰仓23.0m","H/工字钢","HN450X200X9X14",1,45468,450,200,9,14,{"v":66.928896,"d":"66.93"},"翼板重合",null,6,"/",72.53,null,"一般性腐蚀","环氧富锌漆"]
["总灰仓HA/BA/H1/H2列框架","圆钢","φ273X8",1,229150,273,"/","/","/",{"v":196.431963,"d":"196.43"},"无重合面",null,6,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["总灰仓楼梯及平台",null,"/","/","/","/","/","/","/","",null,null,6,"/",77.78,null,"一般性腐蚀","环氧富锌漆"]
["排灰管","圆钢","φ250",1,8000,250,"/","/","/",6.28,"无重合面",null,6,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["总灰仓本体仓壁","其他","圆柱直径d：7.1m、高h：9m\n圆锥底直径7.1m、圆锥斜边L5.55m","/","/","/","/","/","/","需手动计算",null,{"v":262.51185000000004,"d":"262.51"},7,"/","/","圆锥体侧面积 = π * (底直径/2) * 斜边长","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["总灰仓二层西面小平台",null,"/","/","/","/","/","/","/","",null,null,7,"/",24.5,null,"一般性腐蚀","环氧富锌漆"]
["一次除尘风道外壳南北面共134.4㎡及南北两面楼梯（下部平台16.8㎡）及一次除尘(底部灰仓下部锥斗4.71㎡)、装入装置尾焦槽7.2㎡。",null,"平台、墙体、槽体面积","/","/","/","/","/","/","",null,null,7,489.33,"/","三座炉总量","一般性腐蚀","环氧富锌漆"]
["冷却塔南北两面楼梯及锅炉给水泵房南面楼梯钢构","[槽钢","槽钢：H160X60X5X5",1,76600,160,60,5,5,42.13,"无重合面",null,8,"/","/",null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["冷却塔南北两面楼梯及锅炉给水泵房南面楼梯踏板",null,"/","/","/","/","/","/","/","",null,null,9,null,94.576,null,"重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["1#、2#、3#锅炉西面管廊阀门平台",null,"/","/","/","/","/","/","/","",null,null,9,"/",61.44,null,"一般性腐蚀","环氧富锌漆"]
["1#/2#/3#干熄炉电梯挡雨棚（外侧）",null,"仅外侧","/","/","/","/","/","/","",null,null,9,{"v":73.6,"d":"73.60"},"/",null,"一般性腐蚀","环氧富锌漆"]
["干熄炉楼梯3.441-6.082m/11.227m-13.731m平面图",null,"/","/","/","/","/","/","/","",null,null,10,"/",41.64,"平台尺寸参考图纸，双面防腐，三座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯8.723m平面图",null,"/","/","/","/","/","/","/","",null,null,11,"/",69.87,"平台尺寸参考图纸，双面防腐，三座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯16.234m平面图",null,"/","/","/","/","/","/","/","",null,null,12,"/",67.17,"平台尺寸参考图纸，双面防腐，三座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯20.184m平面图",null,"/","/","/","/","/","/","/","",null,null,13,"/",67.17,"平台尺寸参考图纸，双面防腐，三座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯29.412m平面图",null,"/","/","/","/","/","/","/","",null,null,14,"/",54.57000000000001,"平台尺寸参考图纸，双面防腐，三座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯34.029m平面图",null,"/","/","/","/","/","/","/","",null,null,15,"/",76.17,"平台尺寸参考图纸，双面防腐，三座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯40.389m平面图",null,"/","/","/","/","/","/","/","",null,null,16,"/",67.17,"平台尺寸参考图纸，双面防腐，三座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯22.384-24.584m/42.489m-44.589m平面图",null,"/","/","/","/","/","/","/","",null,null,17,"/",41.64,"平台尺寸参考图纸，双面防腐，三座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯49.189m平面图",null,"/","/","/","/","/","/","/","",null,null,18,"/",54.57000000000001,"平台尺寸参考图纸，双面防腐，三座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯51.379m-53.569m平面图",null,"/","/","/","/","/","/","/","",null,null,19,"/",41.64,"平台尺寸参考图纸，双面防腐，三座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯57.979m平面图",null,"/","/","/","/","/","/","/","",null,null,20,"/",57.045,"平台尺寸参考图纸，双面防腐，三座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯3.435-6.076m钢梯平台结构布置图","H/工字钢","HN200X100X5.5X8",12,1300,200,100,5.5,8,{"v":10.6704,"d":"10.67"},"翼板重合",null,21,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯3.435-6.076m钢梯平台结构布置图","[槽钢","C10槽钢",3,8800,100,50,6,6,{"v":8.9232,"d":"8.92"},"翼板重合",null,22,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯3.435-6.076m钢梯平台结构布置图","[槽钢","C20A槽钢",6,1200,200,73,5,5,{"v":4.3848,"d":"4.38"},"翼板重合",null,23,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯3.435-6.076m钢梯平台结构布置图","[槽钢","C20A槽钢",6,4200,200,73,5,5,{"v":15.3468,"d":"15.35"},"翼板重合",null,24,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯3.435-6.076m钢梯平台结构布置图","[槽钢","C20A槽钢",6,5400,200,73,5,5,{"v":19.7316,"d":"19.73"},"翼板重合",null,25,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯8.717m钢梯平台结构布置图","H/工字钢","HM244X175X7X11",3,5000,244,175,7,11,{"v":14.865,"d":"14.87"},"翼板重合",null,26,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯8.717m钢梯平台结构布置图","H/工字钢","HM194X150X6X9",3,5000,194,150,6,9,{"v":12.3,"d":"12.30"},"翼板重合",null,27,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯8.717m钢梯平台结构布置图","H/工字钢","HN200X100X5.5X8",6,1300,200,100,5.5,8,{"v":5.3352,"d":"5.34"},"翼板重合",null,28,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯8.717m钢梯平台结构布置图","[槽钢","C10槽钢",12,1200,100,50,6,6,{"v":4.8672,"d":"4.87"},"翼板重合",null,29,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯8.717m钢梯平台结构布置图","[槽钢","C20A槽钢",6,1200,200,73,5,5,{"v":4.3848,"d":"4.38"},"翼板重合",null,30,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯8.717m钢梯平台结构布置图","[槽钢","C20A槽钢",6,3000,200,73,5,5,{"v":10.962,"d":"10.96"},"翼板重合",null,31,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯8.717m钢梯平台结构布置图","[槽钢","C20A槽钢",6,4200,200,73,5,5,{"v":15.3468,"d":"15.35"},"翼板重合",null,32,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯8.717m钢梯平台结构布置图","圆钢","φ140x7",3,3500,140,"/","/","/",{"v":4.6158,"d":"4.62"},"无重合面",null,33,null,null,"已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯16.228m钢梯平台结构布置图","H/工字钢","HM244X175X7X11",3,4700,244,175,7,11,{"v":13.9731,"d":"13.97"},"翼板重合",null,34,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯16.228m钢梯平台结构布置图","H/工字钢","HM194X150X6X9",3,4700,194,150,6,9,{"v":11.562,"d":"11.56"},"翼板重合",null,35,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯16.228m钢梯平台结构布置图","H/工字钢","HN200X100X5.5X8",3,3300,200,100,5.5,8,{"v":6.7716,"d":"6.77"},"翼板重合",null,36,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯16.228m钢梯平台结构布置图","[槽钢","C10槽钢",12,1200,100,50,6,6,{"v":4.8672,"d":"4.87"},"翼板重合",null,37,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯16.228m钢梯平台结构布置图","[槽钢","C20A槽钢",6,4200,200,73,5,5,{"v":15.3468,"d":"15.35"},"翼板重合",null,38,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯16.228m钢梯平台结构布置图","[槽钢","C20A槽钢",6,4200,200,73,5,5,{"v":15.3468,"d":"15.35"},"翼板重合",null,39,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯16.228m钢梯平台结构布置图","圆钢","φ140x7",3,3500,140,"/","/","/",{"v":4.6158,"d":"4.62"},"无重合面",null,40,null,null,"已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯20.178m钢梯平台结构布置图","H/工字钢","HM244X175X7X11",3,4700,244,175,7,11,{"v":13.9731,"d":"13.97"},"翼板重合",null,41,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯20.178m钢梯平台结构布置图","H/工字钢","HM194X150X6X9",3,8475,194,150,6,9,{"v":20.8485,"d":"20.85"},"翼板重合",null,42,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯20.178m钢梯平台结构布置图","H/工字钢","HN200X100X5.5X8",3,3300,200,100,5.5,8,{"v":6.7716,"d":"6.77"},"翼板重合",null,43,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯20.178m钢梯平台结构布置图","[槽钢","C10槽钢",12,1200,100,50,6,6,{"v":4.8672,"d":"4.87"},"翼板重合",null,44,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯20.178m钢梯平台结构布置图","[槽钢","C20A槽钢",6,4200,200,73,5,5,{"v":15.3468,"d":"15.35"},"翼板重合",null,45,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯20.178m钢梯平台结构布置图","[槽钢","C20A槽钢",6,4200,200,73,5,5,{"v":15.3468,"d":"15.35"},"翼板重合",null,46,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯20.178m钢梯平台结构布置图","圆钢","φ140x7",3,3500,140,"/","/","/",{"v":4.6158,"d":"4.62"},"无重合面",null,47,null,null,"已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯22.378-24.578m钢梯平台结构布置图","H/工字钢","HN200X100X5.5X8",12,1300,200,100,5.5,8,{"v":10.6704,"d":"10.67"},"翼板重合",null,48,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯22.378-24.578m钢梯平台结构布置图","[槽钢","C10槽钢",3,3600,100,50,6,6,{"v":3.6504,"d":"3.65"},"翼板重合",null,49,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯22.378-24.578m钢梯平台结构布置图","[槽钢","C20A槽钢",6,4200,200,73,5,5,{"v":15.3468,"d":"15.35"},"翼板重合",null,50,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯22.378-24.578m钢梯平台结构布置图","[槽钢","C20A槽钢",6,4200,200,73,5,5,{"v":15.3468,"d":"15.35"},"翼板重合",null,51,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯29.406m钢梯平台结构布置图","H/工字钢","HM194X150X6X9",6,1300,194,150,6,9,{"v":6.396,"d":"6.40"},"翼板重合",null,52,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯29.406m钢梯平台结构布置图","H/工字钢","HN200X100X5.5X8",6,1300,200,100,5.5,8,{"v":5.3352,"d":"5.34"},"翼板重合",null,53,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯29.406m钢梯平台结构布置图","[槽钢","C10槽钢",3,10600,100,50,6,6,{"v":10.7484,"d":"10.75"},"翼板重合",null,54,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯29.406m钢梯平台结构布置图","[槽钢","C20A槽钢",12,4200,200,73,5,5,{"v":30.6936,"d":"30.69"},"翼板重合",null,55,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯34.023m钢梯平台结构布置图","H/工字钢","HM244X175X7X11",3,4700,244,175,7,11,{"v":13.9731,"d":"13.97"},"翼板重合",null,56,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯34.023m钢梯平台结构布置图","H/工字钢","HM194X150X6X9",3,7700,194,150,6,9,{"v":18.942,"d":"18.94"},"翼板重合",null,57,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯34.023m钢梯平台结构布置图","H/工字钢","HN200X100X5.5X8",6,1300,200,100,5.5,8,{"v":5.3352,"d":"5.34"},"翼板重合",null,58,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯34.023m钢梯平台结构布置图","[槽钢","C10槽钢",3,3000,100,50,6,6,{"v":3.042,"d":"3.04"},"翼板重合",null,59,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯34.023m钢梯平台结构布置图","[槽钢","C20A槽钢",6,4200,200,73,5,5,{"v":15.3468,"d":"15.35"},"翼板重合",null,60,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯34.023m钢梯平台结构布置图","[槽钢","C20A槽钢",6,4200,200,73,5,5,{"v":15.3468,"d":"15.35"},"翼板重合",null,61,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯34.023m钢梯平台结构布置图","圆钢","φ140x7",3,3500,140,"/","/","/",{"v":4.6158,"d":"4.62"},"无重合面",null,62,null,null,"已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯40.383m钢梯平台结构布置图","H/工字钢","HM244X175X7X11",3,4700,244,175,7,11,{"v":13.9731,"d":"13.97"},"翼板重合",null,63,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯40.383m钢梯平台结构布置图","H/工字钢","HM194X150X6X9",3,4700,194,150,6,9,{"v":11.562,"d":"11.56"},"翼板重合",null,64,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯40.383m钢梯平台结构布置图","H/工字钢","HN200X100X5.5X8",6,1300,200,100,5.5,8,{"v":5.3352,"d":"5.34"},"翼板重合",null,65,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯40.383m钢梯平台结构布置图","[槽钢","C10槽钢",3,3000,100,50,6,6,{"v":3.042,"d":"3.04"},"翼板重合",null,66,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯40.383m钢梯平台结构布置图","[槽钢","C20A槽钢",6,4200,200,73,5,5,{"v":15.3468,"d":"15.35"},"翼板重合",null,67,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯40.383m钢梯平台结构布置图","[槽钢","C20A槽钢",6,4200,200,73,5,5,{"v":15.3468,"d":"15.35"},"翼板重合",null,68,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯40.383m钢梯平台结构布置图","圆钢","φ140x7",3,3500,140,"/","/","/",{"v":4.6158,"d":"4.62"},"无重合面",null,69,null,null,"已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯42.483-44.583m钢梯平台结构布置图","H/工字钢","HN200X100X5.5X8",12,1300,200,100,5.5,8,{"v":10.6704,"d":"10.67"},"翼板重合",null,70,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯42.483-44.583m钢梯平台结构布置图","[槽钢","C10槽钢",3,9600,100,50,6,6,{"v":9.7344,"d":"9.73"},"翼板重合",null,71,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯42.483-44.583m钢梯平台结构布置图","[槽钢","C20A槽钢",6,4200,200,73,5,5,{"v":15.3468,"d":"15.35"},"翼板重合",null,72,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯42.483-44.583m钢梯平台结构布置图","[槽钢","C20A槽钢",6,4200,200,73,5,5,{"v":15.3468,"d":"15.35"},"翼板重合",null,73,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯49.183m钢梯平台结构布置图","H/工字钢","HN200X100X5.5X8",9,1300,200,100,5.5,8,{"v":8.0028,"d":"8.00"},"翼板重合",null,74,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯49.183m钢梯平台结构布置图","H/工字钢","HM194X150X6X9",3,2000,194,150,6,9,4.92,"翼板重合",null,75,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯49.183m钢梯平台结构布置图","[槽钢","C10槽钢",3,9600,100,50,6,6,{"v":9.7344,"d":"9.73"},"翼板重合",null,76,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯49.183m钢梯平台结构布置图","[槽钢","C20A槽钢",9,5700,200,73,5,5,{"v":31.2417,"d":"31.24"},"翼板重合",null,77,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯49.183m钢梯平台结构布置图","圆钢","φ140x7",3,3500,140,"/","/","/",{"v":4.6158,"d":"4.62"},"无重合面",null,78,null,null,"已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯57.973m钢梯平台结构布置图","H/工字钢","HM244X175X7X11",3,3650,244,175,7,11,{"v":10.85145,"d":"10.85"},"翼板重合",null,79,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯57.973m钢梯平台结构布置图","H/工字钢","HM194X150X6X9",3,3300,194,150,6,9,{"v":8.118,"d":"8.12"},"翼板重合",null,80,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯57.973m钢梯平台结构布置图","H/工字钢","HN200X100X5.5X8",6,1300,200,100,5.5,8,{"v":5.3352,"d":"5.34"},"翼板重合",null,81,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯57.973m钢梯平台结构布置图","[槽钢","C10槽钢",3,4800,100,50,6,6,{"v":4.8672,"d":"4.87"},"翼板重合",null,82,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["干熄炉楼梯57.973m钢梯平台结构布置图","[槽钢","C20A槽钢",12,4200,200,73,5,5,{"v":30.6936,"d":"30.69"},"翼板重合",null,83,null,null,"扣除了重合面积，已算3座炉防腐量","重度腐蚀","石墨烯改性钛基纳米重防腐涂料"]
["楼梯框架钢柱构件C-C","H/工字钢","HM390X300X10X16",6,57973,390,300,10,16,{"v":677.588424,"d":"677.59"},"无重合面",null,83,null,null,"已算3座炉防腐量","一般性腐蚀","环氧富锌漆"]
["楼梯框架钢柱构件C-C","H/工字钢","HN200X100X7X10",72,3000,200,100,7,10,168.48,"无重合面",null,83,null,null,"已算3座炉防腐量","一般性腐蚀","环氧富锌漆"]
["楼梯框架钢柱构件C-C","2L型钢","2L75X6",144,3905,0,75,6,0,{"v":84.348,"d":"84.35"},"无重合面",null,83,null,null,"已算3座炉防腐量","一般性腐蚀","环氧富锌漆"]
["钢梯柱与平台拉结框架8.717m","H/工字钢","HM194X150X6X9",3,3000,194,150,6,9,8.73,"无重合面",null,83,null,null,"已算3座炉防腐量","一般性腐蚀","环氧富锌漆"]
["钢梯柱与平台拉结框架8.717m","H/工字钢","HN200X100X7X10",3,3000,200,100,7,10,7.02,"无重合面",null,83,null,null,"已算3座炉防腐量","一般性腐蚀","环氧富锌漆"]
["钢梯柱与平台拉结框架8.717m","2L型钢","2L90X8",6,4242,0,90,8,0,{"v":4.58136,"d":"4.58"},"无重合面",null,83,null,null,"已算3座炉防腐量","一般性腐蚀","环氧富锌漆"]
["钢梯柱与平台拉结框架16.228m/34.023m/40.383m","H/工字钢","HM194X150X6X9",9,2800,194,150,6,9,{"v":24.444,"d":"24.44"},"无重合面",null,83,null,null,"已算3座炉防腐量","一般性腐蚀","环氧富锌漆"]
["钢梯柱与平台拉结框架16.228m/34.023m/40.383m","H/工字钢","HN200X100X7X10",9,2800,200,100,7,10,{"v":19.656,"d":"19.66"},"无重合面",null,83,null,null,"已算3座炉防腐量","一般性腐蚀","环氧富锌漆"]
["钢梯柱与平台拉结框架16.228m/34.023m/40.383m","L型钢","2L90X8",18,4103,0,90,8,0,{"v":13.29372,"d":"13.29"},"无重合面",null,83,null,null,"已算3座炉防腐量","一般性腐蚀","环氧富锌漆"]
["钢梯柱与平台拉结框架20.178m","H/工字钢","HM194X150X6X9",3,2800,194,150,6,9,{"v":8.148,"d":"8.15"},"无重合面",null,83,null,null,"已算3座炉防腐量","一般性腐蚀","环氧富锌漆"]
["钢梯柱与平台拉结框架20.178m","H/工字钢","HN200X100X7X10",3,2800,200,100,7,10,{"v":6.552,"d":"6.55"},"无重合面",null,83,null,null,"已算3座炉防腐量","一般性腐蚀","环氧富锌漆"]
["钢梯柱与平台拉结框架20.178m","2L型钢","2L90X8",3,4103,0,70,8,0,{"v":1.72326,"d":"1.72"},"无重合面",null,83,null,null,"已算3座炉防腐量","一般性腐蚀","环氧富锌漆"]
["楼梯槽钢","[槽钢","C20A槽钢",30,3720,200,73,5,5,{"v":76.1112,"d":"76.11"},"无重合面",null,83,null,null,"已算3座炉防腐量","一般性腐蚀","环氧富锌漆"]
["楼梯槽钢","[槽钢","C20A槽钢",42,3905,200,73,5,5,{"v":111.85482,"d":"111.85"},"无重合面",null,83,null,null,"已算3座炉防腐量","一般性腐蚀","环氧富锌漆"]
["楼梯槽钢","[槽钢","C20A槽钢",36,3720,200,73,5,5,{"v":91.33344,"d":"91.33"},"无重合面",null,83,null,null,"已算3座炉防腐量","一般性腐蚀","环氧富锌漆"]
["楼梯槽钢","[槽钢","C20A槽钢",36,3720,200,73,5,5,{"v":91.33344,"d":"91.33"},"无重合面",null,83,null,null,"已算3座炉防腐量","一般性腐蚀","环氧富锌漆"]
["钢梯踏板",null,"/","/","/","/","/","/","/","",null,null,83,null,388.79999999999995,"踏板长0.9m，宽0.25m，共288级，参考JG01.07-08钢梁钢梯一览表，已算3座炉防腐量","一般性腐蚀","环氧富锌漆"]
["缓冲仓底北面除尘管平台及楼梯",null,"/","/","/","/","/","/","/","",null,null,83,null,34.766,"平台长11m，宽2.25m。楼梯踏板长0.8m，宽0.25m，共23级。楼梯斜支撑为厚板，长7m，宽0.2m，共2块。","一般性腐蚀","环氧富锌漆"]
["缓冲仓底北面除尘管平台支撑钢构","H/工字钢","HW400X200X10X10",1,26500,400,200,10,10,36.57,"翼板重合",null,83,null,null,"扣除了重合面积","一般性腐蚀","环氧富锌漆"]
["缓冲仓底北面除尘管平台支撑钢构","H/工字钢","HW200X200X10X7",1,11800,200,200,10,7,{"v":11.6348,"d":"11.63"},"翼板重合",null,83,null,null,"扣除了重合面积","一般性腐蚀","环氧富锌漆"]
["缓冲仓至筛焦除尘站除尘管平台及支架1","H/工字钢","HW300X200X10X10",1,43000,300,200,10,10,50.74,"翼板重合",null,83,null,24.4,"扣除2个平台支撑钢构贴合面,长3.6m，宽1m平台、长2m，宽1m平台。护笼及护栏估算3㎡","一般性腐蚀","环氧富锌漆"]
["缓冲仓至筛焦除尘站除尘管平台及支架1","H/工字钢","HW200X200X10X10",1,11500,200,200,10,10,13.57,"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["缓冲仓至筛焦除尘站除尘管平台及支架1","H/工字钢","L100X100X7",1,48000,0,100,7,0,{"v":19.2,"d":"19.20"},"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["缓冲仓至筛焦除尘站除尘管支架2","H/工字钢","HW250X170X10X10",2,7000,250,170,10,10,16.24,"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["缓冲仓至筛焦除尘站除尘管支架2","L型钢","L50X50X6",1,16400,0,50,6,0,1.64,"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["缓冲仓至筛焦除尘站除尘管支架3","H/工字钢","HW300X200X10X10",2,7800,300,200,10,10,{"v":21.528,"d":"21.53"},"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["缓冲仓至筛焦除尘站除尘管支架3","L型钢","L70X70X6",1,12800,0,70,6,0,{"v":1.792,"d":"1.79"},"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["缓冲仓至筛焦除尘站除尘管支架4","H/工字钢","HW250X170X10X10",2,7000,250,170,10,10,16.24,"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["缓冲仓至筛焦除尘站除尘管支架4","L型钢","L50X50X6",1,16400,0,50,6,0,1.64,"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["缓冲仓至筛焦除尘站除尘管支架5","H/工字钢","HW250X170X10X10",2,8000,250,170,10,10,18.56,"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["缓冲仓至筛焦除尘站除尘管支架5","L型钢","L50X50X6",1,25700,0,50,6,0,2.57,"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["筛焦除尘站楼梯","[槽钢","槽钢160X60X6X6",2,13000,160,60,6,6,{"v":14.248,"d":"14.25"},"无重合面",null,83,null,22.5,"楼梯踏板长1m，宽0.25m，共45级，双面防腐。","一般性腐蚀","环氧富锌漆"]
["筛焦除尘站西面冷却水管支架","H/工字钢","HW350X170X10X10",4,7600,350,170,10,10,{"v":41.344,"d":"41.34"},"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["筛焦除尘站西面冷却水管支架","其他","HW350X170X10X10切割蜂窝梁",2,13000,350,170,10,10,"需手动计算",null,33.68,83,null,null,"扣除正六边形镂空：边长100mm，共56个。","一般性腐蚀","环氧富锌漆"]
["环境总灰仓西面输灰管支架","H/工字钢","HW250X100X10X10",2,18000,250,100,10,10,31.68,"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["环境总灰仓西面输灰管支架","[槽钢","槽钢200X70X5X5",4,8000,200,70,5,5,21.44,"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["环境除尘站北面出口风道支架1","H/工字钢","HW300X150X10X10",2,14500,300,150,10,10,34.22,"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["环境除尘站北面出口风道支架1","L型钢","L50X50X6",1,45000,0,50,6,0,{"v":4.5,"d":"4.50"},"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["环境除尘站北面出口风道支架2","H/工字钢","HW200X150X10X10",1,9000,200,150,10,10,8.82,"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["环境除尘站北面出口风道支架3","H/工字钢","HW200X150X10X10",1,9000,200,150,10,10,8.82,"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["转运站南至环境除尘站南面支架1","H/工字钢","HW150X150X10X10",4,5000,150,150,10,10,{"v":17.6,"d":"17.60"},"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["转运站南至环境除尘站南面支架1","L型钢","L50X50X6",4,11000,0,50,6,0,{"v":4.4,"d":"4.40"},"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["转运站南至环境除尘站南面支架2","H/工字钢","HW150X150X10X10",4,5000,150,150,10,10,{"v":17.6,"d":"17.60"},"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["转运站南至环境除尘站南面支架2","L型钢","L50X50X6",4,11000,0,50,6,0,{"v":4.4,"d":"4.40"},"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["转运站南至环境除尘站南面支架3","H/工字钢","HW150X150X10X10",4,5000,150,150,10,10,{"v":17.6,"d":"17.60"},"无重合面",null,83,null,2.4,"包含长1.2m，宽1m平台，双面防腐","一般性腐蚀","环氧富锌漆"]
["转运站南至环境除尘站南面支架3","L型钢","L50X50X6",4,11000,0,50,6,0,{"v":4.4,"d":"4.40"},"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["三座炉副省煤器出口风道支架及平台","H/工字钢","HW400X200X10X10",2,14500,400,200,10,10,45.82,"无重合面",null,83,null,11.440000000000001,"钢构已算3座炉，平台长5.2m，宽1.1m仅3#炉有。","一般性腐蚀","环氧富锌漆"]
["三座炉副省煤器出口风道支架及平台","H/工字钢","HW200X200X10X10",1,5000,200,200,10,10,{"v":5.9,"d":"5.90"},"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["三座炉副省煤器出口风道支架及平台","[槽钢","槽钢140X60X6X6",4,7000,140,60,6,6,{"v":14.224,"d":"14.22"},"无重合面",null,83,null,null,"钢构已算3座炉","一般性腐蚀","环氧富锌漆"]
["三座炉副省煤器出口风道支架及平台","H/工字钢","HW150X100X10X10",2,1100,150,100,10,10,{"v":1.276,"d":"1.28"},"翼板重合",null,83,null,null,"已扣除与平台重合面","一般性腐蚀","环氧富锌漆"]
["1#炉一次除尘北面线缆架钢构","其他","HW400X200X10X10切割蜂窝梁",2,14000,400,200,10,10,"需手动计算",null,{"v":40.865,"d":"40.87"},83,null,null,"扣除正六边形镂空：边长150mm，共50个。","一般性腐蚀","环氧富锌漆"]
["三座炉与大间台西面楼梯平台","[槽钢","槽钢120X25X6X6",1,14000,120,25,6,6,{"v":4.592,"d":"4.59"},"无重合面",null,83,null,15.24,"楼梯踏板长0.9m，宽0.2m，共11级。平台宽1.1m*1m、2m*1m。已算三座炉楼梯平台面积","一般性腐蚀","环氧富锌漆"]
["干熄炉三楼周边风道通道平台",null,"/","/","/","/","/","/","/","",null,null,83,null,18,"平台长3m，宽1m，已算3座炉。","一般性腐蚀","环氧富锌漆"]
["缓冲仓东西两侧面四套楼梯平台及钢构架","[槽钢","槽钢160X60X6X6",4,38000,160,60,6,6,{"v":83.296,"d":"83.30"},"无重合面",null,83,null,279.8,"平台包含1m*2m共4个、1m*1m共2个。楼梯踏板长0.9m，宽0.25m，共111级。双面防腐，4套楼梯平台","一般性腐蚀","环氧富锌漆"]
["缓冲仓东西两侧面四套楼梯平台及钢构架","[槽钢","槽钢180X70X5X5",2,4500,180,70,5,5,5.67,"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["缓冲仓东西两侧面四套楼梯平台及钢构架","L型钢","L75X75X6",1,35500,0,75,6,0,{"v":5.325,"d":"5.33"},"无重合面",null,83,{"$nulls":3},"一般性腐蚀","环氧富锌漆"]
["汇总",{"$nulls":8},{"v":1024.08625,"d":"1024.09"},null,{"v":262.51185,"d":"262.51"},null,{"v":0,"d":"0.00"},{"v":733.231,"d":"733.23"}]
["防腐区域2防腐面积汇总",{"$nulls":8},{"v":1286.5981,"d":"钢结构： 1286.60㎡"},{"$nulls":3},{"v":733.231,"d":"平台733.23㎡"}]
[]
["干熄焦防腐区域3","钢构展开面积计算（忽略截断面）     无翼板、腹板概念的钢材例如方钢，长边按腹板计，短边按翼板计。圆钢直径计入“F”列单元格。",{"$nulls":11},"平台防腐"]
["区域/部位","材料型号","规格","数量：根","单根长","腹板H","翼板B","翼板厚t2","腹板厚t1","面积：㎡","重合情况","手动计算","序号","单面","双面","备注","腐蚀程度","推荐采用防腐涂料"]
["锅炉出口风道","H/工字钢","长4.8m/宽2.4m/高12m","/","/","/","/","/","/","",null,null,0,{"v":172.8,"d":"172.80"},"/","风道外壳：高12m、宽2.4m、长4.8m","一般性腐蚀","环氧富锌漆"]
["锅炉GRID-1立面布置图","方（扁）钢","方形钢400X400",1,71960,400,400,0,0,{"v":115.136,"d":"115.14"},"无重合面",null,0,{"v":0,"d":"0.00"},"/","包含4根12000mm，2根11980mm主梁方钢","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HW250X250X9X14",3,12000,250,250,9,14,{"v":52.992,"d":"52.99"},"无重合面",null,0,"/","/","包含3根12000mm","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN800X300X14X26",1,10196,800,300,14,26,{"v":28.018608,"d":"28.02"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HM488X300X11X18",1,10196,488,300,11,18,{"v":21.81944,"d":"21.82"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN700X300X13X24",1,10196,700,300,13,24,{"v":26.020192,"d":"26.02"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN300X150X6.5X9",1,10196,300,150,6.5,9,{"v":12.051672,"d":"12.05"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN400X200X8X13",1,10196,400,200,8,13,{"v":16.048504,"d":"16.05"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN600X200X10X17",1,10196,600,200,10,17,{"v":20.045336,"d":"20.05"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HW300X300X10X15",1,39020,300,300,10,15,{"v":69.0654,"d":"69.07"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HW200X200X8X12",1,35476,200,200,8,12,{"v":41.719776,"d":"41.72"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN300X150X6.5X9",1,2671,300,150,6.5,9,{"v":3.157122,"d":"3.16"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN250X125X6X9",1,21755,250,125,6,9,{"v":21.36341,"d":"21.36"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["锅炉GRID-2立面布置图","方（扁）钢","方形钢400X400",1,71960,400,400,0,0,{"v":115.136,"d":"115.14"},"无重合面",null,0,{"v":0,"d":"0.00"},"/",null,"一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HW300X300X10X15",1,40316,300,300,10,15,{"v":71.35932,"d":"71.36"},"无重合面",null,0,"/","/","LC-4:3781*2/LC-5:5807*4/LC-6:4763*2 同规格长度不一共8根","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HW250X250X9X14",1,24096,250,250,9,14,{"v":29.445312,"d":"29.45"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HW200X200X8X12",1,23684,200,200,8,12,{"v":23.115584,"d":"23.12"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN450X200X9X14",1,10196,450,200,9,14,{"v":15.008512,"d":"15.01"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HM488X300X11X18",1,10196,488,300,11,18,{"v":18.76064,"d":"18.76"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN400X200X8X13",6,10196,400,200,8,13,{"v":84.055824,"d":"84.06"},"翼板重合",null,0,"/","/","同规格，同长度共6根，扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN350X175X7X11",1,2198,350,175,7,11,{"v":2.644194,"d":"2.64"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN300X150X6.5X9",1,2671,300,150,6.5,9,{"v":2.756472,"d":"2.76"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN250X125X6X9",8,2671,250,125,6,9,{"v":18.312376,"d":"18.31"},"翼板重合",null,0,"/","/","ZL-77:2根，其他各1根，共8根，扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN200X100X5.5X8",1,2567,200,100,5.5,8,{"v":1.755828,"d":"1.76"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN200X100X8X12",1,21202,200,100,8,12,{"v":16.452752,"d":"16.45"},"无重合面",null,0,"/","/","LC-28两根，其他1根，各规格长度具体看图纸","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HW250X250X9X14",3,12000,250,250,9,14,{"v":52.992,"d":"52.99"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["锅炉GRID-3立面布置图","H/工字钢","HW250X250X9X14",1,69840,250,250,9,14,{"v":102.80448,"d":"102.80"},"无重合面",null,0,{"v":0,"d":"0.00"},"/",null,"一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN200X100X5.5X8",1,12930,200,100,5.5,8,{"v":8.84412,"d":"8.84"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN250X125X6X9",1,13730,250,125,6,9,{"v":11.76661,"d":"11.77"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN400X200X8X13",5,10346,400,200,8,13,{"v":71.07702,"d":"71.08"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HW175X175X7.5X11",1,58284,175,175,7.5,11,{"v":59.915952,"d":"59.92"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["/","L型钢","L100X7角钢",1,22845,0,100,7,0,{"v":4.569,"d":"4.57"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["锅炉GRID-A立面布置图","H/工字钢","Hi1000-16-36X300",1,9576,1000,300,16,36,{"v":27.080928,"d":"27.08"},"翼板重合",null,0,{"v":0,"d":"0.00"},"/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN500X200X10X16",2,9576,500,200,10,16,{"v":30.030336,"d":"30.03"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN350X175X7X11",1,71840,350,175,7,11,{"v":86.42352,"d":"86.42"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HW350X350X12X19",2,5033,350,350,12,19,{"v":20.756092,"d":"20.76"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HW175X175X7.5X11",2,5756,175,175,7.5,11,{"v":11.834336,"d":"11.83"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HW150X150X7X10",1,17878,150,150,7,11,{"v":15.696884,"d":"15.70"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HW250X250X9X14",1,51240,250,250,9,14,{"v":75.42528,"d":"75.43"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["锅炉GRID-B立面布置图","H/工字钢","Hi1000-16-36X300",1,9576,1000,300,16,36,{"v":27.080928,"d":"27.08"},"翼板重合",null,0,{"v":0,"d":"0.00"},"/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN500X200X10X16",2,9576,500,200,10,16,{"v":30.030336,"d":"30.03"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN350X175X7X11",1,71840,350,175,7,11,{"v":86.42352,"d":"86.42"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HW175X175X7.5X11",1,21578,175,175,7.5,11,{"v":22.182184,"d":"22.18"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HW150X150X7X10",1,17878,150,150,7,10,{"v":15.73264,"d":"15.73"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HW250X250X9X14",1,51240,250,250,9,14,{"v":75.42528,"d":"75.43"},"无重合面",null,0,"/","/",null,"一般性腐蚀","环氧富锌漆"]
["锅炉GRID-C立面布置图","H/工字钢","HN300X150X6.5X9",5,4987,300,150,6.5,9,{"v":25.73292,"d":"25.73"},"翼板重合",null,0,{"v":0,"d":"0.00"},"/","扣除支撑重合面,ZL-16:2根，其他1根","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN350X175X7X11",8,9967,350,175,7,11,{"v":95.922408,"d":"95.92"},"翼板重合",null,0,"/","/","扣除支撑重合面,ZL-78/81:2根，其他1根","一般性腐蚀","环氧富锌漆"]
["锅炉PLAN EL+4.6m布置图","H/工字钢","HN250X125X6X9",7,4992,250,125,6,9,{"v":29.947008,"d":"29.95"},"翼板重合",null,0,"/",106,"锅炉2楼西面大平台面积53㎡","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN200X100X5.5X8",1,40160,200,100,5.5,8,{"v":27.46944,"d":"27.47"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","L型钢","L75X6角钢",1,38557,75,75,6,0,{"v":8.675325,"d":"8.68"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","[槽钢","C16槽钢",4,1142,140,58,6,6,{"v":2.019056,"d":"2.02"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","[槽钢","C20A槽钢",1,1601,200,73,7,7,{"v":0.968605,"d":"0.97"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","L型钢","L90X10角钢",10,1101,90,90,10,0,{"v":2.9727,"d":"2.97"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["锅炉PLAN EL+9.3m布置图","H/工字钢","HN350X175X7X11",1,11817,350,175,7,11,{"v":14.215851,"d":"14.22"},"翼板重合",null,0,{"v":0,"d":"0.00"},"/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN400X200X8X13",1,10593,400,200,8,13,{"v":14.554782,"d":"14.55"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN300X150X6.5X9",2,9172,300,150,6.5,9,{"v":18.931008,"d":"18.93"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN200X100X5.5X8",1,34626,200,100,5.5,8,{"v":23.684184,"d":"23.68"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN250X125X6X9",1,40930,250,125,6,9,{"v":35.07701,"d":"35.08"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","[槽钢","C16槽钢",1,17940,140,58,6,6,{"v":7.92948,"d":"7.93"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","L型钢","L75X6角钢",1,34593,75,75,6,0,{"v":7.783425,"d":"7.78"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","L型钢","L90X10角钢",1,20050,90,90,10,0,{"v":5.4135,"d":"5.41"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["锅炉PLAN EL+13.7m布置图","H/工字钢","HN300X150X6.9X9",1,32023,300,150,6.9,9,{"v":33.047736,"d":"33.05"},"翼板重合",null,0,{"v":0,"d":"0.00"},"/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN200X100X5.5X8",1,2993,200,100,5.5,8,{"v":2.047212,"d":"2.05"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN250X125X6X9",7,2993,250,125,6,9,{"v":17.955007,"d":"17.96"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","L型钢","L75X6角钢",1,27886,75,75,6,0,{"v":6.27435,"d":"6.27"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["锅炉PLAN EL+18.1m布置图","H/工字钢","HN400X200X8X13",1,10592,400,200,8,13,{"v":14.553408,"d":"14.55"},"翼板重合",null,0,{"v":0,"d":"0.00"},"/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HI650-16-45X300",1,10590,650,300,16,45,{"v":22.3449,"d":"22.34"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN350X175X7X11",2,8241,350,175,7,11,{"v":19.827846,"d":"19.83"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN200X100X5.5X8",1,9963,200,100,5.5,8,{"v":6.814692,"d":"6.81"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN250X125X6X9",1,37937,250,125,6,9,{"v":32.512009,"d":"32.51"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","[槽钢","C16槽钢",1,14978,140,58,6,6,{"v":6.620276,"d":"6.62"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","L型钢","L75X6角钢",1,25402,75,75,6,0,{"v":5.71545,"d":"5.72"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["锅炉PLAN EL+23m布置图","H/工字钢","HN350X175X7X11",1,30914,350,175,7,11,{"v":37.189542,"d":"37.19"},"翼板重合",null,0,{"v":0,"d":"0.00"},"/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN400X200X8X13",1,11950,400,200,8,13,{"v":16.4193,"d":"16.42"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN200X100X5.5X8",1,21327,200,100,5.5,8,{"v":14.587668,"d":"14.59"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","[槽钢","C16槽钢",1,20156,140,58,6,6,{"v":8.908952,"d":"8.91"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","L型钢","L75X6角钢",1,37608,75,75,6,0,{"v":8.4618,"d":"8.46"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["锅炉PLAN EL+27.4m布置图","H/工字钢","HN250X125X6X9",1,20364,250,125,6,9,{"v":17.451948,"d":"17.45"},"翼板重合",null,0,{"v":0,"d":"0.00"},"/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN700X300X13X24",1,10593,700,300,13,24,{"v":23.855436,"d":"23.86"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","[槽钢","C16槽钢",1,24885,140,58,6,6,{"v":10.99917,"d":"11.00"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","[槽钢","C20A槽钢",1,4763,200,73,7,7,{"v":2.881615,"d":"2.88"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","[槽钢","C25B槽钢",8,1138,250,80,9,12,{"v":6.573088,"d":"6.57"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN350X175X7X11",1,10593,350,175,7,11,{"v":12.743379,"d":"12.74"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN200X100X5.5X8",1,5182,200,100,5.5,8,{"v":3.544488,"d":"3.54"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","L型钢","L75X6角钢",1,30755,75,75,6,0,{"v":6.919875,"d":"6.92"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["锅炉PLAN EL+21.4m布置图","[槽钢","C20槽钢",1,2993,200,75,7,7,{"v":1.828723,"d":"1.83"},"翼板重合",null,0,{"v":0,"d":"0.00"},"/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN250X125X6X9",2,10593,250,125,6,9,{"v":18.156402,"d":"18.16"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN200X100X5.5X8",15,1394,200,100,5.5,8,{"v":14.30244,"d":"14.30"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["锅炉PLAN EL+31.7m布置图","H/工字钢","HN350X175X7X11",1,21570,350,175,7,11,{"v":25.94871,"d":"25.95"},"翼板重合",null,0,{"v":0,"d":"0.00"},"/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN250X125X6X9",2,7891,250,125,6,9,{"v":13.525174,"d":"13.53"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN400X200X8X13",1,10593,400,200,8,13,{"v":14.554782,"d":"14.55"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","[槽钢","C20A槽钢",1,4763,200,73,7,7,{"v":2.881615,"d":"2.88"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","[槽钢","C16槽钢",1,22737,140,58,6,6,{"v":10.049754,"d":"10.05"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","L型钢","L75X6角钢",1,25896,75,75,6,0,{"v":5.8266,"d":"5.83"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["锅炉PLAN EL+36.3m布置图","H/工字钢","HN400X200X8X13",1,13794,400,200,8,13,{"v":18.952956,"d":"18.95"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","[槽钢","C16槽钢",1,4285,140,58,6,6,{"v":1.89397,"d":"1.89"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN250X125X6X9",1,20516,250,125,6,9,{"v":17.582212,"d":"17.58"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN200X100X5.5X8",1,9961,200,100,5.5,8,{"v":6.813324,"d":"6.81"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN350X175X7X11",1,12557,350,175,7,11,{"v":15.106071,"d":"15.11"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HW150X150X7X10",2,1710,150,150,7,10,{"v":2.4966,"d":"2.50"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","HN250X100X5.5X8",2,1727,250,100,5.5,8,{"v":2.707936,"d":"2.71"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","H/工字钢","TM122X175X7X11",1,18647,122,175,7,11,{"v":13.929309,"d":"13.93"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","L型钢","L75X6角钢",1,17116,75,75,6,0,{"v":3.8511,"d":"3.85"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","[槽钢","C20A槽钢",1,20095,200,73,7,7,{"v":12.157475,"d":"12.16"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["/","[槽钢","C28C槽钢",4,2737,280,86,11.5,12.5,{"v":8.70366,"d":"8.70"},"翼板重合",null,0,"/","/","扣除支撑重合面","一般性腐蚀","环氧富锌漆"]
["35.9m/23.995m/24.2m/28.6m/28.7m各小层合计估算",null,"/","/","/","/","/","/","/","",null,null,0,{"v":5,"d":"5.00"},10,"/","一般性腐蚀","环氧富锌漆"]
["汇总",{"$nulls":8},{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},null,{"v":0,"d":"0.00"},{"v":0,"d":"0.00"}]
["干熄焦防腐区域3（3座锅炉）工程量汇总",{"$nulls":8},{"v":0,"d":"钢结构： 0.00㎡"},{"$nulls":3},{"v":0,"d":"平台： 0.00㎡"}]
["干熄焦防腐区域1+2+3",{"v":15768.488136,"d":"钢结构： 15768.49㎡"},null,{"v":4817.58292552,"d":"平台： 4817.58㎡"}]

{"sheet":"7.工程预算表","index":6,"n_rows":22,"n_cols":13,"rows_kept":22,"merged":[[0,1,0,12],[1,0,1,12],[2,0,3,0],[2,1,3,1],[4,6,5,6],[4,12,5,12],[6,6,7,6],[6,12,7,12],[8,6,9,6],[8,12,9,12],[10,0,10,12],[11,0,12,0],[11,1,12,1],[13,6,14,6],[13,12,14,12],[20,11,20,12],[21,0,21,1],[21,2,21,4],[21,11,21,12],[22,11,22,12]],"flags":["formulas_cached_only"]}
[null,"广西钢铁焦化厂除锈防腐检修工程—工程量及预算总表"]
["一、非高温钢构部分"]
["车间","腐蚀程度","防腐工程量",{"$nulls":4},"综合单价",null,"总价",null,"总计"]
[null,null,"钢结构","平台","管道","汇总1","汇总2","材料费","施工费","材料费","施工费","分项","合计"]
["干熄焦","重度",{"v":15768.488136,"d":"15768.49㎡"},{"v":4817.58292552,"d":"4817.58㎡"},{"v":659.160104,"d":"659.16㎡"},{"v":21245.23116552,"d":"21245.23㎡"},{"v":36303.14124652,"d":"36303.14㎡"},null,null,{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"}]
["干熄焦","一般",{"v":10352.411031,"d":"10352.41㎡"},{"v":2673.032,"d":"2673.03㎡"},{"v":2032.46705,"d":"2032.47㎡"},{"v":15057.910080999998,"d":"15057.91㎡"},{"$nulls":3},{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"}]
["化产","重度",{"v":8458.56145955999,"d":"8458.56㎡"},{"v":3518.6104824,"d":"3518.61㎡"},{"v":12911.83609,"d":"12911.84㎡"},{"v":24889.00803195999,"d":"24889.01㎡"},{"v":111864.7938485425,"d":"111864.79㎡"},null,null,{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"}]
["化产","一般",{"v":63303.7531963425,"d":"63303.75㎡"},{"v":12794.51087424,"d":"12794.51㎡"},{"v":10877.521746,"d":"10877.52㎡"},{"v":86975.7858165825,"d":"86975.79㎡"},{"$nulls":3},{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"}]
["焦炉","重度",{"v":4411.52189376,"d":"4411.52㎡"},{"v":1289.946,"d":"1289.95㎡"},{"v":0,"d":"0.00㎡"},{"v":5701.46789376,"d":"5701.47㎡"},{"v":83168.77725376,"d":"83168.78㎡"},null,null,{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"}]
["焦炉","一般",{"v":57181.6452,"d":"57181.65㎡"},{"v":8892.9152,"d":"8892.92㎡"},{"v":11392.74896,"d":"11392.75㎡"},{"v":77467.30936,"d":"77467.31㎡"},{"$nulls":3},{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"}]
["二、 高温钢构部分"]
["车间","腐蚀程度","防腐工程量",{"$nulls":4},"综合单价",null,"总价",null,"总计"]
[null,null,"钢结构","平台","管道","汇总1","汇总2","材料费","施工费","材料费","施工费","分项","合计"]
["干熄焦","重度",{"v":0,"d":"0.00㎡"},{"v":0,"d":"0.00㎡"},{"v":903.849,"d":"903.85㎡"},{"v":903.849,"d":"903.85㎡"},{"v":2382.161,"d":"2382.16㎡"},null,null,{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"}]
["干熄焦","一般",{"v":0,"d":"0.00㎡"},{"v":0,"d":"0.00㎡"},{"v":1478.312,"d":"1478.31㎡"},{"v":1478.312,"d":"1478.31㎡"},{"$nulls":3},{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"}]
["备注：材料单价包含稀释剂的费用"]
["2024年计划实施的工程量及预算表",{"$nulls":9},"总费用",null,{"v":0,"d":"0.00万元"}]
["构件温度类别","材料费","施工费","重度防腐工程量","一般防腐工程量",{"$nulls":5},"一般性腐蚀",null,{"v":0,"d":"0.00万元"}]
["非高温构件",{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"},{"v":51835.707091239994,"d":"51835.71㎡"},{"v":0,"d":"0.00㎡"},{"$nulls":5},"重度腐蚀",null,{"v":0,"d":"0.00万元"}]
["高温构件",{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"},{"v":903.849,"d":"903.85㎡"},{"v":0,"d":"0.00㎡"},{"$nulls":5},"2024年度防腐资金限额:"]
["汇总",{"v":0,"d":"0.00万元"},{"v":0,"d":"0.00万元"},{"v":52739.556091239996,"d":"52739.56㎡"},{"v":0,"d":"0.00万元"}]
["总费用：材料费+施工费",null,{"v":0,"d":"0.00万元"}]

{"sheet":"数据源","index":7,"n_rows":9,"n_cols":4,"rows_kept":9,"hidden":true,"flags":["formulas_cached_only"]}
["材料型号","重合情况","防腐部位","腐蚀程度"]
["H/工字钢","无重合面","单面","重度腐蚀"]
["[槽钢","翼板重合","双面","一般性腐蚀"]
["L型钢","腹板重合",null,"高温重度腐蚀"]
["2L型钢",null,null,"高温+一般性腐蚀"]
["方（扁）钢"]
["圆钢"]
["其他"]
["2[槽钢"]

{"sheet":"Sheet10","index":8,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}